{"text_format":"1","workbook":"xlsx","n_sheets":31,"sheets":["README","Certification","Certification Table","LSE Showing","Resource Custom Profiles","Profile Optimization","Validation Overview","Check Capacity","Check Local","Check Flex","Check Contract Dates","Check Custom Profiles","Check Shown Hours","Check Storage Excess Capacity","Check Storage SOC","Check Grouped Resources","Check Hybrid Deliverability","Check MCC Bucket 4","LSE Showing Complete","Hourly Availability Chart","Hourly Availability","Local Availability Chart","Local Availability","Flex Availability Chart","Flex Availability","Requirements and Allocations","Resource Database","Resource NQC","Resource Default Profiles","Resource Profile Categories","Regions"],"not_rendered":{"charts":6,"images":0,"macros":1,"external_links":0,"defined_names":63,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Hourly Availability Chart","index":19,"reason":"not_a_worksheet"},{"sheet":"Local Availability Chart","index":21,"reason":"not_a_worksheet"},{"sheet":"Flex Availability Chart","index":23,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"README","index":0,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["This template ingests data into tables in tabbed worksheets and uses queries and connections to process and validate inputs. Validation test results are queries loaded into hidden worksheets and retrieved via standard Excel workbook functions in the \"Validation Overview\" worksheet with a golden tab. All queries can be accessed from the \"Data\" menu -> \"Queries & Connections\" -> \"Queries & Connections\".\n\nA valid monthly showing consists of general resource allocations specified in the table on the A1\"LSE Showing\" worksheet along with custom slice-of-day profiles for any resources for which the default profile is not desired, and a certification of showing with information about the load-serving entity submitting the showing. The \"LSEShowing\" query merges the general showing, custom profiles, and default profiles to build the complete showing data table. Only the three worksheets corresponding to these tables, denoted with blue tabs, should be altered when preparing a monthly showing: \"Certification\", \"LSE Showing\", and \"Resource Custom Profiles\". A fourth worksheet, denoted with a lighter blue tab and labelled \"Profile Optimization\", provides a tool for automatically allocating operating hours for resources shown using default profiles from the Resource Database.\n\nAll showing data for each resource, including custom and automatically optimized profiles along, is presented in the \"LSE Showing Complete\" worksheet. This sheet is for reference only and should not be edited. Hidden worksheets may be unhidden by right-clicking on any tab and selecting \"Unhide Sheets\"."]

{"sheet":"Certification","index":1,"n_rows":27,"n_cols":2,"rows_kept":27,"cut":false,"hidden":false,"merged":[[7,0,7,1],[9,0,9,1],[15,0,15,1],[21,0,21,1]]}
["Monthly Showing Certification Form"]
["Load Serving Entity:","LSE_1"]
["Showing Month:",45536]
["Date of Filing:",45457]
["Load Basis:"]
["Flex Category:"]
[]
["Consistent with Rules 1 and 2.4 of the CPUC's Rules of Practice and Procedure, this resource adequacy showing has been verified by an officer of the corporation, who shall expressly certify, under penalty of perjury, the following:\n1. I have responsibility for the activities reflected in this showing;\n2. I have reviewed, or have caused to be reviewed, this showing;\n3. Based on my knowledge, information, or belief, this filing does not contain any untrue statement of a material fact or omit to state a material fact necessary to make the statements made;\n4. Based on my knowledge, information, or belief, this filing contains all of the information required to be provided by CPUC orders, rules, and regulations."]
[]
["LSE Officer Information"]
["Title:","Manager"]
["Name:","Janet Doe"]
["Email:","jdoe@lse1.com"]
["Phone:","123-555-0000"]
[]
["Backup Contact Information"]
["Title:","Assistant to the Manager"]
["Name:","Jimothy Dee"]
["Email:","jdee@lse1.com"]
["Phone:","123-555-0001"]
[]
["Load Serving Entity Information"]
["LSE Address Line 1:","123 Fake Street"]
["LSE Address Line 2:"]
["LSE City:","Rancho Irreal"]
["LSE State:","CA"]
["LSE Zip:",97531]

{"sheet":"Certification Table","index":2,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["Key","Value"]
["Load Serving Entity",{"$f":"'Certification'!B2","v":"LSE_1"}]
["Showing Month",{"$f":"'Certification'!B3","v":"2024-09-01"}]
["Date of Filing",{"$f":"'Certification'!B4","v":"2024-06-14"}]
["Load Basis",{"$f":"'Certification'!B5","v":0}]
["Flex Category",{"$f":"'Certification'!B6","v":0}]
["Contact 1 Title",{"$f":"'Certification'!B11","v":"Manager"}]
["Contact 1 Name",{"$f":"'Certification'!B12","v":"Janet Doe"}]
["Contact 1 Email",{"$f":"'Certification'!B13","v":"jdoe@lse1.com"}]
["Contact 1 Phone",{"$f":"'Certification'!B14","v":"123-555-0000"}]
["Contact 2 Title",{"$f":"'Certification'!B17","v":"Assistant to the Manager"}]
["Contact 2 Name",{"$f":"'Certification'!B18","v":"Jimothy Dee"}]
["Contact 2 Email",{"$f":"'Certification'!B19","v":"jdee@lse1.com"}]
["Contact 2 Phone",{"$f":"'Certification'!B20","v":"123-555-0001"}]
["Address 1",{"$f":"'Certification'!B23","v":"123 Fake Street"}]
["Address 2",{"$f":"'Certification'!B24","v":0}]
["City",{"$f":"'Certification'!B25","v":"Rancho Irreal"}]
["State",{"$f":"'Certification'!B26","v":"CA"}]
["Zip",{"$f":"'Certification'!B27","v":97531}]

{"sheet":"LSE Showing","index":3,"n_rows":17,"n_cols":12,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Contract ID","Resource ID","Resource SubID","NQC or VER Under Contract (MW)","Local RA (MW)","Committed Flexible RA (MW)","Capacity Effective Start Date","Capacity Effective End Date","SCID or Counterparty if not available","MCC Bucket 4","Unspecified Import","Use Default Profile"]
["CAM Storage","CAM Storage 2",null,20,0,0,"2024-09-01","2024-09-30","TEST",false,false,false]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN",3,0,3,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR",5.25,0,5.25,"2024-09-01","2024-09-30","TEST",true,false,false]
["Contract 2","PWEST_1_UNIT",null,2.1,0,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 3","PRIMM_2_SOLAR1",null,10,0,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 4","TIGRCK_7_UNITS",null,5,0,5,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 5","ACACIA_6_SOLAR",null,20,2.2200000000000002,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 6","ALAMO_6_UNIT",null,9.5399999999999991,9.5399999999999991,9.5399999999999991,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 7","VOYAGR_2_VOYWD3",null,42.45,0,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 7","JOANEC_2_ST3BT3",null,20,0,40,"2024-09-01","2024-09-30","TEST",false,false,false]
["Contract 8","7STDRD_1_SOLAR1",null,20,0,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 9","ALTWD_2_COAWD1",null,5.67,5.67,0,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 10","ALAMIT_7_ES1",null,10,10,20,"2024-09-01","2024-09-30","TEST",true,false,false]
["Contract 11","SUTTER_2_CISO",null,25,null,25,"2024-09-01","2024-09-30","TEST",false,false,true]
["Contract 12","SCE1_MALIN500_I_F_121212",null,10,null,null,"2024-09-01","2024-09-30","TEST",false,true,false]
["Contract 13","SCE1_MALIN500_I_F_131313",null,10,null,null,"2024-09-01","2024-09-30","TEST",false,true,false]

{"sheet":"Resource Custom Profiles","index":4,"n_rows":3,"n_cols":26,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Resource ID","Resource SubID","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]
["SCE1_MALIN500_I_F_121212",null,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10]
["SCE1_MALIN500_I_F_131313",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,10,10,10,10,0,0,0]

{"sheet":"Profile Optimization","index":5,"n_rows":98,"n_cols":23,"rows_kept":98,"cut":false,"hidden":false,"merged":[[5,0,62,2]]}
[null,null,null,null,"Resource or Group Hourly Optimization",null,null,null,null,null,"Unshown Resource Adequacy",null,null,null,null,"Resource or Group Information"]
[null,null,null,null,"Optimization Group ID","Hour Ending","Show Hour","Shown MW","State-of-Charge",null,"Hour Ending","Remaining Required MW","Shown MW","Objective Function",null,"Optimization Group ID","Combined IDs","NQC or VER Under Contract (MW)","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","Difference Daily MWh"]
[null,null,null,null,"ALAMIT_7_ES1",1,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":2.2749999999999999E-2},null,1,-10.662000000000006,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":113.67824400000013},null,"ALAMIT_7_ES1","ALAMIT_7_ES1",10,2.86,0.91,400,1142,{"$f":"Export_ResourceGroupsForOptimization[[#This Row],[Storage Maximum Daily MWh]]-SUMIF(Table_LSEShowingProfilesForOptimization[Optimization Group ID],Export_ResourceGroupsForOptimization[[#This Row],[Optimization Group ID]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":1132.4394105223621}]
[null,null,null,null,"ALAMIT_7_ES1",2,1.4472359989002797E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.14472359989002798},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":2.2388191000274931E-2},null,2,-8.6576000000000022,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":1.3423983423007506},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":99.999966846017799},null,"CAM Storage 2","CAM Storage 2",20,2.79,0.87,80,1000,{"$f":"Export_ResourceGroupsForOptimization[[#This Row],[Storage Maximum Daily MWh]]-SUMIF(Table_LSEShowingProfilesForOptimization[Optimization Group ID],Export_ResourceGroupsForOptimization[[#This Row],[Optimization Group ID]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":961.75766128577584}]
[null,null,null,null,"ALAMIT_7_ES1",3,4.1448448905949939E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.41448448905949942},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":2.1351979777626182E-2},null,3,-6.1554000000000002,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":3.8445992831240519},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":99.999985662481535},null,"JOANEC_2_ST3BT3","JOANEC_2_ST3BT3",20,1,0.8,160,160,{"$f":"Export_ResourceGroupsForOptimization[[#This Row],[Storage Maximum Daily MWh]]-SUMIF(Table_LSEShowingProfilesForOptimization[Optimization Group ID],Export_ResourceGroupsForOptimization[[#This Row],[Optimization Group ID]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":121.7576612857759}]
["How to Optimize Storage Resources:\n1. Add one or more storage resources to the LSE Showing worksheet and set \"Default Profile\" to \"FALSE\".\n2. Do not create an entry in the Resource Custom Profiles worksheet for these resources.\n3. Click the \"Refresh Tables\" button and wait for the three tables to finish updating (refresh status appears at the bottom of the Excel window).\n4. Click the \"Reset Shown Hours\" button to set all values in the Show Hour column to zero.\n5. Click the \"Optimize Shown Hours\" button and wait for Solver to finish setting new values in the Show Hour column.\n6. Check that values in the \"Shown MW\" column equal all positive values in the Required Remaining MW column. If not, additional resources may need to be shown in the LSE Showing worksheet.\n\nThis sheet uses Excel's Solver tool to minimize the objective cell at the bottom of the Objective Function column. Solver sets usage in the Show Hour column of the Resources or Groups Hourly Optimization table as a fraction of each resource's or group's  NQC or VER capacity under contract indicated on the LSE Showing.\n\nThe objective cell calculates the sum of the squared differences between  Remaining Required MW and Shown MW. This function provides a smooth surface for the solver to descend to a minimum, bounded by the constraints, and prioritizes showing capacities during the hours with greater deficits if there is not sufficient storage capacity to fulfil.\n\nThe Capacity Persistence column calculates the cumulative shown capacity with a falloff based on contracted capacity and storage efficiency when 0 capacity is shown. The solver uses this column to ensure that multi-cycle storage has sufficient time to charge between discharging hours. Both single- and multi-cycle storage are additionally  constrained by total daily MWh.\n\nNote: Excel's Solver Add-In is limited to 200 variables, which means only 8 resources can be optimized. Queries will group resources in order to constrain the number of decision variables passed to Solver. The GRG Nonlinear method is used to accomodate multicycle storage, thus solutions are not guaranteed to be the absolute optimum.",null,null,null,"ALAMIT_7_ES1",4,7.3838743830876116E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.73838743830876119},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1.9506011181854278E-2},null,4,-3.1510000000000105,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":6.8490029114365276},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":100.00005822873925},null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR","LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",5.25,1,0.8,21,21,{"$f":"Export_ResourceGroupsForOptimization[[#This Row],[Storage Maximum Daily MWh]]-SUMIF(Table_LSEShowingProfilesForOptimization[Optimization Group ID],Export_ResourceGroupsForOptimization[[#This Row],[Optimization Group ID]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":18.364860860265974}]
[null,null,null,null,"ALAMIT_7_ES1",5,9.5400638060325935E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.95400638060325937},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1.7120995230346131E-2},null,5,-1.1510000000000105,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":8.8490032239832264},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":100.00006447967513}]
[null,null,null,null,"ALAMIT_7_ES1",6,3.7862945362659968E-3,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.7862945362659967E-2},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1.7026337866939481E-2},null,6,0.35120000000000573,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0.35119972862737864},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":7.3643102734803599E-14}]
[null,null,null,null,"ALAMIT_7_ES1",7,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":3.977633786693948E-2},null,7,-3.8765999999999963,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":15.028027559999972}]
[null,null,null,null,"ALAMIT_7_ES1",8,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":6.252633786693948E-2},null,8,-9.4444000000000017,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":89.196691360000031}]
[null,null,null,null,"ALAMIT_7_ES1",9,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":8.5276337866939472E-2},null,9,-25.604399999999998,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":655.58529935999991}]
[null,null,null,null,"ALAMIT_7_ES1",10,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.10802633786693946},null,10,-33.944400000000002,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":1152.2222913600001}]
[null,null,null,null,"ALAMIT_7_ES1",11,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.13077633786693946},null,11,-26.044399999999996,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":678.31077135999976}]
[null,null,null,null,"ALAMIT_7_ES1",12,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.15352633786693945},null,12,-17.066599999999994,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":291.26883555999979}]
[null,null,null,null,"ALAMIT_7_ES1",13,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.17627633786693944},null,13,-5.526600000000002,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":30.54330756000002}]
[null,null,null,null,"ALAMIT_7_ES1",14,1.9394934376640992E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.19394934376640993},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.17579146450752342},null,14,1.7990000000000066,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":1.7989973604628635},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":6.96715632969228E-12}]
[null,null,null,null,"ALAMIT_7_ES1",15,0.14684945221426898,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":1.4684945221426897},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.17212022820216669},null,15,13.621199999999988,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":13.62120030650591},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":9.3945880751098831E-14}]
[null,null,null,null,"ALAMIT_7_ES1",16,0.19827458430098202,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":1.9827458430098202},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.16716336359464212},null,16,18.391199999999998,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":18.391203647347247},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":1.3303141955618469E-11}]
[null,null,null,null,"ALAMIT_7_ES1",17,0.2109723797262387,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":2.109723797262387},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.16188905410148616},null,17,19.569000000000017,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":19.569003352070862},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":1.1236378949212012E-11}]
[null,null,null,null,"ALAMIT_7_ES1",18,8.0775183793507663E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.80775183793507666},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.15986967450664846},null,18,7.4924000000000035,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":7.4923993496463437},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":4.2295988283422397E-13}]
[null,null,null,null,"ALAMIT_7_ES1",19,7.0845928029740032E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.70845928029740035},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.15809852630590496},null,19,6.571399999999997,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":6.5713985403150623},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":2.1306801085945209E-12}]
[null,null,null,null,"ALAMIT_7_ES1",20,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.18084852630590495},null,20,-5.0708000000000055,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":25.713012640000056}]
[null,null,null,null,"ALAMIT_7_ES1",21,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.20359852630590494},null,21,-17.070800000000006,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":291.41221264000018}]
[null,null,null,null,"ALAMIT_7_ES1",22,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.22634852630590493},null,22,-6.5641999999999996,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":43.088721639999996}]
[null,null,null,null,"ALAMIT_7_ES1",23,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.24909852630590493},null,23,-12.5642,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":157.85912163999998}]
[null,null,null,null,"ALAMIT_7_ES1",24,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.27184852630590495},null,24,-14.061999999999998,{"$f":"SUMIF(Table_LSEShowingProfilesForOptimization[Hour Ending],Export_LSEShowingUnshownRequirement[[#This Row],[Hour Ending]],Table_LSEShowingProfilesForOptimization[Shown MW])","v":0},{"$f":"(Export_LSEShowingUnshownRequirement[[#This Row],[Remaining Required MW]]-Export_LSEShowingUnshownRequirement[[#This Row],[Shown MW]])^2","v":197.73984399999992}]
[null,null,null,null,"CAM Storage 2",1,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.21749999999999997},null,null,null,null,{"$f":"SUBTOTAL(109,Export_LSEShowingUnshownRequirement[Objective Function])","v":4141.6464558969483}]
[null,null,null,null,"CAM Storage 2",2,2.8944629088115847E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.57889258176231695},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.210263842727971}]
[null,null,null,null,"CAM Storage 2",3,8.2896809228238597E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":1.657936184564772},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.18953964042091134}]
[null,null,null,null,"CAM Storage 2",4,0.14767742899498726,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":2.9535485798997452},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.15262028317216453}]
[null,null,null,null,"CAM Storage 2",5,0.1908012145366689,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.8160242907333779},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.10491997953799731}]
[null,null,null,null,"CAM Storage 2",6,7.5725151049457519E-3,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.15145030209891502},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.10302685076176087}]
[null,null,null,null,"CAM Storage 2",7,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.32052685076176085}]
[null,null,null,null,"CAM Storage 2",8,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.53802685076176082}]
[null,null,null,null,"CAM Storage 2",9,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.75552685076176074}]
[null,null,null,null,"CAM Storage 2",10,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.97302685076176076}]
[null,null,null,null,"CAM Storage 2",11,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",12,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",13,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",14,3.8789766069147351E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.77579532138294705},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.9903025584827132}]
[null,null,null,null,"CAM Storage 2",15,0.29369879804741145,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":5.8739759609482292},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.91687785897086038}]
[null,null,null,null,"CAM Storage 2",16,0.39654908332096461,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":7.9309816664192923},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.81774058814061923}]
[null,null,null,null,"CAM Storage 2",17,0.42194466928099156,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":8.4388933856198314},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.71225442082037138}]
[null,null,null,null,"CAM Storage 2",18,0.16155026985003107,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.2310053970006214},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.67186685335786356}]
[null,null,null,null,"CAM Storage 2",19,0.14169175218970287,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":2.8338350437940574},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.63644391531043787}]
[null,null,null,null,"CAM Storage 2",20,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.85394391531043778}]
[null,null,null,null,"CAM Storage 2",21,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",22,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",23,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"CAM Storage 2",24,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"JOANEC_2_ST3BT3",1,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.1}]
[null,null,null,null,"JOANEC_2_ST3BT3",2,2.8944629088115847E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.57889258176231695},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":9.6381921363985518E-2}]
[null,null,null,null,"JOANEC_2_ST3BT3",3,8.2896809228238597E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":1.657936184564772},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":8.6019820210455691E-2}]
[null,null,null,null,"JOANEC_2_ST3BT3",4,0.14767742899498726,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":2.9535485798997452},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":6.7560141586082284E-2}]
[null,null,null,null,"JOANEC_2_ST3BT3",5,0.1908012145366689,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.8160242907333779},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":4.3709989768998675E-2}]
[null,null,null,null,"JOANEC_2_ST3BT3",6,7.5725151049457519E-3,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.15145030209891502},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":4.2763425380880453E-2}]
[null,null,null,null,"JOANEC_2_ST3BT3",7,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.14276342538088047}]
[null,null,null,null,"JOANEC_2_ST3BT3",8,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.24276342538088047}]
[null,null,null,null,"JOANEC_2_ST3BT3",9,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.34276342538088045}]
[null,null,null,null,"JOANEC_2_ST3BT3",10,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.44276342538088043}]
[null,null,null,null,"JOANEC_2_ST3BT3",11,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.5427634253808804}]
[null,null,null,null,"JOANEC_2_ST3BT3",12,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.64276342538088038}]
[null,null,null,null,"JOANEC_2_ST3BT3",13,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.74276342538088036}]
[null,null,null,null,"JOANEC_2_ST3BT3",14,3.8789766069147351E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.77579532138294705},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.73791470462223696}]
[null,null,null,null,"JOANEC_2_ST3BT3",15,0.29369879804741145,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":5.8739759609482292},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.70120235486631055}]
[null,null,null,null,"JOANEC_2_ST3BT3",16,0.39654908332096461,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":7.9309816664192923},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.65163371945118997}]
[null,null,null,null,"JOANEC_2_ST3BT3",17,0.42194466928099156,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":8.4388933856198314},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.59889063579106605}]
[null,null,null,null,"JOANEC_2_ST3BT3",18,0.16155026985003107,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.2310053970006214},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.57869685205981214}]
[null,null,null,null,"JOANEC_2_ST3BT3",19,0.14169175218970287,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":2.8338350437940574},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.56098538303609924}]
[null,null,null,null,"JOANEC_2_ST3BT3",20,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.66098538303609922}]
[null,null,null,null,"JOANEC_2_ST3BT3",21,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.76098538303609919}]
[null,null,null,null,"JOANEC_2_ST3BT3",22,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.86098538303609917}]
[null,null,null,null,"JOANEC_2_ST3BT3",23,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.96098538303609915}]
[null,null,null,null,"JOANEC_2_ST3BT3",24,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",1,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.2}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",2,7.5980150259216664E-3,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":3.9889578886088746E-2},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.19810049624351961}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",3,2.1760461892382624E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.11424242493500877},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.19266038077042394}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",4,3.8765393014909763E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.20351831332827625},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.18296903251669649}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",5,5.0085383221564091E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.26294826191321147},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.17044768671130547}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",6,1.9878436317883018E-3,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":1.0436179066888585E-2},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.1699507258033584}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",7,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.36995072580335842}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",8,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.56995072580335848}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",9,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.76995072580335844}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",10,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.96995072580335839}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",11,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",12,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",13,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",14,1.0182356939154202E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":5.3457373930559562E-2},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.99745441076521146}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",15,7.7095973803192719E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.40475386246676176},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.9781804173144133}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",16,0.10409418504739885,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.546494471498844},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.95215687105256364}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",17,0.1107605302035834,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.58149278356881284},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.92446673850166783}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",18,4.2406993849528431E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.22263671771002427},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.91386499003928567}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",19,3.7194128081818649E-2,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0.19526917242954792},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":0.90456645801883107}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",20,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",21,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",22,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",23,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]
[null,null,null,null,"LNCSTR_6_SOLAR2/LNCSTR_6_SOLAR2_LESR",24,0,{"$f":"Table_LSEShowingProfilesForOptimization[[#This Row],[Show Hour]]*SUMIF(Export_ResourceGroupsForOptimization[Optimization Group ID],Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[NQC or VER Under Contract (MW)])","v":0},{"$f":"IF(\n    Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]]<=OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[Hour Ending]],-1,0),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        -Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]],\n        MIN(\n            100%,\n            VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6)\n        )\n    ),\n    IF(\n        Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]>0,\n        OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)-Table_LSEShowingProfilesForOptimization[[#This Row],[Shown MW]]/VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n        MIN(\n            OFFSET(Table_LSEShowingProfilesForOptimization[[#This Row],[State-of-Charge]],-1,0)\n                +VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],3)\n                *VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],5)\n                /VLOOKUP(Table_LSEShowingProfilesForOptimization[[#This Row],[Optimization Group ID]],Export_ResourceGroupsForOptimization[],6),\n            100%\n        )\n    )\n)","v":1}]

{"sheet":"Validation Overview","index":6,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[9,3,10,3],[9,5,10,5],[9,4,10,4]]}
["Test","Result","Description","Worksheet","Review","Refresh"]
["Hourly System Capacity",{"$f":"IF(AND(Export_CheckCapacity[Hour Ending]>=0),\"Pass\",\"Fail\")","v":"Pass"},"Checks whether the total MWh shown available across all 24 hours meet the hourly requirements.","Check Capacity"]
["Local Capacity",{"$f":"IF(AND(SUM(Export_CheckLocal[LA Basin])>=0,SUM(Export_CheckLocal[Big Creek-Ventura])>=0,SUM(Export_CheckLocal[San Diego-IV])>=0,SUM(Export_CheckLocal[Bay Area])>=0,SUM(Export_CheckLocal[Fresno])>=0,SUM(Export_CheckLocal[Sierra])>=0,SUM(Export_CheckLocal[Stockton])>=0,SUM(Export_CheckLocal[Kern])>=0,SUM(Export_CheckLocal[Humboldt])>=0,SUM(Export_CheckLocal[NBNC])>=0),\"Pass\",\"Fail\")","v":"Pass"},"Checks whether shown local capacity meets local requirements.","Check Local"]
["Flexible Capacity",{"$f":"IF(AND(SUM(Export_CheckFlex[Category 1])>=0,SUM(Export_CheckFlex[Category 2])>=0,SUM(Export_CheckFlex[Category 3])>=0),\"Pass\",\"Fail\")","v":"Pass"},"Checks whether shown local capacity meets flex requirements.","Check Flex"]
["Contract Date",{"$f":"IFERROR(IF(AND(Export_CheckContractDates[Check Dates]),\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Checks that each shown resource is available for the current showing month according to the contract period.","Check Contract Dates"]
["Custom Profile",{"$f":"IFERROR(IF(MIN(Export_CheckCustomProfiles[[Delta MW HE 1]:[Delta MW HE 24]])>=0,\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Checks whether any custom resource profiles exceed the current monthly NQC or contracted NQC or VER.","Check Custom Profiles"]
["Shown Hours",{"$f":"IF(IFERROR(AND(Export_CheckShownHours[Valid Hours]),FALSE),\"Pass\",\"Fail\")","v":"Pass"},"Passes if the shown hours of usage for each resource are below the maximum allowed in the resource database.","Check Shown Hours"]
["Storage Excess Capacity",{"$f":"IF(Export_CheckStorageExcessCapacity[CheckStorageExcessCapacity]>=0,\"Pass\",\"Fail\")","v":"Pass"},"Checks that sufficient excess capacity above system requirements across all hours are shown to supply the total storage charging needs, accounting for efficiency losses.","Check Storage Excess Capacity"]
["MCC Bucket 4 Storage Excess Capacity",{"$f":"IF(Export_CheckMCCBucket4StorageExcessCapacity[CheckMCCBucket4StorageExcessCapacity]>=0,\"Pass\",\"Fail\")","v":"Pass"},"Applies the Storage Excess Capacity test only to Storage Resources indicated with the MCC Bucket 4 flag","Check MCC Bucket 4"]
["Storage Minimum State-of-Charge",{"$f":"IFERROR(IF(AND(Export_CheckStorageSOC[[SOC HE 1]:[SOC HE 24]]>=0),\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Checks the state-of-charge for each hour to ensure storage resources doesn't supply unavailable capacity.","Check Storage SOC"]
["Storage Energy",{"$f":"IFERROR(IF(AND(Export_CheckStorageSOC[[SOC HE 1]:[SOC HE 24]]<=1),\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Checks that storage resources don't exceed their listed maximum energy capacities."]
["Grouped Resource Interconnection",{"$f":"IFERROR(IF(AND(Export_CheckGroupedResources[Interconnection Limit (MW)]>=_xlfn.BYROW(Export_CheckGroupedResources[[MW HE 1]:[MW HE 24]],_xlfn.LAMBDA(_xlpm.array,MAX(_xlpm.array)))),\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Compares groups of resources--either hybrid pairs or colocated resources--and checks that their combined effects do not exceed interconnection limits.","Check Grouped Resources"]
["Hybrid Deliverability",{"$f":"IFERROR(IF(AND(Export_CheckHybridDeliverability[Hybrid Check]),\"Pass\",\"Fail\"),\"N/A\")","v":"Pass"},"Checks hybrid solar resources against their paired storage according to their deliverability statuses.","Check Hybrid Deliverability"]
["Overall",{"$f":"IF(OR(B2:B13=\"Fail\"),\"Fail\",\"Pass\")","v":"Pass"},"All applicable individual tests above must pass."]

{"sheet":"Check Capacity","index":7,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
["Hour Ending","Delta Capacity (MW)"]
[1,1.877]
[2,0.72160000000000002]
[3,0]
[4,0]
[5,0]
[6,3.4108000000000001]
[7,7.8631000000000002]
[8,8.2553999999999998]
[9,11.4154]
[10,13.7554]
[11,4.0553999999999997]
[12,0]
[13,0]
[14,0]
[15,0]
[16,0]
[17,0]
[18,0]
[19,0]
[20,0]
[21,0]
[22,0]
[23,3.3546999999999998]
[24,5.2770000000000001]

{"sheet":"Check Local","index":8,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","LA Basin","Big Creek-Ventura","San Diego-IV","Bay Area","Fresno","Sierra","Stockton","Kern","Humboldt","NBNC"]
["DR Allocation","",""]
["Local Requirement","","",-6,-4]
["Contract 8","7STDRD_1_SOLAR1","",null,null,null,null,null,null,null,0]
["Contract 5","ACACIA_6_SOLAR","",null,2.2200000000000002]
["Contract 10","ALAMIT_7_ES1","",10]
["Contract 6","ALAMO_6_UNIT","",null,9.5399999999999991]
["Contract 9","ALTWD_2_COAWD1","",5.67]
["Contract 7","JOANEC_2_ST3BT3","",0]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR"]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN"]
["Contract 3","PRIMM_2_SOLAR1",""]
["Contract 2","PWEST_1_UNIT","",0]
["Contract 12","SCE1_MALIN500_I_F_121212",""]
["Contract 11","SUTTER_2_CISO",""]
["Contract 4","TIGRCK_7_UNITS",""]
["Contract 7","VOYAGR_2_VOYWD3",""]

{"sheet":"Check Flex","index":9,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Category 1","Category 2","Category 3"]
["Flex RA",null,null,-2,-3]
["Contract 10","ALAMIT_7_ES1","",0]
["Contract 9","ALTWD_2_COAWD1",""]
["Contract 5","DIABLO_7_UNIT 1",""]
["Contract 7","JOANEC_2_ST3BT3",""]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR",null,5.25]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN",null,3]
["Contract 8","MIRLOM_2_MLBBTA","",0]
["Contract 6","MIRLOM_2_MLBBTB","",0]
["Contract 3","PRIMM_2_SOLAR1",""]
["Contract 2","PWEST_1_UNIT",""]
["Contract 7","SANBRN_2_ESBBT1","",null,10]
["Contract 12","SCE1_MALIN500_I_F_121212",""]
["Contract 11","SUTTER_2_CISO",""]
["Contract 4","TIGRCK_7_UNITS","",5]

{"sheet":"Check Contract Dates","index":10,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Capacity Effective Start Date","Capacity Effective End Date","Check Dates"]
["Contract 10","ALAMIT_7_ES1","","2024-09-01","2024-09-30",true]
["Contract 9","ALTWD_2_COAWD1","","2024-09-01","2024-09-30",true]
["CAM Storage","CAM Storage 2","","2024-09-01","2024-09-30",true]
["Contract 5","DIABLO_7_UNIT 1","","2024-09-01","2024-09-30",true]
["Contract 7","JOANEC_2_ST3BT3","","2024-09-01","2024-09-30",true]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR","2024-09-01","2024-09-30",true]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN","2024-09-01","2024-09-30",true]
["Contract 8","MIRLOM_2_MLBBTA","","2024-09-01","2024-09-30",true]
["Contract 6","MIRLOM_2_MLBBTB","","2024-09-01","2024-09-30",true]
["Contract 3","PRIMM_2_SOLAR1","","2024-09-01","2024-09-30",true]
["Contract 2","PWEST_1_UNIT","","2024-09-01","2024-09-30",true]
["Contract 7","SANBRN_2_ESBBT1","","2024-09-01","2024-09-30",true]
["Contract 4","TIGRCK_7_UNITS","","2024-09-01","2024-09-30",true]
["Contract 11","SUTTER_2_CISO","","2024-09-01","2024-09-30",true]
["Contract 12","SCE1_MALIN500_I_F_121212","","2024-09-01","2024-09-30",true]

{"sheet":"Check Custom Profiles","index":11,"n_rows":2,"n_cols":26,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Resource ID","Resource SubID","Delta MW HE 1","Delta MW HE 2","Delta MW HE 3","Delta MW HE 4","Delta MW HE 5","Delta MW HE 6","Delta MW HE 7","Delta MW HE 8","Delta MW HE 9","Delta MW HE 10","Delta MW HE 11","Delta MW HE 12","Delta MW HE 13","Delta MW HE 14","Delta MW HE 15","Delta MW HE 16","Delta MW HE 17","Delta MW HE 18","Delta MW HE 19","Delta MW HE 20","Delta MW HE 21","Delta MW HE 22","Delta MW HE 23","Delta MW HE 24"]
["SCE1_MALIN500_I_F_121212","",10,10,10,10,10,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,10,10]

{"sheet":"Check Shown Hours","index":12,"n_rows":18,"n_cols":10,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","First Hour Shown","Last Hour Shown","Total Hours Shown","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","Valid Hours"]
["CAM Storage","CAM Storage 2","",3,22,14,1,24,11.16578,true]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR",3,22,14,1,24,24,true]
["Contract 10","ALAMIT_7_ES1","",3,22,14,1,24,11.42,true]
["Contract 6","MIRLOM_2_MLBBTB","",3,22,14,1,24,24,true]
["Contract 7","JOANEC_2_ST3BT3","",3,22,14,1,24,24,true]
["Contract 7","SANBRN_2_ESBBT1","",3,22,14,1,24,24,true]
["Contract 8","MIRLOM_2_MLBBTA","",3,22,14,1,24,24,true]
["Contract 9","ALTWD_2_COAWD1","",1,24,24,1,24,24,true]
["Contract 5","DIABLO_7_UNIT 1","",1,24,24,1,24,24,true]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN",7,19,13,1,24,24,true]
["Contract 3","PRIMM_2_SOLAR1","",7,19,13,1,24,24,true]
["Contract 2","PWEST_1_UNIT","",1,24,24,1,24,24,true]
["Contract 4","TIGRCK_7_UNITS","",8,18,11,1,24,24,true]
["Contract 11","SUTTER_2_CISO","",1,24,24,null,null,null,true]
["Contract 12","SCE1_MALIN500_I_F_121212","",6,12,7,null,null,null,true]
["CAM DR Allocation","","",17,20,4,null,null,null,true]
["Other CAM Allocation","","",1,24,24,null,null,null,true]

{"sheet":"Check Storage Excess Capacity","index":13,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["CheckStorageExcessCapacity"]
[33.26129923365886]

{"sheet":"Check Storage SOC","index":14,"n_rows":8,"n_cols":34,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","SOC HE 1","SOC HE 2","SOC HE 3","SOC HE 4","SOC HE 5","SOC HE 6","SOC HE 7","SOC HE 8","SOC HE 9","SOC HE 10","SOC HE 11","SOC HE 12","SOC HE 13","SOC HE 14","SOC HE 15","SOC HE 16","SOC HE 17","SOC HE 18","SOC HE 19","SOC HE 20","SOC HE 21","SOC HE 22","SOC HE 23","SOC HE 24"]
["CAM Storage","CAM Storage 2","",2.79,0.87,80,1000,1,24,11.16578,0.21749999999999997,0.43499999999999994,0.43433419472022738,0.43260887436965906,0.4299219021554942,0.64742190215549411,0.86492190215549414,1,1,1,1,0.99941804607219364,0.98754310183621985,0.97162176523772481,0.95000787035959089,0.92635102496043187,0.90368621266308735,0.886526161258818,0.87398956877291922,0.86775245389420141,0.86740147179245408,0.8673527804263953,1,1]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR",1,0.8,21,21,1,24,24,0.2,0.4,0.39841458614369063,0.39430620223869822,0.38790788473432408,0.58790788473432409,0.78790788473432416,0.98790788473432412,1,1,1,0.9986142570450558,0.97033707931504865,0.93242442986261631,0.88095637552595907,0.82462354865878773,0.7706530008899577,0.72979066274429849,0.69993793500509927,0.68508584102262848,0.68425009990157759,0.6840691770781433,0.88406917707814325,1]
["Contract 10","ALAMIT_7_ES1","",2.86,0.91,400,1142,1,24,11.42,0.22750000000000001,0.45500000000000002,0.45332520145923477,0.44900235960022966,0.44199117019490536,0.66949117019490534,0.89699117019490537,1,1,1,1,0.98823959047573617,0.95271385314912249,0.90707213378756635,0.84719902061701136,0.78221853313233591,0.71971812704088756,0.67097962426896318,0.63379976786045233,0.61236860533285664,0.60565277498208769,0.60000000000000009,0.82750000000000012,1]
["Contract 6","MIRLOM_2_MLBBTB","",2.79,0.87,40,112,1,24,24,0.21749999999999997,0.43499999999999994,0.43433419472022738,0.43260887436965906,0.4299219021554942,0.64742190215549411,0.86492190215549414,1,1,1,1,0.99941804607219364,0.98754310183621985,0.97162176523772481,0.95000787035959089,0.92635102496043187,0.90368621266308735,0.886526161258818,0.87398956877291922,0.86775245389420141,0.86740147179245408,0.8673527804263953,1,1]
["Contract 7","JOANEC_2_ST3BT3","",1,0.8,160,160,1,24,24,0.2,0.4,0.39841458614369063,0.39430620223869822,0.38790788473432408,0.58790788473432409,0.78790788473432416,0.98790788473432412,1,1,1,0.9986142570450558,0.97033707931504865,0.93242442986261631,0.88095637552595907,0.82462354865878773,0.77065300088995758,0.72979066274429838,0.69993793500509915,0.68508584102262837,0.68425009990157748,0.68406917707814319,0.88406917707814325,1]
["Contract 7","SANBRN_2_ESBBT1","",1,0.8,400,400,1,24,24,0.1,0.2,0.19920729307184531,0.19715310111934911,0.19395394236716204,0.29395394236716205,0.39395394236716208,0.49395394236716206,0.59395394236716204,0.69395394236716201,0.79395394236716199,0.79326107088968989,0.77912248202468637,0.76016615729847015,0.73443213013014153,0.7062657166965558,0.67928044281214073,0.65884927373931113,0.64392290986971146,0.63649686287847607,0.63607899231795062,0.63598853090623353,0.73598853090623351,0.83598853090623348]
["Contract 8","MIRLOM_2_MLBBTA","",2.79,0.87,40,112,1,24,24,0.21749999999999997,0.43499999999999994,0.43433419472022738,0.43260887436965906,0.4299219021554942,0.64742190215549411,0.86492190215549414,1,1,1,1,0.99941804607219364,0.98754310183621985,0.97162176523772481,0.95000787035959089,0.92635102496043187,0.90368621266308735,0.886526161258818,0.87398956877291922,0.86775245389420141,0.86740147179245408,0.8673527804263953,1,1]

{"sheet":"Check Grouped Resources","index":15,"n_rows":2,"n_cols":26,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Associated Resources","Interconnection Limit (MW)","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]
["LNCSTR_6_SOLAR2.LNCSTR_6_SOLAR2_LESR,LNCSTR_6_SOLAR2.LNCSTR_6_SOLAR2_SUN",8.25,0,0,3.2803587047497182E-2,8.4941995703032888E-2,0.13332132460705909,0,0.03,0.60000000000000009,1.56,2.0999999999999996,2.4000000000000004,2.649339683668841,3.2291757096176599,3.3981260626054617,3.5586706075017029,3.3895415446634747,2.7402694844080866,1.6602185976759227,0.74287198113065123,0.37281604016711201,0.2034883350660826,6.3988913397708833E-2,0,0]

{"sheet":"Check Hybrid Deliverability","index":16,"n_rows":2,"n_cols":31,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Resource Type","Deliverable MW","Hybrid Pair","Hybrid Check","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN","Hybrid_SolarFixed",6.9,true,true,0,0,0,0,0,0,0.03,0.60000000000000009,1.56,2.0999999999999996,2.4000000000000004,2.52,2.58,2.5499999999999998,2.4300000000000002,2.16,1.6800000000000002,0.75,0.06,0,0,0,0,0]

{"sheet":"Check MCC Bucket 4","index":17,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["CheckMCCBucket4StorageExcessCapacity"]
[125.02093379221382]

{"sheet":"LSE Showing Complete","index":18,"n_rows":19,"n_cols":52,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Colocated Resource IDs","NQC MW","NQC or VER Under Contract (MW)","Local RA (MW)","Local Capacity Area","Committed Flexible RA (MW)","Flexible Category","Deliverability Status","Deliverable %","Deliverable MW","Capacity Effective Start Date","Capacity Effective End Date","Resource Type","Path 26 Designation","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","Interconnection Limit (MW)","MCC Bucket 4","Unspecified Import","Profile Source","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]
["CAM Storage","CAM Storage 2","","",null,20,0,"CAISO System",0,null,null,null,null,45536,45565,"Battery Storage","South",2.79,0.87,80,1000,1,24,11.16578,null,false,false,"Optimized",0,0.57889258176231695,1.657936184564772,2.9535485798997452,3.8160242907333779,0.15145030209891502,0,0,0,0,0,0,0,0.77579532138294705,5.8739759609482292,7.9309816664192923,8.4388933856198314,3.2310053970006214,2.8338350437940574,0,0,0,0,0]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR","",5.26,5.25,0,"SEPV Sierra NGR",5.25,2,null,null,null,45536,45565,"Hybrid_Storage","",1,0.8,21,21,1,24,24,8.25,true,false,"Optimized",0,3.9889578886088746E-2,0.11424242493500877,0.20351831332827625,0.26294826191321147,1.0436179066888585E-2,0,0,0,0,0,0,0,5.3457373930559562E-2,0.40475386246676176,0.546494471498844,0.58149278356881284,0.22263671771002427,0.19526917242954792,0,0,0,0,0]
["Contract 10","ALAMIT_7_ES1","","",100,10,10,"LA Basin",20,1,"FC",null,null,45536,45565,"Battery Storage","South",2.86,0.91,400,1142,1,24,11.42,null,true,false,"Optimized",0,0.14472359989002798,0.41448448905949942,0.73838743830876119,0.95400638060325937,3.7862945362659967E-2,0,0,0,0,0,0,0,0.19394934376640993,1.4684945221426897,1.9827458430098202,2.109723797262387,0.80775183793507666,0.70845928029740035,0,0,0,0,0]
["Contract 7","JOANEC_2_ST3BT3","","",40,20,0,"LA Basin",40,null,"FC",null,null,45536,45565,"Battery Storage","South",1,0.8,160,160,1,24,24,null,false,false,"Optimized",0,0.57889258176231695,1.657936184564772,2.9535485798997452,3.8160242907333779,0.15145030209891502,0,0,0,0,0,0,0,0.77579532138294705,5.8739759609482292,7.9309816664192923,8.4388933856198314,3.2310053970006214,2.8338350437940574,0,0,0,0,0]
["Contract 8","7STDRD_1_SOLAR1","","",2.2200000000000002,20,0,"Kern",0,null,"FC",null,null,45536,45565,"Solar_1Axis","North",null,null,null,null,1,24,24,null,false,false,"Default",0,0,0,0,0,0,0,2.8000000000000003,10.4,13.799999999999999,14.6,14.8,14.6,14.6,14.6,14.8,13.4,8.1999999999999993,1.2,0,0,0,0,0]
["Contract 5","ACACIA_6_SOLAR","","",2.2200000000000002,20,2.2200000000000002,"Big Creek-Ventura",0,null,"FC",null,null,45536,45565,"Solar_Fixed","South",null,null,null,null,1,24,24,null,false,false,"Default",0,0,0,0,0,0,0.2,4,10.4,14,16,16.8,17.2,17,16.200000000000003,14.399999999999999,11.200000000000001,5,0.4,0,0,0,0,0]
["Contract 6","ALAMO_6_UNIT","","",9.5399999999999991,9.5399999999999991,9.5399999999999991,"Big Creek-Ventura",9.5399999999999991,2,"FC",null,null,45536,45565,"Hydro","South",null,null,null,null,1,24,24,null,false,false,"Default",9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991,9.5399999999999991]
["Contract 9","ALTWD_2_COAWD1","","",5.67,5.67,5.67,"LA Basin",0,null,"FC",null,null,45536,45565,"Wind","South",null,null,null,null,1,24,24,null,false,false,"Default",0.56700000000000006,0.4536,0.39690000000000003,0.28350000000000003,0.28350000000000003,0.2268,0.1701,0.1134,0.1134,0.1134,0.1134,0.1701,0.1701,0.28350000000000003,0.2268,0.2268,0.28350000000000003,0.4536,0.73709999999999998,0.79380000000000006,0.79380000000000006,0.62370000000000003,0.62370000000000003,0.56700000000000006]
["Contract 1","LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN","",5.26,3,0,"SEPV Sierra NGR",3,2,"PD",null,6.9,45536,45565,"Hybrid_SolarFixed","South",null,null,null,null,1,24,24,8.25,false,false,"Default",0,0,0,0,0,0,0.03,0.60000000000000009,1.56,2.0999999999999996,2.4000000000000004,2.52,2.58,2.5499999999999998,2.4300000000000002,2.16,1.6800000000000002,0.75,0.06,0,0,0,0,0]
["Contract 3","PRIMM_2_SOLAR1","","",27.75,10,0,"CAISO System",0,null,"FC",null,null,45536,45565,"Solar_Fixed","South",null,null,null,null,1,24,24,null,false,false,"Default",0,0,0,0,0,0,0.1,2,5.2,7,8,8.4,8.6,8.5,8.1000000000000014,7.1999999999999993,5.6000000000000005,2.5,0.2,0,0,0,0,0]
["Contract 2","PWEST_1_UNIT","","",0.24,2.1,0,"LA Basin",0,null,"FC",null,null,45536,45565,"Wind","South",null,null,null,null,1,24,24,null,false,false,"Default",0.21000000000000002,0.16800000000000001,0.14700000000000002,0.10500000000000001,0.10500000000000001,8.4000000000000005E-2,6.3E-2,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2,4.2000000000000003E-2,6.3E-2,6.3E-2,0.10500000000000001,8.4000000000000005E-2,8.4000000000000005E-2,0.10500000000000001,0.16800000000000001,0.27300000000000002,0.29400000000000004,0.29400000000000004,0.23100000000000001,0.23100000000000001,0.21000000000000002]
["Contract 4","TIGRCK_7_UNITS","","",36.299999999999997,5,0,"CAISO System",5,1,"FC",null,null,45536,45565,"Hydro","North",null,null,null,null,1,24,24,null,false,false,"Default",5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5]
["Contract 7","VOYAGR_2_VOYWD3","","",4.7699999999999996,42.45,0,"CAISO System",0,null,"FC",null,null,45536,45565,"Wind","South",null,null,null,null,1,24,24,null,false,false,"Default",4.2450000000000001,3.3960000000000004,2.9715000000000007,2.1225000000000001,2.1225000000000001,1.6980000000000002,1.2735000000000001,0.84900000000000009,0.84900000000000009,0.84900000000000009,0.84900000000000009,1.2735000000000001,1.2735000000000001,2.1225000000000001,1.6980000000000002,1.6980000000000002,2.1225000000000001,3.3960000000000004,5.5185000000000004,5.9430000000000014,5.9430000000000014,4.6695000000000002,4.6695000000000002,4.2450000000000001]
["Contract 11","SUTTER_2_CISO","","",null,25,null,null,25,null,null,null,null,45536,45565,null,null,null,null,null,null,null,null,null,null,false,false,"Default",25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25,25]
["Contract 12","SCE1_MALIN500_I_F_121212","","",null,10,null,null,null,null,null,null,null,45536,45565,null,null,null,null,null,null,null,null,null,null,false,true,"Custom",10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10]
["Contract 13","SCE1_MALIN500_I_F_131313","","",null,10,null,null,null,null,null,null,null,45536,45565,null,null,null,null,null,null,null,null,null,null,false,true,"Custom",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,10,10,10,10,0,0,0]
["DR Allocation","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Allocation",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,5,5,5,5,0,0,0]
["Other CAM Allocation","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Allocation",42.1,42.1,42.1,42.1,42.1,42.1,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5]

{"sheet":"Hourly Availability","index":20,"n_rows":9,"n_cols":25,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["Label","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24"]
["Requirements and Allocations",43.9,44.9,46.9,48.9,50.9,51.9,47.5,50.5,52.5,53.5,65.5,76.5,88.5,96.5,106.5,108.5,103.5,87.5,74.5,61.5,49.5,48.5,42.5,40.5]
["Battery Storage",0,1.3423983423007506,3.8445992831240519,6.8490029114365276,8.8490032239832264,0.35119972862737864,0,0,0,0,0,0,0,1.7989973604628635,13.62120030650591,18.391203647347247,19.569003352070862,7.4923993496463437,6.5713985403150623,0,0,0,0,0]
["Other",39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54,39.54]
["Solar Fixed",0,0,0,0,0,0,0.33,6.6,17.16,23.1,26.4,27.72,28.380000000000003,28.05,26.730000000000004,23.759999999999998,18.48,8.25,0.66,0,0,0,0,0]
["Solar Thermal",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Solar Tracking",0,0,0,0,0,0,0,2.8000000000000003,10.4,13.799999999999999,14.6,14.8,14.6,14.6,14.6,14.8,13.4,8.1999999999999993,1.2,0,0,0,0,0]
["Unspecified Imports",10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,10,20,20,20,20,10,10,10]
["Wind",5.0220000000000002,4.0176000000000007,3.5154000000000005,2.5110000000000001,2.5110000000000001,2.0088000000000004,1.5066000000000002,1.0044000000000002,1.0044000000000002,1.0044000000000002,1.0044000000000002,1.5066000000000002,1.5066000000000002,2.5110000000000001,2.0088000000000004,2.0088000000000004,2.5110000000000001,4.0176000000000007,6.5286000000000008,7.030800000000001,7.030800000000001,5.5242000000000004,5.5242000000000004,5.0220000000000002]

{"sheet":"Local Availability","index":22,"n_rows":9,"n_cols":11,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["Label","LA Basin","Big Creek-Ventura","San Diego-IV","Bay Area","Fresno","Sierra","Stockton","Kern","Humboldt","NBNC"]
["Local Requirement",6,4,0,0,0,0,0,0,0,0]
["Battery Storage",10,0,0,0,0,0,0,0,0,0]
["Other",0,0,0,0,0,0,0,0,0,0]
["Solar Fixed",0,0,0,0,0,0,0,0,0,0]
["Solar Thermal",0,0,0,0,0,0,0,0,0,0]
["Solar Tracking",0,0,0,0,0,0,0,0,0,0]
["Unspecified Imports",0,0,0,0,0,0,0,0,0,0]
["Wind",5.67,0,0,0,0,0,0,0,0,0]

{"sheet":"Flex Availability","index":24,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["Label","Flexible Category 1","Flexible Category 2","Flexible Category 3"]
["Flexible Requirement",2,3,0]
["Battery Storage",0,15.25,0]
["Other",5,0,0]
["Solar Fixed",0,3,0]
["Solar Thermal",0,0,0]
["Solar Tracking",0,0,0]
["Unspecified Imports",0,0,0]
["Wind",0,0,0]

{"sheet":"Requirements and Allocations","index":25,"n_rows":685,"n_cols":7,"rows_kept":685,"cut":false,"hidden":false,"merged":[]}
["LSE","Year","Month","Name","Option","Value","Units"]
["LSE_1",2024,1,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,1,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,2,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,2,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,3,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,3,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,4,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,4,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,5,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,5,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,6,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,6,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,7,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,7,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,8,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,8,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,9,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,9,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,10,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,10,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,11,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,11,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,12,"Flexible Requirement","Category 1",2,"MW"]
["LSE_1",2024,12,"Flexible Requirement","Category 2",3,"MW"]
["LSE_1",2024,1,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,2,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,3,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,4,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,5,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,6,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,7,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,8,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,9,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,10,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,11,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,12,"Local Requirement","LA Basin",6,"MW"]
["LSE_1",2024,1,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,2,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,3,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,4,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,5,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,6,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,7,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,8,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,9,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,10,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,11,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,12,"Local Requirement","Big Creek-Ventura",4,"MW"]
["LSE_1",2024,9,"System Requirement","HE 1",86,"MW"]
["LSE_1",2024,9,"System Requirement","HE 10",102,"MW"]
["LSE_1",2024,9,"System Requirement","HE 11",114,"MW"]
["LSE_1",2024,9,"System Requirement","HE 12",125,"MW"]
["LSE_1",2024,9,"System Requirement","HE 13",137,"MW"]
["LSE_1",2024,9,"System Requirement","HE 14",145,"MW"]
["LSE_1",2024,9,"System Requirement","HE 15",155,"MW"]
["LSE_1",2024,9,"System Requirement","HE 16",157,"MW"]
["LSE_1",2024,9,"System Requirement","HE 17",152,"MW"]
["LSE_1",2024,9,"System Requirement","HE 18",141,"MW"]
["LSE_1",2024,9,"System Requirement","HE 19",128,"MW"]
["LSE_1",2024,9,"System Requirement","HE 2",87,"MW"]
["LSE_1",2024,9,"System Requirement","HE 20",115,"MW"]
["LSE_1",2024,9,"System Requirement","HE 21",103,"MW"]
["LSE_1",2024,9,"System Requirement","HE 22",97,"MW"]
["LSE_1",2024,9,"System Requirement","HE 23",91,"MW"]
["LSE_1",2024,9,"System Requirement","HE 24",89,"MW"]
["LSE_1",2024,9,"System Requirement","HE 3",89,"MW"]
["LSE_1",2024,9,"System Requirement","HE 4",91,"MW"]
["LSE_1",2024,9,"System Requirement","HE 5",93,"MW"]
["LSE_1",2024,9,"System Requirement","HE 6",94,"MW"]
["LSE_1",2024,9,"System Requirement","HE 7",96,"MW"]
["LSE_1",2024,9,"System Requirement","HE 8",99,"MW"]
["LSE_1",2024,9,"System Requirement","HE 9",101,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,1,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,2,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,3,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,4,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,5,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,6,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,7,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,8,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,9,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,10,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,11,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 1",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 2",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 3",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 4",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 5",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 6",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 7",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 8",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 9",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 10",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 11",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 12",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 13",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 14",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 15",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 16",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 17",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 18",5,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 19",5,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 20",5,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 21",5,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 22",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 23",0,"MW"]
["LSE_1",2024,12,"DR Allocation","HE 24",0,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,1,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,2,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,3,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,4,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,5,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,6,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,7,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,8,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,9,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,10,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,11,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 1",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 2",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 3",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 4",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 5",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 6",42.1,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 7",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 8",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 9",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 10",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 11",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 12",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 13",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 14",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 15",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 16",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 17",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 18",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 19",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 20",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 21",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 22",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 23",48.5,"MW"]
["LSE_1",2024,12,"Other CAM Allocation","HE 24",48.5,"MW"]
["LSE_1",2024,1,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,2,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,3,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,4,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,5,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,6,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,7,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,8,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,9,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,10,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,11,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,12,"CAM Storage Allocation","Total Energy Available",20,"MWh"]
["LSE_1",2024,1,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,2,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,3,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,4,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,5,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,6,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,7,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,8,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,9,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,10,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,11,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,12,"CAM Storage Allocation","Daily Storage Cycle Physical Capability",1.5,"MW"]
["LSE_1",2024,1,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,2,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,3,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,4,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,5,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,6,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,7,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,8,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,9,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,10,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,11,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]
["LSE_1",2024,12,"CAM Storage Allocation","Maximum Discharge Rate",6,"MW"]

{"sheet":"Resource Database","index":26,"n_rows":1203,"n_cols":24,"rows_kept":1203,"cut":false,"hidden":false,"merged":[]}
["Resource ID","Resource SubID","Resource Name","Colocated Resource IDs","Technology","Resource Type","Fuel","Balancing Authority Area","Path 26 Designation","Local Capacity Area","Sub-Local Capacity Area","Interconnection Limit (MW)","Flexible Category","Pmax (MW)","Deliverable %","Deliverable MW","Deliverability Status","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours"]
["7STDRD_1_SOLAR1",null,"Shafter Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["ACACIA_6_SOLAR",null,"West Antelope Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["ADERA_1_SOLAR1",null,"Adera Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["ADLIN_1_UNITS",null,"GEYSERS AIDLIN AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",null,1,22,null,null,"FC"," "," "," "," ",1,24,24]
["ADMEST_6_SOLAR",null,"Adams East",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,null,19,null,null,"EO"," "," "," "," ",1,24,24]
["ADOBEE_1_SOLAR",null,"Adobe Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["AGRICO_6_PL3N5",null,"Fresno Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon",null,1,22.69,null,null,"FC"," "," "," "," ",1,24,24]
["AGRICO_7_UNIT",null,"Fresno Cogen",null,"OTHER","CHP","NATURAL GAS","CISO","North","Fresno","Herndon",null,1,50.6,null,null,"FC"," "," "," "," ",1,24,24]
["AGUCAL_5_SOLAR1",null,"Agua Caliente Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,290,null,null,"EO"," "," "," "," ",1,24,24]
["AKINGS_6_AMESR1",null,"American Kings Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Hanford",null,null,123,null,null,"FC"," "," "," "," ",1,24,24]
["ALAMIT_2_PL1X3",null,"Alamitos Energy Center Unit 7",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",null,1,674.7,null,null,"FC"," "," "," "," ",1,24,24]
["ALAMIT_7_ES1",null,"Alamitos Energy Storage",null,"4Hr_Li","Battery Storage","LESR","CISO","South","LA Basin","Western",null,1,100,null,null,"FC",2.86,0.91,400,1142,1,24,11.42]
["ALAMIT_7_UNIT 3",null,"ALAMITOS GEN STA. UNIT 3",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,326.76,null,null,"FC"," "," "," "," ",1,24,24]
["ALAMIT_7_UNIT 4",null,"ALAMITOS GEN STA. UNIT 4",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,334.43,null,null,"FC"," "," "," "," ",1,24,24]
["ALAMIT_7_UNIT 5",null,"ALAMITOS GEN STA. UNIT 5",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,480,null,null,"FC"," "," "," "," ",1,24,24]
["ALAMO_6_UNIT",null,"ALAMO POWER PLANT ",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,null,2,17,null,null,"FC"," "," "," "," ",1,24,24]
["ALLGNY_6_HYDRO1",null,"Salmon Creek Hydroelectric Project",null,"OTHER","Hydro","WATER","CISO","North","Sierra",null,null,null,0.52,null,null,"FC"," "," "," "," ",1,24,24]
["ALMASL_2_AL6BT6",null,"Almasol 6 BES","ALMASL_2_GS6SR6","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,55.57,1,50,null,null,"FC",1,0.8,200,200,1,24,4]
["ALMASL_2_GS1SR1",null,"Almasol Generating Station 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,125,null,null,"FC"," "," "," "," ",1,24,24]
["ALMASL_2_GS4SR4",null,"Almasol Generating Station 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,100,null,null,"FC"," "," "," "," ",1,24,24]
["ALMASL_2_GS6SR6",null,"Almasol Generating Station 6","ALMASL_2_AL6BT6","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,55.57,null,100,null,null,"FC"," "," "," "," ",1,24,24]
["ALMASL_2_GS7SR7",null,"Almasol Generating Station 7",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,132,null,null,"FC"," "," "," "," ",1,24,24]
["ALMEGT_1_UNIT 1",null,"ALAMEDA GT UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Oakland",null,1,25,null,null,"FC"," "," "," "," ",1,24,24]
["ALMEGT_1_UNIT 2",null,"ALAMEDA GT UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Oakland",null,1,25,null,null,"FC"," "," "," "," ",1,24,24]
["ALPSLR_1_NTHSLR",null,"Alpaugh North, LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["ALPSLR_1_SPSSLR",null,"Alpaugh 50 LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,50,null,null,"FC"," "," "," "," ",1,24,24]
["ALT6DN_2_WIND7",null,"Pinyon Pines 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,164.31,null,null,"FC"," "," "," "," ",1,24,24]
["ALT6DS_2_WIND9",null,"Pinyon Pines 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,132,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA3A_2_CPCE4",null,"Alta Wind 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,102,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA3A_2_CPCE5",null,"Alta Wind 5",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,168,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA3A_2_CPCE8",null,"Alta Wind 8",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA4A_2_CPCW1",null,"Alta Wind 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA4B_2_CPCW2",null,"Alta Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA4B_2_CPCW3",null,"Alta Wind 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA4B_2_CPCW6",null,"Mustang Hills",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA6B_2_WIND11",null,"Alta Wind 11",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,88.15,null,null,"FC"," "," "," "," ",1,24,24]
["ALTA6E_2_WIND10",null,"Alta Wind 10",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,134.84,null,null,"FC"," "," "," "," ",1,24,24]
["ALTWD_2_AT3WD3",null,"Altech 3",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,9.8000000000000007,null,null,"FC"," "," "," "," ",1,24,24]
["ALTWD_2_COAWD1",null,"Coachella 1",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,50.4,null,null,"FC"," "," "," "," ",1,24,24]
["ANAHM_2_CANYN1",null,"CANYON POWER PLANT UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,49.21,null,null,"FC"," "," "," "," ",1,24,24]
["ANAHM_2_CANYN2",null,"CANYON POWER PLANT UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,48.04,null,null,"FC"," "," "," "," ",1,24,24]
["ANAHM_2_CANYN3",null,"CANYON POWER PLANT UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,46.49,null,null,"FC"," "," "," "," ",1,24,24]
["ANAHM_2_CANYN4",null,"CANYON POWER PLANT UNIT 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,49.8,null,null,"FC"," "," "," "," ",1,24,24]
["ANTLPE_2_QF",null,"ANTELOPE QFS",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,4,null,null,"FC"," "," "," "," ",1,24,24]
["APLHIL_1_SFKHY1",null,"South Fork Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,null,2.68,null,null,"EO"," "," "," "," ",1,24,24]
["AQUAWS_2_AQWSR1",null,"Aquamarine Westside",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,250,1,null,"ID"," "," "," "," ",1,24,24]
["ARBWD_6_QF",null,"Wind Resource II",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,19.95,null,null,"FC"," "," "," "," ",1,24,24]
["ARCOGN_2_UNITS",null,"WATSON COGENERATION",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","LA Basin","Western",null,null,305,null,null,"FC"," "," "," "," ",1,24,24]
["ARLNTN_2_AR1SR1",null,"Arlington","SUNCAT_2_A2ABT2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,144.31,null,100,1,null,"ID"," "," "," "," ",1,24,24]
["ARLNTN_2_ASUSR1",null,"Arlington Solar Unit 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,131,1,null,"ID"," "," "," "," ",1,24,24]
["ARVINN_6_ORION1",null,"Orion 1 Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,12,null,null,"FC"," "," "," "," ",1,24,24]
["ARVINN_6_ORION2",null,"Orion 2 Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,8,null,null,"FC"," "," "," "," ",1,24,24]
["ASTORA_2_SOLAR1",null,"Astoria 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,100,null,null,"FC"," "," "," "," ",1,24,24]
["ASTORA_2_SOLAR2",null,"Astoria 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,75,null,null,"FC"," "," "," "," ",1,24,24]
["ATHOS_5_AP1X2",null,"Athos Power Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,250,null,null,"FC"," "," "," "," ",1,24,24]
["ATHOS_5_AP2X2",null,"Athos Power Plant 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,200,null,null,"FC"," "," "," "," ",1,24,24]
["ATWEL2_1_SOLAR1",null,"Atwell West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["ATWELL_1_SOLAR",null,"Atwell Island PV Solar Generating Faci.",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["AVENAL_6_AVPARK",null,"Avenal Park Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,null,6,1,null,"ID"," "," "," "," ",1,24,24]
["AVENAL_6_AVSLR1",null,"Avenal Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga",null,null,7.9,null,null,"EO"," "," "," "," ",1,24,24]
["AVENAL_6_AVSLR2",null,"Avenal Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga",null,null,7.9,null,null,"EO"," "," "," "," ",1,24,24]
["AVENAL_6_SANDDG",null,"Sand Drag Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Fresno","Coalinga",null,null,19,0.83579999999999999,null,"ID"," "," "," "," ",1,24,24]
["AVENAL_6_SUNCTY",null,"Sun City Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,null,20,1,null,"ID"," "," "," "," ",1,24,24]
["AVSOLR_2_SOLAR",null,"AV SOLAR RANCH 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,241.5,null,null,"FC"," "," "," "," ",1,24,24]
["BAHIA_2_LKHSR1",null,"Lake Herman Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,5,null,null,"EO"," "," "," "," ",1,24,24]
["BALCHS_7_UNIT 1",null,"BALCH 1 PH UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,1,31,null,null,"FC"," "," "," "," ",1,24,24]
["BALCHS_7_UNIT 2",null,"BALCH 2 PH UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,1,52.5,null,null,"FC"," "," "," "," ",1,24,24]
["BALCHS_7_UNIT 3",null,"BALCH 2 PH UNIT 3",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,1,54.6,null,null,"FC"," "," "," "," ",1,24,24]
["BANKPP_2_NSPIN",null,"BANKPP_2_NSPIN",null,"PUMP","Pump","WATER","CISO","North","Bay Area","Contra Costa",null,null,270,null,null,"FC"," "," "," "," ",1,24,24]
["BARRE_2_QF",null,"BARRE QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Western",null,null,0.2,null,null,"FC"," "," "," "," ",1,24,24]
["BARRE_6_PEAKER",null,"Barre Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,49,null,null,"FC"," "," "," ",449,1,24,9.17]
["BASICE_2_UNITS",null,"King City Cogen",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,120,null,null,"FC"," "," "," "," ",1,24,24]
["BDGRCK_1_UNITS",null,"BADGER CREEK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",null,1,48.08,null,null,"FC"," "," "," "," ",1,24,24]
["BEARDS_7_UNIT 1",null,"Beardsley Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,1,11.5,null,null,"FC"," "," "," "," ",1,24,24]
["BEARMT_1_UNIT",null,"Bear Mountain Limited",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP, Westpark",null,1,49.21,null,null,"FC"," "," "," "," ",1,24,24]
["BELDEN_7_UNIT 1",null,"BELDEN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,119,null,null,"FC"," "," "," "," ",1,24,24]
["BGSKYN_2_AS2SR1",null,"Antelope Solar 2","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,105,1,null,"ID"," "," "," "," ",1,24,24]
["BGSKYN_2_ASPSR2",null,"Antelope Solar 2 San Pablo","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,100,1,null,"ID"," "," "," "," ",1,24,24]
["BGSKYN_2_ASSR1B",null,"Antelope Solar 1B ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_AS2SR2, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,17,1,null,"ID",null,null,null,null,1,24,24]
["BGSKYN_2_ASSR3A",null,"Antelope Solar 3A ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,15,1,null,"ID"," "," "," "," ",1,24,24]
["BGSKYN_2_ASSR3B",null,"Antelope Solar 3B ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,5,1,null,"ID"," "," "," "," ",1,24,24]
["BGSKYN_2_BS3SR3",null,"Big Sky Solar 3","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGCRK_2_EXESWD",null,"BIG CREEK HYDRO PROJECT PSP",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,1,820,null,null,"FC"," "," "," "," ",1,24,24]
["BIGCRK_7_DAM7",null,"DAM 7 AT BIG CREEK (FISHWATER GEN)",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,0.3,null,null,"EO"," "," "," "," ",1,24,24]
["BIGCRK_7_MAMRES",null,"MAMMOTH POOL RESERVOIR (FISHWATER",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,1.25,null,null,"EO"," "," "," "," ",1,24,24]
["BIGSKY_2_AS2BT1",null,"Antelope Solar 2 LAB","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3","OTHER","Paired_BattStorage","LESR","CISO","South","Big Creek-Ventura",null,1792.24,2,127,1,null,"ID",1,0.8,508,508,1,24,4]
["BIGSKY_2_ASLBT2",null,"Antelope Solar 2 Luna",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura",null,null,2,100,1,null,"ID",1,0.8,400,400,1,24,4]
["BIGSKY_2_BSKSR6",null,"Big Sky Solar 6","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2,BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_BSKSR7",null,"Big Sky Solar 7","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_BSKSR8",null,"Big Sky Solar 8","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR1",null,"Antelope Big Sky Ranch ","BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR2",null,"Big Sky Solar 4","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,40,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR3",null,"Big Sky Summer ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2,BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR4",null,"Western Antelope Blue Sky Ranch B","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR5",null,"Big Sky Solar 2","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,5,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR6",null,"Solverde 1","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,85,null,null,"FC"," "," "," "," ",1,24,24]
["BIGSKY_2_SOLAR7",null,"Big Sky Solar 1","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,1792.24,null,50,null,null,"FC"," "," "," "," ",1,24,24]
["BIOMAS_1_UNIT 1",null,"WOODLAND BIOMASS",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,25.5,null,null,"FC"," "," "," "," ",1,24,24]
["BISHOP_1_ALAMO",null,"BISHOP CREEK PLANT 2  AND  6",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,null,13.4,null,null,"FC"," "," "," "," ",1,24,24]
["BISHOP_1_UNITS",null,"BISHOP CREEK PLANT 3  AND  4",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,null,15.8,null,null,"FC"," "," "," "," ",1,24,24]
["BKRFLD_2_SOLAR1",null,"Bakersfield 111",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP",null,null,1.38,null,null,"FC"," "," "," "," ",1,24,24]
["BLACK_7_UNIT 1",null,"JAMES B. BLACK 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,85,null,null,"FC"," "," "," "," ",1,24,24]
["BLACK_7_UNIT 2",null,"JAMES B. BLACK 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,84.1,null,null,"FC"," "," "," "," ",1,24,24]
["BLAST_1_WIND",null,"Mountain View IV Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,49,null,null,"FC"," "," "," "," ",1,24,24]
["BLCKBT_2_STONEY",null,"BLACK BUTTE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,6.2,null,null,"FC"," "," "," "," ",1,24,24]
["BLCKWL_6_SOLAR1",null,"Blackwell Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,12,null,null,"FC"," "," "," "," ",1,24,24]
["BLKCRK_2_GMCBT1",null,"Genesis McCoy Bess","BLKCRK_2_SOLAR1, GENESI_2_STG","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,258.91000000000003,1,230,null,null,"FC",2.84,0.9,920,2616,1,24,11.38]
["BLKCRK_2_SOLAR1",null,"McCoy Station","BLKCRK_2_GMCBT1, GENESI_2_STG","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,258.91000000000003,null,250,null,null,"EO"," "," "," "," ",1,24,24]
["BLKDIA_2_BDEBT1",null,"Black Diamond Energy Storage ",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","Pittsburg",null,1,200,null,null,"FC",1,0.8,800,800,1,24,4]
["BLM W_2_COSBT1",null,"Coso Battery Storage",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,2,60,null,null,"FC",1,0.8,240,240,1,24,4]
["BLM_2_UNITS",null,"BLM EAST Facility",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,1,72,null,47,"PD"," "," "," "," ",1,24,24]
["BLYTHE_1_SOLAR1",null,"Blythe Solar 1 Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,21,null,null,"EO"," "," "," "," ",1,24,24]
["BLYTHE_1_SOLAR2",null,"Blythe Green 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["BNNIEN_7_ALTAPH",null,"ALTA POWER HOUSE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,1,null,null,"FC"," "," "," "," ",1,24,24]
["BOGUE_1_UNITA1",null,"Feather River Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Bogue, Drum-Rio Oso",null,1,48.69,null,null,"FC"," "," "," "," ",1,24,24]
["BORDER_6_UNITA1",null,"CalPeak Power Border Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",null,1,51.25,null,null,"FC"," "," "," "," ",1,24,24]
["BOWMN_6_HYDRO",null,"NID Hydro Bowman Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,3.6,null,null,"FC"," "," "," "," ",1,24,24]
["BRDGVL_7_BAKER",null,"Baker Station Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,null,1.49,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_HIWIND",null,"High Winds Energy Center",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,162,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_MTZUM2",null,"NextEra Energy Montezuma Wind II",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,78.2,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_MTZUMA",null,"FPL Energy Montezuma Wind",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,36.799999999999997,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_SHILO1",null,"Shiloh I Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_SHILO2",null,"SHILOH WIND PROJECT 2",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_SHLO3A",null,"Shiloh III Wind Project, LLC",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,102.5,null,null,"FC"," "," "," "," ",1,24,24]
["BRDSLD_2_SHLO3B",null,"Shiloh IV Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,100,null,null,"FC"," "," "," "," ",1,24,24]
["BREGGO_6_DEGRSL",null,"Desert Green Solar Farm",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","South","San Diego-IV","San Diego",null,null,6.3,null,null,"FC"," "," "," "," ",1,24,24]
["BREGGO_6_SOLAR",null,"NRG Borrego Solar One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,null,26,null,null,"FC"," "," "," "," ",1,24,24]
["BRODIE_2_WIND",null,"Coram Brodie Wind Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,102,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKBL_2_PL1X3",null,"Blythe Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,null,1,493.63,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKCK_2_HYDRO",null,"Lassen Station Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,null,0.99,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKCK_7_OAKFLT",null,"Oak Flat",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,null,1.3,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKCK_7_PL1X2",null,"BUCKS CREEK AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,57.25,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKWD_1_NPALM1",null,"North Palm Springs 1A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,2.4,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKWD_1_QF",null,"Buckwind Re-powering project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,16.5,null,null,"FC"," "," "," "," ",1,24,24]
["BUCKWD_7_WINTCV",null,"Wintec Energy, Ltd.",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,1.32,null,null,"FC"," "," "," "," ",1,24,24]
["BURNYF_2_UNIT 1",null,"Burney Forest Power",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,29,null,null,"FC"," "," "," "," ",1,24,24]
["BUTTVL_7_UNIT 1",null,"BUTT VALLEY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,39.5,null,null,"FC"," "," "," "," ",1,24,24]
["CABALO_2_M2BSR1",null,"Mustang 2 Barbaro Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,50,1,null,"ID"," "," "," "," ",1,24,24]
["CABALO_2_M2WSR2",null,"Mustang 2 Whirlaway Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,100,1,null,"ID"," "," "," "," ",1,24,24]
["CABZON_1_WINDA1",null,"Cabazon Wind Project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,41,null,null,"FC"," "," "," "," ",1,24,24]
["CALFTN_2_CFSBT1",null,"California Flats Solar Battery","CALFTN_2_SOLAR","OTHER","Paired_BattStorage","LESR","CISO","North","CAISO System",null,72.599999999999994,3,60,null,null,"FC",1,0.8,240,240,1,24,4]
["CALFTN_2_SOLAR",null,"California Flats North","CALFTN_2_CFSBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","North","CAISO System",null,72.599999999999994,null,130,0.82,null,"ID"," "," "," "," ",1,24,24]
["CALFTS_2_CFSSR1",null,"California Flats Solar South",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24,24]
["CALGEN_1_UNITS",null,"Coso Navy 1",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,1,80,null,null,"FC"," "," "," "," ",1,24,24]
["CALPIN_1_AGNEW",null,"Agnews Power Plant",null,"COMBUSTION TURBINE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,28.56,null,null,"FC"," "," "," "," ",1,24,24]
["CAMCHE_1_PL1X3",null,"CAMANCHE UNITS  1, 2 &  3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota",null,null,9.99,null,null,"FC"," "," "," "," ",1,24,24]
["CAMLOT_2_SOLAR1",null,"Camelot",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,45,null,null,"FC"," "," "," "," ",1,24,24]
["CAMLOT_2_SOLAR2",null,"Columbia Two",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,15,null,null,"FC"," "," "," "," ",1,24,24]
["CAMPFW_7_FARWST",null,"CAMP FAR WEST HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,1,6.8,null,null,"FC"," "," "," "," ",1,24,24]
["CANTUA_1_SOLAR",null,"Cantua Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Panoche 115 kV",null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["CAPWD_1_QF",null,"Edom Hills Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,19.55,null,null,"FC"," "," "," "," ",1,24,24]
["CARBOU_7_PL2X3",null,"CARIBOU PH 1 UNIT 2 & 3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,49,null,null,"FC"," "," "," "," ",1,24,24]
["CARBOU_7_PL4X5",null,"CARIBOU PH 2 UNIT 4 & 5 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,120,null,null,"FC"," "," "," "," ",1,24,24]
["CARBOU_7_UNIT 1",null,"CARIBOU PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,24,null,null,"FC"," "," "," "," ",1,24,24]
["CARLS1_2_CARCT1",null,"Carlsbad 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,422,null,null,"FC"," "," "," "," ",7,24,18]
["CARLS2_1_CARCT1",null,"Carlsbad 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,2,105.5,null,null,"FC"," "," "," "," ",7,24,18]
["CASADB_1_CD4GT1",null,"Casa Diablo 4",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,null,40.700000000000003,null,null,"FC"," "," "," "," ",1,24,24]
["CATLNA_2_SOLAR",null,"Catalina Solar - Phases 1 and 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,110,null,null,"FC"," "," "," "," ",1,24,24]
["CATLNA_2_SOLAR2",null,"Catalina Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,18,null,null,"FC"," "," "," "," ",1,24,24]
["CAVLSR_2_BSOLAR",null,"California Valley Solar Ranch-Phase B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,40,null,null,"FC"," "," "," "," ",1,24,24]
["CAVLSR_2_RSOLAR",null,"California Valley Solar Ranch-Phase A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,210,null,null,"FC"," "," "," "," ",1,24,24]
["CAYTNO_2_VASCO",null,"Vasco Road",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Contra Costa",null,null,4.3,null,null,"FC"," "," "," "," ",1,24,24]
["CDWR07_2_GEN",null,"CDWR07_2_GEN",null,"PUMP","Pumped Hydro","WATER","CISO","North","CAISO System",null,null,null,415.3,null,null,"FC"," "," "," "," ",1,24,24]
["CEDRCK_6_UNIT",null,"Water Wheel Ranch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.98,null,null,"FC"," "," "," "," ",1,24,24]
["CEDUCR_2_SOLAR1",null,"Ducor Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["CEDUCR_2_SOLAR2",null,"Ducor Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["CEDUCR_2_SOLAR3",null,"Ducor Solar 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,15,null,null,"EO"," "," "," "," ",1,24,24]
["CEDUCR_2_SOLAR4",null,"Ducor Solar 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["CENT40_1_C40SR1",null,"CENTRAL 40",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,null,40,null,null,"FC"," "," "," "," ",1,24,24]
["CENTER_2_RHONDO",null,"MWD Rio Hondo Hydroelectric Recovery Pla",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",null,1,1.91,null,null,"FC"," "," "," "," ",1,24,24]
["CENTER_2_SOLAR1",null,"Pico Rivera",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,0.9,null,null,"EO"," "," "," "," ",1,24,24]
["CENTER_2_TECNG1",null,"TECHNICAST",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","LA Basin","Western",null,null,0.99,null,null,"EO"," "," "," "," ",1,24,24]
["CENTER_6_PEAKER",null,"Center Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,47.3,null,null,"FC"," "," "," ",402,1,24,8.5]
["CENTPD_2_BMSSX2",null,"Blythe Mesa Solar","CENTPD_2_BMSX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,134.69,null,223.6,null,null,"FC",null,null,null,null,1,24,24]
["CENTPD_2_BMSX2",null,"Blythe Mesa Solar 2 BESS","CENTPD_2_BMSSX2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,134.69,2,112,null,null,"FC",1,0.8,448,448,1,24,4]
["CENTRY_6_PL1X4",null,"CENTURY GENERATING PLANT (AGGREGATE)",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,41.4,null,null,"FC"," "," "," "," ",1,24,24]
["CHALK_1_UNIT",null,"CHALK CLIFF LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,48.67,null,null,"FC"," "," "," "," ",1,24,24]
["CHARMN_2_PGONG1",null,"PROCTER  AND  GAMBLE OXNARD I",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,19.87,null,null,"FC"," "," "," "," ",1,24,24]
["CHEVCD_6_UNIT",null,"CHEVRON USA (TAFT/CADET)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,11.5,null,null,"FC"," "," "," "," ",1,24,24]
["CHEVCO_6_UNIT 1",null,"CHEVRON USA (COALINGA)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,16.5,null,null,"FC"," "," "," "," ",1,24,24]
["CHEVCO_6_UNIT 2",null,"AERA ENERGY LLC. (COALINGA)",null,"FTUR","CHP","NATURAL GAS","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,8.5,null,null,"FC"," "," "," "," ",1,24,24]
["CHEVCY_1_UNIT",null,"CHEVRON USA (CYMRIC)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,24.3,null,null,"FC"," "," "," "," ",1,24,24]
["CHEVMN_2_UNITS",null,"CHEVRON U.S.A. UNITS 1 & 2 AGGREGATE",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","LA Basin","Western, El Nido",null,null,124.87,null,null,"FC"," "," "," "," ",1,24,24]
["CHICPK_7_UNIT 1",null,"Chicago Park Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1,42,null,null,"FC"," "," "," "," ",1,24,24]
["CHILLS_1_SYCENG",null,"Sycamore Energy 1",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,null,1.5,null,null,"FC"," "," "," "," ",1,24,24]
["CHILLS_7_UNITA1",null,"Sycamore Energy 2",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,1,2.25,null,null,"FC"," "," "," "," ",1,24,24]
["CHINO_2_APEBT1",null,"Pomona Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",null,3,20,null,null,"FC",1,0.8,80,80,1,24,4]
["CHINO_2_JURUPA",null,"Jurupa",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["CHINO_2_QF",null,"CHINO QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,null,0.19,null,null,"FC"," "," "," "," ",1,24,24]
["CHINO_2_SASOLR",null,"SS San Antonio West LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["CHINO_2_SOLAR",null,"Chino RT Solar 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"FC"," "," "," "," ",1,24,24]
["CHINO_2_SOLAR2",null,"Kona Solar - Terra Francesca",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,1.49,null,null,"EO"," "," "," "," ",1,24,24]
["CHINO_6_CIMGEN",null,"Chino Co-Generation",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,26,null,null,"FC"," "," "," "," ",1,24,24]
["CHWCHL_1_BIOMAS",null,"Chow II Biomass to Energy",null,"STEAM","Biomass","BIOMASS","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,null,10.8,null,null,"FC"," "," "," "," ",1,24,24]
["CHWCHL_1_UNIT",null,"CHOW 2 PEAKER PLANT",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,1,48.6,null,null,"FC"," "," "," "," ",1,24,24]
["CLOVDL_1_SOLAR",null,"Cloverdale Solar I",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","NCNB","Eagle Rock, Fulton",null,null,1.5,null,null,"FC"," "," "," "," ",1,24,24]
["CLOVER_2_UNIT",null,"Clover Creek",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.99,null,null,"FC"," "," "," "," ",1,24,24]
["CLRMTK_1_QF",null,"SMALL QF AGGREGATION - OAKLAND",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","Oakland",null,null,1.25,null,null,"FC"," "," "," "," ",1,24,24]
["CNTNLA_2_SOLAR1",null,"Centinela Solar Energy I ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,null,125,null,null,"FC"," "," "," "," ",1,24,24]
["CNTNLA_2_SOLAR2",null,"Centinels Solar Energy 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,null,45.6,null,null,"FC"," "," "," "," ",1,24,24]
["COCOPP_2_CTG1",null,"Marsh Landing 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,204.2,null,null,"FC"," "," "," "," ",1,24,24]
["COCOPP_2_CTG2",null,"Marsh Landing 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,202.7,null,null,"FC"," "," "," "," ",1,24,24]
["COCOPP_2_CTG3",null,"Marsh Landing 3",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,208.96,null,null,"FC"," "," "," "," ",1,24,24]
["COCOPP_2_CTG4",null,"Marsh Landing 4",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,204.29,null,null,"FC"," "," "," "," ",1,24,24]
["COCOSB_6_SOLAR",null,"Oakley Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Bay Area","Contra Costa",null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["COGNAT_1_UNIT",null,"Stockton Biomas",null,"STEAM","CHP","BIOMASS","CISO","North","CAISO System",null,null,null,45,null,null,"FC"," "," "," "," ",1,24,24]
["COLEMN_2_UNIT",null,"Coleman",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,13,null,null,"FC"," "," "," "," ",1,24,24]
["COLGAT_7_UNIT 1",null,"Colgate Powerhouse Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,1,176.72,null,null,"FC"," "," "," "," ",1,24,24]
["COLGAT_7_UNIT 2",null,"Colgate Powerhouse Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,1,175.67,null,null,"FC"," "," "," "," ",1,24,24]
["COLPIN_6_COLLNS",null,"Collins Pine",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,3.3,null,null,"EO"," "," "," "," ",1,24,24]
["COLTON_6_AGUAM1",null,"AGUA MANSA UNIT 1 (CITY OF COLTON)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,43,null,null,"FC"," "," "," "," ",1,24,24]
["COLUSA_2_PL1X3",null,"Colusa Generating Station",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,641,null,null,"FC"," "," "," "," ",1,24,24]
["COLVIL_7_PL1X2",null,"COLLIERVILLE HYDRO UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,246.86,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_CASAD1",null,"Mammoth G1",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,null,7.2,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_CASAD2",null,"Mammoth G2",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,null,10.5,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_CASAD3",null,"Mammoth G3",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,null,14,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_LUNDY",null,"LUNDY",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,null,3,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_OXBOW",null,"Dixie Valley Geo",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,null,60,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_POOLE",null,"POOLE HYDRO PLANT 1",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,1,10.9,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_QF",null,"CONTROL QFS",null,"OTHER","CHP","OTHER","CISO","South","CAISO System",null,null,null,2.5499999999999998,null,null,"FC"," "," "," "," ",1,24,24]
["CONTRL_1_RUSHCK",null,"RUSH CREEK",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,1,11.94,null,null,"FC"," "," "," "," ",1,24,24]
["COPMT2_2_SOLAR2",null,"CMS2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,155,null,null,"FC"," "," "," "," ",1,24,24]
["COPMT4_2_SOLAR4",null,"Copper Mountain Solar 4",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,92,null,null,"FC"," "," "," "," ",1,24,24]
["COPMTN_2_CM10",null,"Copper Mountain 10",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,10,null,7.25,"PD"," "," "," "," ",1,24,24]
["COPMTN_2_SOLAR1",null,"Copper Mountain 48",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,48,null,16.5,"PD"," "," "," "," ",1,24,24]
["CORCAN_1_SOLAR1",null,"CID Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["CORCAN_1_SOLAR2",null,"Corcoran City",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Hanford",null,null,11,null,null,"FC"," "," "," "," ",1,24,24]
["CORONS_2_SOLAR",null,"Master Development Corona",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,0.99,null,null,"EO"," "," "," "," ",1,24,24]
["CORONS_6_CLRWTR",null,"Clearwater Power Plant",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,28,null,null,"FC"," "," "," "," ",1,24,24]
["CORRAL_6_SJOAQN",null,"Ameresco San Joaquin",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,4.3,null,null,"FC"," "," "," "," ",1,24,24]
["COTTLE_2_FRNKNH",null,"Frankenheimer Power Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,5.3,null,null,"FC"," "," "," "," ",1,24,24]
["COVERD_2_HCKHY1",null,"HATCHET CREEK",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,6.89,null,null,"FC"," "," "," "," ",1,24,24]
["COVERD_2_MCKHY1",null,"Montgomery Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,2.8,null,null,"FC"," "," "," "," ",1,24,24]
["COVERD_2_QFUNTS",null,"Cove Hydroelectric Project",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,5.5,null,null,"FC"," "," "," "," ",1,24,24]
["COVERD_2_RCKHY1",null,"ROARING CREEK",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24,24]
["COWCRK_2_UNIT",null,"Cow Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24,24]
["CPVERD_2_SOLAR",null,"Campo Verde Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,null,139,null,null,"FC"," "," "," "," ",1,24,24]
["CRELMN_6_RAMON1",null,"Ramona 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,null,2,null,null,"FC"," "," "," "," ",1,24,24]
["CRELMN_6_RAMON2",null,"Ramona 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,null,5,null,null,"FC"," "," "," "," ",1,24,24]
["CRELMN_6_RAMSR3",null,"Ramona Solar Energy",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,null,4.32,0.8,null,"PD"," "," "," "," ",1,24,24]
["CRESSY_1_PARKER",null,"PARKER POWERHOUSE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,2.83,null,null,"FC"," "," "," "," ",1,24,24]
["CRESTA_7_PL1X2",null,"CRESTA PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,70.400000000000006,null,null,"FC"," "," "," "," ",1,24,24]
["CRIMSN_2_CRMBT1",null,"Crimson",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,1,200,1,null,"ID",1,0.8,800,800,1,24,4]
["CRIMSN_2_CRMBT2",null,"Crimson 2",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,1,150,1,null,"ID",1,0.8,600,600,1,24,4]
["CRNEVL_6_CRNVA",null,"Crane Valley ",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,null,0.9,null,null,"FC"," "," "," "," ",1,24,24]
["CRNEVL_6_SJQN 2",null,"SAN JOAQUIN 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,null,3.2,null,null,"FC"," "," "," "," ",1,24,24]
["CROKET_7_UNIT",null,"CROCKETT COGEN",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,null,240,null,null,"FC"," "," "," "," ",1,24,24]
["CRSTWD_6_KUMYAY",null,"Kumeyaay Wind Farm",null,"WIND","Wind","WIND","CISO","South","San Diego-IV","San Diego",null,null,50,null,null,"FC"," "," "," "," ",1,24,24]
["CRWCKS_1_SOLAR1",null,"Crow Creek Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,null,20,null,null,"EO"," "," "," "," ",1,24,24]
["CSCCOG_1_UNIT 1",null,"SANTA CLARA CO-GEN",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,7,null,null,"FC"," "," "," "," ",1,24,24]
["CSCGNR_1_UNIT 1",null,"GIANERA PEAKER UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,24.75,null,null,"FC"," "," "," "," ",1,24,24]
["CSCGNR_1_UNIT 2",null,"GIANERA PEAKER UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,24.75,null,null,"FC"," "," "," "," ",1,24,24]
["CSLR4S_2_SOLAR",null,"Csolar IV South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,null,130,null,null,"FC"," "," "," "," ",1,24,24]
["CSTOGA_6_LNDFIL",null,"Clover Flat Land Fill Gas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB","Fulton",null,null,0.85,null,null,"EO"," "," "," "," ",1,24,24]
["CSTRVL_7_PL1X2",null,"Marina Land Fill Gas",null,"RECIPROCATING ENGINE","Biogas","OTHER","CISO","North","CAISO System",null,null,1,4.53,null,null,"FC"," "," "," "," ",1,24,24]
["CSTRVL_7_QFUNTS",null,"Castroville QF Aggregate",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24,24]
["CTNWDP_1_QF",null,"SMALL QF AGGREGATION - BURNEY",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.5,null,null,"FC"," "," "," "," ",1,24,24]
["CUMBIA_1_SOLAR",null,"Columbia Solar Energy II",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area","Pittsburg",null,null,19,null,null,"FC"," "," "," "," ",1,24,24]
["CUMMNG_6_SUNCT1",null,"SunSelect 1",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","CAISO System",null,null,1,4,null,null,"FC"," "," "," "," ",1,24,24]
["CURTIS_1_CANLCK",null,"Canal Creek Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,0.9,null,null,"FC"," "," "," "," ",1,24,24]
["CURTIS_1_FARFLD",null,"Fairfield Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,0.9,null,null,"FC"," "," "," "," ",1,24,24]
["CUYAMS_6_CUYSR1",null,"Cuyama Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,40,null,null,"FC"," "," "," "," ",1,24,24]
["DAIRLD_1_MD1SL1",null,"Madera 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["DAIRLD_1_MD2BM1",null,"Madera Digester Genset 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,null,null,0.8,null,null,"EO"," "," "," "," ",1,24,24]
["DAVIS_1_SOLAR1",null,"Grasslands 3",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,1,null,null,"EO"," "," "," "," ",1,24,24]
["DAVIS_1_SOLAR2",null,"Grasslands 4",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,1,null,null,"EO"," "," "," "," ",1,24,24]
["DAVIS_7_MNMETH",null,"MM Yolo Power LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,4,null,null,"FC"," "," "," "," ",1,24,24]
["DEADCK_1_UNIT",null,"DEADCK_1_UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,null,1.96,null,null,"FC"," "," "," "," ",1,24,24]
["DEERCR_6_UNIT 1",null,"DEER CREEK",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,7,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR1",null,"Golden Springs Building H",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,1.5,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR2",null,"Golden Springs Building M",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,1.75,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR3",null,"Golden Springs Building G",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,1.25,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR4",null,"Golden Springs Building F",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,1.3,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR5",null,"Golden Springs Building L",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,1,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLAR6",null,"Freeway Springs",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,null,2,null,null,"FC"," "," "," "," ",1,24,24]
["DELAMO_2_SOLRC1",null,"Golden Springs Building C1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,null,1.1599999999999999,null,null,"EO"," "," "," "," ",1,24,24]
["DELAMO_2_SOLRD",null,"Golden Solar Building D",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,null,1.25,null,null,"EO"," "," "," "," ",1,24,24]
["DELSUR_6_BSOLAR",null,"Central Antelope Dry Ranch B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24,24]
["DELSUR_6_CREST",null,"Delsur Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,null,10,null,null,"EO"," "," "," "," ",1,24,24]
["DELSUR_6_DRYFRB",null,"Dry Farm Ranch B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,5,null,null,"FC"," "," "," "," ",1,24,24]
["DELSUR_6_SOLAR1",null,"Summer Solar North ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,6.5,null,null,"FC"," "," "," "," ",1,24,24]
["DELSUR_6_SOLAR4",null,"Radiance Solar 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["DELSUR_6_SOLAR5",null,"Radiance Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24,24]
["DELTA_2_PL1X4",null,"DELTA ENERGY CENTER AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,1,880,null,null,"FC"," "," "," "," ",1,24,24]
["DEVERS_1_SEPV05",null,"SEPV 5",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,2,null,null,"EO"," "," "," "," ",1,24,24]
["DEVERS_1_SOLAR",null,"Cascade Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,18.5,null,null,"EO"," "," "," "," ",1,24,24]
["DEVERS_1_SOLAR1",null,"SEPV8",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,12,null,null,"EO"," "," "," "," ",1,24,24]
["DEVERS_1_SOLAR2",null,"SEPV9",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,9,null,null,"EO"," "," "," "," ",1,24,24]
["DEVERS_2_CS2SR4",null,"Caliente Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,0.91,null,null,"EO"," "," "," "," ",1,24,24]
["DEVERS_2_DHSPG2",null,"Desert Hot Springs 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,1.4,null,null,"EO"," "," "," "," ",1,24,24]
["DEXZEL_1_UNIT",null,"Western Power and Steam Cogeneration",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,null,20,null,null,"FC"," "," "," "," ",1,24,24]
["DIABLO_7_UNIT 1",null,"Diablo Canyon Unit 1",null,"STEAM","Nuclear","URANIUM","CISO","North","CAISO System",null,null,null,1150,null,null,"FC"," "," "," "," ",1,24,24]
["DIABLO_7_UNIT 2",null,"Diablo Canyon Unit 2",null,"STEAM","Nuclear","URANIUM","CISO","North","CAISO System",null,null,null,1150,null,null,"FC"," "," "," "," ",1,24,24]
["DISCOV_1_CHEVRN",null,"CHEVRON USA (EASTRIDGE)",null,"FTUR","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,null,48.8,null,null,"FC"," "," "," "," ",1,24,24]
["DIXNLD_1_LNDFL",null,"Zero Waste Energy",null,"RECIPROCATING ENGINE","Biomass","BIOMASS","CISO","North","Bay Area",null,null,null,1.6,null,null,"FC"," "," "," "," ",1,24,24]
["DMDVLY_1_UNITS",null,"DIAMOND VALLEY LAKE PUMP-GEN PLANT",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,21,null,null,"FC"," "," "," "," ",1,24,24]
["DONNLS_7_UNIT",null,"Donnells Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,1,72,null,null,"FC"," "," "," "," ",1,24,24]
["DOSMGO_2_NSPIN",null,"DOSMGO_2_NSPIN",null,"PUMP","Pump","WATER","CISO","North","CAISO System",null,null,null,159,null,null,"FC"," "," "," "," ",1,24,24]
["DOUBLC_1_UNITS",null,"DOUBLE \"C\" LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",null,1,52.23,null,null,"FC"," "," "," "," ",1,24,24]
["DRACKR_2_D4SR4B",null,"Dracker Solar Unit 4B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,62.5,null,null,"FC"," "," "," "," ",1,24,24]
["DRACKR_2_DS3SR3",null,"Dracker Solar Unit 3","DRACKR_2_DSUBT3","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,115,null,125,null,null,"EO"," "," "," "," ",1,24,24]
["DRACKR_2_DS4SR4",null,"Dracker Solar Unit 4A","DRACKR_2_DSUBT4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,53.01,null,62.5,null,null,"FC"," "," "," "," ",1,24,24]
["DRACKR_2_DSUBT1",null,"Dracker Solar Unit 1 BESS","DRACKR_2_SOLAR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,74.97,3,63,null,null,"FC",1,0.8,252,252,1,24,4]
["DRACKR_2_DSUBT2",null,"Dracker Solar Unit 2 BESS","DRACKR_2_SOLAR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,115,1,115,null,null,"FC",2.84,0.9,460,1308,1,24,11.38]
["DRACKR_2_DSUBT3",null,"Dracker Solar Unit 3 BESS","DRACKR_2_DS3SR3","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,115,1,115,null,null,"FC",2.85,0.9,460,1310,1,24,11.39]
["DRACKR_2_DSUBT4",null,"Dracker Solar Unit 4 BESS","DRACKR_2_DS4SR4","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,53.01,3,47,1,null,"ID",1,0.8,188,188,1,24,4]
["DRACKR_2_SOLAR1",null,"Dracker Solar Unit 1","DRACKR_2_DSUBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,74.97,null,110,null,null,"FC"," "," "," "," ",1,24,24]
["DRACKR_2_SOLAR2",null,"Dracker Solar Unit 2","DRACKR_2_DSUBT2","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,115,null,125,null,null,"EO"," "," "," "," ",1,24,24]
["DREWS_6_PL1X4",null,"Drews Generating Plant",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,41.4,null,null,"FC"," "," "," "," ",1,24,24]
["DRUM_7_PL1X2",null,"Drum PH 1 Units 1 & 2 Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,26,null,null,"FC"," "," "," "," ",1,24,24]
["DRUM_7_PL3X4",null,"Drum PH 1 Units 3 & 4 Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,28.9,null,null,"FC"," "," "," "," ",1,24,24]
["DRUM_7_UNIT 5",null,"DRUM PH 2 UNIT 5",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,50,null,null,"FC"," "," "," "," ",1,24,24]
["DSABLA_7_UNIT",null,"De Sabla Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,18.5,null,null,"FC"," "," "," "," ",1,24,24]
["DSFLWR_2_WS2SR1",null,"Willow Springs 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,100,null,null,"FC"," "," "," "," ",1,24,24]
["DSFLWR_2_W9CSB1",null,"Willy 9 Chap 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,102,1,null,"ID",null,null,null,null,1,24,24]
["DSFLWR_2_W9CSB2",null,"Willy 9 Chap 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,72,1,null,"ID",null,null,null,null,1,24,24]
["DSRTHV_2_DH1SR1",null,"Desert Harvest",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,80,null,null,"FC"," "," "," "," ",1,24,24]
["DSRTHV_2_DH2BT1",null,"Desert Harvest BESS","DSRTHV_2_DH2SR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,38.92,1,35,null,35,"PD",1,0.8,140,140,1,24,4]
["DSRTHV_2_DH2SR2",null,"Desert Harvest 2","DSRTHV_2_DH2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,38.92,null,70,null,null,"FC"," "," "," "," ",1,24,24]
["DSRTSL_2_SOLAR1",null,"Desert Stateline",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,296.19,null,null,"FC"," "," "," "," ",1,24,24]
["DSRTSN_2_DS2X2",null,"Desert Sunlight PV II Storage","DSRTSN_2_SOLAR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,251.02,1,230,null,null,"FC",2.78,0.87,920,2560,1,24,11.13]
["DSRTSN_2_SOLAR1",null,"Desert Sunlight 300",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,300,null,null,"FC"," "," "," "," ",1,24,24]
["DSRTSN_2_SOLAR2",null,"Desert Sunlight 250","DSRTSN_2_DS2X2","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,251.02,null,250,null,null,"FC"," "," "," "," ",1,24,24]
["DTCHWD_2_BT3WND",null,"Brookfield Tehachapi 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,4.5,null,null,"FC"," "," "," "," ",1,24,24]
["DTCHWD_2_BT4WND",null,"Brookfield Tehachapi 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,6.52,null,null,"FC"," "," "," "," ",1,24,24]
["DUANE_1_PL1X3",null,"DONALD VON RAESFELD POWER PROJECT",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,147.80000000000001,null,null,"FC"," "," "," "," ",1,24,24]
["DUTCH1_7_UNIT 1",null,"DUTCH FLAT 1 PH",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1,22,null,null,"FC"," "," "," "," ",1,24,24]
["DUTCH2_7_UNIT 1",null,"DUTCH FLAT 2 PH",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,26,null,null,"FC"," "," "," "," ",1,24,24]
["DVLCYN_1_UNITS",null,"DEVIL CANYON HYDRO UNITS 1-4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,1,235,null,null,"FC"," "," "," "," ",1,24,24]
["DYERSM_6_DSWWD1",null,"Dyer Summit Wind Repower",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,44.8,null,null,"FC"," "," "," "," ",1,24,24]
["EASTWD_7_UNIT",null,"EASTWOOD PUMP-GEN",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,1,200,null,null,"FC"," "," "," "," ",1,24,24]
["EDMONS_2_NSPIN",null,"EDMONS_2_NSPIN",null,"PUMP","Pump","WATER","CISO","South","Big Creek-Ventura",null,null,null,775.8,null,null,"FC"," "," "," "," ",1,24,24]
["EDWARD_2_E21SB1","EDWARD_2_E21SB1_SUN","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,166,2,130,1,null,"ID"," "," "," "," ",1,24,24]
["EDWARD_2_E21SB1","EDWARD_2_E21SB1_LESR","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"CAISO System",null,166,2,71,null,null,null,1,0.8,284,284,1,24,4]
["EDWARD_2_E23SB1","EDWARD_2_E23SB1_SUN","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,24,2,24,1,null,"ID"," "," "," "," ",1,24,24]
["EDWARD_2_E23SB1","EDWARD_2_E23SB1_LESR","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"CAISO System",null,24,2,6,null,null,null,1,0.8,24,24,1,24,4]
["EDWARD_2_ES2BT3","EDWARD_2_ES2BT3_SUN","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,151,2,118,1,null,"ID"," "," "," "," ",1,24,24]
["EDWARD_2_ES2BT3","EDWARD_2_ES2BT3_LESR","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"CAISO System",null,151,2,66,null,null,null,1,0.8,264,264,1,24,4]
["EDWARD_2_ESSSB1",null,"Sanborn Solar 2 Edwards 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,116,0,0,"ID",null,null,null,null,1,24]
["EDWARD_2_ESSSB2",null,"Sanborn Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,132,0,0,"ID",null,null,null,null,1,24]
["EEKTMN_6_SOLAR1",null,"EE K Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["ELCAJN_6_EB1BT1",null,"Eastern BESS 1",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego, El Cajon",null,1,7.5,null,null,"FC",1,0.8,30,30,1,24]
["ELCAJN_6_LM6K",null,"El Cajon Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, El Cajon",null,1,48.1,null,null,"FC"," "," "," "," ",1,24]
["ELCAJN_6_UNITA1",null,"Cuyamaca Peak Energy Plant",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, El Cajon",null,1,45.42,null,null,"FC"," "," "," "," ",1,24]
["ELCAP_1_SOLAR",null,"2097 Helton",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["ELDORO_7_UNIT 1",null,"El Dorado Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,null,11,null,null,"FC"," "," "," "," ",1,24]
["ELDORO_7_UNIT 2",null,"El Dorado Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,null,11,null,null,"FC"," "," "," "," ",1,24]
["ELECTR_7_PL1X3",null,"ELECTRA PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,93,null,null,"FC"," "," "," "," ",1,24]
["ELKCRK_6_STONYG",null,"STONEY GORGE HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,4.9000000000000004,null,null,"FC"," "," "," "," ",1,24]
["ELKHIL_2_PL1X3",null,"ELK HILLS COMBINED CYCLE (AGGREGATE)",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,551.70000000000005,null,null,"FC"," "," "," "," ",1,24]
["ELKHRN_1_EESX3",null,"Elkhorn Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",null,1,182.5,null,null,"FC",1,0.8,730,730,1,24]
["ELLIS_2_QF",null,"ELLIS QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Western",null,null,12,null,null,"FC"," "," "," "," ",1,24]
["ELNIDP_6_BIOMAS",null,"El Nido Biomass to Energy",null,"STEAM","Biomass","BIOMASS","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,10.5,0.97,null,"FC"," "," "," "," ",1,24]
["ELSEGN_2_UN1011",null,"El Segundo Energy Center 5/6",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western, El Nido",null,1,274.31,null,null,"FC"," "," "," "," ",1,24]
["ELSEGN_2_UN2021",null,"El Segundo Energy Center 7/8",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western, El Nido",null,1,271.74,null,null,"FC"," "," "," "," ",1,24]
["ENERSJ_2_WIND",null,"ESJ Wind Energy",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,null,151,null,null,"FC"," "," "," "," ",1,24]
["ENERSJ_5_ESJWD2",null,"Energia Sierra Juarez Wind 2",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,null,105,null,null,"FC"," "," "," "," ",1,24]
["ENWIND_2_WIND1",null,"Cameron Ridge",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,47.1,null,null,"FC"," "," "," "," ",1,24]
["ENWIND_2_WIND2",null,"Ridgetop I",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,38.24,null,null,"FC"," "," "," "," ",1,24]
["ESCNDO_6_EB1BT1",null,"Escondido BESS 1",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,10,null,null,"FC",1,0.8,40,40,1,24]
["ESCNDO_6_EB2BT2",null,"Escondido BESS 2",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,10,null,null,"FC",1,0.8,40,40,1,24]
["ESCNDO_6_EB3BT3",null,"Escondido BESS 3",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,10,null,null,"FC",1,0.8,40,40,1,24]
["ESCNDO_6_PL1X2",null,"MMC Escondido Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,48.71,null,null,"FC"," "," "," "," ",1,24]
["ESCNDO_6_UNITB1",null,"CalPeak Power Enterprise Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,48.04,null,null,"FC"," "," "," "," ",1,24]
["ESCO_6_GLMQF",null,"Goal Line Cogen",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","San Diego-IV","San Diego",null,1,49.9,null,null,"FC"," "," "," "," ",1,24]
["ESNHWR_2_WC1BT1",null,"Wildcat I BESS",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern, Valley-Devers",null,3,3,1,null,"ID",1,0.8,6,6,1,24]
["ESQUON_6_LNDFIL",null,"Neal Road Landfill Generating Facility",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,2.1,null,null,"EO"," "," "," "," ",1,24]
["ESTWND_2_OPPWD1",null,"Oasis Power Plant Eastwind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,57.14,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_CHMPNE",null,"Champagne",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"EO"," "," "," "," ",1,24]
["ETIWND_2_FONTNA",null,"FONTANALYTLE CREEK POWERHOUSE P",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,2.56,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS010",null,"SPVP010 Fontana RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS015",null,"SPVP015",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,3,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS017",null,"SPVP017",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,3.5,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS018",null,"SPVP018 Fontana RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS023",null,"SPVP023 Fontana RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS026",null,"SPVP026",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,6,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_RTS027",null,"SPVP027",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,2,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_SOLAR1",null,"Dedeaux Ontario",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_2_SOLAR2",null,"Rochester",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"EO"," "," "," "," ",1,24]
["ETIWND_2_SOLAR5",null,"Dulles",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,2,null,null,"EO"," "," "," "," ",1,24]
["ETIWND_2_UNIT1",null,"ETIWND_2_UNIT1",null,"FTUR","CHP","NATURAL GAS","CISO","South","LA Basin","Eastern",null,null,33.6,null,null,"FC"," "," "," "," ",1,24]
["ETIWND_6_GRPLND",null,"Grapeland Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,45.64,null,null,"FC"," "," "," ",408,1,24]
["ETIWND_6_MWDETI",null,"ETIWANDA RECOVERY HYDRO",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,24,null,null,"FC"," "," "," "," ",1,24]
["EXCHEC_7_UNIT 1",null,"EXCHEQUER HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,1,94.5,0.97,null,"FC"," "," "," "," ",1,24]
["EXCLSG_1_SOLAR",null,"Excelsior Solar ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,null,60,null,null,"FC"," "," "," "," ",1,24]
["FALBRK_6_FESBT1",null,"Fallbrook Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV",null,null,1,40,null,null,"FC",1,0.8,160,160,1,24]
["FELLOW_7_QFUNTS",null,"Fellow QF Aggregate",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,6.2,null,null,"FC"," "," "," "," ",1,24]
["FIFTHS_2_FSSBT",null,"Fifth Standard Solar BESS",null,"OTHER","Battery Storage","LESR","CISO","North","CAISO System",null,null,null,137,null,null,"FC",1,0.8,548,548,1,24]
["FLOWD2_2_FPLWND",null,"DIABLO WINDS",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,18,null,null,"FC"," "," "," "," ",1,24]
["FLOWD_2_RT2WD2",null,"Ridgetop 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,27.39,null,null,"FC"," "," "," "," ",1,24]
["FLOWD_2_WIND1",null,"Cameron Ridge 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,11.9,null,null,"FC"," "," "," "," ",1,24]
["FMEADO_6_HELLHL",null,"FMEADO_6_HELLHL",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,null,0.6,null,null,"FC"," "," "," "," ",1,24]
["FMEADO_7_UNIT",null,"FRENCH MEADOWS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,1,16,null,null,"FC"," "," "," "," ",1,24]
["FORBST_7_UNIT 1",null,"FORBESTOWN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,1,37.5,null,null,"FC"," "," "," "," ",1,24]
["FRESHW_1_SOLAR1",null,"Corcoran 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,null,20,null,null,"EO"," "," "," "," ",1,24]
["FRIANT_6_UNITS",null,"FRIANT DAM",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,null,25,null,null,"FC"," "," "," "," ",1,24]
["FRITO_1_LAY",null,"FRITO-LAY",null,"FTUR","CHP","NATURAL GAS",null,"North","CAISO System",null,null,null,6,null,null,"FC"," "," "," "," ",1,24]
["FRNTBW_6_SOLAR1",null,"Frontier Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["FROGTN_1_UTICAA",null,"Angels Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,1.4,null,null,"FC"," "," "," "," ",1,24]
["FROGTN_1_UTICAM",null,"Murphys Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,3.6,null,null,"FC"," "," "," "," ",1,24]
["FTSWRD_6_TRFORK",null,"Three Forks Water Power Project",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,null,1.63,0.8,null,"PD"," "," "," "," ",1,24]
["FTSWRD_7_QFUNTS",null,"FTSWRD_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,null,1.6,null,null,"FC"," "," "," "," ",1,24]
["FULTON_1_QF",null,"SMALL QF AGGREGATION - ZENIA",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["GALE_1_SR3SR3",null,"Sunray 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,13.8,null,null,"FC"," "," "," "," ",1,24]
["GANSO_1_WSTBM1",null,"Weststar Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1,null,null,"EO"," "," "," "," ",1,24]
["GARLND_2_GARBT1",null,"Garland B BESS","GARLND_2_GASLR, GARLND_2_GASLRA","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,109.58,1,88,null,null,"FC",2.76,0.85,352,971,1,24]
["GARLND_2_GASLR",null,"Garland B","GARLND_2_GARBT1, GARLND_2_GASLRA","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,109.58,null,180,null,null,"FC"," "," "," "," ",1,24]
["GARLND_2_GASLRA",null,"Garland A","GARLND_2_GARBT1, GARLND_2_GASLR","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,109.58,null,20,null,null,"FC"," "," "," "," ",1,24]
["GARNET_1_SOLAR",null,"North Palm Springs 4A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,4,null,null,"EO"," "," "," "," ",1,24]
["GARNET_1_SOLAR2",null,"Garnet Solar Power Generation Station 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,4,null,null,"FC"," "," "," "," ",1,24]
["GARNET_1_WIND",null,"GARNET WIND ENERGY CENTER",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,6.5,null,null,"FC"," "," "," "," ",1,24]
["GARNET_1_WINDS",null,"Garnet Winds Aggregation",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,22.5,null,null,"FC"," "," "," "," ",1,24]
["GARNET_1_WT3WND",null,"Wagner Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,6,null,null,"EO"," "," "," "," ",1,24]
["GARNET_2_COAWD2",null,"Coachella 2",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,10.8,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_HYDRO",null,"Whitewater Hydro",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_WIND1",null,"Phoenix",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,11.2,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_WIND2",null,"Karen Avenue Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,11.7,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_WIND3",null,"San Gorgonio East",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,12.6,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_WIND4",null,"Windustries",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,9.8000000000000007,null,null,"FC"," "," "," "," ",1,24]
["GARNET_2_WIND5",null,"Eastwind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,3,null,null,"FC"," "," "," "," ",1,24]
["GASKW1_2_GW1SR1",null,"Gaskell West 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["GASKW1_2_GW2SR1",null,"Gaskell West 2a",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,16,1,null,"ID"," "," "," "," ",1,24]
["GASKW1_2_GW2SR2",null,"Gaskell West 2b",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,29,1,null,"ID"," "," "," "," ",1,24]
["GASKW1_2_GW3SR1",null,"Gaskell West 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,1,null,"ID"," "," "," "," ",1,24]
["GASKW1_2_GW4SR1",null,"Gaskell West 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,1,null,"ID"," "," "," "," ",1,24]
["GASKW1_2_GW5SR1",null,"Gaskell West 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,1,null,"ID"," "," "," "," ",1,24]
["GATES_2_SOLAR",null,"Gates Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["GATES_2_WSOLAR",null,"West Gates Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,10,null,null,"FC"," "," "," "," ",1,24]
["GATEWY_2_GESBT1",null,"Gateway Energy Stroage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,250,null,null,"FC",1,0.8,1000,1000,1,24]
["GATWAY_2_PL1X3",null,"GATEWAY GENERATING STATION",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,585,null,null,"FC"," "," "," "," ",1,24]
["GENESI_2_STG",null,"Genesis Station","BLKCRK_2_GMCBT1, BLKCRK_2_SOLAR1","STEAM","Paired_Solar_Thermal","SUN","CISO","South","CAISO System",null,258.91000000000003,null,250,null,null,"FC"," "," "," "," ",1,24]
["GEYS11_7_UNIT11",null,"GEYSERS UNIT 11 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",null,1,86.8,null,null,"FC"," "," "," "," ",1,24]
["GEYS12_7_UNIT12",null,"GEYSERS UNIT 12 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,1,57,null,null,"FC"," "," "," "," ",1,24]
["GEYS13_7_UNIT13",null,"GEYSERS UNIT 13 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,73,null,null,"FC"," "," "," "," ",1,24]
["GEYS14_7_UNIT14",null,"GEYSERS UNIT 14 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,1,70,null,null,"FC"," "," "," "," ",1,24]
["GEYS16_7_UNIT16",null,"GEYSERS UNIT 16 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,1,63,null,null,"FC"," "," "," "," ",1,24]
["GEYS17_7_UNIT17",null,"GEYSERS UNIT 17 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,1,75.5,null,null,"FC"," "," "," "," ",1,24]
["GEYS18_7_UNIT18",null,"GEYSERS UNIT 18 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,72,null,null,"FC"," "," "," "," ",1,24]
["GEYS20_7_UNIT20",null,"GEYSERS UNIT 20 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,50,null,null,"FC"," "," "," "," ",1,24]
["GIFENS_6_BUGSL1",null,"Burford Giffen",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["GIFFEN_6_SOLAR",null,"Giffen Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,null,10,null,null,"FC"," "," "," "," ",1,24]
["GIFFEN_6_SOLAR1",null,"Aspiration Solar G",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,null,9,null,null,"EO"," "," "," "," ",1,24]
["GILROY_1_UNIT",null,"GILROY COGEN AGGREGATE",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",null,1,120,null,null,"FC"," "," "," "," ",1,24]
["GILRPP_1_PL1X2",null,"GILROY ENERGY CENTER UNITS 1&2 AGGREGATE",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",null,1,95.2,null,null,"FC"," "," "," "," ",1,24]
["GILRPP_1_PL3X4",null,"GILROY ENERGY CENTER, UNIT #3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",null,1,46.2,null,null,"FC"," "," "," "," ",1,24]
["GLDFGR_6_SOLAR1",null,"Portal Ridge B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["GLDFGR_6_SOLAR2",null,"Portal Ridge C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,11.4,null,null,"FC"," "," "," "," ",1,24]
["GLDTWN_6_COLUM3",null,"Columbia 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,10,null,null,"FC"," "," "," "," ",1,24]
["GLDTWN_6_SOLAR",null,"Rio Grande",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,5,null,null,"FC"," "," "," "," ",1,24]
["GLNARM_2_UNIT 5",null,"Glenarm Turbine 5",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",null,1,65.81,null,65,"PD"," "," "," "," ",1,24]
["GLNARM_7_UNIT 1",null,"GLEN ARM UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,22.13,null,null,"FC"," "," "," "," ",1,24]
["GLNARM_7_UNIT 2",null,"GLEN ARM UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,22.38,null,null,"FC"," "," "," "," ",1,24]
["GLNARM_7_UNIT 3",null,"GLEN ARM UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,44.83,null,null,"FC"," "," "," "," ",1,24]
["GLNARM_7_UNIT 4",null,"GLEN ARM UNIT 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,42.42,null,null,"FC"," "," "," "," ",1,24]
["GLOW_6_SOLAR",null,"Antelope Power Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["GOLETA_2_QF",null,"GOLETA QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,null,0.25,null,null,"FC"," "," "," "," ",1,24]
["GOLETA_2_VALBT1",null,"Vallecito Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,3,10,null,null,"FC",1,0.8,40,40,1,24]
["GOLETA_6_ELLWOD",null,"ELLWOOD ENERGY SUPPORT FACILITY",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,1,54,null,null,"FC"," "," "," "," ",1,24]
["GOLETA_6_EXGEN",null,"EXXON COMPANY USA",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,null,48.2,null,null,"FC"," "," "," "," ",1,24]
["GONZLS_6_UNIT",null,"Johnson Canyon Landfill",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1.42,null,null,"FC"," "," "," "," ",1,24]
["GOOSLK_1_SOLAR1",null,"Goose Lake",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,12,null,null,"FC"," "," "," "," ",1,24]
["GRIDLY_6_SOLAR",null,"GRIDLEY MAIN TWO",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Sierra","Pease",null,null,2.5,null,null,"EO"," "," "," "," ",1,24]
["GRIZLY_1_UNIT 1",null,"GRIZZLY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,20,null,null,"FC"," "," "," "," ",1,24]
["GRNLF2_1_UNIT",null,"GREENLEAF II COGEN",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",null,1,49.2,null,null,"FC"," "," "," "," ",1,24]
["GRNVLY_7_SCLAND",null,"SANTA CRUZ LANDFILL GENERATING PLANT",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,3.04,null,null,"FC"," "," "," "," ",1,24]
["GRSCRK_6_BGCKWW",null,"BIG CREEK WATER WORKS - CEDAR FLAT",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,5,null,null,"FC"," "," "," "," ",1,24]
["GRZZLY_1_BERKLY",null,"Berkeley Cogeneration",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","Bay Area",null,null,null,26.35,null,null,"FC"," "," "," "," ",1,24]
["GUERNS_6_HD3BM3",null,"Hanford Digester Genset 3",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,null,null,1,null,null,"EO"," "," "," "," ",1,24]
["GUERNS_6_SOLAR",null,"Guernsey Solar Station",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["GUERNS_6_VH2BM1",null,"Hanford Digester Genset 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,null,null,1,null,null,"EO"," "," "," "," ",1,24]
["GWFPWR_1_UNITS",null,"Hanford Peaker Plant",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Hanford",null,1,98.46,null,null,"FC"," "," "," "," ",1,24]
["GYS5X6_7_UNITS",null,"GEYSERS UNITS 5 & 6 AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",null,1,98.43,null,null,"FC"," "," "," "," ",1,24]
["GYS7X8_7_UNITS",null,"GEYSERS UNITS 7 & 8 AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",null,1,95.8,null,null,"FC"," "," "," "," ",1,24]
["GYSRVL_7_WSPRNG",null,"Warm Springs Hydro",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,null,3.75,null,null,"FC"," "," "," "," ",1,24]
["HAASPH_7_PL1X2",null,"HAAS PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,1,144,null,null,"FC"," "," "," "," ",1,24]
["HALSEY_6_UNIT",null,"HALSEY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1,13.5,null,null,"FC"," "," "," "," ",1,24]
["HARBGN_7_UNITS",null,"HARBOR COGEN COMBINED CYCLE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",null,1,109.01,null,null,"FC"," "," "," "," ",1,24]
["HARDWK_6_STWBM1",null,"Still Water Ranch Dairy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,null,null,1,null,null,"EO"," "," "," "," ",1,24]
["HATCR1_7_UNIT",null,"Hat Creek  #1 ",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,8.5,null,null,"FC"," "," "," "," ",1,24]
["HATCR2_7_UNIT",null,"Hat Creek  #2  ",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,8.5,null,null,"FC"," "," "," "," ",1,24]
["HATLOS_6_BWDHY1",null,"Bidwell Ditch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["HATLOS_6_LSCRK",null,"Lost Creek 1 & 2 Hydro Conversion",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.7,null,null,"FC"," "," "," "," ",1,24]
["HATRDG_2_WIND",null,"Hatchet Ridge Wind Farm",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,102,null,null,"FC"," "," "," "," ",1,24]
["HAYPRS_6_HAYHD1",null,"Haypress Lower",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,5.8,null,null,"FC"," "," "," "," ",1,24]
["HAYPRS_6_HAYHD2",null,"Haypress Middle",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,6.7,null,null,"FC"," "," "," "," ",1,24]
["HELMPG_7_UNIT 1",null,"HELMS PUMP-GEN UNIT 1",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,null,1,407,null,null,"FC"," "," "," "," ",1,24]
["HELMPG_7_UNIT 2",null,"HELMS PUMP-GEN UNIT 2",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,null,1,407,null,null,"FC"," "," "," "," ",1,24]
["HELMPG_7_UNIT 3",null,"HELMS PUMP-GEN UNIT 3",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,null,1,404,null,null,"FC"," "," "," "," ",1,24]
["HENRTA_6_HDEBT1",null,"Henrietta D Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Fresno",null,null,2,10,1,null,"ID",1,0.8,40,40,1,24]
["HENRTA_6_SOLAR1",null,"Lemoore 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,1,null,"ID"," "," "," "," ",1,24]
["HENRTA_6_SOLAR2",null,"Westside Solar Power PV1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,2,null,null,"EO"," "," "," "," ",1,24]
["HENRTA_6_UNITA1",null,"GWF HENRIETTA PEAKER PLANT UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno",null,null,1,49.98,null,null,"FC"," "," "," "," ",1,24]
["HENRTA_6_UNITA2",null,"GWF HENRIETTA PEAKER PLANT UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno",null,null,1,49.42,null,null,"FC"," "," "," "," ",1,24]
["HENRTS_1_SOLAR",null,"Henrietta Solar Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,null,100,null,null,"FC"," "," "," "," ",1,24]
["HERDLN_6_BYHSR1",null,"Byron Highway Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,5,null,null,"EO",null,null,null,null,1,24]
["HIDSRT_2_UNITS",null,"HIGH DESERT POWER PROJECT AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,null,1,850,null,null,"FC"," "," "," "," ",1,24]
["HIGGNS_1_COMBIE",null,"Combie South",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["HIGGNS_7_QFUNTS",null,"HIGGNS_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,0.5,null,null,"FC"," "," "," "," ",1,24]
["HIGHDS_2_H5SBT1",null,"High 5 Solar BESS","HIGHDS_2_H5SSR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,61.14,2,50,null,null,"FC",1,0.8,200,200,1,24]
["HIGHDS_2_H5SSR1",null,"High 5 Solar","HIGHDS_2_H5SBT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,61.14,null,100,null,null,"FC"," "," "," "," ",1,24]
["HILAND_7_YOLOWD",null,"CLEAR LAKE UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,null,3.75,null,null,"EO"," "," "," "," ",1,24]
["HINSON_6_LBECH1",null,"Long Beach Unit 1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,63,null,null,"FC"," "," "," "," ",1,24]
["HINSON_6_LBECH2",null,"Long Beach Unit 2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,63,null,null,"FC"," "," "," "," ",1,24]
["HINSON_6_LBECH3",null,"Long Beach Unit 3",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,63,null,null,"FC"," "," "," "," ",1,24]
["HINSON_6_LBECH4",null,"Long Beach Unit 4",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,63,null,null,"FC"," "," "," "," ",1,24]
["HINSON_6_SERRGN",null,"Southeast Resource Recovery",null,"STEAM","CHP","WASTE TO POWER","CISO","South","LA Basin","Western",null,null,34,null,null,"FC"," "," "," "," ",1,24]
["HNTGBH_2_PL1X3",null,"Huntington Beach Energy",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",null,1,673.8,null,null,"FC"," "," "," "," ",1,24]
["HNTGBH_7_UNIT 2",null,"HUNTINGTON BEACH GEN STA. UNIT 2",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,226.84,null,null,"FC"," "," "," "," ",1,24]
["HOLGAT_1_BORAX",null,"U.S. Borax, Unit 1",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","CAISO System",null,null,null,48.2,null,null,"FC"," "," "," "," ",1,24]
["HOLSTR_1_SOLAR",null,"San Benito Smart Park",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["HOLSTR_1_SOLAR2",null,"Hollister Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["HUMBPP_1_UNITS3",null,"Humboldt Bay Generating Station 3",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Humboldt",null,null,1,65.08,null,null,"FC"," "," "," "," ",1,24]
["HUMBPP_6_UNITS",null,"Humboldt Bay Generating Station 1",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Humboldt",null,null,1,97.62,null,null,"FC"," "," "," "," ",1,24]
["HURON_6_SOLAR",null,"Huron Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["HYTTHM_2_UNITS",null,"HYATT-THERMALITO PUMP-GEN (AGGREGATE)",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,933.1,null,null,"FC"," "," "," "," ",1,24]
["IGNACO_1_QF",null,"SMALL QF AGGREGATION - VALLEJO/DINSMORE",null,"OTHER","CHP","OTHER","CISO","North","NCNB",null,null,null,0.5,null,null,"FC"," "," "," "," ",1,24]
["INDIGO_1_UNIT 1",null,"INDIGO PEAKER UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,45.3,null,null,"FC"," "," "," "," ",1,24]
["INDIGO_1_UNIT 2",null,"INDIGO PEAKER UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,45.3,null,null,"FC"," "," "," "," ",1,24]
["INDIGO_1_UNIT 3",null,"INDIGO PEAKER UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,45.3,null,null,"FC"," "," "," "," ",1,24]
["INDVLY_1_UNITS",null,"Indian Valley Hydro",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,null,3.01,null,null,"FC"," "," "," "," ",1,24]
["INTKEP_2_UNITS",null,"CCSF Hetch_Hetchy Hydro Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,405,null,null,"FC"," "," "," "," ",1,24]
["INTTRB_6_UNIT",null,"International Turbine Research",null,"WIND","Wind","WIND","CISO","North","Fresno",null,null,null,18.399999999999999,null,null,"FC"," "," "," "," ",1,24]
["IVANPA_1_UNIT1",null,"Ivanpah 1",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,null,126,null,null,"FC"," "," "," "," ",1,24]
["IVANPA_1_UNIT2",null,"Ivanpah 2",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,null,133,null,null,"FC"," "," "," "," ",1,24]
["IVANPA_1_UNIT3",null,"Ivanpah 3",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,null,133,null,null,"FC"," "," "," "," ",1,24]
["IVSLR2_2_SM2SR1",null,"Silver Ridge Mount Signal 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,null,150,null,null,"FC"," "," "," "," ",1,24]
["IVSLRP_2_SOLAR1",null,"Silver Ridge Mount Signal",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,null,200,null,null,"FC"," "," "," "," ",1,24]
["IVWEST_2_SOLAR1",null,"Imperial Valley West ( Q # 608) ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,null,150,null,null,"FC"," "," "," "," ",1,24]
["JACMSR_1_JACSR1",null,"Jacumba Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["JAVASR_1_JAVSR1",null,"Java Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,13.5,1,null,"ID"," "," "," "," ",1,24]
["JAWBNE_2_NSRWND",null,"North Sky River Wind Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,160,null,null,"FC"," "," "," "," ",1,24]
["JAWBNE_2_SRWND",null,"Sky River Wind Repower A",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,30,null,null,"FC"," "," "," "," ",1,24]
["JAWBNE_2_SRWWD2",null,"Sky River Wind Repower B",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,30.2,null,null,"FC"," "," "," "," ",1,24]
["JAYNE_6_WLSLR",null,"Westlands Solar Farm PV 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,null,18,null,null,"EO"," "," "," "," ",1,24]
["JOANEC_2_ST3BT3",null,"Santa Ana Storage 3",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,null,null,40,null,null,"FC",1,0.8,160,160,1,24]
["JOANEC_2_STABT1",null,"Santa Ana Storage 1",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,2,20,null,null,"FC",1,0.8,80,80,1,24]
["JOANEC_2_STABT2",null,"Santa Ana Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,1,20,null,null,"FC",1,0.8,80,80,1,24]
["JOHANN_2_JOSBT1",null,"Johanna Storage 1",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,3,10,null,null,"FC",1,0.8,40,40,1,24]
["JOHANN_2_JOSBT2",null,"Johanna Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,2,10,null,null,"FC",1,0.8,40,40,1,24]
["JOHANN_2_OCEBT2",null,"Orange County Energy Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,3,9,null,null,"FC",1,0.8,36,36,1,24]
["JOHANN_2_OCEBT3",null,"Orange County Energy Storage 3",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,3,6,null,null,"FC",1,0.8,24,24,1,24]
["KANSAS_6_SOLAR",null,"RE Kansas South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["KEARNY_6_NESBT1",null,"Kearny North Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,10,null,null,"FC",1,0.8,40,40,1,24]
["KEARNY_6_SESBT2",null,"Kearny South Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,10,null,null,"FC",1,0.8,40,40,1,24]
["KEKAWK_6_UNIT",null,"STS HYDROPOWER LTD. (KEKAWAKA)",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,null,5.5,null,null,"FC"," "," "," "," ",1,24]
["KELSO_2_UNITS",null,"Mariposa Energy",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,198.03,null,null,"FC"," "," "," "," ",1,24]
["KELYRG_6_UNIT",null,"KELLY RIDGE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,1,11,null,null,"FC"," "," "," "," ",1,24]
["KERKH2_7_UNIT 1",null,"KERKHOFF PH 2 UNIT #1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon, Wilson 115 kV",null,1,153.9,null,null,"FC"," "," "," "," ",1,24]
["KERMAN_6_SOLAR1",null,"Fresno Solar South",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["KERMAN_6_SOLAR2",null,"Fresno Solar West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["KERNFT_1_UNITS",null,"KERN FRONT LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",null,1,52.4,null,null,"FC"," "," "," "," ",1,24]
["KERNRG_1_UNITS",null,"South Belridge Cogen Facility",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,null,55.2,null,null,"FC"," "," "," "," ",1,24]
["KERRGN_1_UNIT 1",null,"KERN RIVER HYDRO UNITS 1-4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,null,25.6,null,null,"FC"," "," "," "," ",1,24]
["KINGCO_1_KINGBR",null,"Kingsburg Cogen",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Hanford",null,1,34.5,null,null,"FC"," "," "," "," ",1,24]
["KINGRV_7_UNIT 1",null,"KINGS RIVER HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon, Reedley",null,1,51.2,null,null,"FC"," "," "," "," ",1,24]
["KIRKER_7_KELCYN",null,"KELLER CANYON LANDFILL GEN FACILICITY",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Pittsburg",null,null,3.56,null,null,"FC"," "," "," "," ",1,24]
["KNGBRD_2_SOLAR1",null,"Kingbird Solar A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["KNGBRD_2_SOLAR2",null,"Kingbird Solar B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["KNGBRG_1_KBSLR1",null,"Kingsburg1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["KNGBRG_1_KBSLR2",null,"Kingsburg2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["KNGCTY_6_UNITA1",null,"King City Energy Center, Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,44.6,null,null,"FC"," "," "," "," ",1,24]
["KNTSTH_6_SOLAR",null,"Kent South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["KRAMER_2_SEGS 9",null,"Kramer Junction 9",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,null,80,null,null,"FC"," "," "," "," ",1,24]
["KRNCNY_6_UNIT",null,"KERN CANYON POWERHOUSE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,10.6,null,null,"FC"," "," "," "," ",1,24]
["KYCORA_6_KMSBT1",null,"Kearny Mesa Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,null,1,null,null,"EO",1,0.8,4,4,1,24]
["LACIEN_2_VENICE",null,"MWD Venice Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western, El Nido",null,null,9.9499999999999993,null,null,"FC"," "," "," "," ",1,24]
["LAKHDG_6_UNIT 1",null,"Lake Hodges Pumped Storage-Unit1",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","San Diego-IV","San Diego",null,1,20,null,null,"FC"," "," "," "," ",1,24]
["LAKHDG_6_UNIT 2",null,"Lake Hodges Pumped Storage-Unit2",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","San Diego-IV","San Diego",null,1,20,null,null,"FC"," "," "," "," ",1,24]
["LAMONT_1_SOLAR1",null,"Regulus Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,null,60,null,null,"FC"," "," "," "," ",1,24]
["LAMONT_1_SOLAR2",null,"Redwood Solar Farm 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["LAMONT_1_SOLAR3",null,"Woodmere Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,null,14.99,null,null,"FC"," "," "," "," ",1,24]
["LAMONT_1_SOLAR4",null,"Hayworth Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,null,26.66,null,null,"FC"," "," "," "," ",1,24]
["LAMONT_1_SOLAR5",null,"Redcrest Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,null,16.66,null,null,"FC"," "," "," "," ",1,24]
["LAPLMA_2_UNIT 1",null,"La Paloma Generating Plant Unit #1",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,267,null,null,"FC"," "," "," "," ",1,24]
["LAPLMA_2_UNIT 2",null,"La Paloma Generating Plant Unit #2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,266,null,null,"FC"," "," "," "," ",1,24]
["LAPLMA_2_UNIT 3",null,"La Paloma Generating Plant Unit #3",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,266,null,null,"FC"," "," "," "," ",1,24]
["LAPLMA_2_UNIT 4",null,"LA PALOMA GENERATING PLANT, UNIT #4",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,267,null,null,"FC"," "," "," "," ",1,24]
["LARKSP_6_UNIT 1",null,"LARKSPUR PEAKER UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",null,1,49,null,null,"FC"," "," "," "," ",1,24]
["LARKSP_6_UNIT 2",null,"LARKSPUR PEAKER UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",null,1,49,null,null,"FC"," "," "," "," ",1,24]
["LAROA2_2_UNITA1",null,"LR2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV",null,null,1,322,null,null,"FC"," "," "," "," ",1,24]
["LASSEN_6_UNITS",null,"Honey Lake Power",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,1,30,null,null,"FC"," "," "," "," ",1,24]
["LAWRNC_7_SUNYVL",null,"City of Sunnyvale Unit 1 and 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area",null,null,null,0.3,null,null,"FC"," "," "," "," ",1,24]
["LEBECS_2_UNITS",null,"Pastoria Energy Facility",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,799.47,null,null,"FC"," "," "," "," ",1,24]
["LECEF_1_UNITS",null,"LOS ESTEROS ENERGY FACILITY AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,309.83999999999997,null,null,"FC"," "," "," "," ",1,24]
["LECONT_2_LESBT1",null,"LeConte Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV",null,null,1,125,1,null,"ID",1,0.8,500,500,1,24]
["LEPRFD_1_KANSAS",null,"Kansas",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["LGHTHP_6_ICEGEN",null,"CARSON COGENERATION",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,48,null,null,"FC"," "," "," "," ",1,24]
["LHILLS_6_SOLAR1",null,"Lost Hills Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["LILIAC_6_SOLAR",null,"Mesa Crest",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,null,3,null,null,"FC"," "," "," "," ",1,24]
["LITLRK_6_GBCSR1",null,"Green Beanworks C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["LITLRK_6_SEPV01",null,"Gestamp Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,2,null,null,"EO"," "," "," "," ",1,24]
["LITLRK_6_SOLAR1",null,"Lancaster Little Rock C ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,5,null,null,"FC"," "," "," "," ",1,24]
["LITLRK_6_SOLAR2",null,"Palmdale 18",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["LITLRK_6_SOLAR3",null,"One Ten Partners",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["LITLRK_6_SOLAR4",null,"Little Rock Pham Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["LIVEOK_6_SOLAR",null,"Harris",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Sierra","Pease",null,null,1.25,0.4,null,"PD"," "," "," "," ",1,24]
["LIVOAK_1_UNIT 1",null,"LIVE OAK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,1,49.7,null,null,"FC"," "," "," "," ",1,24]
["LMBEPK_2_UNITA1",null,"Lambie Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,47.5,null,null,"FC"," "," "," "," ",1,24]
["LMBEPK_2_UNITA2",null,"Creed Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,47.6,null,null,"FC"," "," "," "," ",1,24]
["LMBEPK_2_UNITA3",null,"Goose Haven Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,47.75,null,null,"FC"," "," "," "," ",1,24]
["LMEC_1_PL1X3",null,"Los Medanos Energy Center AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,1,580,null,null,"FC"," "," "," "," ",1,24]
["LNCSTR_6_CREST",null,"Lanacaster Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,5.5,null,null,"EO"," "," "," "," ",1,24]
["LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN","SEPV Sierra NGR",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","South","SEPV Sierra NGR",null,8.25,2,3,null,6.9,"PD"," "," "," "," ",1,24]
["LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR","SEPV Sierra NGR",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"SEPV Sierra NGR",null,8.25,2,5.25,null,null,null,1,0.8,21,21,1,24]
["LOCKFD_1_BEARCK",null,"Bear Creek Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["LOCKFD_1_KSOLAR",null,"Kettleman Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["LODI25_2_UNIT 1",null,"LODI GAS TURBINE",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Stockton","Lockeford",null,1,25,null,null,"FC"," "," "," "," ",1,24]
["LODIEC_2_PL1X2",null,"Lodi Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,1,302.58,null,null,"FC"," "," "," "," ",1,24]
["LOTUS_6_LSFSR1",null,"Lotus Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Borden",null,null,50,null,null,"FC"," "," "," "," ",1,24]
["LOWGAP_1_SUPHR",null,"Mill & Sulphur Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.99,null,null,"FC"," "," "," "," ",1,24]
["LOWGAP_7_QFUNTS",null,"Matthews Dam Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.35,null,null,"FC"," "," "," "," ",1,24]
["LTBEAR_1_LB3SR3",null,"Little Bear 3 Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,20,1,null,"ID"," "," "," "," ",1,24]
["LTBEAR_1_LB4SR4",null,"Little Bear 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,50,1,null,"ID"," "," "," "," ",1,24]
["LTBEAR_1_LB4SR5",null,"Little Bear 4 Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,50,1,null,"ID"," "," "," "," ",1,24]
["LTBERA_1_LB1SR1",null,"Little Bear Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,40,1,null,"ID"," "," "," "," ",1,24]
["MAGUND_1_BKISR1",null,"Bakersfield Industrial 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["MAGUND_1_BKSSR2",null,"Bakersfield Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,null,5.25,null,null,"FC"," "," "," "," ",1,24]
["MALAGA_1_PL1X2",null,"Malaga Power Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon",null,1,96.61,null,null,"FC"," "," "," "," ",1,24]
["MALCHQ_7_UNIT 1",null,"MALACHA HYDRO L.P.",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,32.5,null,null,"FC"," "," "," "," ",1,24]
["MANTEC_1_ML1SR1",null,"Manteca  Land 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,null,1,null,null,"EO"," "," "," "," ",1,24]
["MANZNA_2_WIND",null,"Manzana Wind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,189,null,null,"FC"," "," "," "," ",1,24]
["MARCPW_6_SOLAR1",null,"Maricopa West Solar PV",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["MARTIN_1_SUNSET",null,"Sunset Reservoir - North Basin",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Bay Area",null,null,null,4.5,null,null,"FC"," "," "," "," ",1,24]
["MCARTH_6_FRIVRB",null,"Fall River Mills Project B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.5,1,null,"ID"," "," "," "," ",1,24]
["MCCALL_1_QF",null,"Fish Water",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,null,0.52,null,null,"FC"," "," "," "," ",1,24]
["MCSWAN_6_UNITS",null,"MC SWAIN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,1,9,0.97,null,"FC"," "," "," "," ",1,24]
["MDFKRL_2_PROJCT",null,"MIDDLE FORK AND RALSTON PSP",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,1,210,null,null,"FC"," "," "," "," ",1,24]
["MENBIO_6_RENEW1",null,"CalRENEW - 1(A)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["MERCED_1_SOLAR1",null,"Mission Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["MERCED_1_SOLAR2",null,"Merced Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["MERCFL_6_UNIT",null,"Merced Falls Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,1,3.5,0.97,null,"FC"," "," "," "," ",1,24]
["MESAP_1_QF",null,"SMALL QF AGGREGATION - SAN LUIS OBISPO",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,null,1,null,null,"FC"," "," "," "," ",1,24]
["METEC_2_PL1X3",null,"Metcalf Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",null,1,597.04999999999995,null,null,"FC"," "," "," "," ",1,24]
["MIDWD_2_WIND2",null,"Coram Energy",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["MIDWD_7_CORAMB",null,"CELLC 7.5 MW Tehachapi Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,7.5,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_CORONA",null,"MWD Corona Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,2.85,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_CREST",null,"Temescal Canyon RV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["MIRLOM_2_LNDFL",null,"Milliken Landfill Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,3,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_MLBBTA",null,"Mira Loma BESS A",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",null,1,10,null,null,"FC",2.79,0.87,40,112,1,24]
["MIRLOM_2_MLBBTB",null,"Mira Loma BESS B",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",null,1,10,null,null,"FC",2.79,0.87,40,112,1,24]
["MIRLOM_2_ONTARO",null,"Ontario RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,5.5,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_RTS032",null,"SPVP032",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_RTS033",null,"SPVP033",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_2_TEMESC",null,"MWD Temescal Hydroelectric Recovery Plan",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,2.85,null,null,"FC"," "," "," "," ",1,24]
["MIRLOM_6_PEAKER",null,"Mira Loma Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,47.18,null,null,"FC"," "," "," ",423,1,24]
["MIRLOM_7_MWDLKM",null,"Lake Mathews Hydroelectric Recovery Plan",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,1,5,null,null,"FC"," "," "," "," ",1,24]
["MISSIX_1_QF",null,"SMALL QF AGGREGATION - SAB FRABCUSCI",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","Ames",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["MKTRCK_1_UNIT 1",null,"MCKITTRICK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,47.72,null,null,"FC"," "," "," "," ",1,24]
["MLPTAS_7_QFUNTS",null,"MLPTAS_7_QFUNTS",null,"OTHER","CHP","OTHER","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["MNDALY_6_MCGRTH",null,"McGrath Beach Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,1,48.56,null,null,"FC"," "," "," ",1165,1,24]
["MNDOTA_1_SOLAR1",null,"North Star Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,null,60,null,null,"FC"," "," "," "," ",1,24]
["MNDOTA_1_SOLAR2",null,"Citizen Solar B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,5,null,null,"EO"," "," "," "," ",1,24]
["MOJAVE_1_SIPHON",null,"MOJAVE SIPHON POWER PLANT",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,2,14.36,null,null,"FC"," "," "," "," ",1,24]
["MOJAVW_2_SOLAR",null,"Mojave West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["MONTPH_7_UNITS",null,"MONTICELLO HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,null,12.5,null,null,"FC"," "," "," "," ",1,24]
["MOORPK_2_ACOBT1",null,"Acorn I BESS",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","Moorpark",null,3,1.95,null,null,"FC",1,0.8,4,4,1,24]
["MOORPK_2_CALABS",null,"Calabasas Gas-to-Energy Facility",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura","Moorpark",null,null,6.96,null,null,"FC"," "," "," "," ",1,24]
["MOORPK_6_QF",null,"MOORPARK QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","Moorpark",null,null,0.8,null,null,"FC"," "," "," "," ",1,24]
["MORWD_6_QF",null,"Morwind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,38.159999999999997,null,null,"FC"," "," "," "," ",1,24]
["MOSSLD_1_QF",null,"SMALL QF AGGREGATION - SANTA CRUZ",null,"COMBUSTION TURBINE","Biomass",null,null,"North","Bay Area",null,null,null,null,null,null,"FC"," "," "," "," ",1,24]
["MOSSLD_2_PSP1",null,"MOSS LANDING POWER BLOCK 1",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",null,1,510,null,null,"FC"," "," "," "," ",1,24]
["MOSSLD_2_PSP2",null,"MOSS LANDING POWER BLOCK 2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",null,1,510,null,null,"FC"," "," "," "," ",1,24]
["MRCHNT_2_PL1X3",null,"Desert Star Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,null,1,494.58,null,419.25,"PD"," "," "," "," ",1,24]
["MRGT_6_MEF2",null,"Miramar Energy Facility II",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,44,null,null,"FC"," "," "," "," ",1,24]
["MRGT_6_MMAREF",null,"Miramar Energy Facility",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,45,null,null,"FC"," "," "," "," ",1,24]
["MRGT_6_TGEBT1",null," Top Gun Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,30,null,null,"FC",1,0.8,120,120,1,24]
["MRLSDS_6_SOLAR1",null,"Morelos Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,15,null,null,"FC"," "," "," "," ",1,24]
["MSHGTS_6_MMARLF",null,"MIRAMAR LANDFILL",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["MSOLAR_2_SOLAR1",null,"Mesquite Solar 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,165,null,null,"FC"," "," "," "," ",1,24]
["MSOLAR_2_SOLAR2",null,"Mesquite Solar 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,100.81,null,null,"FC"," "," "," "," ",1,24]
["MSOLAR_2_SOLAR3",null,"Mesquite Solar 3, LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,152,null,null,"FC"," "," "," "," ",1,24]
["MSSION_2_QF",null,"SMALL QF AGGREGATION - SAN DIEGO",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","San Diego-IV","San Diego",null,null,2,null,null,"FC"," "," "," "," ",1,24]
["MSTANG_2_MTGBT1",null,"Mustang 1 BESS","MSTANG_2_SOLAR, MSTANG_2_SOLAR3, MSTANG_2_SOLAR4","OTHER","Paired_BattStorage","LESR","CISO","North","Fresno",null,null,1,75,null,null,"FC",1,0.8,300,300,1,24]
["MSTANG_2_SOLAR",null,"Mustang","MSTANG_2_MTGBT1, MSTANG_2_SOLAR3, MSTANG_2_SOLAR4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,30,null,null,"EO"," "," "," "," ",1,24]
["MSTANG_2_SOLAR3",null,"Mustang 3","MSTANG_2_SOLAR, MSTANG_2_MTGBT1, MSTANG_2_SOLAR4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,40,0.37369999999999998,null,"PD"," "," "," "," ",1,24]
["MSTANG_2_SOLAR4",null,"Mustang 4","MSTANG_2_SOLAR, MSTANG_2_MTGBT1, MSTANG_2_SOLAR3","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,30,null,null,"FC"," "," "," "," ",1,24]
["MTNPOS_1_UNIT",null,"MT.POSO COGENERATION CO.",null,"STEAM","CHP","BIOMASS","CISO","North","Kern","South Kern PP, Kern Oil",null,null,46.64,null,null,"FC"," "," "," "," ",1,24]
["MTWIND_1_MVPWD1",null,"Mountain View Power Project I Repower",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,66.599999999999994,null,null,"FC"," "," "," "," ",1,24]
["MTWIND_1_UNIT 3",null,"Mountain View Power Project III",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,22.44,null,null,"FC"," "," "," "," ",1,24]
["MURRAY_6_UNIT",null,"Grossmont Hospital",null,"FTUR","CHP","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,null,4.12,null,null,"EO"," "," "," "," ",1,24]
["NAROW1_2_UNIT",null,"NARROWS PH 1 UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,1,12,null,null,"FC"," "," "," "," ",1,24]
["NAROW2_2_UNIT",null,"Narrows Powerhouse Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,2,55,null,null,"FC"," "," "," "," ",1,24]
["NAVYII_2_UNITS",null,"COSO POWER DEVELOPER (NAVY II) AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,1,90,null,55,"PD"," "," "," "," ",1,24]
["NCPA_7_GP1UN1",null,"NCPA GEO PLANT 1 UNIT 1",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,38.85,null,null,"FC"," "," "," "," ",1,24]
["NCPA_7_GP1UN2",null,"NCPA GEO PLANT 1 UNIT 2",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,39.94,null,null,"FC"," "," "," "," ",1,24]
["NCPA_7_GP2UN3",null,"NCPA GEO PLANT 2 UNIT 3",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,null,42.42,null,null,"FC"," "," "," "," ",1,24]
["NCPA_7_GP2UN4",null,"NCPA GEO PLANT 2 UNIT 4",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",null,1,52.73,null,null,"FC"," "," "," "," ",1,24]
["NEENCH_6_SOLAR",null,"Alpine Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,null,66,null,null,"FC"," "," "," "," ",1,24]
["NEWARK_1_QF",null,"NEWARK 1 QF",null,"OTHER","CHP","OTHER","CISO","North","Bay Area",null,null,null,0.1,null,null,"FC"," "," "," "," ",1,24]
["NHOGAN_6_UNITS",null,"NEW HOGAN PH AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,4,null,null,"FC"," "," "," "," ",1,24]
["NOVATO_6_LNDFL",null,"Redwood Renewable Energy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB",null,null,null,3.9,null,null,"FC"," "," "," "," ",1,24]
["NWCSTL_7_UNIT 1",null,"NEWCASTLE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,12,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_2_WDSTR5",null,"Windstream 6111",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,6.31,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_6_CALWND",null,"Wind Resource I",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,9,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_6_WDSTR",null,"Windstream 39",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,3.35,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_6_WDSTR2",null,"Windstream 6040",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,4.07,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_6_WDSTR3",null,"Windstream 6041",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,3.86,null,null,"FC"," "," "," "," ",1,24]
["NZWIND_6_WDSTR4",null,"Windstream 6042",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,6.77,null,null,"FC"," "," "," "," ",1,24]
["OAK C_1_EBMUD",null,"MWWTP PGS 1 - ENGINES",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Oakland",null,null,6.9,null,null,"FC"," "," "," "," ",1,24]
["OAK C_7_UNIT 1",null,"OAKLAND STATION C GT UNIT 1",null,"COMBUSTION TURBINE","Peaker","DISTILLATE","CISO","North","Bay Area","Oakland",null,1,55,null,null,"FC"," "," "," "," ",1,24]
["OAK C_7_UNIT 3",null,"OAKLAND STATION C GT UNIT 3",null,"COMBUSTION TURBINE","Peaker","DISTILLATE","CISO","North","Bay Area","Oakland",null,1,55,null,null,"FC"," "," "," "," ",1,24]
["OAK L_1_GTG1",null,"MWWTP PGS 2 - Turbine",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","North","Bay Area","Oakland",null,null,4.5999999999999996,null,null,"EO"," "," "," "," ",1,24]
["OAKWD_6_QF",null,"Oak Creek",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,27.87,null,null,"FC"," "," "," "," ",1,24]
["OAKWD_6_ZEPHWD",null,"Zephyr Park",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,3.5,null,null,"FC"," "," "," "," ",1,24]
["OASIS_6_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,10.5,null,null,"EO"," "," "," "," ",1,24]
["OASIS_6_GBDSR4",null,"Green Beanworks D",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["OASIS_6_SOLAR1",null,"Morgan Lancaster I",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["OASIS_6_SOLAR2",null,"Oasis Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["OASIS_6_SOLAR3",null,"Soccer Center",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"EO"," "," "," "," ",1,24]
["OCTILO_5_WIND",null,"Ocotillo Wind Energy Facility",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,null,265,null,null,"FC"," "," "," "," ",1,24]
["OGROVE_6_PL1X2",null,"Orange Grove Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,96,null,null,"FC"," "," "," "," ",1,24]
["OILFLD_7_QFUNTS",null,"Nacimiento Hydroelectric Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,3.8,null,null,"FC"," "," "," "," ",1,24]
["OLDRIV_6_BIOGAS",null,"Bidart Old River 1",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,2,null,null,"FC"," "," "," "," ",1,24]
["OLDRIV_6_CESDBM",null,"Ces Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["OLDRIV_6_LKVBM1",null,"Lakeview Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["OLDRV1_6_SOLAR",null,"Old River One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["OLINDA_2_COYCRK",null,"MWD Coyote Creek Hydroelectric Recovery ",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",null,1,3.13,null,null,"FC"," "," "," "," ",1,24]
["OLINDA_2_LNDFL2",null,"Brea Power II",null,"COMBINED CYCLE","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,null,28.1,null,null,"FC"," "," "," "," ",1,24]
["OLINDA_7_BLKSND",null,"BlackSand Generating Facility",null,"COMBUSTION TURBINE","Biomass","WASTE TO POWER","CISO","South","LA Basin","Western",null,null,8,null,null,"FC"," "," "," "," ",1,24]
["OLIVEP_1_SOLAR",null,"White River Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["OLIVEP_1_SOLAR2",null,"White River West",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,19.75,null,null,"FC"," "," "," "," ",1,24]
["OLSEN_2_UNIT",null,"OLSEN POWER PARTNERS",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,5.5,null,null,"FC"," "," "," "," ",1,24]
["OMAR_2_UNIT 1",null,"KERN RIVER COGENERATION CO. UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,75,null,null,"FC"," "," "," "," ",1,24]
["OMAR_2_UNIT 2",null,"KERN RIVER COGENERATION CO. UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,75,null,null,"FC"," "," "," "," ",1,24]
["OMAR_2_UNIT 3",null,"KERN RIVER COGENERATION CO. UNIT 3",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,75,null,null,"FC"," "," "," "," ",1,24]
["OMAR_2_UNIT 4",null,"KERN RIVER COGENERATION CO. UNIT 4",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,75,null,null,"FC"," "," "," "," ",1,24]
["ONLLPP_6_UNITS",null,"O'NEILL PUMP-GEN (AGGREGATE)",null,"HYDRO","Pumped Hydro","WATER","CISO","North","Fresno",null,null,null,25.2,null,null,"FC"," "," "," "," ",1,24]
["ORLND_6_HIGHLI",null,"High Line Canal Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.5,null,null,"FC"," "," "," "," ",1,24]
["ORLND_6_SOLAR1",null,"Enerparc California 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["ORMOND_7_UNIT 1",null,"ORMOND BEACH GEN STA. UNIT 1",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","Big Creek-Ventura","Moorpark",null,1,741.27,null,null,"FC"," "," "," "," ",1,24]
["ORMOND_7_UNIT 2",null,"ORMOND BEACH GEN STA. UNIT 2",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","Big Creek-Ventura","Moorpark",null,1,750,null,null,"FC"," "," "," "," ",1,24]
["OROLOM_1_SOLAR1",null,"Oro Loma Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,null,10,null,null,"EO"," "," "," "," ",1,24]
["OROLOM_1_SOLAR2",null,"Oro Loma Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,null,10,null,null,"EO"," "," "," "," ",1,24]
["OROVIL_6_UNIT",null,"Oroville Cogeneration, LP",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","North","Sierra","Drum-Rio Oso",null,1,7.5,null,null,"FC"," "," "," "," ",1,24]
["ORTGA_6_ME1SL1",null,"Merced 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["OSO_6_NSPIN",null,"OSO_6_NSPIN",null,"PUMP","Pump","WATER","CISO","South","Big Creek-Ventura",null,null,null,70,null,null,"FC"," "," "," "," ",1,24]
["OTAY_6_PL1X2",null,"Chula Vista Energy Center, LLC",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,39.57,null,null,"FC"," "," "," "," ",1,24]
["OTMESA_2_PL1X3",null,"OTAY MESA ENERGY CENTER",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,603.67999999999995,null,null,"FC"," "," "," "," ",1,24]
["OXBOW_6_DRUM",null,"OXBOW HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,5.8,null,null,"FC"," "," "," "," ",1,24]
["OXMTN_6_LNDFIL",null,"Ox Mountain Landfill Generating Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Ames",null,null,10.62,null,null,"FC"," "," "," "," ",1,24]
["PACLUM_6_UNIT",null,"Humboldt Redwood",null,"STEAM","Biomass","BIOMASS","CISO","North","Humboldt",null,null,null,28.8,null,null,"FC"," "," "," "," ",1,24]
["PADUA_2_ONTARO",null,"ONTARIO/SIERRA HYDRO PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,null,1.92,null,null,"FC"," "," "," "," ",1,24]
["PADUA_2_SOLAR1",null,"Kona Solar - Rancho DC #1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,1.75,null,null,"EO"," "," "," "," ",1,24]
["PADUA_6_MWDSDM",null,"San Dimas Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,1,9.9,null,null,"FC"," "," "," "," ",1,24]
["PADUA_6_QF",null,"PADUA QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,null,1.82,null,null,"FC"," "," "," "," ",1,24]
["PADUA_7_SDIMAS",null,"San Dimas Wash Hydro",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,1,1.05,null,null,"FC"," "," "," "," ",1,24]
["PAIGES_6_SOLAR",null,"Paige Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,20,null,null,"EO"," "," "," "," ",1,24]
["PALALT_7_COBUG",null,"Cooperatively Owned Back Up Generator",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area",null,null,null,4.5,null,null,"FC"," "," "," "," ",1,24]
["PALOMR_2_PL1X3",null,"Palomar Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,588.21,null,null,"FC"," "," "," "," ",1,24]
["PARDEB_6_UNITS",null,"Pardee Power House",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,30,null,null,"FC"," "," "," "," ",1,24]
["PBLOSM_2_SOLAR",null,"PearBlossom",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,9.5,null,null,"FC"," "," "," "," ",1,24]
["PEABDY_2_LNDFIL",null,"G2 Energy Hay Road Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1.6,null,null,"FC"," "," "," "," ",1,24]
["PEABDY_2_LNDFL1",null,"Potrero Hills Energy Producers",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,8,null,null,"FC"," "," "," "," ",1,24]
["PEARBL_2_NSPIN",null,"PEARBL_2_NSPIN",null,"PUMP","Pump","WATER","CISO","South","CAISO System",null,null,null,118,null,null,"FC"," "," "," "," ",1,24]
["PEASE_1_TBEBT1",null,"Tierra Buena Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Sierra","Pease, Drum-Rio Oso",null,3,6,1,null,"ID",1,0.8,24,24,1,24]
["PEORIA_1_SOLAR",null,"Sonora 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["PHOENX_1_UNIT",null,"PHOENIX PH",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,2,null,null,"FC"," "," "," "," ",1,24]
["PINFLT_7_UNITS",null,"PINE FLAT HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,1,198.51,null,null,"FC"," "," "," "," ",1,24]
["PIOPIC_2_CTG1",null,"Pio Pico Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,111.3,null,null,"FC"," "," "," "," ",1,24]
["PIOPIC_2_CTG2",null,"Pio Pico Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,112.7,null,null,"FC"," "," "," "," ",1,24]
["PIOPIC_2_CTG3",null,"Pio Pico Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,1,112,null,null,"FC"," "," "," "," ",1,24]
["PIT1_6_FRIVRA",null,"Fall River Mills Project A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.5,1,null,"ID"," "," "," "," ",1,24]
["PIT1_7_UNIT 1",null,"PIT PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,32,null,null,"FC"," "," "," "," ",1,24]
["PIT1_7_UNIT 2",null,"PIT PH 1 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,32,null,null,"FC"," "," "," "," ",1,24]
["PIT3_7_PL1X3",null,"PIT PH 3 UNITS 1, 2 & 3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,70.599999999999994,null,null,"FC"," "," "," "," ",1,24]
["PIT4_7_PL1X2",null,"PIT PH 4 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,95,null,null,"FC"," "," "," "," ",1,24]
["PIT5_7_PL1X2",null,"PIT PH 5 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,82,null,null,"FC"," "," "," "," ",1,24]
["PIT5_7_PL3X4",null,"PIT PH 5 UNITS 3 & 4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,82,null,null,"FC"," "," "," "," ",1,24]
["PIT5_7_QFUNTS",null,"GRASSHOPPER FLAT HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.1000000000000001,null,null,"FC"," "," "," "," ",1,24]
["PIT6_7_UNIT 1",null,"PIT PH 6 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,39,null,null,"FC"," "," "," "," ",1,24]
["PIT6_7_UNIT 2",null,"PIT PH 6 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,40,null,null,"FC"," "," "," "," ",1,24]
["PIT7_7_UNIT 1",null,"PIT PH 7 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,55.7,null,null,"FC"," "," "," "," ",1,24]
["PIT7_7_UNIT 2",null,"PIT PH 7 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,54.6,null,null,"FC"," "," "," "," ",1,24]
["PIUTE_6_GNBSR1",null,"Green Beanworks B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["PLACVL_1_CHILIB",null,"Chili Bar Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,null,8.34,null,null,"FC"," "," "," "," ",1,24]
["PLACVL_1_RCKCRE",null,"Rock Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["PLAINV_6_BSOLAR",null,"Western Antelope Blue Sky Ranch A ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["PLAINV_6_DSOLAR",null,"Western Antelope Dry Ranch ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,10,null,null,"FC"," "," "," "," ",1,24]
["PLAINV_6_NLRSR1",null,"North Lancaster Ranch ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["PLAINV_6_SOLAR3",null,"Sierra Solar Greenworks LLC",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["PLAINV_6_SOLARC",null,"Central Antelope Dry Ranch C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["PLMSSR_6_HISIER",null,"High Sierra Cogeneration Aggregate",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,1,6,null,null,"FC"," "," "," "," ",1,24]
["PLSNTG_7_LNCLND",null,"Lincoln Landfill Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,4.9800000000000004,null,null,"FC"," "," "," "," ",1,24]
["PMDLET_6_SOLAR1",null,"SEPV Palmdale East, LLC",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,10,null,null,"FC"," "," "," "," ",1,24]
["PMPJCK_1_RB2SLR",null,"Rio Bravo Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["PMPJCK_1_SOLAR1",null,"Pumpjack Solar I",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["PMPJCK_1_SOLAR2",null,"Rio Bravo Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["PNCHEG_2_PL1X4",null,"PANOCHE ENERGY CENTER (Aggregated)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,417,1,null,"ID"," "," "," "," ",1,24]
["PNCHPP_1_PL1X2",null,"Midway Peaking Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Panoche 115 kV",null,1,119.91,null,null,"FC"," "," "," "," ",1,24]
["PNCHVS_2_SOLAR",null,"Panoche Valley Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,140,null,null,"FC"," "," "," "," ",1,24]
["PNOCHE_1_PL1X2",null,"Panoche Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Panoche 115 kV",null,1,49.97,null,null,"FC"," "," "," "," ",1,24]
["PNOCHE_1_UNITA1",null,"CalPeak Power Panoche Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Panoche 115 kV",null,1,52.3,null,null,"FC"," "," "," "," ",1,24]
["POEPH_7_UNIT 1",null,"POE HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,68,null,null,"FC"," "," "," "," ",1,24]
["POEPH_7_UNIT 2",null,"POE HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,68.5,null,null,"FC"," "," "," "," ",1,24]
["POTTER_6_UNITS",null,"Potter Valley",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,null,10.1,null,null,"FC"," "," "," "," ",1,24]
["POTTER_7_VECINO",null,"Vecino Vineyards LLC",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,null,1.25,null,null,"FC"," "," "," "," ",1,24]
["PRCTVY_1_MIGBT1",null,"Miguel BESS",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,null,2,null,null,"EO",1,0.8,8,8,1,24]
["PRIMM_2_SOLAR1",null,"Silver State South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,250,null,null,"FC"," "," "," "," ",1,24]
["PSWEET_1_STCRUZ",null,"Santa Cruz Energy LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1.6,null,null,"EO"," "," "," "," ",1,24]
["PSWEET_7_QFUNTS",null,"PSWEET_7_QFUNTS",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,null,1,null,null,"FC"," "," "," "," ",1,24]
["PUTHCR_1_PCNSB1","PUTHCR_1_PCNSB1_SUN","Putah Creek Solar Farm North",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","North","CAISO System",null,3,null,3,null,null,"ID"," "," "," "," ",1,24]
["PUTHCR_1_PCNSB1","PUTHCR_1_PCNSB1_LESR","Putah Creek Solar Farm North",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","CAISO System",null,3,null,3,1,null,"ID",1,0.8,12,12,1,24]
["PUTHCR_1_SOLAR1",null,"Putah Creek Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.98,null,null,"FC"," "," "," "," ",1,24]
["PWEST_1_UNIT",null,"PACIFIC WEST 1 WIND GENERATION",null,"WIND","Wind","WIND","CISO","South","LA Basin","Western",null,null,2.1,null,null,"FC"," "," "," "," ",1,24]
["RATSKE_2_NROSR1",null,"North Rosamond Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24]
["RATSKE_2_RBSSB1","RATSKE_2_RBSSB1_SUN","Rabbitbrush Solar 1",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","Rabbitbrush Solar 1",null,60,2,60,1,null,"ID"," "," "," "," ",1,24]
["RATSKE_2_RBSSB1","RATSKE_2_RBSSB1_LESR","Rabbitbrush Solar 2",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Rabbitbrush Solar 1",null,60,2,7.5,null,null,null,1,0.8,30,30,1,24]
["RATSKE_2_RBSSB2","RATSKE_2_RBSSB2_SUN","Rabbitbrush Solar 2",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","Rabbitbrush Solar 2",null,40,2,40,1,null,"ID"," "," "," "," ",1,24]
["RATSKE_2_RBSSB2","RATSKE_2_RBSSB2_LESR","Rabbitbrush Solar 3",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Rabbitbrush Solar 2",null,40,2,5,null,null,null,1,0.8,20,20,1,24]
["RCKCRK_7_UNIT 1",null,"ROCK CREEK HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,57,null,null,"FC"," "," "," "," ",1,24]
["RCKCRK_7_UNIT 2",null,"ROCK CREEK HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1,56.9,null,null,"FC"," "," "," "," ",1,24]
["RDWAY_1_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,6.5,null,null,"EO"," "," "," "," ",1,24]
["RECTOR_2_CREST",null,"Rector Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,10.5,null,null,"EO"," "," "," "," ",1,24]
["RECTOR_2_IVANPV",null,"Ivanhoe Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,3.5,null,null,"EO"," "," "," "," ",1,24]
["RECTOR_2_KAWEAH",null,"KAWEAH PH 2 & 3 PSP AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,6.55,null,null,"FC"," "," "," "," ",1,24]
["RECTOR_2_KAWH 1",null,"KAWEAH PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,2.25,null,null,"FC"," "," "," "," ",1,24]
["RECTOR_2_QF",null,"Kaweah Unit 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,20.09,null,null,"FC"," "," "," "," ",1,24]
["RECTOR_2_TFDBM1",null,"Two Fiets Dairy Digester",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,0.8,null,null,"EO"," "," "," "," ",1,24]
["RECTOR_7_TULARE",null,"MM Tulare ",null,"RECIPROCATING ENGINE","Biomass","BIOMASS","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["REDBLF_6_UNIT",null,"RED BLUFF PEAKER PLANT",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","CAISO System",null,null,1,44,null,null,"FC"," "," "," "," ",1,24]
["REDMAN_2_SOLAR",null,"Lancaster East Avenue F",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3.75,null,null,"FC"," "," "," "," ",1,24]
["REDMAN_6_AVSSR1",null,"Antelope Valley Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["REDOND_7_UNIT 5",null,"REDONDO GEN STA. UNIT 5",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,178.87,null,null,"FC"," "," "," "," ",1,24]
["REDOND_7_UNIT 6",null,"REDONDO GEN STA. UNIT 6",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,174.29,null,null,"FC"," "," "," "," ",1,24]
["REDOND_7_UNIT 8",null,"REDONDO GEN STA. UNIT 8",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",null,1,480,null,null,"FC"," "," "," "," ",1,24]
["REEDLY_6_SOLAR",null,"Terzian",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Fresno","Herndon, Reedley",null,null,1.23,null,null,"EO"," "," "," "," ",1,24]
["RENWD_1_QF",null,"Renwind re-powering project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,10,null,null,"FC"," "," "," "," ",1,24]
["RICHMN_1_CHVSR2",null,"Chevron 8.5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area",null,null,null,8.5,1,null,"ID"," "," "," "," ",1,24]
["RICHMN_1_SOLAR",null,"Chevron 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area",null,null,null,2,1,null,"ID"," "," "," "," ",1,24]
["RICHMN_7_BAYENV",null,"BAY ENVIRONMENTAL (NOVE POWER)",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area",null,null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["RIOBRV_6_UNIT 1",null,"RIO BRAVO HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,14,null,null,"FC"," "," "," "," ",1,24]
["RIOOSO_1_QF",null,"SMALL QF AGGREGATION - GRASS VALLEY",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,1.1100000000000001,null,null,"FC"," "," "," "," ",1,24]
["RNDMTN_2_SLSPHY1",null,"Silver Springs",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.6,null,null,"FC"," "," "," "," ",1,24]
["RNDSBG_1_HZASR1",null,"Hazel A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,2.99,null,null,"FC"," "," "," "," ",1,24]
["ROLLIN_6_UNIT",null,"ROLLINS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,2,13.5,null,null,"FC"," "," "," "," ",1,24]
["ROSMDW_2_WIND1",null,"Pacific Wind - Phase 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,140,null,null,"FC"," "," "," "," ",1,24]
["ROSMND_6_SOLAR",null,"Lancaster B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["RSMSLR_6_SOLAR1",null,"Rosamond One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["RSMSLR_6_SOLAR2",null,"Rosamond Two",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SC1SR3",null,"Rosamond West Solar Clean",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,40,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SEBSR3",null,"Rosamond West Solar East Bay 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,56,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SEBSR4",null,"Rosamond West Solar East Bay 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,56,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SOLAR1",null,"Rosamond West Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,54,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SOLAR2",null,"Rosamond West Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,54,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SPASR4",null,"Rosamond West Solar Palo Alto",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,26,null,null,"FC"," "," "," "," ",1,24]
["RTEDDY_2_SRXSR4",null,"Rosamond West Solar Rosie X",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,13.6,null,null,"FC"," "," "," "," ",1,24]
["RTREE_2_WIND1",null,"Rising Tree 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,79.2,null,null,"FC"," "," "," "," ",1,24]
["RTREE_2_WIND2",null,"Rising Tree 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,19.8,null,null,"FC"," "," "," "," ",1,24]
["RTREE_2_WIND3",null,"Rising Tree 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,99,null,null,"FC"," "," "," "," ",1,24]
["RUSCTY_2_UNITS",null,"Russell City Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Ames",null,1,615.17999999999995,null,null,"FC"," "," "," "," ",1,24]
["RVRVEW_1_UNITA1",null,"Riverview Energy Center (GP Antioch)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",null,1,48.7,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_2_RERCU3",null,"Riverside Energy Res. Ctr Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,49,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_2_RERCU4",null,"Riverside Energy Res. Ctr Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,49,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_6_RERCU1",null,"Riverside Energy Res. Ctr Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,48.35,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_6_RERCU2",null,"Riverside Energy Res. Ctr Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,48.5,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_6_SOLAR1",null,"Tequesquite Landfill Solar Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,null,7.5,null,null,"FC"," "," "," "," ",1,24]
["RVSIDE_6_SPRING",null,"SPRINGS GENERATION PROJECT AGGREGATE",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",null,1,36,null,null,"FC"," "," "," "," ",1,24]
["S_RITA_6_SOLAR1",null,"Sun Harvest Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["SALIRV_2_UNIT",null,"Salinas River Cogeneration",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,39,null,null,"FC"," "," "," "," ",1,24]
["SALTSP_7_UNITS",null,"SALT SPRINGS HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,46,null,null,"FC"," "," "," "," ",1,24]
["SAMPSN_6_KELCO1",null,"KELCO QUALIFYING FACILITY",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","San Diego-IV","San Diego",null,null,25,null,null,"FC"," "," "," "," ",1,24]
["SANBRN_2_EESSB2",null,"Edsan 2 Edwards Sanborn E1B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,166,1,null,"ID"," "," "," "," ",1,24]
["SANBRN_2_ES1BT3","SANBRN_2_ES1BT3_SUN","EdSan 1 Edwards 1",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","EdSan 1 Edwards 1",null,50.43,2,40,1,null,"ID"," "," "," "," ",1,24]
["SANBRN_2_ES1BT3","SANBRN_2_ES1BT3_LESR","EdSan 1 Edwards 2",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"EdSan 1 Edwards 1",null,50.43,2,22,null,null,null,1,0.8,88,88,1,24]
["SANBRN_2_ES2SB3","SANBRN_2_ES2SB3_SUN","EdSan 2 Sanborn 3",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","EdSan 2 Sanborn 3",null,42,2,33,1,null,"ID"," "," "," "," ",1,24]
["SANBRN_2_ES2SB3","SANBRN_2_ES2SB3_LESR","EdSan 2 Sanborn 4",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"EdSan 2 Sanborn 3",null,42,2,18,null,null,null,1,0.8,72,72,1,24]
["SANBRN_2_ESABT1",null,"EdSan 1A",null,"OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,null,2,100,1,null,"ID",1,0.8,400,400,1,24]
["SANBRN_2_ESBBT1",null,"EdSan 1B",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,2,100,1,null,"ID",1,0.8,400,400,1,24]
["SANBRN_2_SS2SB4",null,"Sanborn Solar 2 Edwards Sanborn S4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,36,0,0,"ID"," "," "," "," ",1,24]
["SANDLT_2_SUNITS",null,"Mojave Solar",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,null,275,null,null,"FC"," "," "," "," ",1,24]
["SANITR_6_UNITS",null,"LACSD CARSON WATER POLLUTION AGGREGATE",null,"COMBINED CYCLE","Biogas","NATURAL GAS","CISO","South","LA Basin","Eastern",null,null,8,null,null,"FC"," "," "," "," ",1,24]
["SANLOB_1_LNDFIL",null,"Cold Canyon",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["SANLOB_1_OSFBM1",null,"Old Santa Fe Road",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,0.85,null,null,"EO"," "," "," "," ",1,24]
["SANTFG_7_UNITS",null,"GEYSERS CALISTOGA AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,72,null,null,"FC"," "," "," "," ",1,24]
["SANTGO_2_LNDFL1",null,"Bowerman Power",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,null,19.600000000000001,null,null,"FC"," "," "," "," ",1,24]
["SANTGO_2_MABBT1",null,"Millikan Avenue BESS",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",null,3,2,null,null,"FC",1,0.8,8,8,1,24]
["SANWD_1_QF",null,"San Gorgonio Farms Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,31,null,null,"FC"," "," "," "," ",1,24]
["SAUGUS_6_CREST",null,"East Portal Hydro",null,"HYDRO","Hydro",null,null,"South","Big Creek-Ventura",null,null,null,null,null,null,"EO"," "," "," "," ",1,24]
["SAUGUS_6_MWDFTH",null,"Foothill Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,null,1,9.1,null,null,"FC"," "," "," "," ",1,24]
["SAUGUS_6_QF",null,"SAUGUS QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura",null,null,null,2.19,null,null,"FC"," "," "," "," ",1,24]
["SAUGUS_7_CHIQCN",null,"Chiquita Canyon Landfill Fac",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,null,8,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_PSP3",null,"Mountainview Gen Sta. Unit 3",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern, West of Devers",null,1,555,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_PSP4",null,"Mountainview Gen Sta. Unit 4",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern, West of Devers",null,1,555,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_REDLND",null,"Redlands RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,2,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS005",null,"SPVP005 Redlands RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS007",null,"SPVP007 Redlands RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS011",null,"SPVP011",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,3.5,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS013",null,"SPVP013",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,3.5,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS016",null,"SPVP016 Redlands RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_2_RTS048",null,"SPVP048",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, West of Devers",null,null,5,null,null,"EO"," "," "," "," ",1,24]
["SBERDO_2_SNTANA",null,"SANTA ANA PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, West of Devers",null,null,6.95,null,null,"FC"," "," "," "," ",1,24]
["SBERDO_6_MILLCK",null,"MILL CREEK PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, West of Devers",null,null,3.93,null,null,"FC"," "," "," "," ",1,24]
["SCHLTE_1_PL1X3",null,"Tracy Combined Cycle Power Plant",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Stockton","Tesla-Bellota",null,1,336.04,null,null,"FC"," "," "," "," ",1,24]
["SCHNDR_1_FIVPTS",null,"Five Points Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,15,null,null,"FC"," "," "," "," ",1,24]
["SCHNDR_1_OS2BM2",null,"Open Sky Digester Genset 2",null,"COMBUSTION TURBINE","Biogas",null,null,"North","Fresno","Coalinga",null,null,null,null,null,"EO"," "," "," "," ",1,24]
["SCHNDR_1_WSTSDE",null,"Westside Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,15,null,null,"FC"," "," "," "," ",1,24]
["SEARLS_7_ARGUS",null,"Argus Cogeneration",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","CAISO System",null,null,null,19,null,null,"FC"," "," "," "," ",1,24]
["SEGS_1_SR2SL2",null,"Sunray 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG1",null,"Sentinel Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,107.68,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG2",null,"Sentinel Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,104.19,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG3",null,"Sentinel Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,105.69,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG4",null,"Sentinel Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,106.55,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG5",null,"Sentinel Unit 5",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,107.52,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG6",null,"Sentinel Unit 6",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,105,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG7",null,"Sentinel Unit 7",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,106.73,null,null,"FC"," "," "," "," ",1,24]
["SENTNL_2_CTG8",null,"Sentinel Unit 8",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,106.85,null,null,"FC"," "," "," "," ",1,24]
["SGREGY_6_SANGER",null,"Algonquin Power Sanger 2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Fresno","Herndon",null,1,48.3,null,null,"FC"," "," "," "," ",1,24]
["SHELRF_1_UNITS",null,"SHELL OIL REFINERY AGGREGATE",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,null,100,null,null,"FC"," "," "," "," ",1,24]
["SHUTLE_6_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,null,4,null,null,"EO"," "," "," "," ",1,24]
["SIERRA_1_UNITS",null,"HIGH SIERRA LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",null,1,52.43,null,null,"FC"," "," "," "," ",1,24]
["SISQUC_1_SMARIA",null,"Santa Maria II LFG Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,1.42,null,null,"FC"," "," "," "," ",1,24]
["SKERN_6_SOLAR1",null,"South Kern Solar PV Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["SKERN_6_SOLAR2",null,"SKIC Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,null,10,null,null,"FC"," "," "," "," ",1,24]
["SLATE_2_SLASR1",null,"Slate",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,50.5,1,null,"ID"," "," "," "," ",1,24]
["SLATE_2_SLASR2","SLATE_2_SLASR2_SUN","SLATE_2",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,93,2,93,1,null,"ID"," "," "," "," ",1,24]
["SLATE_2_SLASR2","SLATE_2_SLASR2_LESR","SLATE_2",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Fresno",null,93,2,46.5,null,null,null,1,0.8,186,186,1,24]
["SLATE_2_SLASR3","SLATE_2_SLASR3_SUN","SLATE_3",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,67.5,2,67.5,1,null,"ID"," "," "," "," ",1,24]
["SLATE_2_SLASR3","SLATE_2_SLASR3_LESR","SLATE_3",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Fresno",null,67.5,2,33.75,null,null,null,1,0.8,135,135,1,24]
["SLATE_2_SLASR4","SLATE_2_SLASR4_SUN","SLATE_4",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,63,3,63,1,null,"ID"," "," "," "," ",1,24]
["SLATE_2_SLASR4","SLATE_2_SLASR4_LESR","SLATE_4",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Fresno",null,63,3,50,null,null,null,1,0.8,200,200,1,24]
["SLATE_2_SLASR5","SLATE_2_SLASR5_SUN","Slate 5",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,26,2,26,1,null,"ID"," "," "," "," ",1,24]
["SLATE_2_SLASR5","SLATE_2_SLASR5_LESR","Slate 5",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"Fresno",null,26,2,10,null,null,null,1,0.8,40,40,1,24]
["SLRMS3_2_SRMSR1",null,"SILVER RIDGE MOUNT SIGNAL 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,null,250,null,null,"FC"," "," "," "," ",1,24]
["SLST13_2_SOLAR1",null,"Quinto Solar PV Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,107.6,null,null,"FC"," "," "," "," ",1,24]
["SLSTR1_2_SOLAR1",null,"Solar Star 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,310,null,null,"FC"," "," "," "," ",1,24]
["SLSTR2_2_SOLAR2",null,"Solar Star 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,276,null,null,"FC"," "," "," "," ",1,24]
["SLUISP_2_UNITS",null,"SAN LUIS (GIANELLI) PUMP-GEN (AGGREGATE)",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","CAISO System",null,null,null,374.43,null,null,"FC"," "," "," "," ",1,24]
["SLYCRK_1_UNIT 1",null,"SLY CREEK HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,1,13,null,null,"FC"," "," "," "," ",1,24]
["SMPRIP_1_SMPSON",null,"Ripon Cogeneration Unit 1",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,1,46.05,null,null,"FC"," "," "," "," ",1,24]
["SMRCOS_6_LNDFIL",null,"San Marcos Energy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["SMUDGO_7_UNIT 1",null,"SONOMA POWER PLANT",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,null,1,64.8,null,null,"FC"," "," "," "," ",1,24]
["SMYRNA_1_DL1SR1",null,"Delano Land 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,1,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_2_HOWLNG",null,"Houwelings Nurseries Oxnard, Inc",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,12.71,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_2_SILBT1",null,"Silverstrand BESS",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,3,11,null,null,"FC",1,0.8,44,44,1,24]
["SNCLRA_2_SPRHYD",null,"Springville Hydroelectric Generator",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_2_UNIT",null,"Channel Islands Power",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,1,27.5,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_2_UNIT1",null,"New Indy Oxnard",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,27.8,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_2_VESBT1",null,"Ventura Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,3,100,null,null,"FC",1,0.8,400,400,1,24]
["SNCLRA_6_OXGEN",null,"OXGEN",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,2,47.7,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_6_PROCGN",null,"Procter and Gamble Oxnard 2",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,47.9,null,null,"FC"," "," "," "," ",1,24]
["SNCLRA_6_QF",null,"SANTA CLARA QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,null,1.65,null,null,"FC"," "," "," "," ",1,24]
["SNDBAR_7_UNIT 1",null,"SANDBAR",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,16.2,null,null,"FC"," "," "," "," ",1,24]
["SNMALF_6_UNITS",null,"Sonoma County Landfill",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB","Fulton",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["SOUTH_2_UNIT",null,"SOUTH HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,7.1,null,null,"FC"," "," "," "," ",1,24]
["SPAULD_6_UNIT 3",null,"SPAULDING HYDRO PH 3 UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,null,6.5,null,null,"FC"," "," "," "," ",1,24]
["SPAULD_6_UNIT12",null,"SPAULDING HYDRO PH 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,11.4,null,null,"FC"," "," "," "," ",1,24]
["SPBURN_2_UNIT 1",null,"Burney Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,22,null,null,"FC"," "," "," "," ",1,24]
["SPBURN_7_SNOWMT",null,"Burney Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,3,null,null,"FC"," "," "," "," ",1,24]
["SPI LI_2_UNIT 1",null,"Lincoln Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,17.2,null,null,"FC"," "," "," "," ",1,24]
["SPIAND_1_ANDSN2",null,"SPI Anderson 2",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,27.15,null,null,"FC"," "," "," "," ",1,24]
["SPICER_1_UNITS",null,"SPICER HYDRO UNITS 1-3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,6,null,null,"FC"," "," "," "," ",1,24]
["SPIFBD_1_PL1X2",null,"SIERRA PACIFIC IND. (SONORA)",null,"STEAM","CHP","BIOMASS","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,7.5,null,null,"FC"," "," "," "," ",1,24]
["SPQUIN_6_SRPCQU",null,"Quincy Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,24,null,null,"FC"," "," "," "," ",1,24]
["SPRGAP_1_UNIT 1",null,"SPRING GAP HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,7,null,null,"FC"," "," "," "," ",1,24]
["SPRGVL_2_CREST",null,"Springerville Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,3,null,null,"EO"," "," "," "," ",1,24]
["SPRGVL_2_EXETPV",null,"Exeter Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,3.5,null,null,"EO"," "," "," "," ",1,24]
["SPRGVL_2_LINDPV",null,"Lindsay Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,4,null,null,"EO"," "," "," "," ",1,24]
["SPRGVL_2_PORTPV",null,"Porterville Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,3.5,null,null,"EO"," "," "," "," ",1,24]
["SPRGVL_2_TULESC",null,"TULE RIVER HYDRO PLANT (SCE)",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["SRINTL_6_UNIT",null,"SRI INTERNATIONAL",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Bay Area",null,null,null,6.9,null,null,"FC"," "," "," "," ",1,24]
["STANIS_7_UNIT 1",null,"STANISLAUS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,1,91,null,null,"FC"," "," "," "," ",1,24]
["STANTN_2_STAGT1",null,"Stanton 1",null,"OTHER","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,49.65,null,null,"FC"," "," "," "," ",1,24]
["STANTN_2_STAGT2",null,"Stanton 2",null,"OTHER","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,49.65,null,null,"FC"," "," "," "," ",1,24]
["STIGCT_2_LODI",null,"LODI STIG UNIT",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,1,49.9,null,null,"FC"," "," "," "," ",1,24]
["STNRES_1_UNIT",null,"Covanta Stanislaus",null,"STEAM","Biomass","WASTE TO POWER","CISO","North","Stockton","Tesla-Bellota",null,null,19.899999999999999,null,null,"FC"," "," "," "," ",1,24]
["STOILS_1_UNITS",null,"Chevron Richmond Refinery",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,null,56.2,null,null,"FC"," "," "," "," ",1,24]
["STOREY_2_MDRCH2",null,"Madera Chowchilla 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,0.56000000000000005,null,null,"FC"," "," "," "," ",1,24]
["STOREY_2_MDRCH3",null,"Madera Chowchilla 3",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,0.42,null,null,"FC"," "," "," "," ",1,24]
["STOREY_2_MDRCH4",null,"Madera Chowchilla 4",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,0.92,null,null,"FC"," "," "," "," ",1,24]
["STOREY_7_MDRCHW",null,"Madera Canal Site 980",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,1.84,null,null,"FC"," "," "," "," ",1,24]
["STROUD_6_SOLAR",null,"Stroud Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["STROUD_6_WWHSR1",null,"Winter Wheat Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["SUMWHT_6_SWSSR1",null,"Summer Wheat Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,18.5,null,null,"FC"," "," "," "," ",1,24]
["SUNCAT_2_A1ABT1",null,"Arlington Solar Unit 1A BESS ",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,2,47,1,null,"ID",1,0.8,188,188,1,24]
["SUNCAT_2_A1BBT1",null,"Arlington Solar Unit 1B BESS ",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,2,63,1,null,"ID",1,0.8,252,252,1,24]
["SUNCAT_2_A2ABT2",null,"Arlington Solar Unit 2A BESS ","ARLNTN_2_AR1SR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,144.31,2,132,1,null,"ID",1,0.8,528,528,1,24]
["SUNRIS_2_PL1X3",null,"Sunrise Power Project AGGREGATE II",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,null,1,586.02,null,null,"FC"," "," "," "," ",1,24]
["SUNSET_2_UNITS",null,"MIDWAY SUNSET COGENERATION PLANT",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,1,248,null,null,"FC"," "," "," "," ",1,24]
["SUNSHN_2_LNDFL",null,"Sunshine Gas Producers",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["SUNSLR_1_SSVSR1",null,"Sunshine Valley Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,100,null,null,"FC"," "," "," "," ",1,24]
["SUNSPT_2_WNASR1",null,"Windhub Solar A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["SUNST2_5_SS2SR1",null,"Sun Streams Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,150,null,null,"FC"," "," "," "," ",1,24]
["SYCAMR_2_UNIT 1",null,"Sycamore Cogeneration Unit 1",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,null,74,null,null,"FC"," "," "," "," ",1,24]
["SYCAMR_2_UNIT 2",null,"Sycamore Cogeneration Unit 2",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,76,null,null,"FC"," "," "," "," ",1,24]
["SYCAMR_2_UNIT 3",null,"Sycamore Cogeneration Unit 3",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,74,null,null,"FC"," "," "," "," ",1,24]
["SYCAMR_2_UNIT 4",null,"Sycamore Cogeneration Unit 4",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,1,76,null,null,"FC"," "," "," "," ",1,24]
["TANHIL_6_SOLART",null,"Berry Cogen 18",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,17,null,null,"FC"," "," "," "," ",1,24]
["TBLMTN_6_QF",null,"SMALL QF AGGREGATION - PARADISE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.7,null,null,"FC"," "," "," "," ",1,24]
["TEHAPI_2_PW1WD1",null,"Point Wind 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,47.49,null,null,"FC"," "," "," "," ",1,24]
["TEHAPI_2_PW2WD2",null,"Point Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,14.4,null,null,"FC"," "," "," "," ",1,24]
["TEHAPI_2_WIND1",null,"Wind Wall Monolith 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,19.850000000000001,0.75,null,"PD"," "," "," "," ",1,24]
["TEHAPI_2_WIND2",null,"Wind Wall Monolith 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,23.66,0.85,null,"PD"," "," "," "," ",1,24]
["TENGEN_2_PL1X2",null,"Placerita Canyon Cogen",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,null,37.700000000000003,null,null,"FC"," "," "," "," ",1,24]
["TERMEX_2_PL1X3",null,"TDM",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV",null,null,1,625,null,null,"FC"," "," "," "," ",1,24]
["TESLA_1_QF",null,"SMALL QF AGGREGATION - STOCKTON",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["TIDWTR_2_UNITS",null,"MARTINEZ COGEN LIMITED PARTNERSHIP",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,null,114.8,null,null,"FC"," "," "," "," ",1,24]
["TIFFNY_1_DILLON",null,"TIFFNY_1_DILLON",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,45,null,null,"FC"," "," "," "," ",1,24]
["TIGRCK_7_UNITS",null,"TIGER CREEK HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,62,null,null,"FC"," "," "," "," ",1,24]
["TKOPWR_6_HYDRO",null,"Bear Creek Hydroelectric Project",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,2.83,null,null,"FC"," "," "," "," ",1,24]
["TMPLTN_2_SOLAR",null,"Vintner Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["TOADTW_6_UNIT",null,"TOAD TOWN",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["TOPAZ_2_SOLAR",null,"Topaz Solar Farms",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,550,null,null,"FC"," "," "," "," ",1,24]
["TORTLA_1_SOLAR",null,"Longboat Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["TRNQL8_2_AMASR1",null,"Tranquillity 8 Amarillo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,1,null,"ID"," "," "," "," ",1,24]
["TRNQL8_2_AZUSR1",null,"Tranquillity 8 Azul",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,1,null,"ID"," "," "," "," ",1,24]
["TRNQL8_2_ROJSR1",null,"Tranquillity 8 Rojo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,100,1,null,"ID"," "," "," "," ",1,24]
["TRNQL8_2_VERSR1",null,"Tranquillity 8 Verde",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,60,1,null,"ID"," "," "," "," ",1,24]
["TRNQLT_2_RETBT1",null,"RE Tranquillity BESS","TRNQLT_2_SOLAR","OTHER","Paired_BattStorage","LESR","CISO","North","Fresno",null,96.76,1,72,null,null,"FC",2.8,0.88,288,807,1,24]
["TRNQLT_2_SOLAR",null,"Tranquillity","TRNQLT_2_RETBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","North","Fresno",null,96.76,null,200,null,null,"FC"," "," "," "," ",1,24]
["TRNSWD_1_QF",null,"FPL Energy C Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,38.97,null,null,"FC"," "," "," "," ",1,24]
["TULARE_2_TULBM1",null,"Tulare BioMAT Fuel Cell",null,"OTHER","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,null,2.8,null,null,"EO"," "," "," "," ",1,24]
["TULEWD_1_TULWD1",null,"Tule Wind",null,"WIND","Wind","WIND","CISO","South","San Diego-IV","Eastern, Valley-Devers",null,null,130.5,null,null,"FC"," "," "," "," ",1,24]
["TULLCK_7_UNITS",null,"Tullock Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota",null,null,25.9,null,null,"FC"," "," "," "," ",1,24]
["TUPMAN_1_BIOGAS",null,"ABEC Bidart-Stockale #1",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,0.6,null,null,"FC"," "," "," "," ",1,24]
["TVYVLY_6_KRSHY1",null,"Kings River Syphon",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,null,1.3,null,null,"FC"," "," "," "," ",1,24]
["TWISSL_6_SOLAR",null,"Nickel 1 (\"NLH1\")",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"FC"," "," "," "," ",1,24]
["TWISSL_6_SOLAR1",null,"Coronal Lost Hills",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["TX-ELK_6_ECKSR2",null,"Eagle Creek",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,3,null,null,"EO"," "," "," "," ",1,24]
["TX-ELK_6_SOLAR1",null,"Castor",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["TXMCKT_6_UNIT",null,"McKittrick Cogen",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,11.2,null,null,"FC"," "," "," "," ",1,24]
["UKIAH_7_LAKEMN",null,"UKIAH LAKE MENDOCINO HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,1,3.5,null,null,"FC"," "," "," "," ",1,24]
["ULTPCH_1_UNIT 1",null,"Pacific Ultrapower Chinese Station",null,"STEAM","Biomass","BIOMASS","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,18,null,null,"FC"," "," "," "," ",1,24]
["ULTPFR_1_UNIT 1",null,"Rio Bravo Fresno",null,"STEAM","Biomass","BIOMASS","CISO","North","Fresno","Herndon",null,null,24.3,null,null,"FC"," "," "," "," ",1,24]
["ULTRCK_2_UNIT",null,"Rio Bravo Rocklin",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,24.4,null,null,"FC"," "," "," "," ",1,24]
["UNCHEM_1_UNIT",null,"CONTRA COSTA CARBON PLANT",null,"STEAM","CHP","COAL","CISO","North","Bay Area","Pittsburg",null,null,19,null,null,"FC"," "," "," "," ",1,24]
["UNOCAL_1_UNITS",null,"TOSCO (RODEO PLANT)",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,null,49.85,null,null,"FC"," "," "," "," ",1,24]
["UNVRSY_1_UNIT 1",null,"Berry Cogen 38 - Unit 1",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,null,38,null,null,"FC"," "," "," "," ",1,24]
["USWND2_1_WIND1",null,"Golden Hills A",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,42.96,null,null,"FC"," "," "," "," ",1,24]
["USWND2_1_WIND2",null,"Golden Hills B",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,42.96,null,null,"FC"," "," "," "," ",1,24]
["USWND2_1_WIND3",null,"Golden Hills C",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,null,46,null,null,"FC"," "," "," "," ",1,24]
["USWND4_2_UNIT2",null,"Altamont Landfill Gas to Energy",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1,7.4,null,null,"FC"," "," "," "," ",1,24]
["USWNDR_2_LABWD1",null,"LaBrisa Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,9,null,null,"FC"," "," "," "," ",1,24]
["USWNDR_2_SMUD",null,"SOLANO WIND FARM",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,102.18,null,null,"FC"," "," "," "," ",1,24]
["USWNDR_2_SMUD2",null,"Solano Wind Project Phase 3",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,127.8,null,null,"FC"," "," "," "," ",1,24]
["USWPFK_6_FRICK",null,"Frick Summit Wind Repower",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,10,null,null,"FC"," "," "," "," ",1,24]
["USWPJR_2_UNITS",null,"Vasco Wind",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,78.2,null,null,"FC"," "," "," "," ",1,24]
["VACADX_1_SOLAR",null,"Vaca-Dixon Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["VACADX_1_UNITA1",null,"CalPeak Power Vaca Dixon Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,51.91,null,null,"FC"," "," "," "," ",1,24]
["VALLEY_5_PERRIS",null,"MWD Perris Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,1,7.94,null,null,"FC"," "," "," "," ",1,24]
["VALLEY_5_REDMTN",null,"MWD Red Mountain Hydroelectric Recovery ",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,null,5.9,null,null,"FC"," "," "," "," ",1,24]
["VALLEY_5_SOLAR1",null,"Kona Solar - Meridian #1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,null,1.49,null,null,"EO"," "," "," "," ",1,24]
["VALLEY_5_SOLAR2",null,"AP North Lake Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["VALTNE_2_AVASR1",null,"Valentine Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,100,null,null,"FC"," "," "," "," ",1,24]
["VALTNE_2_TBBBT1","VALTNE_2_TBBBT1_SUN","Tropico Solar Big Beau",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,58,1,58,1,null,"ID",null,null,null,null,1,24]
["VALTNE_2_TBBBT1","VALTNE_2_TBBBT1_LESR","Tropico Solar Big Beau",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"CAISO System",null,58,1,18,null,null,null,1,0.8,72,72,1,24]
["VALTNE_2_TRSBT1","VALTNE_2_TRSBT1_SUN","Tropico Solar Big Beau",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,70,1,70,1,null,"ID",null,null,null,null,1,24]
["VALTNE_2_TRSBT1","VALTNE_2_TRSBT1_LESR","Tropico Solar Big Beau",null,"OTHER","Hybrid_Storage","HYBD","CISO",null,"CAISO System",null,70,1,22,null,null,null,1,0.8,88,88,1,24]
["VEAVST_1_SOLAR",null,"Community Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,14.4,null,null,"EO"," "," "," "," ",1,24]
["VEDDER_1_SEKERN",null,"TEXACO EXPLORATION & PROD (SE KERN RIVER",null,"FTUR","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,null,34.47,null,null,"FC"," "," "," "," ",1,24]
["VEGA_6_SOLAR1",null,"Vega Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["VENWD_1_WIND3",null,"Painted Hills",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,44.53,null,null,"FC"," "," "," "," ",1,24]
["VERNON_6_GONZL1",null,"H. Gonzales Unit #1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,5.75,null,null,"FC"," "," "," "," ",1,24]
["VERNON_6_GONZL2",null,"H. Gonzales Unit #2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,5.75,null,null,"FC"," "," "," "," ",1,24]
["VERNON_6_MALBRG",null,"Malburg Generating Station",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",null,1,139,null,134,"PD"," "," "," "," ",1,24]
["VESTAL_2_KERN",null,"KERN RIVER PH 3 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Vestal",null,null,36.799999999999997,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_2_RTS042",null,"SPVP042 Porterville Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,5,null,null,"EO"," "," "," "," ",1,24]
["VESTAL_2_SOLAR1",null,"NICOLIS",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_2_SOLAR2",null,"TROPICO",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,14,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_2_TS5SR1",null,"Tulare Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,null,55.83,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_2_UNIT1",null,"CALGREN-PIXLEY",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","Vestal",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_2_WELLHD",null,"Wellhead Power Delano",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","Vestal",null,1,49,null,null,"FC"," "," "," "," ",1,24]
["VESTAL_6_QF",null,"Isabella Hydro Dam 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Vestal",null,null,11.95,null,null,"FC"," "," "," "," ",1,24]
["VICTOR_1_CREST",null,"Victor Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,24.5,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_EXSLRA",null,"Expressway Solar A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["VICTOR_1_EXSLRB",null,"Expressway Solar B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,2,null,null,"FC"," "," "," "," ",1,24]
["VICTOR_1_LVSLR1",null,"Lone Valley Solar Park 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,10,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_LVSLR2",null,"Lone Valley Solar Park 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_SLRHES",null,"Sunedison - Hesperia",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_SOLAR1",null,"Victor Phelan Solar One",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,17.5,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_SOLAR2",null,"Alamo Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_SOLAR3",null,"Adelanto Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,7,null,null,"FC"," "," "," "," ",1,24]
["VICTOR_1_SOLAR4",null,"Adelanto Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,20,null,null,"EO"," "," "," "," ",1,24]
["VICTOR_1_VDRYFA",null,"Victor Dry Farm Ranch A ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,5,null,null,"FC"," "," "," "," ",1,24]
["VICTOR_1_VDRYFB",null,"Victor Dry Farm Ranch B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,null,5,null,null,"EO"," "," "," "," ",1,24]
["VILLPK_2_VALLYV",null,"MWD Valley View Hydroelectric Recovery P",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",null,1,4.0999999999999996,null,null,"FC"," "," "," "," ",1,24]
["VILLPK_6_MWDYOR",null,"Yorba Linda Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",null,1,5.0999999999999996,null,null,"FC"," "," "," "," ",1,24]
["VISTA_2_FCELL",null,"CSUSB fuel cell",null,"OTHER","Fuel Cell",null,null,"South","LA Basin",null,null,null,null,null,null,"EO"," "," "," "," ",1,24]
["VISTA_2_RIALTO",null,"Rialto RT Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,1,null,null,"FC"," "," "," "," ",1,24]
["VISTA_2_RTS028",null,"SPVP028",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,null,3.5,null,null,"FC"," "," "," "," ",1,24]
["VISTA_6_QF",null,"VISTA QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,null,0.18,null,null,"FC"," "," "," "," ",1,24]
["VISTRA_5_DALBT1",null,"Dallas Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",null,1,100,null,null,"FC",1,0.8,400,400,1,24]
["VISTRA_5_DALBT2",null,"Dallas Energy Storage 2",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",null,1,100,null,null,"FC",1,0.8,400,400,1,24]
["VISTRA_5_DALBT3",null,"Dallas Energy Storage 3",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",null,1,100,null,null,"FC",1,0.8,400,400,1,24]
["VISTRA_5_DALBT4",null,"Dallas Energy Storage 4",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",null,1,100,null,null,"FC",1,0.8,400,400,1,24]
["VISTRA_5_PLABT1",null,"Plano Storage 1",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,null,1,100.4,null,null,"FC",1,0.8,401.6,401.6,1,24]
["VISTRA_5_PLABT3",null,"Plano Storage 3",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,null,1,74.599999999999994,null,null,"FC",1,0.8,298.39999999999998,298.39999999999998,1,24]
["VLCNTR_6_VCEBT1",null,"Valley Center Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,54,null,54,"PD",1,0.8,216,216,1,24]
["VLCNTR_6_VCEBT2",null,"Valley Center Energy Storage B",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,2,85,null,50,"PD",1,0.8,340,340,1,24]
["VLCNTR_6_VCSLR",null,"Cole Grade",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,null,2.33,null,null,"FC"," "," "," "," ",1,24]
["VLCNTR_6_VCSLR1",null,"Valley Center 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,null,2.5,null,null,"FC"," "," "," "," ",1,24]
["VLCNTR_6_VCSLR2",null,"Valley Center 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,null,5,null,null,"FC"," "," "," "," ",1,24]
["VLYHOM_7_SSJID",null,"Woodward Power Plant",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,null,3,null,null,"FC"," "," "," "," ",1,24]
["VOLTA_2_UNIT 1",null,"VOLTA HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,9.1,null,null,"FC"," "," "," "," ",1,24]
["VOLTA_2_UNIT 2",null,"Volta Hydro Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1,null,null,"FC"," "," "," "," ",1,24]
["VOLTA_6_BAILCK",null,"Bailey Creek Ranch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.63,null,null,"EO"," "," "," "," ",1,24]
["VOLTA_6_DIGHYD",null,"Digger Creek Ranch Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.6,null,null,"FC"," "," "," "," ",1,24]
["VOLTA_7_PONHY1",null,"Ponderosa Bailey Hydroelectric",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,1.25,null,null,"FC"," "," "," "," ",1,24]
["VOLTA_7_QFUNTS",null,"VOLTA_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,null,0.15,null,null,"FC"," "," "," "," ",1,24]
["VOYAGR_2_VOAWD5",null,"Voyager Wind Oasis Alta",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,13.98,null,null,"FC"," "," "," "," ",1,24]
["VOYAGR_2_VOYWD1",null,"Voyager 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,128.91,null,null,"FC"," "," "," "," ",1,24]
["VOYAGR_2_VOYWD2",null,"Voyager Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,126.35,null,null,"FC"," "," "," "," ",1,24]
["VOYAGR_2_VOYWD3",null,"Voyager Wind 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,42.45,null,null,"FC"," "," "," "," ",1,24]
["VOYAGR_2_VOYWD4",null,"Voyager Wind 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,21.01,null,null,"FC"," "," "," "," ",1,24]
["VSTAES_6_VESBT1",null,"Vista Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,1,40,null,30,"PD",1,0.8,160,160,1,24]
["WADHAM_6_UNIT",null,"Wadham Energy LP",null,"STEAM","Biomass","WASTE TO POWER","CISO","North","CAISO System",null,null,null,29.07,null,null,"FC"," "," "," "," ",1,24]
["WALCRK_2_CTG1",null,"Walnut Creek Energy Park Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,97.32,null,null,"FC"," "," "," "," ",1,24]
["WALCRK_2_CTG2",null,"Walnut Creek Energy Park Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,96.91,null,null,"FC"," "," "," "," ",1,24]
["WALCRK_2_CTG3",null,"Walnut Creek Energy Park Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,96.65,null,null,"FC"," "," "," "," ",1,24]
["WALCRK_2_CTG4",null,"Walnut Creek Energy Park Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,96.6,null,null,"FC"," "," "," "," ",1,24]
["WALCRK_2_CTG5",null,"Walnut Creek Energy Park Unit 5",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",null,1,96.65,null,null,"FC"," "," "," "," ",1,24]
["WALNUT_2_SOLAR",null,"Industry MetroLink PV 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["WALNUT_6_HILLGEN",null,"Puente Hills",null,"OTHER","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,null,47,null,null,"FC"," "," "," "," ",1,24]
["WALNUT_7_WCOVST",null,"MM West Covina - ST Unit",null,"STEAM","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,null,6.5,null,null,"FC"," "," "," "," ",1,24]
["WARNE_2_UNIT",null,"WARNE HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,null,1,76,null,null,"FC"," "," "," "," ",1,24]
["WAUKNA_1_SOLAR",null,"Corcoran Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,null,20,null,null,"FC"," "," "," "," ",1,24]
["WAUKNA_1_SOLAR2",null,"Corcoran 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Hanford",null,null,19.75,null,null,"FC"," "," "," "," ",1,24]
["WDLEAF_7_UNIT 1",null,"WOODLEAF HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,1,60,null,null,"FC"," "," "," "," ",1,24]
["WEBER_6_FORWRD",null,"Forward",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,null,4.2,null,null,"FC"," "," "," "," ",1,24]
["WESTPT_2_UNIT",null,"West Point Hydro Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,14,null,null,"FC"," "," "," "," ",1,24]
["WFRESN_1_SOLAR",null,"Joya Del Sol",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,null,1.5,null,null,"EO"," "," "," "," ",1,24]
["WHEATL_6_LNDFIL",null,"G2 ENERGY, OSTROM ROAD LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra",null,null,null,3.55,null,null,"FC"," "," "," "," ",1,24]
["WHITNY_6_SOLAR",null,"Whitney Point Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,null,20,null,null,"EO"," "," "," "," ",1,24]
["WHTWTR_1_WINDA1",null,"Whitewater Hill Wind Project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,null,61.5,null,null,"FC"," "," "," "," ",1,24]
["WISE_1_UNIT 1",null,"Wise Hydro Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1,14.5,null,null,"FC"," "," "," "," ",1,24]
["WISE_1_UNIT 2",null,"WISE HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,null,3.2,null,null,"FC"," "," "," "," ",1,24]
["WISHON_6_UNITS",null,"Wishon/San Joaquin  #1-A AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,2,18.399999999999999,null,null,"FC"," "," "," "," ",1,24]
["WISTRA_2_WRSSR1",null,"Wistaria Ranch Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,null,100,null,null,"FC"," "," "," "," ",1,24]
["WLDWD_1_SOLAR1",null,"Wildwood Solar I",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,20,null,null,"FC"," "," "," "," ",1,24]
["WLDWD_1_SOLAR2",null,"Wildwood Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,null,15,null,null,"FC"," "," "," "," ",1,24]
["WNDMAS_2_UNIT 1",null,"BUENA VISTA ENERGY, LLC",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,38,null,null,"FC"," "," "," "," ",1,24]
["WNDSTR_2_WIND",null,"Windstar",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,120,null,null,"FC"," "," "," "," ",1,24]
["WOLFSK_1_UNITA1",null,"Wolfskill Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,1,48.68,null,null,"FC"," "," "," "," ",1,24]
["WOODWR_1_HYDRO",null,"Quinten Luallen",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,null,7.3,null,null,"EO"," "," "," "," ",1,24]
["WRGHTP_7_AMENGY",null,"SMALL QF AGGREGATION - LOS BANOS",null,"HYDRO","Hydro",null,null,"North","Fresno",null,null,null,null,null,null,"FC"," "," "," "," ",1,24]
["WRGTSR_2_WSFSR1",null,"Wright Solar Freeman",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,null,200,null,null,"FC"," "," "," "," ",1,24]
["WSENGY_1_UNIT 1",null,"Wheelabrator Shasta",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,null,50,null,null,"FC"," "," "," "," ",1,24]
["WSTWND_2_M89BT2",null,"Mojave 89 BESS 2B",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,null,70.599999999999994,null,null,"EO",1,0.8,282.39999999999998,282.39999999999998,1,24]
["WSTWND_2_M89WD1",null,"Mojave 89",null,"OTHER","Wind","HYBD","CISO","South","CAISO System",null,null,1,82.65,null,null,"FC"," "," "," "," ",1,24]
["WSTWND_2_M89WD2",null,"Mojave 89 Wind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,82.65,null,null,"FC"," "," "," "," ",1,24]
["WSTWND_2_M90WD2",null,"Mojave 90",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,null,64.819999999999993,null,null,"FC"," "," "," "," ",1,24]
["WSTWND_2_SBSBT1",null,"Sagebrush Solar 2",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,null,80,1,null,"ID",1,0.8,320,320,1,24]
["YELPIN_2_YP2BT1",null,"Yellow Pine 2 BESS",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,null,null,65,null,65,"ID",1,0.8,260,260,1,24]
["YUBACT_1_SUNSWT",null,"YUBA CITY COGEN",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",null,1,49.97,null,null,"FC"," "," "," "," ",1,24]
["YUBACT_6_UNITA1",null,"Yuba City Energy Center (Calpine)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",null,1,47.16,null,null,"FC"," "," "," "," ",1,24]
["ZOND_6_UNIT",null,"ZOND WINDSYSTEMS INC.",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,null,17.100000000000001,null,null,"FC"," "," "," "," ",1,24]
["ALHMBR_1_ALHSLR",null,"Alhambra (Solar Gen 2) ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["ANZA_6_SOLAR1",null,"Seville Solar One",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID",null,null,null,null,null,20,null,null,null," "," "," "," ",1,24]
["ARKANS_1_ARKSLR",null,"Arkansas (Solar Gen 2)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["ARLINT_5_SCEDYN",null,"Arlington Valley CC",null,"COMBINED CYCLE","CCGT","NATURAL GAS","AZPS",null,null,null,null,null,565,null,null,null," "," "," "," ",1,24]
["ARLVAL_5_SOLAR",null,"Arlington Valley Solar Energy II",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","SRP",null,null,null,null,null,127,null,null,null," "," "," "," ",1,24]
["BCTSYS_5_PWXDYN",null,"BCTSYS_5_PWXDYN",null,"HYDRO","Hydro","WATER","BPAT",null,null,null,null,null,428,null,null,null," "," "," "," ",1,24]
["BEJNLS_5_BV2SCEDYN",null,"Broadview 2",null,"WIND","Wind","WIND","AZPS",null,null,null,null,null,167,null,null,null," "," "," "," ",1,24]
["BEKWJS_5_BV1SCEDYN",null,"Broadview 1",null,"WIND","Wind","WIND","AZPS",null,null,null,null,null,130,null,null,null," "," "," "," ",1,24]
["CALPSS_6_SOLAR1",null,"Calipatria Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,19.899999999999999,null,null,null," "," "," "," ",1,24]
["CLINESCO_3_PVDYN",null,"CLINES CORNERS",null,"WIND","Wind","WIND","PNM",null,null,null,null,null,129.94,null,null,null," "," "," "," ",1,24]
["CLINESCO_3_WBDYN",null,"CLINES CORNERS B",null,"WIND","Wind","WIND","PNM",null,null,null,null,null,194.28,null,null,null," "," "," "," ",1,24]
["COLGNS_2_CNSSR1",null,"ColGreen North Shore ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,74.8,null,null,null," "," "," "," ",1,24]
["DURNMESA_3_WBDYN",null,"DURAN MESA",null,"WIND","Wind","WIND","PNM",null,null,null,null,null,105.08,null,null,null," "," "," "," ",1,24]
["ELCABO_5_ECWSCEDYN",null,"El Cabo Wind",null,"WIND","Wind","WIND","AZPS",null,null,null,null,null,298,null,null,null," "," "," "," ",1,24]
["GRADYW_5_GDYWD1",null,"Grady Wind",null,"WIND","Wind","WIND","AZPS",null,null,null,null,null,200,null,null,null," "," "," "," ",1,24]
["GRIFFI_2_LSPDYN",null,"Griffith Energy",null,"COMBINED CYCLE","CCGT","NATURAL GAS","WALC",null,null,null,null,null,570,null,null,null," "," "," "," ",1,24]
["HOOV_2_ANAPT",null,"Hoover Power Plant",null,"HYDRO","Hydro","WATER","WALC",null,null,null,null,null,40.39,null,null,null," "," "," "," ",1,24]
["HOOVER_2_MWDPT",null,"HOOVER MWD",null,"HYDRO","Hydro","WATER","WALC",null,null,null,null,1,249,null,null,null," "," "," "," ",1,24]
["HOOVER_2_SCEPT",null,"Hoover DAM - SCE Share",null,"HYDRO","Hydro","WATER","WALC",null,null,null,null,1,287,null,null,null," "," "," "," ",1,24]
["HOOVER_2_VEAPT",null,"HOOVER VEA",null,"HYDRO","Hydro","WATER","WALC",null,null,null,null,1,16,null,null,null," "," "," "," ",1,24]
["INTMNT_3_ANAHEIM",null,"Intermountain Power Project",null,"STEAM","Coal","COAL","LADWP",null,null,null,null,1,234,null,null,null," "," "," "," ",1,24]
["INTMNT_3_PASADENA",null,"Intermountain Power Project",null,"STEAM","Coal","COAL","LADWP",null,null,null,null,null,107,null,null,null," "," "," "," ",1,24]
["INTMNT_3_RIVERSIDE",null,"IPPDYN",null,"STEAM","Coal","COAL","LADWP",null,null,null,null,1,136,null,null,null," "," "," "," ",1,24]
["MAGNLA_6_ANAHEIM",null,"Magnolia Power Plant Anaheim",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP",null,null,null,null,1,109,null,null,null," "," "," "," ",1,24]
["MAGNLA_6_CERRITOS",null,"Magnolia Power Plant Cerritos",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP",null,null,null,null,null,12,null,null,null," "," "," "," ",1,24]
["MAGNLA_6_COLTON",null,"Magnolia Power Project",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP",null,null,null,null,null,12,null,null,null," "," "," "," ",1,24]
["MAGNLA_6_PASADENA",null,"Magnolia Power Plant - PASADENA",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP",null,null,null,null,null,18,null,null,null," "," "," "," ",1,24]
["MALIN_5_BPADYN",null,"MALIN_5_BPADYN",null,"HYDRO","Hydro","WATER","BPAT",null,null,null,null,null,700,null,null,null," "," "," "," ",1,24]
["MALIN_5_GCPDDYN",null,"Grant County Hydro Facilities",null,"HYDRO","Hydro","WATER","BPAT",null,null,null,null,null,125,null,null,null," "," "," "," ",1,24]
["MALIN_5_HERMDYN",null,"MALIN_5_HERMDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","BPAT",null,null,null,null,null,308,null,null,null," "," "," "," ",1,24]
["MALIN_5_IBERDR",null,"Iberdrola Centroid Sytem Resource",null,"WIND","Wind","WIND","BPAT",null,null,null,null,null,100,null,null,null," "," "," "," ",1,24]
["MALIN_5_INHRED",null,"CSF Columbia Gorge",null,"WIND","Wind","WIND","BPAT",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["MALIN_5_INHRPG",null,"BIGLOW CANYON",null,"WIND","Wind","WIND","BPAT",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["MIDWY3_2_MDSSR1",null,"Midway South Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,20,null,null,null," "," "," "," ",1,24]
["MIDWYS_2_MIDSL1",null,"Midway Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,49.9,null,null,null," "," "," "," ",1,24]
["MILFRD_7_PASADENA",null,"Milford I",null,"WIND","Wind","WIND","LADWP",null,null,null,null,null,5,null,null,null," "," "," "," ",1,24]
["MSQUIT_5_SERDYN",null,"MSQUIT_5_SERDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","SRP",null,null,null,null,null,625,null,null,null," "," "," "," ",1,24]
["NGILAA_5_SDGDYN",null,"NGILAA_5_SDGDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","AZPS",null,null,null,null,null,55,null,null,null," "," "," "," ",1,24]
["PVERDE_5_SCEDYN",null,"PVERDE_5_SCEDYN",null,"STEAM","Nuclear","URANIUM","SRP",null,null,null,null,null,635,null,null,null," "," "," "," ",1,24]
["RAMON_2_SCEDYN",null,"RAMON_2_SCEDYN",null,"OTHER","Geothermal","GEOTHERMAL","IID",null,null,null,null,null,106.18,null,null,null," "," "," "," ",1,24]
["SIGHEB_6_HE2SCEDYN",null,"Heber 2",null,"COMBUSTION TURBINE","Geothermal","GEOTHERMAL","IID",null,null,null,null,null,28,null,null,null," "," "," "," ",1,24]
["SIGHEB_6_MIRDYN",null,"Heber South",null,"COMBUSTION TURBINE","Geothermal","GEOTHERMAL","IID",null,null,null,null,null,17,null,null,null," "," "," "," ",1,24]
["SNORA_2_SNRSLR",null,"Sonora (Solar Gen 2)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["SUNSTR_5_SS1SCEDYN",null,"Sunstream Solar 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","AZPS",null,null,null,null,null,150,null,null,null," "," "," "," ",1,24]
["SUTTER_2_CISO",null,"Sutter Power Plant Pseudo-CISO",null,"COMBINED CYCLE","CCGT","NATURAL GAS","BANC",null,null,null,null,null,275,null,null,null," "," "," "," ",1,24]
["TECOLOTE_3_WBDYN",null,"TECOLOTE WIND",null,"WIND","Wind","WIND","PNM",null,null,null,null,null,271.68,null,null,null," "," "," "," ",1,24]
["TITANS_2_TTSSR1",null,"Titan Solar 1 Pseudo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID",null,null,null,null,null,70,null,null,null," "," "," "," ",1,24]
["TOWNSITE_2_MEADDYN","TOWNSITE_2_MEADDYN_SUN","Townsite Solar BESS",null,"OTHER","Hybrid_Solar1Axis","OTHER","WALC",null,null,null,180,2,180,null,null,null," "," "," "," ",1,24]
["TOWNSITE_2_MEADDYN","TOWNSITE_2_MEADDYN_LESR","Townsite Solar BESS",null,"OTHER","Hybrid_Storage","OTHER","WALC",null,null,null,180,2,180,null,null,null,1,0.8,720,720,1,24]
["WHITEH_2_MEADDYN1",null,"White Hills A",null,"WIND","Wind","WIND","WALC",null,null,null,null,null,50,null,null,null," "," "," "," ",1,24]
["WHITEH_2_MEADDYN2",null,"White Hills B",null,"WIND","Wind","WIND","WALC",null,null,null,null,null,300,null,null,null," "," "," "," ",1,24]
["WISTER_2_WISSR1",null,"Wister Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID",null,null,null,null,null,20,null,null,null," "," "," "," ",1,24]
["WSNR_2_CVPDYN",null,"Central Valley 1",null,"HYDRO","Hydro","WATER","BANC",null,null,null,null,null,10,null,null,null," "," "," "," ",1,24]
["WSNR_2_TESLADYN",null,"Central Valley Tesla",null,"HYDRO","Hydro","WATER","BANC",null,null,null,null,null,10,null,null,null," "," "," "," ",1,24]
["WSNR_5_TRCYDYN",null,"Central Valley Tracy",null,"HYDRO","Hydro","WATER","BANC",null,null,null,null,null,10,null,null,null," "," "," "," ",1,24]
["CAM Storage 1",null,"CAM Storage Allocation Group #1",null,"4Hr_Li","Battery Storage","LESR","CISO","North","CAISO System",null,null,null,482.5,null,null,null,1,0.8,1930,800,1,24,4]
["CAM Storage 2",null,"CAM Storage Allocation Group #2",null,"4Hr_Li","Battery Storage","LESR","CISO","South","CAISO System",null,null,null,20,null,null,null,2.79,0.87,80,1000,1,24,11.16578]

{"sheet":"Resource NQC","index":27,"n_rows":13483,"n_cols":3,"rows_kept":13483,"cut":false,"hidden":false,"merged":[]}
["Resource ID","Month","NQC MW"]
["7STDRD_1_SOLAR1",1,0.08]
["7STDRD_1_SOLAR1",2,0.6]
["7STDRD_1_SOLAR1",3,0.7]
["7STDRD_1_SOLAR1",4,0.88]
["7STDRD_1_SOLAR1",5,1.28]
["7STDRD_1_SOLAR1",6,2.62]
["7STDRD_1_SOLAR1",7,2.88]
["7STDRD_1_SOLAR1",8,2.48]
["7STDRD_1_SOLAR1",9,2.2200000000000002]
["7STDRD_1_SOLAR1",10,1.48]
["7STDRD_1_SOLAR1",11,1.1399999999999999]
["7STDRD_1_SOLAR1",12,0.7]
["ACACIA_6_SOLAR",1,0.08]
["ACACIA_6_SOLAR",2,0.6]
["ACACIA_6_SOLAR",3,0.7]
["ACACIA_6_SOLAR",4,0.88]
["ACACIA_6_SOLAR",5,1.28]
["ACACIA_6_SOLAR",6,2.62]
["ACACIA_6_SOLAR",7,2.88]
["ACACIA_6_SOLAR",8,2.48]
["ACACIA_6_SOLAR",9,2.2200000000000002]
["ACACIA_6_SOLAR",10,1.48]
["ACACIA_6_SOLAR",11,1.1399999999999999]
["ACACIA_6_SOLAR",12,0.7]
["ADERA_1_SOLAR1",1,0]
["ADERA_1_SOLAR1",2,0]
["ADERA_1_SOLAR1",3,0]
["ADERA_1_SOLAR1",4,0]
["ADERA_1_SOLAR1",5,0]
["ADERA_1_SOLAR1",6,0]
["ADERA_1_SOLAR1",7,0]
["ADERA_1_SOLAR1",8,0]
["ADERA_1_SOLAR1",9,0]
["ADERA_1_SOLAR1",10,0]
["ADERA_1_SOLAR1",11,0]
["ADERA_1_SOLAR1",12,0]
["ADLIN_1_UNITS",1,22]
["ADLIN_1_UNITS",2,22]
["ADLIN_1_UNITS",3,22]
["ADLIN_1_UNITS",4,22]
["ADLIN_1_UNITS",5,22]
["ADLIN_1_UNITS",6,22]
["ADLIN_1_UNITS",7,22]
["ADLIN_1_UNITS",8,22]
["ADLIN_1_UNITS",9,22]
["ADLIN_1_UNITS",10,22]
["ADLIN_1_UNITS",11,22]
["ADLIN_1_UNITS",12,22]
["ADMEST_6_SOLAR",1,0]
["ADMEST_6_SOLAR",2,0]
["ADMEST_6_SOLAR",3,0]
["ADMEST_6_SOLAR",4,0]
["ADMEST_6_SOLAR",5,0]
["ADMEST_6_SOLAR",6,0]
["ADMEST_6_SOLAR",7,0]
["ADMEST_6_SOLAR",8,0]
["ADMEST_6_SOLAR",9,0]
["ADMEST_6_SOLAR",10,0]
["ADMEST_6_SOLAR",11,0]
["ADMEST_6_SOLAR",12,0]
["ADOBEE_1_SOLAR",1,0.08]
["ADOBEE_1_SOLAR",2,0.6]
["ADOBEE_1_SOLAR",3,0.7]
["ADOBEE_1_SOLAR",4,0.88]
["ADOBEE_1_SOLAR",5,1.28]
["ADOBEE_1_SOLAR",6,2.62]
["ADOBEE_1_SOLAR",7,2.88]
["ADOBEE_1_SOLAR",8,2.48]
["ADOBEE_1_SOLAR",9,2.2200000000000002]
["ADOBEE_1_SOLAR",10,1.48]
["ADOBEE_1_SOLAR",11,1.1399999999999999]
["ADOBEE_1_SOLAR",12,0.7]
["AGRICO_6_PL3N5",1,22.69]
["AGRICO_6_PL3N5",2,22.69]
["AGRICO_6_PL3N5",3,22.69]
["AGRICO_6_PL3N5",4,22.69]
["AGRICO_6_PL3N5",5,22.69]
["AGRICO_6_PL3N5",6,22.69]
["AGRICO_6_PL3N5",7,22.69]
["AGRICO_6_PL3N5",8,22.69]
["AGRICO_6_PL3N5",9,22.69]
["AGRICO_6_PL3N5",10,22.69]
["AGRICO_6_PL3N5",11,22.69]
["AGRICO_6_PL3N5",12,22.69]
["AGRICO_7_UNIT",1,48.58]
["AGRICO_7_UNIT",2,48.58]
["AGRICO_7_UNIT",3,48.58]
["AGRICO_7_UNIT",4,48.58]
["AGRICO_7_UNIT",5,48.58]
["AGRICO_7_UNIT",6,48.58]
["AGRICO_7_UNIT",7,48.58]
["AGRICO_7_UNIT",8,48.58]
["AGRICO_7_UNIT",9,48.58]
["AGRICO_7_UNIT",10,48.58]
["AGRICO_7_UNIT",11,48.58]
["AGRICO_7_UNIT",12,48.58]
["AGUCAL_5_SOLAR1",1,0]
["AGUCAL_5_SOLAR1",2,0]
["AGUCAL_5_SOLAR1",3,0]
["AGUCAL_5_SOLAR1",4,0]
["AGUCAL_5_SOLAR1",5,0]
["AGUCAL_5_SOLAR1",6,0]
["AGUCAL_5_SOLAR1",7,0]
["AGUCAL_5_SOLAR1",8,0]
["AGUCAL_5_SOLAR1",9,0]
["AGUCAL_5_SOLAR1",10,0]
["AGUCAL_5_SOLAR1",11,0]
["AGUCAL_5_SOLAR1",12,0]
["AKINGS_6_AMESR1",1,0.49]
["AKINGS_6_AMESR1",2,3.69]
["AKINGS_6_AMESR1",3,4.3099999999999996]
["AKINGS_6_AMESR1",4,5.41]
["AKINGS_6_AMESR1",5,7.87]
["AKINGS_6_AMESR1",6,16.11]
["AKINGS_6_AMESR1",7,17.71]
["AKINGS_6_AMESR1",8,15.25]
["AKINGS_6_AMESR1",9,13.65]
["AKINGS_6_AMESR1",10,9.1]
["AKINGS_6_AMESR1",11,7.01]
["AKINGS_6_AMESR1",12,4.3099999999999996]
["ALAMIT_2_PL1X3",1,674.7]
["ALAMIT_2_PL1X3",2,674.7]
["ALAMIT_2_PL1X3",3,674.7]
["ALAMIT_2_PL1X3",4,674.7]
["ALAMIT_2_PL1X3",5,674.7]
["ALAMIT_2_PL1X3",6,674.7]
["ALAMIT_2_PL1X3",7,674.7]
["ALAMIT_2_PL1X3",8,674.7]
["ALAMIT_2_PL1X3",9,674.7]
["ALAMIT_2_PL1X3",10,674.7]
["ALAMIT_2_PL1X3",11,674.7]
["ALAMIT_2_PL1X3",12,674.7]
["ALAMIT_7_ES1",1,100]
["ALAMIT_7_ES1",2,100]
["ALAMIT_7_ES1",3,100]
["ALAMIT_7_ES1",4,100]
["ALAMIT_7_ES1",5,100]
["ALAMIT_7_ES1",6,100]
["ALAMIT_7_ES1",7,100]
["ALAMIT_7_ES1",8,100]
["ALAMIT_7_ES1",9,100]
["ALAMIT_7_ES1",10,100]
["ALAMIT_7_ES1",11,100]
["ALAMIT_7_ES1",12,100]
["ALAMIT_7_UNIT 3",1,326.76]
["ALAMIT_7_UNIT 3",2,326.76]
["ALAMIT_7_UNIT 3",3,326.76]
["ALAMIT_7_UNIT 3",4,326.76]
["ALAMIT_7_UNIT 3",5,326.76]
["ALAMIT_7_UNIT 3",6,326.76]
["ALAMIT_7_UNIT 3",7,326.76]
["ALAMIT_7_UNIT 3",8,326.76]
["ALAMIT_7_UNIT 3",9,326.76]
["ALAMIT_7_UNIT 3",10,326.76]
["ALAMIT_7_UNIT 3",11,326.76]
["ALAMIT_7_UNIT 3",12,326.76]
["ALAMIT_7_UNIT 4",1,334.43]
["ALAMIT_7_UNIT 4",2,334.43]
["ALAMIT_7_UNIT 4",3,334.43]
["ALAMIT_7_UNIT 4",4,334.43]
["ALAMIT_7_UNIT 4",5,334.43]
["ALAMIT_7_UNIT 4",6,334.43]
["ALAMIT_7_UNIT 4",7,334.43]
["ALAMIT_7_UNIT 4",8,334.43]
["ALAMIT_7_UNIT 4",9,334.43]
["ALAMIT_7_UNIT 4",10,334.43]
["ALAMIT_7_UNIT 4",11,334.43]
["ALAMIT_7_UNIT 4",12,334.43]
["ALAMIT_7_UNIT 5",1,480]
["ALAMIT_7_UNIT 5",2,480]
["ALAMIT_7_UNIT 5",3,480]
["ALAMIT_7_UNIT 5",4,480]
["ALAMIT_7_UNIT 5",5,480]
["ALAMIT_7_UNIT 5",6,480]
["ALAMIT_7_UNIT 5",7,480]
["ALAMIT_7_UNIT 5",8,480]
["ALAMIT_7_UNIT 5",9,480]
["ALAMIT_7_UNIT 5",10,480]
["ALAMIT_7_UNIT 5",11,480]
["ALAMIT_7_UNIT 5",12,480]
["ALAMO_6_UNIT",1,2.5499999999999998]
["ALAMO_6_UNIT",2,2.69]
["ALAMO_6_UNIT",3,2.75]
["ALAMO_6_UNIT",4,8.6999999999999993]
["ALAMO_6_UNIT",5,8.33]
["ALAMO_6_UNIT",6,8.4499999999999993]
["ALAMO_6_UNIT",7,14]
["ALAMO_6_UNIT",8,13.07]
["ALAMO_6_UNIT",9,9.5399999999999991]
["ALAMO_6_UNIT",10,4.37]
["ALAMO_6_UNIT",11,0]
["ALAMO_6_UNIT",12,0]
["ALLGNY_6_HYDRO1",1,0.11]
["ALLGNY_6_HYDRO1",2,0.22]
["ALLGNY_6_HYDRO1",3,0.31]
["ALLGNY_6_HYDRO1",4,0.49]
["ALLGNY_6_HYDRO1",5,0.48]
["ALLGNY_6_HYDRO1",6,0.25]
["ALLGNY_6_HYDRO1",7,0.09]
["ALLGNY_6_HYDRO1",8,0.03]
["ALLGNY_6_HYDRO1",9,0]
["ALLGNY_6_HYDRO1",10,0.03]
["ALLGNY_6_HYDRO1",11,0.14000000000000001]
["ALLGNY_6_HYDRO1",12,0.16]
["ALMASL_2_AL6BT6",1,50]
["ALMASL_2_AL6BT6",2,50]
["ALMASL_2_AL6BT6",3,50]
["ALMASL_2_AL6BT6",4,50]
["ALMASL_2_AL6BT6",5,50]
["ALMASL_2_AL6BT6",6,50]
["ALMASL_2_AL6BT6",7,50]
["ALMASL_2_AL6BT6",8,50]
["ALMASL_2_AL6BT6",9,50]
["ALMASL_2_AL6BT6",10,50]
["ALMASL_2_AL6BT6",11,50]
["ALMASL_2_AL6BT6",12,50]
["ALMASL_2_GS1SR1",1,0.5]
["ALMASL_2_GS1SR1",2,3.75]
["ALMASL_2_GS1SR1",3,4.38]
["ALMASL_2_GS1SR1",4,5.5]
["ALMASL_2_GS1SR1",5,8]
["ALMASL_2_GS1SR1",6,16.38]
["ALMASL_2_GS1SR1",7,18]
["ALMASL_2_GS1SR1",8,15.5]
["ALMASL_2_GS1SR1",9,13.88]
["ALMASL_2_GS1SR1",10,9.25]
["ALMASL_2_GS1SR1",11,7.13]
["ALMASL_2_GS1SR1",12,4.38]
["ALMASL_2_GS4SR4",1,0.4]
["ALMASL_2_GS4SR4",2,3]
["ALMASL_2_GS4SR4",3,3.5]
["ALMASL_2_GS4SR4",4,4.4000000000000004]
["ALMASL_2_GS4SR4",5,6.4]
["ALMASL_2_GS4SR4",6,13.1]
["ALMASL_2_GS4SR4",7,14.4]
["ALMASL_2_GS4SR4",8,12.4]
["ALMASL_2_GS4SR4",9,11.1]
["ALMASL_2_GS4SR4",10,7.4]
["ALMASL_2_GS4SR4",11,5.7]
["ALMASL_2_GS4SR4",12,3.5]
["ALMASL_2_GS6SR6",1,0.1]
["ALMASL_2_GS6SR6",2,0.95]
["ALMASL_2_GS6SR6",3,1.18]
["ALMASL_2_GS6SR6",4,1.63]
["ALMASL_2_GS6SR6",5,2.4300000000000002]
["ALMASL_2_GS6SR6",6,5.08]
["ALMASL_2_GS6SR6",7,5.57]
["ALMASL_2_GS6SR6",8,4.7]
["ALMASL_2_GS6SR6",9,4]
["ALMASL_2_GS6SR6",10,2.5]
["ALMASL_2_GS6SR6",11,1.74]
["ALMASL_2_GS6SR6",12,0.84]
["ALMASL_2_GS7SR7",1,0.53]
["ALMASL_2_GS7SR7",2,3.96]
["ALMASL_2_GS7SR7",3,4.62]
["ALMASL_2_GS7SR7",4,5.81]
["ALMASL_2_GS7SR7",5,8.4499999999999993]
["ALMASL_2_GS7SR7",6,17.29]
["ALMASL_2_GS7SR7",7,19.010000000000002]
["ALMASL_2_GS7SR7",8,16.37]
["ALMASL_2_GS7SR7",9,14.65]
["ALMASL_2_GS7SR7",10,9.77]
["ALMASL_2_GS7SR7",11,7.52]
["ALMASL_2_GS7SR7",12,4.62]
["ALMEGT_1_UNIT 1",1,23.4]
["ALMEGT_1_UNIT 1",2,23.4]
["ALMEGT_1_UNIT 1",3,23.4]
["ALMEGT_1_UNIT 1",4,23.4]
["ALMEGT_1_UNIT 1",5,23.4]
["ALMEGT_1_UNIT 1",6,23.4]
["ALMEGT_1_UNIT 1",7,23.4]
["ALMEGT_1_UNIT 1",8,23.4]
["ALMEGT_1_UNIT 1",9,23.4]
["ALMEGT_1_UNIT 1",10,23.4]
["ALMEGT_1_UNIT 1",11,23.4]
["ALMEGT_1_UNIT 1",12,23.4]
["ALMEGT_1_UNIT 2",1,23.5]
["ALMEGT_1_UNIT 2",2,23.5]
["ALMEGT_1_UNIT 2",3,23.5]
["ALMEGT_1_UNIT 2",4,23.5]
["ALMEGT_1_UNIT 2",5,23.5]
["ALMEGT_1_UNIT 2",6,23.5]
["ALMEGT_1_UNIT 2",7,23.5]
["ALMEGT_1_UNIT 2",8,23.5]
["ALMEGT_1_UNIT 2",9,23.5]
["ALMEGT_1_UNIT 2",10,23.5]
["ALMEGT_1_UNIT 2",11,23.5]
["ALMEGT_1_UNIT 2",12,23.5]
["ALPSLR_1_NTHSLR",1,0.08]
["ALPSLR_1_NTHSLR",2,0.6]
["ALPSLR_1_NTHSLR",3,0.7]
["ALPSLR_1_NTHSLR",4,0.88]
["ALPSLR_1_NTHSLR",5,1.28]
["ALPSLR_1_NTHSLR",6,2.62]
["ALPSLR_1_NTHSLR",7,2.88]
["ALPSLR_1_NTHSLR",8,2.48]
["ALPSLR_1_NTHSLR",9,2.2200000000000002]
["ALPSLR_1_NTHSLR",10,1.48]
["ALPSLR_1_NTHSLR",11,1.1399999999999999]
["ALPSLR_1_NTHSLR",12,0.7]
["ALPSLR_1_SPSSLR",1,0.2]
["ALPSLR_1_SPSSLR",2,1.5]
["ALPSLR_1_SPSSLR",3,1.75]
["ALPSLR_1_SPSSLR",4,2.2000000000000002]
["ALPSLR_1_SPSSLR",5,3.2]
["ALPSLR_1_SPSSLR",6,6.55]
["ALPSLR_1_SPSSLR",7,7.2]
["ALPSLR_1_SPSSLR",8,6.2]
["ALPSLR_1_SPSSLR",9,5.55]
["ALPSLR_1_SPSSLR",10,3.7]
["ALPSLR_1_SPSSLR",11,2.85]
["ALPSLR_1_SPSSLR",12,1.75]
["ALT6DN_2_WIND7",1,29.03]
["ALT6DN_2_WIND7",2,30.88]
["ALT6DN_2_WIND7",3,27.13]
["ALT6DN_2_WIND7",4,25.99]
["ALT6DN_2_WIND7",5,27.64]
["ALT6DN_2_WIND7",6,25.34]
["ALT6DN_2_WIND7",7,23.54]
["ALT6DN_2_WIND7",8,17.89]
["ALT6DN_2_WIND7",9,18.48]
["ALT6DN_2_WIND7",10,17.14]
["ALT6DN_2_WIND7",11,23.1]
["ALT6DN_2_WIND7",12,27.98]
["ALT6DS_2_WIND9",1,23.32]
["ALT6DS_2_WIND9",2,24.81]
["ALT6DS_2_WIND9",3,21.8]
["ALT6DS_2_WIND9",4,20.88]
["ALT6DS_2_WIND9",5,22.21]
["ALT6DS_2_WIND9",6,20.350000000000001]
["ALT6DS_2_WIND9",7,18.91]
["ALT6DS_2_WIND9",8,14.37]
["ALT6DS_2_WIND9",9,14.84]
["ALT6DS_2_WIND9",10,13.77]
["ALT6DS_2_WIND9",11,18.559999999999999]
["ALT6DS_2_WIND9",12,22.48]
["ALTA3A_2_CPCE4",1,18.02]
["ALTA3A_2_CPCE4",2,19.170000000000002]
["ALTA3A_2_CPCE4",3,16.84]
["ALTA3A_2_CPCE4",4,16.14]
["ALTA3A_2_CPCE4",5,17.16]
["ALTA3A_2_CPCE4",6,15.73]
["ALTA3A_2_CPCE4",7,14.61]
["ALTA3A_2_CPCE4",8,11.1]
["ALTA3A_2_CPCE4",9,11.47]
["ALTA3A_2_CPCE4",10,10.64]
["ALTA3A_2_CPCE4",11,14.34]
["ALTA3A_2_CPCE4",12,17.37]
["ALTA3A_2_CPCE5",1,29.69]
["ALTA3A_2_CPCE5",2,31.57]
["ALTA3A_2_CPCE5",3,27.74]
["ALTA3A_2_CPCE5",4,26.58]
["ALTA3A_2_CPCE5",5,28.26]
["ALTA3A_2_CPCE5",6,25.91]
["ALTA3A_2_CPCE5",7,24.07]
["ALTA3A_2_CPCE5",8,18.29]
["ALTA3A_2_CPCE5",9,18.89]
["ALTA3A_2_CPCE5",10,17.53]
["ALTA3A_2_CPCE5",11,23.62]
["ALTA3A_2_CPCE5",12,28.61]
["ALTA3A_2_CPCE8",1,26.51]
["ALTA3A_2_CPCE8",2,28.19]
["ALTA3A_2_CPCE8",3,24.77]
["ALTA3A_2_CPCE8",4,23.73]
["ALTA3A_2_CPCE8",5,25.23]
["ALTA3A_2_CPCE8",6,23.13]
["ALTA3A_2_CPCE8",7,21.49]
["ALTA3A_2_CPCE8",8,16.329999999999998]
["ALTA3A_2_CPCE8",9,16.87]
["ALTA3A_2_CPCE8",10,15.65]
["ALTA3A_2_CPCE8",11,21.09]
["ALTA3A_2_CPCE8",12,25.55]
["ALTA4A_2_CPCW1",1,26.51]
["ALTA4A_2_CPCW1",2,28.19]
["ALTA4A_2_CPCW1",3,24.77]
["ALTA4A_2_CPCW1",4,23.73]
["ALTA4A_2_CPCW1",5,25.23]
["ALTA4A_2_CPCW1",6,23.13]
["ALTA4A_2_CPCW1",7,21.49]
["ALTA4A_2_CPCW1",8,16.329999999999998]
["ALTA4A_2_CPCW1",9,16.87]
["ALTA4A_2_CPCW1",10,15.65]
["ALTA4A_2_CPCW1",11,21.09]
["ALTA4A_2_CPCW1",12,25.55]
["ALTA4B_2_CPCW2",1,26.51]
["ALTA4B_2_CPCW2",2,28.19]
["ALTA4B_2_CPCW2",3,24.77]
["ALTA4B_2_CPCW2",4,23.73]
["ALTA4B_2_CPCW2",5,25.23]
["ALTA4B_2_CPCW2",6,23.13]
["ALTA4B_2_CPCW2",7,21.49]
["ALTA4B_2_CPCW2",8,16.329999999999998]
["ALTA4B_2_CPCW2",9,16.87]
["ALTA4B_2_CPCW2",10,15.65]
["ALTA4B_2_CPCW2",11,21.09]
["ALTA4B_2_CPCW2",12,25.55]
["ALTA4B_2_CPCW3",1,26.51]
["ALTA4B_2_CPCW3",2,28.19]
["ALTA4B_2_CPCW3",3,24.77]
["ALTA4B_2_CPCW3",4,23.73]
["ALTA4B_2_CPCW3",5,25.23]
["ALTA4B_2_CPCW3",6,23.13]
["ALTA4B_2_CPCW3",7,21.49]
["ALTA4B_2_CPCW3",8,16.329999999999998]
["ALTA4B_2_CPCW3",9,16.87]
["ALTA4B_2_CPCW3",10,15.65]
["ALTA4B_2_CPCW3",11,21.09]
["ALTA4B_2_CPCW3",12,25.55]
["ALTA4B_2_CPCW6",1,26.51]
["ALTA4B_2_CPCW6",2,28.19]
["ALTA4B_2_CPCW6",3,24.77]
["ALTA4B_2_CPCW6",4,23.73]
["ALTA4B_2_CPCW6",5,25.23]
["ALTA4B_2_CPCW6",6,23.13]
["ALTA4B_2_CPCW6",7,21.49]
["ALTA4B_2_CPCW6",8,16.329999999999998]
["ALTA4B_2_CPCW6",9,16.87]
["ALTA4B_2_CPCW6",10,15.65]
["ALTA4B_2_CPCW6",11,21.09]
["ALTA4B_2_CPCW6",12,25.55]
["ALTA6B_2_WIND11",1,15.58]
["ALTA6B_2_WIND11",2,16.57]
["ALTA6B_2_WIND11",3,14.56]
["ALTA6B_2_WIND11",4,13.95]
["ALTA6B_2_WIND11",5,14.83]
["ALTA6B_2_WIND11",6,13.59]
["ALTA6B_2_WIND11",7,12.63]
["ALTA6B_2_WIND11",8,9.6]
["ALTA6B_2_WIND11",9,9.91]
["ALTA6B_2_WIND11",10,9.1999999999999993]
["ALTA6B_2_WIND11",11,12.39]
["ALTA6B_2_WIND11",12,15.01]
["ALTA6E_2_WIND10",1,23.83]
["ALTA6E_2_WIND10",2,25.34]
["ALTA6E_2_WIND10",3,22.27]
["ALTA6E_2_WIND10",4,21.33]
["ALTA6E_2_WIND10",5,22.68]
["ALTA6E_2_WIND10",6,20.79]
["ALTA6E_2_WIND10",7,19.32]
["ALTA6E_2_WIND10",8,14.68]
["ALTA6E_2_WIND10",9,15.16]
["ALTA6E_2_WIND10",10,14.07]
["ALTA6E_2_WIND10",11,18.96]
["ALTA6E_2_WIND10",12,22.96]
["ALTWD_2_AT3WD3",1,1.73]
["ALTWD_2_AT3WD3",2,1.84]
["ALTWD_2_AT3WD3",3,1.62]
["ALTWD_2_AT3WD3",4,1.55]
["ALTWD_2_AT3WD3",5,1.65]
["ALTWD_2_AT3WD3",6,1.51]
["ALTWD_2_AT3WD3",7,1.4]
["ALTWD_2_AT3WD3",8,1.07]
["ALTWD_2_AT3WD3",9,1.1000000000000001]
["ALTWD_2_AT3WD3",10,1.02]
["ALTWD_2_AT3WD3",11,1.38]
["ALTWD_2_AT3WD3",12,1.67]
["ALTWD_2_COAWD1",1,8.91]
["ALTWD_2_COAWD1",2,9.4700000000000006]
["ALTWD_2_COAWD1",3,8.32]
["ALTWD_2_COAWD1",4,7.97]
["ALTWD_2_COAWD1",5,8.48]
["ALTWD_2_COAWD1",6,7.77]
["ALTWD_2_COAWD1",7,7.22]
["ALTWD_2_COAWD1",8,5.49]
["ALTWD_2_COAWD1",9,5.67]
["ALTWD_2_COAWD1",10,5.26]
["ALTWD_2_COAWD1",11,7.09]
["ALTWD_2_COAWD1",12,8.58]
["ANAHM_2_CANYN1",1,49.21]
["ANAHM_2_CANYN1",2,49.21]
["ANAHM_2_CANYN1",3,49.21]
["ANAHM_2_CANYN1",4,49.21]
["ANAHM_2_CANYN1",5,49.21]
["ANAHM_2_CANYN1",6,49.21]
["ANAHM_2_CANYN1",7,49.21]
["ANAHM_2_CANYN1",8,49.21]
["ANAHM_2_CANYN1",9,49.21]
["ANAHM_2_CANYN1",10,49.21]
["ANAHM_2_CANYN1",11,49.21]
["ANAHM_2_CANYN1",12,49.21]
["ANAHM_2_CANYN2",1,48.04]
["ANAHM_2_CANYN2",2,48.04]
["ANAHM_2_CANYN2",3,48.04]
["ANAHM_2_CANYN2",4,48.04]
["ANAHM_2_CANYN2",5,48.04]
["ANAHM_2_CANYN2",6,48.04]
["ANAHM_2_CANYN2",7,48.04]
["ANAHM_2_CANYN2",8,48.04]
["ANAHM_2_CANYN2",9,48.04]
["ANAHM_2_CANYN2",10,48.04]
["ANAHM_2_CANYN2",11,48.04]
["ANAHM_2_CANYN2",12,48.04]
["ANAHM_2_CANYN3",1,46.49]
["ANAHM_2_CANYN3",2,46.49]
["ANAHM_2_CANYN3",3,46.49]
["ANAHM_2_CANYN3",4,46.49]
["ANAHM_2_CANYN3",5,46.49]
["ANAHM_2_CANYN3",6,46.49]
["ANAHM_2_CANYN3",7,46.49]
["ANAHM_2_CANYN3",8,46.49]
["ANAHM_2_CANYN3",9,46.49]
["ANAHM_2_CANYN3",10,46.49]
["ANAHM_2_CANYN3",11,46.49]
["ANAHM_2_CANYN3",12,46.49]
["ANAHM_2_CANYN4",1,49.8]
["ANAHM_2_CANYN4",2,49.8]
["ANAHM_2_CANYN4",3,49.8]
["ANAHM_2_CANYN4",4,49.8]
["ANAHM_2_CANYN4",5,49.8]
["ANAHM_2_CANYN4",6,49.8]
["ANAHM_2_CANYN4",7,49.8]
["ANAHM_2_CANYN4",8,49.8]
["ANAHM_2_CANYN4",9,49.8]
["ANAHM_2_CANYN4",10,49.8]
["ANAHM_2_CANYN4",11,49.8]
["ANAHM_2_CANYN4",12,49.8]
["ANTLPE_2_QF",1,0.71]
["ANTLPE_2_QF",2,0.75]
["ANTLPE_2_QF",3,0.66]
["ANTLPE_2_QF",4,0.63]
["ANTLPE_2_QF",5,0.67]
["ANTLPE_2_QF",6,0.62]
["ANTLPE_2_QF",7,0.56999999999999995]
["ANTLPE_2_QF",8,0.44]
["ANTLPE_2_QF",9,0.45]
["ANTLPE_2_QF",10,0.42]
["ANTLPE_2_QF",11,0.56000000000000005]
["ANTLPE_2_QF",12,0.68]
["APLHIL_1_SFKHY1",1,0]
["APLHIL_1_SFKHY1",2,0]
["APLHIL_1_SFKHY1",3,0]
["APLHIL_1_SFKHY1",4,0]
["APLHIL_1_SFKHY1",5,0]
["APLHIL_1_SFKHY1",6,0]
["APLHIL_1_SFKHY1",7,0]
["APLHIL_1_SFKHY1",8,0]
["APLHIL_1_SFKHY1",9,0]
["APLHIL_1_SFKHY1",10,0]
["APLHIL_1_SFKHY1",11,0]
["APLHIL_1_SFKHY1",12,0]
["AQUAWS_2_AQWSR1",1,1]
["AQUAWS_2_AQWSR1",2,7.5]
["AQUAWS_2_AQWSR1",3,8.75]
["AQUAWS_2_AQWSR1",4,11]
["AQUAWS_2_AQWSR1",5,16]
["AQUAWS_2_AQWSR1",6,32.75]
["AQUAWS_2_AQWSR1",7,36]
["AQUAWS_2_AQWSR1",8,31]
["AQUAWS_2_AQWSR1",9,27.75]
["AQUAWS_2_AQWSR1",10,18.5]
["AQUAWS_2_AQWSR1",11,14.25]
["AQUAWS_2_AQWSR1",12,8.75]
["ARBWD_6_QF",1,3.53]
["ARBWD_6_QF",2,3.75]
["ARBWD_6_QF",3,3.29]
["ARBWD_6_QF",4,3.16]
["ARBWD_6_QF",5,3.36]
["ARBWD_6_QF",6,3.08]
["ARBWD_6_QF",7,2.86]
["ARBWD_6_QF",8,2.17]
["ARBWD_6_QF",9,2.2400000000000002]
["ARBWD_6_QF",10,2.08]
["ARBWD_6_QF",11,2.8]
["ARBWD_6_QF",12,3.4]
["ARCOGN_2_UNITS",1,305]
["ARCOGN_2_UNITS",2,305]
["ARCOGN_2_UNITS",3,305]
["ARCOGN_2_UNITS",4,305]
["ARCOGN_2_UNITS",5,305]
["ARCOGN_2_UNITS",6,305]
["ARCOGN_2_UNITS",7,305]
["ARCOGN_2_UNITS",8,305]
["ARCOGN_2_UNITS",9,305]
["ARCOGN_2_UNITS",10,305]
["ARCOGN_2_UNITS",11,305]
["ARCOGN_2_UNITS",12,305]
["ARLNTN_2_AR1SR1",1,0]
["ARLNTN_2_AR1SR1",2,0.15]
["ARLNTN_2_AR1SR1",3,0.73]
["ARLNTN_2_AR1SR1",4,2.5299999999999998]
["ARLNTN_2_AR1SR1",5,4.5999999999999996]
["ARLNTN_2_AR1SR1",6,11.36]
["ARLNTN_2_AR1SR1",7,12.31]
["ARLNTN_2_AR1SR1",8,8.89]
["ARLNTN_2_AR1SR1",9,4.9800000000000004]
["ARLNTN_2_AR1SR1",10,1.6]
["ARLNTN_2_AR1SR1",11,0]
["ARLNTN_2_AR1SR1",12,0]
["ARLNTN_2_ASUSR1",1,0.52]
["ARLNTN_2_ASUSR1",2,3.93]
["ARLNTN_2_ASUSR1",3,4.59]
["ARLNTN_2_ASUSR1",4,5.76]
["ARLNTN_2_ASUSR1",5,8.3800000000000008]
["ARLNTN_2_ASUSR1",6,17.16]
["ARLNTN_2_ASUSR1",7,18.86]
["ARLNTN_2_ASUSR1",8,16.239999999999998]
["ARLNTN_2_ASUSR1",9,14.54]
["ARLNTN_2_ASUSR1",10,9.69]
["ARLNTN_2_ASUSR1",11,7.47]
["ARLNTN_2_ASUSR1",12,4.59]
["ARVINN_6_ORION1",1,0.05]
["ARVINN_6_ORION1",2,0.36]
["ARVINN_6_ORION1",3,0.42]
["ARVINN_6_ORION1",4,0.53]
["ARVINN_6_ORION1",5,0.77]
["ARVINN_6_ORION1",6,1.57]
["ARVINN_6_ORION1",7,1.73]
["ARVINN_6_ORION1",8,1.49]
["ARVINN_6_ORION1",9,1.33]
["ARVINN_6_ORION1",10,0.89]
["ARVINN_6_ORION1",11,0.68]
["ARVINN_6_ORION1",12,0.42]
["ARVINN_6_ORION2",1,0.03]
["ARVINN_6_ORION2",2,0.24]
["ARVINN_6_ORION2",3,0.28000000000000003]
["ARVINN_6_ORION2",4,0.35]
["ARVINN_6_ORION2",5,0.51]
["ARVINN_6_ORION2",6,1.05]
["ARVINN_6_ORION2",7,1.1499999999999999]
["ARVINN_6_ORION2",8,0.99]
["ARVINN_6_ORION2",9,0.89]
["ARVINN_6_ORION2",10,0.59]
["ARVINN_6_ORION2",11,0.46]
["ARVINN_6_ORION2",12,0.28000000000000003]
["ASTORA_2_SOLAR1",1,0.4]
["ASTORA_2_SOLAR1",2,3]
["ASTORA_2_SOLAR1",3,3.5]
["ASTORA_2_SOLAR1",4,4.4000000000000004]
["ASTORA_2_SOLAR1",5,6.4]
["ASTORA_2_SOLAR1",6,13.1]
["ASTORA_2_SOLAR1",7,14.4]
["ASTORA_2_SOLAR1",8,12.4]
["ASTORA_2_SOLAR1",9,11.1]
["ASTORA_2_SOLAR1",10,7.4]
["ASTORA_2_SOLAR1",11,5.7]
["ASTORA_2_SOLAR1",12,3.5]
["ASTORA_2_SOLAR2",1,0.3]
["ASTORA_2_SOLAR2",2,2.25]
["ASTORA_2_SOLAR2",3,2.63]
["ASTORA_2_SOLAR2",4,3.3]
["ASTORA_2_SOLAR2",5,4.8]
["ASTORA_2_SOLAR2",6,9.83]
["ASTORA_2_SOLAR2",7,10.8]
["ASTORA_2_SOLAR2",8,9.3000000000000007]
["ASTORA_2_SOLAR2",9,8.33]
["ASTORA_2_SOLAR2",10,5.55]
["ASTORA_2_SOLAR2",11,4.28]
["ASTORA_2_SOLAR2",12,2.63]
["ATHOS_5_AP1X2",1,1]
["ATHOS_5_AP1X2",2,7.5]
["ATHOS_5_AP1X2",3,8.75]
["ATHOS_5_AP1X2",4,11]
["ATHOS_5_AP1X2",5,16]
["ATHOS_5_AP1X2",6,32.75]
["ATHOS_5_AP1X2",7,36]
["ATHOS_5_AP1X2",8,31]
["ATHOS_5_AP1X2",9,27.75]
["ATHOS_5_AP1X2",10,18.5]
["ATHOS_5_AP1X2",11,14.25]
["ATHOS_5_AP1X2",12,8.75]
["ATHOS_5_AP2X2",1,0.8]
["ATHOS_5_AP2X2",2,6]
["ATHOS_5_AP2X2",3,7]
["ATHOS_5_AP2X2",4,8.8000000000000007]
["ATHOS_5_AP2X2",5,12.8]
["ATHOS_5_AP2X2",6,26.2]
["ATHOS_5_AP2X2",7,28.8]
["ATHOS_5_AP2X2",8,24.8]
["ATHOS_5_AP2X2",9,22.2]
["ATHOS_5_AP2X2",10,14.8]
["ATHOS_5_AP2X2",11,11.4]
["ATHOS_5_AP2X2",12,7]
["ATWEL2_1_SOLAR1",1,0.08]
["ATWEL2_1_SOLAR1",2,0.6]
["ATWEL2_1_SOLAR1",3,0.7]
["ATWEL2_1_SOLAR1",4,0.88]
["ATWEL2_1_SOLAR1",5,1.28]
["ATWEL2_1_SOLAR1",6,2.62]
["ATWEL2_1_SOLAR1",7,2.88]
["ATWEL2_1_SOLAR1",8,2.48]
["ATWEL2_1_SOLAR1",9,2.2200000000000002]
["ATWEL2_1_SOLAR1",10,1.48]
["ATWEL2_1_SOLAR1",11,1.1399999999999999]
["ATWEL2_1_SOLAR1",12,0.7]
["ATWELL_1_SOLAR",1,0.08]
["ATWELL_1_SOLAR",2,0.6]
["ATWELL_1_SOLAR",3,0.7]
["ATWELL_1_SOLAR",4,0.88]
["ATWELL_1_SOLAR",5,1.28]
["ATWELL_1_SOLAR",6,2.62]
["ATWELL_1_SOLAR",7,2.88]
["ATWELL_1_SOLAR",8,2.48]
["ATWELL_1_SOLAR",9,2.2200000000000002]
["ATWELL_1_SOLAR",10,1.48]
["ATWELL_1_SOLAR",11,1.1399999999999999]
["ATWELL_1_SOLAR",12,0.7]
["AVENAL_6_AVPARK",1,0.02]
["AVENAL_6_AVPARK",2,0.18]
["AVENAL_6_AVPARK",3,0.21]
["AVENAL_6_AVPARK",4,0.26]
["AVENAL_6_AVPARK",5,0.38]
["AVENAL_6_AVPARK",6,0.79]
["AVENAL_6_AVPARK",7,0.86]
["AVENAL_6_AVPARK",8,0.74]
["AVENAL_6_AVPARK",9,0.67]
["AVENAL_6_AVPARK",10,0.44]
["AVENAL_6_AVPARK",11,0.34]
["AVENAL_6_AVPARK",12,0.21]
["AVENAL_6_AVSLR1",1,0]
["AVENAL_6_AVSLR1",2,0]
["AVENAL_6_AVSLR1",3,0]
["AVENAL_6_AVSLR1",4,0]
["AVENAL_6_AVSLR1",5,0]
["AVENAL_6_AVSLR1",6,0]
["AVENAL_6_AVSLR1",7,0]
["AVENAL_6_AVSLR1",8,0]
["AVENAL_6_AVSLR1",9,0]
["AVENAL_6_AVSLR1",10,0]
["AVENAL_6_AVSLR1",11,0]
["AVENAL_6_AVSLR1",12,0]
["AVENAL_6_AVSLR2",1,0]
["AVENAL_6_AVSLR2",2,0]
["AVENAL_6_AVSLR2",3,0]
["AVENAL_6_AVSLR2",4,0]
["AVENAL_6_AVSLR2",5,0]
["AVENAL_6_AVSLR2",6,0]
["AVENAL_6_AVSLR2",7,0]
["AVENAL_6_AVSLR2",8,0]
["AVENAL_6_AVSLR2",9,0]
["AVENAL_6_AVSLR2",10,0]
["AVENAL_6_AVSLR2",11,0]
["AVENAL_6_AVSLR2",12,0]
["AVENAL_6_SANDDG",1,7.0000000000000007E-2]
["AVENAL_6_SANDDG",2,0.48]
["AVENAL_6_SANDDG",3,0.56000000000000005]
["AVENAL_6_SANDDG",4,0.7]
["AVENAL_6_SANDDG",5,1.02]
["AVENAL_6_SANDDG",6,2.0699999999999998]
["AVENAL_6_SANDDG",7,2.2799999999999998]
["AVENAL_6_SANDDG",8,1.96]
["AVENAL_6_SANDDG",9,1.76]
["AVENAL_6_SANDDG",10,1.18]
["AVENAL_6_SANDDG",11,0.9]
["AVENAL_6_SANDDG",12,0.56000000000000005]
["AVENAL_6_SUNCTY",1,0.08]
["AVENAL_6_SUNCTY",2,0.6]
["AVENAL_6_SUNCTY",3,0.7]
["AVENAL_6_SUNCTY",4,0.88]
["AVENAL_6_SUNCTY",5,1.28]
["AVENAL_6_SUNCTY",6,2.62]
["AVENAL_6_SUNCTY",7,2.88]
["AVENAL_6_SUNCTY",8,2.48]
["AVENAL_6_SUNCTY",9,2.2200000000000002]
["AVENAL_6_SUNCTY",10,1.48]
["AVENAL_6_SUNCTY",11,1.1399999999999999]
["AVENAL_6_SUNCTY",12,0.7]
["AVSOLR_2_SOLAR",1,0.97]
["AVSOLR_2_SOLAR",2,7.25]
["AVSOLR_2_SOLAR",3,8.4499999999999993]
["AVSOLR_2_SOLAR",4,10.63]
["AVSOLR_2_SOLAR",5,15.46]
["AVSOLR_2_SOLAR",6,31.64]
["AVSOLR_2_SOLAR",7,34.78]
["AVSOLR_2_SOLAR",8,29.95]
["AVSOLR_2_SOLAR",9,26.81]
["AVSOLR_2_SOLAR",10,17.87]
["AVSOLR_2_SOLAR",11,13.77]
["AVSOLR_2_SOLAR",12,8.4499999999999993]
["BAHIA_2_LKHSR1",1,0]
["BAHIA_2_LKHSR1",2,0]
["BAHIA_2_LKHSR1",3,0]
["BAHIA_2_LKHSR1",4,0]
["BAHIA_2_LKHSR1",5,0]
["BAHIA_2_LKHSR1",6,0]
["BAHIA_2_LKHSR1",7,0]
["BAHIA_2_LKHSR1",8,0]
["BAHIA_2_LKHSR1",9,0]
["BAHIA_2_LKHSR1",10,0]
["BAHIA_2_LKHSR1",11,0]
["BAHIA_2_LKHSR1",12,0]
["BALCHS_7_UNIT 1",1,24.8]
["BALCHS_7_UNIT 1",2,24.8]
["BALCHS_7_UNIT 1",3,24.8]
["BALCHS_7_UNIT 1",4,24.8]
["BALCHS_7_UNIT 1",5,24.8]
["BALCHS_7_UNIT 1",6,24.8]
["BALCHS_7_UNIT 1",7,31]
["BALCHS_7_UNIT 1",8,31]
["BALCHS_7_UNIT 1",9,31]
["BALCHS_7_UNIT 1",10,28.2]
["BALCHS_7_UNIT 1",11,26.16]
["BALCHS_7_UNIT 1",12,24.8]
["BALCHS_7_UNIT 2",1,42]
["BALCHS_7_UNIT 2",2,52.5]
["BALCHS_7_UNIT 2",3,43.6]
["BALCHS_7_UNIT 2",4,52.5]
["BALCHS_7_UNIT 2",5,52.5]
["BALCHS_7_UNIT 2",6,52.5]
["BALCHS_7_UNIT 2",7,52.5]
["BALCHS_7_UNIT 2",8,52.5]
["BALCHS_7_UNIT 2",9,52.5]
["BALCHS_7_UNIT 2",10,52.5]
["BALCHS_7_UNIT 2",11,52.5]
["BALCHS_7_UNIT 2",12,52.5]
["BALCHS_7_UNIT 3",1,42]
["BALCHS_7_UNIT 3",2,0]
["BALCHS_7_UNIT 3",3,0.4]
["BALCHS_7_UNIT 3",4,43.68]
["BALCHS_7_UNIT 3",5,43.68]
["BALCHS_7_UNIT 3",6,54.18]
["BALCHS_7_UNIT 3",7,54.18]
["BALCHS_7_UNIT 3",8,54.18]
["BALCHS_7_UNIT 3",9,54.18]
["BALCHS_7_UNIT 3",10,54.18]
["BALCHS_7_UNIT 3",11,54.18]
["BALCHS_7_UNIT 3",12,43.68]
["BANKPP_2_NSPIN",1,127]
["BANKPP_2_NSPIN",2,127]
["BANKPP_2_NSPIN",3,127]
["BANKPP_2_NSPIN",4,127]
["BANKPP_2_NSPIN",5,127]
["BANKPP_2_NSPIN",6,127]
["BANKPP_2_NSPIN",7,127]
["BANKPP_2_NSPIN",8,127]
["BANKPP_2_NSPIN",9,127]
["BANKPP_2_NSPIN",10,127]
["BANKPP_2_NSPIN",11,127]
["BANKPP_2_NSPIN",12,127]
["BARRE_2_QF",1,0]
["BARRE_2_QF",2,0]
["BARRE_2_QF",3,0.01]
["BARRE_2_QF",4,0.01]
["BARRE_2_QF",5,0]
["BARRE_2_QF",6,0]
["BARRE_2_QF",7,0]
["BARRE_2_QF",8,0]
["BARRE_2_QF",9,0]
["BARRE_2_QF",10,0]
["BARRE_2_QF",11,0]
["BARRE_2_QF",12,0]
["BARRE_6_PEAKER",1,49]
["BARRE_6_PEAKER",2,49]
["BARRE_6_PEAKER",3,49]
["BARRE_6_PEAKER",4,49]
["BARRE_6_PEAKER",5,49]
["BARRE_6_PEAKER",6,49]
["BARRE_6_PEAKER",7,49]
["BARRE_6_PEAKER",8,49]
["BARRE_6_PEAKER",9,49]
["BARRE_6_PEAKER",10,49]
["BARRE_6_PEAKER",11,49]
["BARRE_6_PEAKER",12,49]
["BASICE_2_UNITS",1,120]
["BASICE_2_UNITS",2,120]
["BASICE_2_UNITS",3,120]
["BASICE_2_UNITS",4,120]
["BASICE_2_UNITS",5,120]
["BASICE_2_UNITS",6,120]
["BASICE_2_UNITS",7,120]
["BASICE_2_UNITS",8,120]
["BASICE_2_UNITS",9,120]
["BASICE_2_UNITS",10,120]
["BASICE_2_UNITS",11,120]
["BASICE_2_UNITS",12,120]
["BDGRCK_1_UNITS",1,48.08]
["BDGRCK_1_UNITS",2,48.08]
["BDGRCK_1_UNITS",3,48.08]
["BDGRCK_1_UNITS",4,48.08]
["BDGRCK_1_UNITS",5,48.08]
["BDGRCK_1_UNITS",6,48.08]
["BDGRCK_1_UNITS",7,48.08]
["BDGRCK_1_UNITS",8,48.08]
["BDGRCK_1_UNITS",9,48.08]
["BDGRCK_1_UNITS",10,48.08]
["BDGRCK_1_UNITS",11,48.08]
["BDGRCK_1_UNITS",12,48.08]
["BEARDS_7_UNIT 1",1,4.5]
["BEARDS_7_UNIT 1",2,0.96]
["BEARDS_7_UNIT 1",3,1.6]
["BEARDS_7_UNIT 1",4,4.0999999999999996]
["BEARDS_7_UNIT 1",5,5]
["BEARDS_7_UNIT 1",6,5.5]
["BEARDS_7_UNIT 1",7,5.0999999999999996]
["BEARDS_7_UNIT 1",8,4.8]
["BEARDS_7_UNIT 1",9,0.8]
["BEARDS_7_UNIT 1",10,0.8]
["BEARDS_7_UNIT 1",11,6.2]
["BEARDS_7_UNIT 1",12,7.48]
["BEARMT_1_UNIT",1,49.21]
["BEARMT_1_UNIT",2,49.21]
["BEARMT_1_UNIT",3,49.21]
["BEARMT_1_UNIT",4,49.21]
["BEARMT_1_UNIT",5,49.21]
["BEARMT_1_UNIT",6,49.21]
["BEARMT_1_UNIT",7,49.21]
["BEARMT_1_UNIT",8,49.21]
["BEARMT_1_UNIT",9,49.21]
["BEARMT_1_UNIT",10,49.21]
["BEARMT_1_UNIT",11,49.21]
["BEARMT_1_UNIT",12,49.21]
["BELDEN_7_UNIT 1",1,40]
["BELDEN_7_UNIT 1",2,1.6]
["BELDEN_7_UNIT 1",3,0]
["BELDEN_7_UNIT 1",4,0]
["BELDEN_7_UNIT 1",5,1.6]
["BELDEN_7_UNIT 1",6,30.4]
["BELDEN_7_UNIT 1",7,82.94]
["BELDEN_7_UNIT 1",8,88]
["BELDEN_7_UNIT 1",9,80.8]
["BELDEN_7_UNIT 1",10,60]
["BELDEN_7_UNIT 1",11,1.6]
["BELDEN_7_UNIT 1",12,1.6]
["BGSKYN_2_AS2SR1",1,0.34]
["BGSKYN_2_AS2SR1",2,2.68]
["BGSKYN_2_AS2SR1",3,3.18]
["BGSKYN_2_AS2SR1",4,4.12]
["BGSKYN_2_AS2SR1",5,6.04]
["BGSKYN_2_AS2SR1",6,12.46]
["BGSKYN_2_AS2SR1",7,13.66]
["BGSKYN_2_AS2SR1",8,11.67]
["BGSKYN_2_AS2SR1",9,10.25]
["BGSKYN_2_AS2SR1",10,6.71]
["BGSKYN_2_AS2SR1",11,4.92]
["BGSKYN_2_AS2SR1",12,2.79]
["BGSKYN_2_ASPSR2",1,0.32]
["BGSKYN_2_ASPSR2",2,2.5499999999999998]
["BGSKYN_2_ASPSR2",3,3.03]
["BGSKYN_2_ASPSR2",4,3.93]
["BGSKYN_2_ASPSR2",5,5.76]
["BGSKYN_2_ASPSR2",6,11.86]
["BGSKYN_2_ASPSR2",7,13.01]
["BGSKYN_2_ASPSR2",8,11.12]
["BGSKYN_2_ASPSR2",9,9.76]
["BGSKYN_2_ASPSR2",10,6.39]
["BGSKYN_2_ASPSR2",11,4.6900000000000004]
["BGSKYN_2_ASPSR2",12,2.66]
["BGSKYN_2_ASSR1B",1,0.05]
["BGSKYN_2_ASSR1B",2,0.43]
["BGSKYN_2_ASSR1B",3,0.51]
["BGSKYN_2_ASSR1B",4,0.67]
["BGSKYN_2_ASSR1B",5,0.98]
["BGSKYN_2_ASSR1B",6,2.02]
["BGSKYN_2_ASSR1B",7,2.21]
["BGSKYN_2_ASSR1B",8,1.89]
["BGSKYN_2_ASSR1B",9,1.66]
["BGSKYN_2_ASSR1B",10,1.0900000000000001]
["BGSKYN_2_ASSR1B",11,0.8]
["BGSKYN_2_ASSR1B",12,0.45]
["BGSKYN_2_ASSR3A",1,0.05]
["BGSKYN_2_ASSR3A",2,0.38]
["BGSKYN_2_ASSR3A",3,0.45]
["BGSKYN_2_ASSR3A",4,0.59]
["BGSKYN_2_ASSR3A",5,0.86]
["BGSKYN_2_ASSR3A",6,1.78]
["BGSKYN_2_ASSR3A",7,1.95]
["BGSKYN_2_ASSR3A",8,1.67]
["BGSKYN_2_ASSR3A",9,1.46]
["BGSKYN_2_ASSR3A",10,0.96]
["BGSKYN_2_ASSR3A",11,0.7]
["BGSKYN_2_ASSR3A",12,0.4]
["BGSKYN_2_ASSR3B",1,0.02]
["BGSKYN_2_ASSR3B",2,0.13]
["BGSKYN_2_ASSR3B",3,0.15]
["BGSKYN_2_ASSR3B",4,0.2]
["BGSKYN_2_ASSR3B",5,0.28999999999999998]
["BGSKYN_2_ASSR3B",6,0.59]
["BGSKYN_2_ASSR3B",7,0.65]
["BGSKYN_2_ASSR3B",8,0.56000000000000005]
["BGSKYN_2_ASSR3B",9,0.49]
["BGSKYN_2_ASSR3B",10,0.32]
["BGSKYN_2_ASSR3B",11,0.23]
["BGSKYN_2_ASSR3B",12,0.13]
["BGSKYN_2_BS3SR3",1,0.06]
["BGSKYN_2_BS3SR3",2,0.51]
["BGSKYN_2_BS3SR3",3,0.61]
["BGSKYN_2_BS3SR3",4,0.79]
["BGSKYN_2_BS3SR3",5,1.1499999999999999]
["BGSKYN_2_BS3SR3",6,2.37]
["BGSKYN_2_BS3SR3",7,2.6]
["BGSKYN_2_BS3SR3",8,2.2200000000000002]
["BGSKYN_2_BS3SR3",9,1.95]
["BGSKYN_2_BS3SR3",10,1.28]
["BGSKYN_2_BS3SR3",11,0.94]
["BGSKYN_2_BS3SR3",12,0.53]
["BIGCRK_2_EXESWD",1,467.32]
["BIGCRK_2_EXESWD",2,472.28]
["BIGCRK_2_EXESWD",3,444.6]
["BIGCRK_2_EXESWD",4,570]
["BIGCRK_2_EXESWD",5,632.20000000000005]
["BIGCRK_2_EXESWD",6,732.04]
["BIGCRK_2_EXESWD",7,702.52]
["BIGCRK_2_EXESWD",8,700]
["BIGCRK_2_EXESWD",9,700]
["BIGCRK_2_EXESWD",10,412.6]
["BIGCRK_2_EXESWD",11,407.32]
["BIGCRK_2_EXESWD",12,374.28]
["BIGCRK_7_DAM7",1,0]
["BIGCRK_7_DAM7",2,0]
["BIGCRK_7_DAM7",3,0]
["BIGCRK_7_DAM7",4,0]
["BIGCRK_7_DAM7",5,0]
["BIGCRK_7_DAM7",6,0]
["BIGCRK_7_DAM7",7,0]
["BIGCRK_7_DAM7",8,0]
["BIGCRK_7_DAM7",9,0]
["BIGCRK_7_DAM7",10,0]
["BIGCRK_7_DAM7",11,0]
["BIGCRK_7_DAM7",12,0]
["BIGCRK_7_MAMRES",1,0]
["BIGCRK_7_MAMRES",2,0]
["BIGCRK_7_MAMRES",3,0]
["BIGCRK_7_MAMRES",4,0]
["BIGCRK_7_MAMRES",5,0]
["BIGCRK_7_MAMRES",6,0]
["BIGCRK_7_MAMRES",7,0]
["BIGCRK_7_MAMRES",8,0]
["BIGCRK_7_MAMRES",9,0]
["BIGCRK_7_MAMRES",10,0]
["BIGCRK_7_MAMRES",11,0]
["BIGCRK_7_MAMRES",12,0]
["BIGSKY_2_AS2BT1",1,127]
["BIGSKY_2_AS2BT1",2,127]
["BIGSKY_2_AS2BT1",3,127]
["BIGSKY_2_AS2BT1",4,127]
["BIGSKY_2_AS2BT1",5,127]
["BIGSKY_2_AS2BT1",6,127]
["BIGSKY_2_AS2BT1",7,127]
["BIGSKY_2_AS2BT1",8,127]
["BIGSKY_2_AS2BT1",9,127]
["BIGSKY_2_AS2BT1",10,127]
["BIGSKY_2_AS2BT1",11,127]
["BIGSKY_2_AS2BT1",12,127]
["BIGSKY_2_ASLBT2",1,100]
["BIGSKY_2_ASLBT2",2,100]
["BIGSKY_2_ASLBT2",3,100]
["BIGSKY_2_ASLBT2",4,100]
["BIGSKY_2_ASLBT2",5,100]
["BIGSKY_2_ASLBT2",6,100]
["BIGSKY_2_ASLBT2",7,100]
["BIGSKY_2_ASLBT2",8,100]
["BIGSKY_2_ASLBT2",9,100]
["BIGSKY_2_ASLBT2",10,100]
["BIGSKY_2_ASLBT2",11,100]
["BIGSKY_2_ASLBT2",12,100]
["BIGSKY_2_BSKSR6",1,0.06]
["BIGSKY_2_BSKSR6",2,0.51]
["BIGSKY_2_BSKSR6",3,0.61]
["BIGSKY_2_BSKSR6",4,0.79]
["BIGSKY_2_BSKSR6",5,1.1499999999999999]
["BIGSKY_2_BSKSR6",6,2.37]
["BIGSKY_2_BSKSR6",7,2.6]
["BIGSKY_2_BSKSR6",8,2.2200000000000002]
["BIGSKY_2_BSKSR6",9,1.95]
["BIGSKY_2_BSKSR6",10,1.28]
["BIGSKY_2_BSKSR6",11,0.94]
["BIGSKY_2_BSKSR6",12,0.53]
["BIGSKY_2_BSKSR7",1,0.06]
["BIGSKY_2_BSKSR7",2,0.51]
["BIGSKY_2_BSKSR7",3,0.61]
["BIGSKY_2_BSKSR7",4,0.79]
["BIGSKY_2_BSKSR7",5,1.1499999999999999]
["BIGSKY_2_BSKSR7",6,2.37]
["BIGSKY_2_BSKSR7",7,2.6]
["BIGSKY_2_BSKSR7",8,2.2200000000000002]
["BIGSKY_2_BSKSR7",9,1.95]
["BIGSKY_2_BSKSR7",10,1.28]
["BIGSKY_2_BSKSR7",11,0.94]
["BIGSKY_2_BSKSR7",12,0.53]
["BIGSKY_2_BSKSR8",1,0.06]
["BIGSKY_2_BSKSR8",2,0.51]
["BIGSKY_2_BSKSR8",3,0.61]
["BIGSKY_2_BSKSR8",4,0.79]
["BIGSKY_2_BSKSR8",5,1.1499999999999999]
["BIGSKY_2_BSKSR8",6,2.37]
["BIGSKY_2_BSKSR8",7,2.6]
["BIGSKY_2_BSKSR8",8,2.2200000000000002]
["BIGSKY_2_BSKSR8",9,1.95]
["BIGSKY_2_BSKSR8",10,1.28]
["BIGSKY_2_BSKSR8",11,0.94]
["BIGSKY_2_BSKSR8",12,0.53]
["BIGSKY_2_SOLAR1",1,0.06]
["BIGSKY_2_SOLAR1",2,0.51]
["BIGSKY_2_SOLAR1",3,0.61]
["BIGSKY_2_SOLAR1",4,0.79]
["BIGSKY_2_SOLAR1",5,1.1499999999999999]
["BIGSKY_2_SOLAR1",6,2.37]
["BIGSKY_2_SOLAR1",7,2.6]
["BIGSKY_2_SOLAR1",8,2.2200000000000002]
["BIGSKY_2_SOLAR1",9,1.95]
["BIGSKY_2_SOLAR1",10,1.28]
["BIGSKY_2_SOLAR1",11,0.94]
["BIGSKY_2_SOLAR1",12,0.53]
["BIGSKY_2_SOLAR2",1,0.13]
["BIGSKY_2_SOLAR2",2,1.02]
["BIGSKY_2_SOLAR2",3,1.21]
["BIGSKY_2_SOLAR2",4,1.57]
["BIGSKY_2_SOLAR2",5,2.2999999999999998]
["BIGSKY_2_SOLAR2",6,4.75]
["BIGSKY_2_SOLAR2",7,5.2]
["BIGSKY_2_SOLAR2",8,4.45]
["BIGSKY_2_SOLAR2",9,3.9]
["BIGSKY_2_SOLAR2",10,2.56]
["BIGSKY_2_SOLAR2",11,1.88]
["BIGSKY_2_SOLAR2",12,1.06]
["BIGSKY_2_SOLAR3",1,0.06]
["BIGSKY_2_SOLAR3",2,0.51]
["BIGSKY_2_SOLAR3",3,0.61]
["BIGSKY_2_SOLAR3",4,0.79]
["BIGSKY_2_SOLAR3",5,1.1499999999999999]
["BIGSKY_2_SOLAR3",6,2.37]
["BIGSKY_2_SOLAR3",7,2.6]
["BIGSKY_2_SOLAR3",8,2.2200000000000002]
["BIGSKY_2_SOLAR3",9,1.95]
["BIGSKY_2_SOLAR3",10,1.28]
["BIGSKY_2_SOLAR3",11,0.94]
["BIGSKY_2_SOLAR3",12,0.53]
["BIGSKY_2_SOLAR4",1,0.06]
["BIGSKY_2_SOLAR4",2,0.51]
["BIGSKY_2_SOLAR4",3,0.61]
["BIGSKY_2_SOLAR4",4,0.79]
["BIGSKY_2_SOLAR4",5,1.1499999999999999]
["BIGSKY_2_SOLAR4",6,2.37]
["BIGSKY_2_SOLAR4",7,2.6]
["BIGSKY_2_SOLAR4",8,2.2200000000000002]
["BIGSKY_2_SOLAR4",9,1.95]
["BIGSKY_2_SOLAR4",10,1.28]
["BIGSKY_2_SOLAR4",11,0.94]
["BIGSKY_2_SOLAR4",12,0.53]
["BIGSKY_2_SOLAR5",1,0.02]
["BIGSKY_2_SOLAR5",2,0.13]
["BIGSKY_2_SOLAR5",3,0.15]
["BIGSKY_2_SOLAR5",4,0.2]
["BIGSKY_2_SOLAR5",5,0.28999999999999998]
["BIGSKY_2_SOLAR5",6,0.59]
["BIGSKY_2_SOLAR5",7,0.65]
["BIGSKY_2_SOLAR5",8,0.56000000000000005]
["BIGSKY_2_SOLAR5",9,0.49]
["BIGSKY_2_SOLAR5",10,0.32]
["BIGSKY_2_SOLAR5",11,0.23]
["BIGSKY_2_SOLAR5",12,0.13]
["BIGSKY_2_SOLAR6",1,0.27]
["BIGSKY_2_SOLAR6",2,2.17]
["BIGSKY_2_SOLAR6",3,2.57]
["BIGSKY_2_SOLAR6",4,3.34]
["BIGSKY_2_SOLAR6",5,4.8899999999999997]
["BIGSKY_2_SOLAR6",6,10.09]
["BIGSKY_2_SOLAR6",7,11.06]
["BIGSKY_2_SOLAR6",8,9.4499999999999993]
["BIGSKY_2_SOLAR6",9,8.3000000000000007]
["BIGSKY_2_SOLAR6",10,5.43]
["BIGSKY_2_SOLAR6",11,3.99]
["BIGSKY_2_SOLAR6",12,2.2599999999999998]
["BIGSKY_2_SOLAR7",1,0.16]
["BIGSKY_2_SOLAR7",2,1.28]
["BIGSKY_2_SOLAR7",3,1.51]
["BIGSKY_2_SOLAR7",4,1.96]
["BIGSKY_2_SOLAR7",5,2.88]
["BIGSKY_2_SOLAR7",6,5.93]
["BIGSKY_2_SOLAR7",7,6.51]
["BIGSKY_2_SOLAR7",8,5.56]
["BIGSKY_2_SOLAR7",9,4.88]
["BIGSKY_2_SOLAR7",10,3.2]
["BIGSKY_2_SOLAR7",11,2.34]
["BIGSKY_2_SOLAR7",12,1.33]
["BIOMAS_1_UNIT 1",1,15.64]
["BIOMAS_1_UNIT 1",2,15.55]
["BIOMAS_1_UNIT 1",3,7.99]
["BIOMAS_1_UNIT 1",4,7.79]
["BIOMAS_1_UNIT 1",5,8]
["BIOMAS_1_UNIT 1",6,8.27]
["BIOMAS_1_UNIT 1",7,8.16]
["BIOMAS_1_UNIT 1",8,7.88]
["BIOMAS_1_UNIT 1",9,15.1]
["BIOMAS_1_UNIT 1",10,7.75]
["BIOMAS_1_UNIT 1",11,11.97]
["BIOMAS_1_UNIT 1",12,15.52]
["BISHOP_1_ALAMO",1,3.71]
["BISHOP_1_ALAMO",2,3.51]
["BISHOP_1_ALAMO",3,4.66]
["BISHOP_1_ALAMO",4,6.84]
["BISHOP_1_ALAMO",5,9.65]
["BISHOP_1_ALAMO",6,9.59]
["BISHOP_1_ALAMO",7,8.6300000000000008]
["BISHOP_1_ALAMO",8,8]
["BISHOP_1_ALAMO",9,5.55]
["BISHOP_1_ALAMO",10,4.41]
["BISHOP_1_ALAMO",11,3.3]
["BISHOP_1_ALAMO",12,2.87]
["BISHOP_1_UNITS",1,5.76]
["BISHOP_1_UNITS",2,4.79]
["BISHOP_1_UNITS",3,2.68]
["BISHOP_1_UNITS",4,8.9600000000000009]
["BISHOP_1_UNITS",5,13.02]
["BISHOP_1_UNITS",6,13.39]
["BISHOP_1_UNITS",7,11.45]
["BISHOP_1_UNITS",8,10.9]
["BISHOP_1_UNITS",9,7.52]
["BISHOP_1_UNITS",10,6.42]
["BISHOP_1_UNITS",11,5.59]
["BISHOP_1_UNITS",12,5.53]
["BKRFLD_2_SOLAR1",1,0.01]
["BKRFLD_2_SOLAR1",2,0.04]
["BKRFLD_2_SOLAR1",3,0.05]
["BKRFLD_2_SOLAR1",4,0.06]
["BKRFLD_2_SOLAR1",5,0.09]
["BKRFLD_2_SOLAR1",6,0.18]
["BKRFLD_2_SOLAR1",7,0.2]
["BKRFLD_2_SOLAR1",8,0.17]
["BKRFLD_2_SOLAR1",9,0.15]
["BKRFLD_2_SOLAR1",10,0.1]
["BKRFLD_2_SOLAR1",11,0.08]
["BKRFLD_2_SOLAR1",12,0.05]
["BLACK_7_UNIT 1",1,84.1]
["BLACK_7_UNIT 1",2,84]
["BLACK_7_UNIT 1",3,82.4]
["BLACK_7_UNIT 1",4,82]
["BLACK_7_UNIT 1",5,84]
["BLACK_7_UNIT 1",6,84]
["BLACK_7_UNIT 1",7,84]
["BLACK_7_UNIT 1",8,84.4]
["BLACK_7_UNIT 1",9,68]
["BLACK_7_UNIT 1",10,68]
["BLACK_7_UNIT 1",11,84.4]
["BLACK_7_UNIT 1",12,84.4]
["BLACK_7_UNIT 2",1,83.3]
["BLACK_7_UNIT 2",2,83.28]
["BLACK_7_UNIT 2",3,82.48]
["BLACK_7_UNIT 2",4,79.760000000000005]
["BLACK_7_UNIT 2",5,83.28]
["BLACK_7_UNIT 2",6,83.28]
["BLACK_7_UNIT 2",7,83.28]
["BLACK_7_UNIT 2",8,83.28]
["BLACK_7_UNIT 2",9,81.28]
["BLACK_7_UNIT 2",10,67.28]
["BLACK_7_UNIT 2",11,83.88]
["BLACK_7_UNIT 2",12,83.88]
["BLAST_1_WIND",1,8.66]
["BLAST_1_WIND",2,9.2100000000000009]
["BLAST_1_WIND",3,8.09]
["BLAST_1_WIND",4,7.75]
["BLAST_1_WIND",5,8.24]
["BLAST_1_WIND",6,7.56]
["BLAST_1_WIND",7,7.02]
["BLAST_1_WIND",8,5.33]
["BLAST_1_WIND",9,5.51]
["BLAST_1_WIND",10,5.1100000000000003]
["BLAST_1_WIND",11,6.89]
["BLAST_1_WIND",12,8.35]
["BLCKBT_2_STONEY",1,2.04]
["BLCKBT_2_STONEY",2,1.6]
["BLCKBT_2_STONEY",3,1.3]
["BLCKBT_2_STONEY",4,3.5]
["BLCKBT_2_STONEY",5,2.7]
["BLCKBT_2_STONEY",6,2.57]
["BLCKBT_2_STONEY",7,2.02]
["BLCKBT_2_STONEY",8,1.83]
["BLCKBT_2_STONEY",9,1.5]
["BLCKBT_2_STONEY",10,1.5]
["BLCKBT_2_STONEY",11,2.1]
["BLCKBT_2_STONEY",12,2.5099999999999998]
["BLCKWL_6_SOLAR1",1,0.05]
["BLCKWL_6_SOLAR1",2,0.36]
["BLCKWL_6_SOLAR1",3,0.42]
["BLCKWL_6_SOLAR1",4,0.53]
["BLCKWL_6_SOLAR1",5,0.77]
["BLCKWL_6_SOLAR1",6,1.57]
["BLCKWL_6_SOLAR1",7,1.73]
["BLCKWL_6_SOLAR1",8,1.49]
["BLCKWL_6_SOLAR1",9,1.33]
["BLCKWL_6_SOLAR1",10,0.89]
["BLCKWL_6_SOLAR1",11,0.68]
["BLCKWL_6_SOLAR1",12,0.42]
["BLKCRK_2_GMCBT1",1,230]
["BLKCRK_2_GMCBT1",2,230]
["BLKCRK_2_GMCBT1",3,230]
["BLKCRK_2_GMCBT1",4,230]
["BLKCRK_2_GMCBT1",5,230]
["BLKCRK_2_GMCBT1",6,230]
["BLKCRK_2_GMCBT1",7,230]
["BLKCRK_2_GMCBT1",8,230]
["BLKCRK_2_GMCBT1",9,230]
["BLKCRK_2_GMCBT1",10,230]
["BLKCRK_2_GMCBT1",11,230]
["BLKCRK_2_GMCBT1",12,230]
["BLKCRK_2_SOLAR1",1,0]
["BLKCRK_2_SOLAR1",2,0]
["BLKCRK_2_SOLAR1",3,0]
["BLKCRK_2_SOLAR1",4,0]
["BLKCRK_2_SOLAR1",5,0]
["BLKCRK_2_SOLAR1",6,0]
["BLKCRK_2_SOLAR1",7,0]
["BLKCRK_2_SOLAR1",8,0]
["BLKCRK_2_SOLAR1",9,0]
["BLKCRK_2_SOLAR1",10,0]
["BLKCRK_2_SOLAR1",11,0]
["BLKCRK_2_SOLAR1",12,0]
["BLKDIA_2_BDEBT1",1,200]
["BLKDIA_2_BDEBT1",2,200]
["BLKDIA_2_BDEBT1",3,200]
["BLKDIA_2_BDEBT1",4,200]
["BLKDIA_2_BDEBT1",5,200]
["BLKDIA_2_BDEBT1",6,200]
["BLKDIA_2_BDEBT1",7,200]
["BLKDIA_2_BDEBT1",8,200]
["BLKDIA_2_BDEBT1",9,200]
["BLKDIA_2_BDEBT1",10,200]
["BLKDIA_2_BDEBT1",11,200]
["BLKDIA_2_BDEBT1",12,200]
["BLM W_2_COSBT1",1,60]
["BLM W_2_COSBT1",2,60]
["BLM W_2_COSBT1",3,60]
["BLM W_2_COSBT1",4,60]
["BLM W_2_COSBT1",5,60]
["BLM W_2_COSBT1",6,60]
["BLM W_2_COSBT1",7,60]
["BLM W_2_COSBT1",8,60]
["BLM W_2_COSBT1",9,60]
["BLM W_2_COSBT1",10,60]
["BLM W_2_COSBT1",11,60]
["BLM W_2_COSBT1",12,60]
["BLM_2_UNITS",1,47]
["BLM_2_UNITS",2,47]
["BLM_2_UNITS",3,47]
["BLM_2_UNITS",4,47]
["BLM_2_UNITS",5,47]
["BLM_2_UNITS",6,47]
["BLM_2_UNITS",7,47]
["BLM_2_UNITS",8,47]
["BLM_2_UNITS",9,47]
["BLM_2_UNITS",10,47]
["BLM_2_UNITS",11,47]
["BLM_2_UNITS",12,47]
["BLYTHE_1_SOLAR1",1,0]
["BLYTHE_1_SOLAR1",2,0]
["BLYTHE_1_SOLAR1",3,0]
["BLYTHE_1_SOLAR1",4,0]
["BLYTHE_1_SOLAR1",5,0]
["BLYTHE_1_SOLAR1",6,0]
["BLYTHE_1_SOLAR1",7,0]
["BLYTHE_1_SOLAR1",8,0]
["BLYTHE_1_SOLAR1",9,0]
["BLYTHE_1_SOLAR1",10,0]
["BLYTHE_1_SOLAR1",11,0]
["BLYTHE_1_SOLAR1",12,0]
["BLYTHE_1_SOLAR2",1,0]
["BLYTHE_1_SOLAR2",2,0]
["BLYTHE_1_SOLAR2",3,0]
["BLYTHE_1_SOLAR2",4,0]
["BLYTHE_1_SOLAR2",5,0]
["BLYTHE_1_SOLAR2",6,0]
["BLYTHE_1_SOLAR2",7,0]
["BLYTHE_1_SOLAR2",8,0]
["BLYTHE_1_SOLAR2",9,0]
["BLYTHE_1_SOLAR2",10,0]
["BLYTHE_1_SOLAR2",11,0]
["BLYTHE_1_SOLAR2",12,0]
["BNNIEN_7_ALTAPH",1,0.32]
["BNNIEN_7_ALTAPH",2,0.28999999999999998]
["BNNIEN_7_ALTAPH",3,0.28999999999999998]
["BNNIEN_7_ALTAPH",4,0.28000000000000003]
["BNNIEN_7_ALTAPH",5,0.15]
["BNNIEN_7_ALTAPH",6,0.42]
["BNNIEN_7_ALTAPH",7,0.53]
["BNNIEN_7_ALTAPH",8,0.66]
["BNNIEN_7_ALTAPH",9,0.35]
["BNNIEN_7_ALTAPH",10,0.41]
["BNNIEN_7_ALTAPH",11,0.41]
["BNNIEN_7_ALTAPH",12,0.28999999999999998]
["BOGUE_1_UNITA1",1,47.38]
["BOGUE_1_UNITA1",2,47.38]
["BOGUE_1_UNITA1",3,47.38]
["BOGUE_1_UNITA1",4,47.38]
["BOGUE_1_UNITA1",5,47.38]
["BOGUE_1_UNITA1",6,47.38]
["BOGUE_1_UNITA1",7,47.38]
["BOGUE_1_UNITA1",8,47.38]
["BOGUE_1_UNITA1",9,47.38]
["BOGUE_1_UNITA1",10,47.38]
["BOGUE_1_UNITA1",11,47.38]
["BOGUE_1_UNITA1",12,47.38]
["BORDER_6_UNITA1",1,51.25]
["BORDER_6_UNITA1",2,51.25]
["BORDER_6_UNITA1",3,51.25]
["BORDER_6_UNITA1",4,51.25]
["BORDER_6_UNITA1",5,51.25]
["BORDER_6_UNITA1",6,51.25]
["BORDER_6_UNITA1",7,51.25]
["BORDER_6_UNITA1",8,51.25]
["BORDER_6_UNITA1",9,51.25]
["BORDER_6_UNITA1",10,51.25]
["BORDER_6_UNITA1",11,51.25]
["BORDER_6_UNITA1",12,51.25]
["BOWMN_6_HYDRO",1,0.2]
["BOWMN_6_HYDRO",2,0.1]
["BOWMN_6_HYDRO",3,0.71]
["BOWMN_6_HYDRO",4,1.17]
["BOWMN_6_HYDRO",5,2.0099999999999998]
["BOWMN_6_HYDRO",6,1.32]
["BOWMN_6_HYDRO",7,2.2200000000000002]
["BOWMN_6_HYDRO",8,2.0299999999999998]
["BOWMN_6_HYDRO",9,1.54]
["BOWMN_6_HYDRO",10,0.98]
["BOWMN_6_HYDRO",11,0.4]
["BOWMN_6_HYDRO",12,0.22]
["BRDGVL_7_BAKER",1,0.76]
["BRDGVL_7_BAKER",2,0.6]
["BRDGVL_7_BAKER",3,0.36]
["BRDGVL_7_BAKER",4,0.16]
["BRDGVL_7_BAKER",5,7.0000000000000007E-2]
["BRDGVL_7_BAKER",6,0]
["BRDGVL_7_BAKER",7,0]
["BRDGVL_7_BAKER",8,0]
["BRDGVL_7_BAKER",9,0]
["BRDGVL_7_BAKER",10,0.01]
["BRDGVL_7_BAKER",11,0]
["BRDGVL_7_BAKER",12,0.15]
["BRDSLD_2_HIWIND",1,53.2]
["BRDSLD_2_HIWIND",2,57.07]
["BRDSLD_2_HIWIND",3,50.9]
["BRDSLD_2_HIWIND",4,53.78]
["BRDSLD_2_HIWIND",5,55.64]
["BRDSLD_2_HIWIND",6,41.04]
["BRDSLD_2_HIWIND",7,36.5]
["BRDSLD_2_HIWIND",8,34.28]
["BRDSLD_2_HIWIND",9,35.200000000000003]
["BRDSLD_2_HIWIND",10,29.49]
["BRDSLD_2_HIWIND",11,37.26]
["BRDSLD_2_HIWIND",12,47.63]
["BRDSLD_2_MTZUM2",1,25.68]
["BRDSLD_2_MTZUM2",2,27.55]
["BRDSLD_2_MTZUM2",3,24.57]
["BRDSLD_2_MTZUM2",4,25.96]
["BRDSLD_2_MTZUM2",5,26.86]
["BRDSLD_2_MTZUM2",6,19.809999999999999]
["BRDSLD_2_MTZUM2",7,17.62]
["BRDSLD_2_MTZUM2",8,16.55]
["BRDSLD_2_MTZUM2",9,16.989999999999998]
["BRDSLD_2_MTZUM2",10,14.24]
["BRDSLD_2_MTZUM2",11,17.989999999999998]
["BRDSLD_2_MTZUM2",12,22.99]
["BRDSLD_2_MTZUMA",1,12.08]
["BRDSLD_2_MTZUMA",2,12.97]
["BRDSLD_2_MTZUMA",3,11.56]
["BRDSLD_2_MTZUMA",4,12.22]
["BRDSLD_2_MTZUMA",5,12.64]
["BRDSLD_2_MTZUMA",6,9.32]
["BRDSLD_2_MTZUMA",7,8.2899999999999991]
["BRDSLD_2_MTZUMA",8,7.79]
["BRDSLD_2_MTZUMA",9,8]
["BRDSLD_2_MTZUMA",10,6.7]
["BRDSLD_2_MTZUMA",11,8.4600000000000009]
["BRDSLD_2_MTZUMA",12,10.82]
["BRDSLD_2_SHILO1",1,49.26]
["BRDSLD_2_SHILO1",2,52.85]
["BRDSLD_2_SHILO1",3,47.13]
["BRDSLD_2_SHILO1",4,49.79]
["BRDSLD_2_SHILO1",5,51.51]
["BRDSLD_2_SHILO1",6,38]
["BRDSLD_2_SHILO1",7,33.799999999999997]
["BRDSLD_2_SHILO1",8,31.74]
["BRDSLD_2_SHILO1",9,32.590000000000003]
["BRDSLD_2_SHILO1",10,27.31]
["BRDSLD_2_SHILO1",11,34.5]
["BRDSLD_2_SHILO1",12,44.1]
["BRDSLD_2_SHILO2",1,49.26]
["BRDSLD_2_SHILO2",2,52.85]
["BRDSLD_2_SHILO2",3,47.13]
["BRDSLD_2_SHILO2",4,49.79]
["BRDSLD_2_SHILO2",5,51.51]
["BRDSLD_2_SHILO2",6,38]
["BRDSLD_2_SHILO2",7,33.799999999999997]
["BRDSLD_2_SHILO2",8,31.74]
["BRDSLD_2_SHILO2",9,32.590000000000003]
["BRDSLD_2_SHILO2",10,27.31]
["BRDSLD_2_SHILO2",11,34.5]
["BRDSLD_2_SHILO2",12,44.1]
["BRDSLD_2_SHLO3A",1,33.659999999999997]
["BRDSLD_2_SHLO3A",2,36.11]
["BRDSLD_2_SHLO3A",3,32.21]
["BRDSLD_2_SHLO3A",4,34.03]
["BRDSLD_2_SHLO3A",5,35.200000000000003]
["BRDSLD_2_SHLO3A",6,25.97]
["BRDSLD_2_SHLO3A",7,23.09]
["BRDSLD_2_SHLO3A",8,21.69]
["BRDSLD_2_SHLO3A",9,22.27]
["BRDSLD_2_SHLO3A",10,18.66]
["BRDSLD_2_SHLO3A",11,23.58]
["BRDSLD_2_SHLO3A",12,30.14]
["BRDSLD_2_SHLO3B",1,32.840000000000003]
["BRDSLD_2_SHLO3B",2,35.229999999999997]
["BRDSLD_2_SHLO3B",3,31.42]
["BRDSLD_2_SHLO3B",4,33.200000000000003]
["BRDSLD_2_SHLO3B",5,34.340000000000003]
["BRDSLD_2_SHLO3B",6,25.33]
["BRDSLD_2_SHLO3B",7,22.53]
["BRDSLD_2_SHLO3B",8,21.16]
["BRDSLD_2_SHLO3B",9,21.73]
["BRDSLD_2_SHLO3B",10,18.21]
["BRDSLD_2_SHLO3B",11,23]
["BRDSLD_2_SHLO3B",12,29.4]
["BREGGO_6_DEGRSL",1,0.03]
["BREGGO_6_DEGRSL",2,0.19]
["BREGGO_6_DEGRSL",3,0.22]
["BREGGO_6_DEGRSL",4,0.28000000000000003]
["BREGGO_6_DEGRSL",5,0.4]
["BREGGO_6_DEGRSL",6,0.83]
["BREGGO_6_DEGRSL",7,0.91]
["BREGGO_6_DEGRSL",8,0.78]
["BREGGO_6_DEGRSL",9,0.7]
["BREGGO_6_DEGRSL",10,0.47]
["BREGGO_6_DEGRSL",11,0.36]
["BREGGO_6_DEGRSL",12,0.22]
["BREGGO_6_SOLAR",1,0.1]
["BREGGO_6_SOLAR",2,0.78]
["BREGGO_6_SOLAR",3,0.91]
["BREGGO_6_SOLAR",4,1.1399999999999999]
["BREGGO_6_SOLAR",5,1.66]
["BREGGO_6_SOLAR",6,3.41]
["BREGGO_6_SOLAR",7,3.74]
["BREGGO_6_SOLAR",8,3.22]
["BREGGO_6_SOLAR",9,2.89]
["BREGGO_6_SOLAR",10,1.92]
["BREGGO_6_SOLAR",11,1.48]
["BREGGO_6_SOLAR",12,0.91]
["BRODIE_2_WIND",1,18.02]
["BRODIE_2_WIND",2,19.170000000000002]
["BRODIE_2_WIND",3,16.84]
["BRODIE_2_WIND",4,16.14]
["BRODIE_2_WIND",5,17.16]
["BRODIE_2_WIND",6,15.73]
["BRODIE_2_WIND",7,14.61]
["BRODIE_2_WIND",8,11.1]
["BRODIE_2_WIND",9,11.47]
["BRODIE_2_WIND",10,10.64]
["BRODIE_2_WIND",11,14.34]
["BRODIE_2_WIND",12,17.37]
["BUCKBL_2_PL1X3",1,493.63]
["BUCKBL_2_PL1X3",2,493.63]
["BUCKBL_2_PL1X3",3,493.63]
["BUCKBL_2_PL1X3",4,493.63]
["BUCKBL_2_PL1X3",5,493.63]
["BUCKBL_2_PL1X3",6,493.63]
["BUCKBL_2_PL1X3",7,493.63]
["BUCKBL_2_PL1X3",8,493.63]
["BUCKBL_2_PL1X3",9,493.63]
["BUCKBL_2_PL1X3",10,493.63]
["BUCKBL_2_PL1X3",11,493.63]
["BUCKBL_2_PL1X3",12,493.63]
["BUCKCK_2_HYDRO",1,0.11]
["BUCKCK_2_HYDRO",2,0.23]
["BUCKCK_2_HYDRO",3,0.23]
["BUCKCK_2_HYDRO",4,0.23]
["BUCKCK_2_HYDRO",5,0.23]
["BUCKCK_2_HYDRO",6,0.16]
["BUCKCK_2_HYDRO",7,0.08]
["BUCKCK_2_HYDRO",8,0.08]
["BUCKCK_2_HYDRO",9,0]
["BUCKCK_2_HYDRO",10,0.02]
["BUCKCK_2_HYDRO",11,0.18]
["BUCKCK_2_HYDRO",12,0.35]
["BUCKCK_7_OAKFLT",1,0.61]
["BUCKCK_7_OAKFLT",2,0.48]
["BUCKCK_7_OAKFLT",3,0.62]
["BUCKCK_7_OAKFLT",4,0.67]
["BUCKCK_7_OAKFLT",5,0.76]
["BUCKCK_7_OAKFLT",6,0.79]
["BUCKCK_7_OAKFLT",7,0.83]
["BUCKCK_7_OAKFLT",8,0.56999999999999995]
["BUCKCK_7_OAKFLT",9,0.4]
["BUCKCK_7_OAKFLT",10,0.21]
["BUCKCK_7_OAKFLT",11,0.2]
["BUCKCK_7_OAKFLT",12,0.35]
["BUCKCK_7_PL1X2",1,55.6]
["BUCKCK_7_PL1X2",2,50.82]
["BUCKCK_7_PL1X2",3,52.25]
["BUCKCK_7_PL1X2",4,50.8]
["BUCKCK_7_PL1X2",5,53.4]
["BUCKCK_7_PL1X2",6,50.8]
["BUCKCK_7_PL1X2",7,54.6]
["BUCKCK_7_PL1X2",8,46.8]
["BUCKCK_7_PL1X2",9,26.4]
["BUCKCK_7_PL1X2",10,26.4]
["BUCKCK_7_PL1X2",11,45.8]
["BUCKCK_7_PL1X2",12,50.8]
["BUCKWD_1_NPALM1",1,0.01]
["BUCKWD_1_NPALM1",2,7.0000000000000007E-2]
["BUCKWD_1_NPALM1",3,0.08]
["BUCKWD_1_NPALM1",4,0.11]
["BUCKWD_1_NPALM1",5,0.15]
["BUCKWD_1_NPALM1",6,0.31]
["BUCKWD_1_NPALM1",7,0.35]
["BUCKWD_1_NPALM1",8,0.3]
["BUCKWD_1_NPALM1",9,0.27]
["BUCKWD_1_NPALM1",10,0.18]
["BUCKWD_1_NPALM1",11,0.14000000000000001]
["BUCKWD_1_NPALM1",12,0.08]
["BUCKWD_1_QF",1,2.92]
["BUCKWD_1_QF",2,3.1]
["BUCKWD_1_QF",3,2.72]
["BUCKWD_1_QF",4,2.61]
["BUCKWD_1_QF",5,2.78]
["BUCKWD_1_QF",6,2.54]
["BUCKWD_1_QF",7,2.36]
["BUCKWD_1_QF",8,1.8]
["BUCKWD_1_QF",9,1.86]
["BUCKWD_1_QF",10,1.72]
["BUCKWD_1_QF",11,2.3199999999999998]
["BUCKWD_1_QF",12,2.81]
["BUCKWD_7_WINTCV",1,0.23]
["BUCKWD_7_WINTCV",2,0.25]
["BUCKWD_7_WINTCV",3,0.22]
["BUCKWD_7_WINTCV",4,0.21]
["BUCKWD_7_WINTCV",5,0.22]
["BUCKWD_7_WINTCV",6,0.2]
["BUCKWD_7_WINTCV",7,0.19]
["BUCKWD_7_WINTCV",8,0.14000000000000001]
["BUCKWD_7_WINTCV",9,0.15]
["BUCKWD_7_WINTCV",10,0.14000000000000001]
["BUCKWD_7_WINTCV",11,0.19]
["BUCKWD_7_WINTCV",12,0.22]
["BURNYF_2_UNIT 1",1,28.8]
["BURNYF_2_UNIT 1",2,28.75]
["BURNYF_2_UNIT 1",3,28.48]
["BURNYF_2_UNIT 1",4,28.79]
["BURNYF_2_UNIT 1",5,28.9]
["BURNYF_2_UNIT 1",6,28.82]
["BURNYF_2_UNIT 1",7,29]
["BURNYF_2_UNIT 1",8,28.65]
["BURNYF_2_UNIT 1",9,29]
["BURNYF_2_UNIT 1",10,28.57]
["BURNYF_2_UNIT 1",11,28.75]
["BURNYF_2_UNIT 1",12,28.98]
["BUTTVL_7_UNIT 1",1,38.799999999999997]
["BUTTVL_7_UNIT 1",2,31.6]
["BUTTVL_7_UNIT 1",3,28.8]
["BUTTVL_7_UNIT 1",4,31.2]
["BUTTVL_7_UNIT 1",5,31.6]
["BUTTVL_7_UNIT 1",6,31.6]
["BUTTVL_7_UNIT 1",7,38.799999999999997]
["BUTTVL_7_UNIT 1",8,31.6]
["BUTTVL_7_UNIT 1",9,38.799999999999997]
["BUTTVL_7_UNIT 1",10,31.6]
["BUTTVL_7_UNIT 1",11,31.6]
["BUTTVL_7_UNIT 1",12,38.799999999999997]
["CABALO_2_M2BSR1",1,0.2]
["CABALO_2_M2BSR1",2,1.5]
["CABALO_2_M2BSR1",3,1.75]
["CABALO_2_M2BSR1",4,2.2000000000000002]
["CABALO_2_M2BSR1",5,3.2]
["CABALO_2_M2BSR1",6,6.55]
["CABALO_2_M2BSR1",7,7.2]
["CABALO_2_M2BSR1",8,6.2]
["CABALO_2_M2BSR1",9,5.55]
["CABALO_2_M2BSR1",10,3.7]
["CABALO_2_M2BSR1",11,2.85]
["CABALO_2_M2BSR1",12,1.75]
["CABALO_2_M2WSR2",1,0.4]
["CABALO_2_M2WSR2",2,3]
["CABALO_2_M2WSR2",3,3.5]
["CABALO_2_M2WSR2",4,4.4000000000000004]
["CABALO_2_M2WSR2",5,6.4]
["CABALO_2_M2WSR2",6,13.1]
["CABALO_2_M2WSR2",7,14.4]
["CABALO_2_M2WSR2",8,12.4]
["CABALO_2_M2WSR2",9,11.1]
["CABALO_2_M2WSR2",10,7.4]
["CABALO_2_M2WSR2",11,5.7]
["CABALO_2_M2WSR2",12,3.5]
["CABZON_1_WINDA1",1,7.24]
["CABZON_1_WINDA1",2,7.71]
["CABZON_1_WINDA1",3,6.77]
["CABZON_1_WINDA1",4,6.49]
["CABZON_1_WINDA1",5,6.9]
["CABZON_1_WINDA1",6,6.32]
["CABZON_1_WINDA1",7,5.87]
["CABZON_1_WINDA1",8,4.46]
["CABZON_1_WINDA1",9,4.6100000000000003]
["CABZON_1_WINDA1",10,4.28]
["CABZON_1_WINDA1",11,5.76]
["CABZON_1_WINDA1",12,6.98]
["CALFTN_2_CFSBT1",1,60]
["CALFTN_2_CFSBT1",2,60]
["CALFTN_2_CFSBT1",3,60]
["CALFTN_2_CFSBT1",4,60]
["CALFTN_2_CFSBT1",5,60]
["CALFTN_2_CFSBT1",6,60]
["CALFTN_2_CFSBT1",7,60]
["CALFTN_2_CFSBT1",8,60]
["CALFTN_2_CFSBT1",9,60]
["CALFTN_2_CFSBT1",10,60]
["CALFTN_2_CFSBT1",11,60]
["CALFTN_2_CFSBT1",12,60]
["CALFTN_2_SOLAR",1,0.24]
["CALFTN_2_SOLAR",2,2.21]
["CALFTN_2_SOLAR",3,2.66]
["CALFTN_2_SOLAR",4,3.67]
["CALFTN_2_SOLAR",5,5.5]
["CALFTN_2_SOLAR",6,11.48]
["CALFTN_2_SOLAR",7,12.6]
["CALFTN_2_SOLAR",8,10.54]
["CALFTN_2_SOLAR",9,8.9499999999999993]
["CALFTN_2_SOLAR",10,5.41]
["CALFTN_2_SOLAR",11,3.61]
["CALFTN_2_SOLAR",12,1.67]
["CALFTS_2_CFSSR1",1,0.6]
["CALFTS_2_CFSSR1",2,4.5]
["CALFTS_2_CFSSR1",3,5.25]
["CALFTS_2_CFSSR1",4,6.6]
["CALFTS_2_CFSSR1",5,9.6]
["CALFTS_2_CFSSR1",6,19.649999999999999]
["CALFTS_2_CFSSR1",7,21.6]
["CALFTS_2_CFSSR1",8,18.600000000000001]
["CALFTS_2_CFSSR1",9,16.649999999999999]
["CALFTS_2_CFSSR1",10,11.1]
["CALFTS_2_CFSSR1",11,8.5500000000000007]
["CALFTS_2_CFSSR1",12,5.25]
["CALGEN_1_UNITS",1,80]
["CALGEN_1_UNITS",2,80]
["CALGEN_1_UNITS",3,80]
["CALGEN_1_UNITS",4,80]
["CALGEN_1_UNITS",5,80]
["CALGEN_1_UNITS",6,80]
["CALGEN_1_UNITS",7,80]
["CALGEN_1_UNITS",8,80]
["CALGEN_1_UNITS",9,80]
["CALGEN_1_UNITS",10,80]
["CALGEN_1_UNITS",11,80]
["CALGEN_1_UNITS",12,80]
["CALPIN_1_AGNEW",1,28.56]
["CALPIN_1_AGNEW",2,28.56]
["CALPIN_1_AGNEW",3,28.56]
["CALPIN_1_AGNEW",4,28.56]
["CALPIN_1_AGNEW",5,28.56]
["CALPIN_1_AGNEW",6,28.56]
["CALPIN_1_AGNEW",7,28.56]
["CALPIN_1_AGNEW",8,28.56]
["CALPIN_1_AGNEW",9,28.56]
["CALPIN_1_AGNEW",10,28.56]
["CALPIN_1_AGNEW",11,28.56]
["CALPIN_1_AGNEW",12,28.56]
["CAMCHE_1_PL1X3",1,2.4900000000000002]
["CAMCHE_1_PL1X3",2,4.6399999999999997]
["CAMCHE_1_PL1X3",3,4.84]
["CAMCHE_1_PL1X3",4,4.95]
["CAMCHE_1_PL1X3",5,5.24]
["CAMCHE_1_PL1X3",6,4.25]
["CAMCHE_1_PL1X3",7,3.62]
["CAMCHE_1_PL1X3",8,2.33]
["CAMCHE_1_PL1X3",9,1.66]
["CAMCHE_1_PL1X3",10,1.75]
["CAMCHE_1_PL1X3",11,1.41]
["CAMCHE_1_PL1X3",12,1.72]
["CAMLOT_2_SOLAR1",1,0.18]
["CAMLOT_2_SOLAR1",2,1.35]
["CAMLOT_2_SOLAR1",3,1.58]
["CAMLOT_2_SOLAR1",4,1.98]
["CAMLOT_2_SOLAR1",5,2.88]
["CAMLOT_2_SOLAR1",6,5.9]
["CAMLOT_2_SOLAR1",7,6.48]
["CAMLOT_2_SOLAR1",8,5.58]
["CAMLOT_2_SOLAR1",9,5]
["CAMLOT_2_SOLAR1",10,3.33]
["CAMLOT_2_SOLAR1",11,2.57]
["CAMLOT_2_SOLAR1",12,1.58]
["CAMLOT_2_SOLAR2",1,0.06]
["CAMLOT_2_SOLAR2",2,0.45]
["CAMLOT_2_SOLAR2",3,0.53]
["CAMLOT_2_SOLAR2",4,0.66]
["CAMLOT_2_SOLAR2",5,0.96]
["CAMLOT_2_SOLAR2",6,1.97]
["CAMLOT_2_SOLAR2",7,2.16]
["CAMLOT_2_SOLAR2",8,1.86]
["CAMLOT_2_SOLAR2",9,1.67]
["CAMLOT_2_SOLAR2",10,1.1100000000000001]
["CAMLOT_2_SOLAR2",11,0.86]
["CAMLOT_2_SOLAR2",12,0.53]
["CAMPFW_7_FARWST",1,0]
["CAMPFW_7_FARWST",2,0]
["CAMPFW_7_FARWST",3,3.28]
["CAMPFW_7_FARWST",4,2]
["CAMPFW_7_FARWST",5,1.06]
["CAMPFW_7_FARWST",6,0.74]
["CAMPFW_7_FARWST",7,3.1]
["CAMPFW_7_FARWST",8,3.7]
["CAMPFW_7_FARWST",9,0]
["CAMPFW_7_FARWST",10,0]
["CAMPFW_7_FARWST",11,0]
["CAMPFW_7_FARWST",12,0]
["CANTUA_1_SOLAR",1,0.08]
["CANTUA_1_SOLAR",2,0.6]
["CANTUA_1_SOLAR",3,0.7]
["CANTUA_1_SOLAR",4,0.88]
["CANTUA_1_SOLAR",5,1.28]
["CANTUA_1_SOLAR",6,2.62]
["CANTUA_1_SOLAR",7,2.88]
["CANTUA_1_SOLAR",8,2.48]
["CANTUA_1_SOLAR",9,2.2200000000000002]
["CANTUA_1_SOLAR",10,1.48]
["CANTUA_1_SOLAR",11,1.1399999999999999]
["CANTUA_1_SOLAR",12,0.7]
["CAPWD_1_QF",1,3.45]
["CAPWD_1_QF",2,3.67]
["CAPWD_1_QF",3,3.23]
["CAPWD_1_QF",4,3.09]
["CAPWD_1_QF",5,3.29]
["CAPWD_1_QF",6,3.01]
["CAPWD_1_QF",7,2.8]
["CAPWD_1_QF",8,2.13]
["CAPWD_1_QF",9,2.2000000000000002]
["CAPWD_1_QF",10,2.04]
["CAPWD_1_QF",11,2.75]
["CAPWD_1_QF",12,3.33]
["CARBOU_7_PL2X3",1,19.600000000000001]
["CARBOU_7_PL2X3",2,1.6]
["CARBOU_7_PL2X3",3,0]
["CARBOU_7_PL2X3",4,0]
["CARBOU_7_PL2X3",5,0]
["CARBOU_7_PL2X3",6,0]
["CARBOU_7_PL2X3",7,22.6]
["CARBOU_7_PL2X3",8,32.4]
["CARBOU_7_PL2X3",9,20]
["CARBOU_7_PL2X3",10,12.8]
["CARBOU_7_PL2X3",11,0]
["CARBOU_7_PL2X3",12,8]
["CARBOU_7_PL4X5",1,47.2]
["CARBOU_7_PL4X5",2,43.2]
["CARBOU_7_PL4X5",3,47.2]
["CARBOU_7_PL4X5",4,16.8]
["CARBOU_7_PL4X5",5,29.52]
["CARBOU_7_PL4X5",6,64]
["CARBOU_7_PL4X5",7,101.19]
["CARBOU_7_PL4X5",8,93.2]
["CARBOU_7_PL4X5",9,93.46]
["CARBOU_7_PL4X5",10,80]
["CARBOU_7_PL4X5",11,25.6]
["CARBOU_7_PL4X5",12,43.44]
["CARBOU_7_UNIT 1",1,19.04]
["CARBOU_7_UNIT 1",2,0]
["CARBOU_7_UNIT 1",3,0]
["CARBOU_7_UNIT 1",4,0]
["CARBOU_7_UNIT 1",5,0]
["CARBOU_7_UNIT 1",6,0]
["CARBOU_7_UNIT 1",7,8.8000000000000007]
["CARBOU_7_UNIT 1",8,19.04]
["CARBOU_7_UNIT 1",9,16.8]
["CARBOU_7_UNIT 1",10,0]
["CARBOU_7_UNIT 1",11,0]
["CARBOU_7_UNIT 1",12,0]
["CARLS1_2_CARCT1",1,422]
["CARLS1_2_CARCT1",2,422]
["CARLS1_2_CARCT1",3,422]
["CARLS1_2_CARCT1",4,422]
["CARLS1_2_CARCT1",5,422]
["CARLS1_2_CARCT1",6,422]
["CARLS1_2_CARCT1",7,422]
["CARLS1_2_CARCT1",8,422]
["CARLS1_2_CARCT1",9,422]
["CARLS1_2_CARCT1",10,422]
["CARLS1_2_CARCT1",11,422]
["CARLS1_2_CARCT1",12,422]
["CARLS2_1_CARCT1",1,105.5]
["CARLS2_1_CARCT1",2,105.5]
["CARLS2_1_CARCT1",3,105.5]
["CARLS2_1_CARCT1",4,105.5]
["CARLS2_1_CARCT1",5,105.5]
["CARLS2_1_CARCT1",6,105.5]
["CARLS2_1_CARCT1",7,105.5]
["CARLS2_1_CARCT1",8,105.5]
["CARLS2_1_CARCT1",9,105.5]
["CARLS2_1_CARCT1",10,105.5]
["CARLS2_1_CARCT1",11,105.5]
["CARLS2_1_CARCT1",12,105.5]
["CASADB_1_CD4GT1",1,31]
["CASADB_1_CD4GT1",2,31]
["CASADB_1_CD4GT1",3,31]
["CASADB_1_CD4GT1",4,31]
["CASADB_1_CD4GT1",5,31]
["CASADB_1_CD4GT1",6,31]
["CASADB_1_CD4GT1",7,31]
["CASADB_1_CD4GT1",8,31]
["CASADB_1_CD4GT1",9,31]
["CASADB_1_CD4GT1",10,31]
["CASADB_1_CD4GT1",11,31]
["CASADB_1_CD4GT1",12,31]
["CATLNA_2_SOLAR",1,0.44]
["CATLNA_2_SOLAR",2,3.3]
["CATLNA_2_SOLAR",3,3.85]
["CATLNA_2_SOLAR",4,4.84]
["CATLNA_2_SOLAR",5,7.04]
["CATLNA_2_SOLAR",6,14.41]
["CATLNA_2_SOLAR",7,15.84]
["CATLNA_2_SOLAR",8,13.64]
["CATLNA_2_SOLAR",9,12.21]
["CATLNA_2_SOLAR",10,8.14]
["CATLNA_2_SOLAR",11,6.27]
["CATLNA_2_SOLAR",12,3.85]
["CATLNA_2_SOLAR2",1,7.0000000000000007E-2]
["CATLNA_2_SOLAR2",2,0.54]
["CATLNA_2_SOLAR2",3,0.63]
["CATLNA_2_SOLAR2",4,0.79]
["CATLNA_2_SOLAR2",5,1.1499999999999999]
["CATLNA_2_SOLAR2",6,2.36]
["CATLNA_2_SOLAR2",7,2.59]
["CATLNA_2_SOLAR2",8,2.23]
["CATLNA_2_SOLAR2",9,2]
["CATLNA_2_SOLAR2",10,1.33]
["CATLNA_2_SOLAR2",11,1.03]
["CATLNA_2_SOLAR2",12,0.63]
["CAVLSR_2_BSOLAR",1,0.16]
["CAVLSR_2_BSOLAR",2,1.2]
["CAVLSR_2_BSOLAR",3,1.4]
["CAVLSR_2_BSOLAR",4,1.76]
["CAVLSR_2_BSOLAR",5,2.56]
["CAVLSR_2_BSOLAR",6,5.24]
["CAVLSR_2_BSOLAR",7,5.76]
["CAVLSR_2_BSOLAR",8,4.96]
["CAVLSR_2_BSOLAR",9,4.4400000000000004]
["CAVLSR_2_BSOLAR",10,2.96]
["CAVLSR_2_BSOLAR",11,2.2799999999999998]
["CAVLSR_2_BSOLAR",12,1.4]
["CAVLSR_2_RSOLAR",1,0.84]
["CAVLSR_2_RSOLAR",2,6.3]
["CAVLSR_2_RSOLAR",3,7.35]
["CAVLSR_2_RSOLAR",4,9.24]
["CAVLSR_2_RSOLAR",5,13.44]
["CAVLSR_2_RSOLAR",6,27.51]
["CAVLSR_2_RSOLAR",7,30.24]
["CAVLSR_2_RSOLAR",8,26.04]
["CAVLSR_2_RSOLAR",9,23.31]
["CAVLSR_2_RSOLAR",10,15.54]
["CAVLSR_2_RSOLAR",11,11.97]
["CAVLSR_2_RSOLAR",12,7.35]
["CAYTNO_2_VASCO",1,3.98]
["CAYTNO_2_VASCO",2,4.08]
["CAYTNO_2_VASCO",3,4.08]
["CAYTNO_2_VASCO",4,4.07]
["CAYTNO_2_VASCO",5,4.0599999999999996]
["CAYTNO_2_VASCO",6,4.04]
["CAYTNO_2_VASCO",7,4.0199999999999996]
["CAYTNO_2_VASCO",8,4.03]
["CAYTNO_2_VASCO",9,4.04]
["CAYTNO_2_VASCO",10,3.91]
["CAYTNO_2_VASCO",11,3.98]
["CAYTNO_2_VASCO",12,4.1100000000000003]
["CDWR07_2_GEN",1,115.6]
["CDWR07_2_GEN",2,115.6]
["CDWR07_2_GEN",3,115.6]
["CDWR07_2_GEN",4,115.6]
["CDWR07_2_GEN",5,115.6]
["CDWR07_2_GEN",6,115.6]
["CDWR07_2_GEN",7,115.6]
["CDWR07_2_GEN",8,115.6]
["CDWR07_2_GEN",9,115.6]
["CDWR07_2_GEN",10,115.6]
["CDWR07_2_GEN",11,115.6]
["CDWR07_2_GEN",12,115.6]
["CEDRCK_6_UNIT",1,0.24]
["CEDRCK_6_UNIT",2,0.27]
["CEDRCK_6_UNIT",3,0.28999999999999998]
["CEDRCK_6_UNIT",4,0.44]
["CEDRCK_6_UNIT",5,0.52]
["CEDRCK_6_UNIT",6,0.26]
["CEDRCK_6_UNIT",7,0.12]
["CEDRCK_6_UNIT",8,0.09]
["CEDRCK_6_UNIT",9,0.08]
["CEDRCK_6_UNIT",10,0.1]
["CEDRCK_6_UNIT",11,0.14000000000000001]
["CEDRCK_6_UNIT",12,0.17]
["CEDUCR_2_SOLAR1",1,0]
["CEDUCR_2_SOLAR1",2,0]
["CEDUCR_2_SOLAR1",3,0]
["CEDUCR_2_SOLAR1",4,0]
["CEDUCR_2_SOLAR1",5,0]
["CEDUCR_2_SOLAR1",6,0]
["CEDUCR_2_SOLAR1",7,0]
["CEDUCR_2_SOLAR1",8,0]
["CEDUCR_2_SOLAR1",9,0]
["CEDUCR_2_SOLAR1",10,0]
["CEDUCR_2_SOLAR1",11,0]
["CEDUCR_2_SOLAR1",12,0]
["CEDUCR_2_SOLAR2",1,0]
["CEDUCR_2_SOLAR2",2,0]
["CEDUCR_2_SOLAR2",3,0]
["CEDUCR_2_SOLAR2",4,0]
["CEDUCR_2_SOLAR2",5,0]
["CEDUCR_2_SOLAR2",6,0]
["CEDUCR_2_SOLAR2",7,0]
["CEDUCR_2_SOLAR2",8,0]
["CEDUCR_2_SOLAR2",9,0]
["CEDUCR_2_SOLAR2",10,0]
["CEDUCR_2_SOLAR2",11,0]
["CEDUCR_2_SOLAR2",12,0]
["CEDUCR_2_SOLAR3",1,0]
["CEDUCR_2_SOLAR3",2,0]
["CEDUCR_2_SOLAR3",3,0]
["CEDUCR_2_SOLAR3",4,0]
["CEDUCR_2_SOLAR3",5,0]
["CEDUCR_2_SOLAR3",6,0]
["CEDUCR_2_SOLAR3",7,0]
["CEDUCR_2_SOLAR3",8,0]
["CEDUCR_2_SOLAR3",9,0]
["CEDUCR_2_SOLAR3",10,0]
["CEDUCR_2_SOLAR3",11,0]
["CEDUCR_2_SOLAR3",12,0]
["CEDUCR_2_SOLAR4",1,0]
["CEDUCR_2_SOLAR4",2,0]
["CEDUCR_2_SOLAR4",3,0]
["CEDUCR_2_SOLAR4",4,0]
["CEDUCR_2_SOLAR4",5,0]
["CEDUCR_2_SOLAR4",6,0]
["CEDUCR_2_SOLAR4",7,0]
["CEDUCR_2_SOLAR4",8,0]
["CEDUCR_2_SOLAR4",9,0]
["CEDUCR_2_SOLAR4",10,0]
["CEDUCR_2_SOLAR4",11,0]
["CEDUCR_2_SOLAR4",12,0]
["CENT40_1_C40SR1",1,0.16]
["CENT40_1_C40SR1",2,1.2]
["CENT40_1_C40SR1",3,1.4]
["CENT40_1_C40SR1",4,1.76]
["CENT40_1_C40SR1",5,2.56]
["CENT40_1_C40SR1",6,5.24]
["CENT40_1_C40SR1",7,5.76]
["CENT40_1_C40SR1",8,4.96]
["CENT40_1_C40SR1",9,4.4400000000000004]
["CENT40_1_C40SR1",10,2.96]
["CENT40_1_C40SR1",11,2.2799999999999998]
["CENT40_1_C40SR1",12,1.4]
["CENTER_2_RHONDO",1,1.91]
["CENTER_2_RHONDO",2,1.91]
["CENTER_2_RHONDO",3,1.91]
["CENTER_2_RHONDO",4,1.91]
["CENTER_2_RHONDO",5,1.91]
["CENTER_2_RHONDO",6,1.91]
["CENTER_2_RHONDO",7,1.91]
["CENTER_2_RHONDO",8,1.91]
["CENTER_2_RHONDO",9,1.91]
["CENTER_2_RHONDO",10,1.91]
["CENTER_2_RHONDO",11,1.91]
["CENTER_2_RHONDO",12,1.91]
["CENTER_2_SOLAR1",1,0]
["CENTER_2_SOLAR1",2,0]
["CENTER_2_SOLAR1",3,0]
["CENTER_2_SOLAR1",4,0]
["CENTER_2_SOLAR1",5,0]
["CENTER_2_SOLAR1",6,0]
["CENTER_2_SOLAR1",7,0]
["CENTER_2_SOLAR1",8,0]
["CENTER_2_SOLAR1",9,0]
["CENTER_2_SOLAR1",10,0]
["CENTER_2_SOLAR1",11,0]
["CENTER_2_SOLAR1",12,0]
["CENTER_2_TECNG1",1,0]
["CENTER_2_TECNG1",2,0]
["CENTER_2_TECNG1",3,0]
["CENTER_2_TECNG1",4,0]
["CENTER_2_TECNG1",5,0]
["CENTER_2_TECNG1",6,0]
["CENTER_2_TECNG1",7,0]
["CENTER_2_TECNG1",8,0]
["CENTER_2_TECNG1",9,0]
["CENTER_2_TECNG1",10,0]
["CENTER_2_TECNG1",11,0]
["CENTER_2_TECNG1",12,0]
["CENTER_6_PEAKER",1,47.3]
["CENTER_6_PEAKER",2,47.3]
["CENTER_6_PEAKER",3,47.3]
["CENTER_6_PEAKER",4,47.3]
["CENTER_6_PEAKER",5,47.3]
["CENTER_6_PEAKER",6,47.3]
["CENTER_6_PEAKER",7,47.3]
["CENTER_6_PEAKER",8,47.3]
["CENTER_6_PEAKER",9,47.3]
["CENTER_6_PEAKER",10,47.3]
["CENTER_6_PEAKER",11,47.3]
["CENTER_6_PEAKER",12,47.3]
["CENTPD_2_BMSSX2",2,4.26]
["CENTPD_2_BMSSX2",3,5.28]
["CENTPD_2_BMSSX2",4,7.27]
["CENTPD_2_BMSSX2",5,10.85]
["CENTPD_2_BMSSX2",6,22.69]
["CENTPD_2_BMSSX2",7,24.9]
["CENTPD_2_BMSSX2",8,21.01]
["CENTPD_2_BMSSX2",9,17.86]
["CENTPD_2_BMSSX2",10,11.19]
["CENTPD_2_BMSSX2",11,7.4]
["CENTPD_2_BMSSX2",12,3.25]
["CENTPD_2_BMSX2",2,112]
["CENTPD_2_BMSX2",3,112]
["CENTPD_2_BMSX2",4,112]
["CENTPD_2_BMSX2",5,112]
["CENTPD_2_BMSX2",6,112]
["CENTPD_2_BMSX2",7,112]
["CENTPD_2_BMSX2",8,112]
["CENTPD_2_BMSX2",9,112]
["CENTPD_2_BMSX2",10,112]
["CENTPD_2_BMSX2",11,112]
["CENTPD_2_BMSX2",12,112]
["CENTRY_6_PL1X4",1,40]
["CENTRY_6_PL1X4",2,40]
["CENTRY_6_PL1X4",3,40]
["CENTRY_6_PL1X4",4,40]
["CENTRY_6_PL1X4",5,40]
["CENTRY_6_PL1X4",6,40]
["CENTRY_6_PL1X4",7,40]
["CENTRY_6_PL1X4",8,40]
["CENTRY_6_PL1X4",9,40]
["CENTRY_6_PL1X4",10,40]
["CENTRY_6_PL1X4",11,40]
["CENTRY_6_PL1X4",12,40]
["CHALK_1_UNIT",1,48.67]
["CHALK_1_UNIT",2,48.67]
["CHALK_1_UNIT",3,48.67]
["CHALK_1_UNIT",4,48.67]
["CHALK_1_UNIT",5,48.67]
["CHALK_1_UNIT",6,48.67]
["CHALK_1_UNIT",7,48.67]
["CHALK_1_UNIT",8,48.67]
["CHALK_1_UNIT",9,48.67]
["CHALK_1_UNIT",10,48.67]
["CHALK_1_UNIT",11,48.67]
["CHALK_1_UNIT",12,48.67]
["CHARMN_2_PGONG1",1,19.87]
["CHARMN_2_PGONG1",2,19.87]
["CHARMN_2_PGONG1",3,19.87]
["CHARMN_2_PGONG1",4,19.87]
["CHARMN_2_PGONG1",5,19.87]
["CHARMN_2_PGONG1",6,19.87]
["CHARMN_2_PGONG1",7,19.87]
["CHARMN_2_PGONG1",8,19.87]
["CHARMN_2_PGONG1",9,19.309999999999999]
["CHARMN_2_PGONG1",10,19.829999999999998]
["CHARMN_2_PGONG1",11,18.36]
["CHARMN_2_PGONG1",12,19.87]
["CHEVCD_6_UNIT",1,0.96]
["CHEVCD_6_UNIT",2,1.66]
["CHEVCD_6_UNIT",3,1.51]
["CHEVCD_6_UNIT",4,1.39]
["CHEVCD_6_UNIT",5,1.28]
["CHEVCD_6_UNIT",6,1.72]
["CHEVCD_6_UNIT",7,1.62]
["CHEVCD_6_UNIT",8,1.64]
["CHEVCD_6_UNIT",9,1.71]
["CHEVCD_6_UNIT",10,1.68]
["CHEVCD_6_UNIT",11,1.87]
["CHEVCD_6_UNIT",12,1.55]
["CHEVCO_6_UNIT 1",1,1.19]
["CHEVCO_6_UNIT 1",2,1.22]
["CHEVCO_6_UNIT 1",3,1.34]
["CHEVCO_6_UNIT 1",4,1.3]
["CHEVCO_6_UNIT 1",5,2.1800000000000002]
["CHEVCO_6_UNIT 1",6,2.19]
["CHEVCO_6_UNIT 1",7,2.31]
["CHEVCO_6_UNIT 1",8,2.71]
["CHEVCO_6_UNIT 1",9,2.87]
["CHEVCO_6_UNIT 1",10,2.42]
["CHEVCO_6_UNIT 1",11,1.5]
["CHEVCO_6_UNIT 1",12,1.1499999999999999]
["CHEVCO_6_UNIT 2",1,0.93]
["CHEVCO_6_UNIT 2",2,1.01]
["CHEVCO_6_UNIT 2",3,1.1100000000000001]
["CHEVCO_6_UNIT 2",4,1.08]
["CHEVCO_6_UNIT 2",5,0.91]
["CHEVCO_6_UNIT 2",6,0.73]
["CHEVCO_6_UNIT 2",7,0.66]
["CHEVCO_6_UNIT 2",8,0.6]
["CHEVCO_6_UNIT 2",9,0.72]
["CHEVCO_6_UNIT 2",10,0.94]
["CHEVCO_6_UNIT 2",11,1.02]
["CHEVCO_6_UNIT 2",12,1]
["CHEVCY_1_UNIT",1,4.8099999999999996]
["CHEVCY_1_UNIT",2,4.08]
["CHEVCY_1_UNIT",3,3.46]
["CHEVCY_1_UNIT",4,3.57]
["CHEVCY_1_UNIT",5,3.18]
["CHEVCY_1_UNIT",6,3.7]
["CHEVCY_1_UNIT",7,3.6]
["CHEVCY_1_UNIT",8,2.92]
["CHEVCY_1_UNIT",9,2.61]
["CHEVCY_1_UNIT",10,3.71]
["CHEVCY_1_UNIT",11,3.21]
["CHEVCY_1_UNIT",12,3.4]
["CHEVMN_2_UNITS",1,3.84]
["CHEVMN_2_UNITS",2,4.1100000000000003]
["CHEVMN_2_UNITS",3,8.2799999999999994]
["CHEVMN_2_UNITS",4,26.35]
["CHEVMN_2_UNITS",5,6.88]
["CHEVMN_2_UNITS",6,5.52]
["CHEVMN_2_UNITS",7,13.32]
["CHEVMN_2_UNITS",8,7.93]
["CHEVMN_2_UNITS",9,13.95]
["CHEVMN_2_UNITS",10,7.64]
["CHEVMN_2_UNITS",11,6.21]
["CHEVMN_2_UNITS",12,1.26]
["CHICPK_7_UNIT 1",1,19.68]
["CHICPK_7_UNIT 1",2,19.940000000000001]
["CHICPK_7_UNIT 1",3,19.8]
["CHICPK_7_UNIT 1",4,19.2]
["CHICPK_7_UNIT 1",5,20.54]
["CHICPK_7_UNIT 1",6,21.6]
["CHICPK_7_UNIT 1",7,27.6]
["CHICPK_7_UNIT 1",8,27.2]
["CHICPK_7_UNIT 1",9,8.8000000000000007]
["CHICPK_7_UNIT 1",10,6.4]
["CHICPK_7_UNIT 1",11,18.8]
["CHICPK_7_UNIT 1",12,23.32]
["CHILLS_1_SYCENG",1,0.68]
["CHILLS_1_SYCENG",2,0.72]
["CHILLS_1_SYCENG",3,0.8]
["CHILLS_1_SYCENG",4,0.79]
["CHILLS_1_SYCENG",5,0.72]
["CHILLS_1_SYCENG",6,0.66]
["CHILLS_1_SYCENG",7,0.85]
["CHILLS_1_SYCENG",8,0.88]
["CHILLS_1_SYCENG",9,0.86]
["CHILLS_1_SYCENG",10,0.79]
["CHILLS_1_SYCENG",11,0.77]
["CHILLS_1_SYCENG",12,0.77]
["CHILLS_7_UNITA1",1,1.82]
["CHILLS_7_UNITA1",2,2]
["CHILLS_7_UNITA1",3,2]
["CHILLS_7_UNITA1",4,2]
["CHILLS_7_UNITA1",5,1.4]
["CHILLS_7_UNITA1",6,1.68]
["CHILLS_7_UNITA1",7,1.56]
["CHILLS_7_UNITA1",8,1.52]
["CHILLS_7_UNITA1",9,1.74]
["CHILLS_7_UNITA1",10,1.75]
["CHILLS_7_UNITA1",11,1.8]
["CHILLS_7_UNITA1",12,1.61]
["CHINO_2_APEBT1",1,20]
["CHINO_2_APEBT1",2,20]
["CHINO_2_APEBT1",3,20]
["CHINO_2_APEBT1",4,20]
["CHINO_2_APEBT1",5,20]
["CHINO_2_APEBT1",6,20]
["CHINO_2_APEBT1",7,20]
["CHINO_2_APEBT1",8,20]
["CHINO_2_APEBT1",9,20]
["CHINO_2_APEBT1",10,20]
["CHINO_2_APEBT1",11,20]
["CHINO_2_APEBT1",12,20]
["CHINO_2_JURUPA",1,0]
["CHINO_2_JURUPA",2,0]
["CHINO_2_JURUPA",3,0]
["CHINO_2_JURUPA",4,0]
["CHINO_2_JURUPA",5,0]
["CHINO_2_JURUPA",6,0]
["CHINO_2_JURUPA",7,0]
["CHINO_2_JURUPA",8,0]
["CHINO_2_JURUPA",9,0]
["CHINO_2_JURUPA",10,0]
["CHINO_2_JURUPA",11,0]
["CHINO_2_JURUPA",12,0]
["CHINO_2_QF",1,0]
["CHINO_2_QF",2,0.02]
["CHINO_2_QF",3,0]
["CHINO_2_QF",4,0]
["CHINO_2_QF",5,0]
["CHINO_2_QF",6,0]
["CHINO_2_QF",7,0]
["CHINO_2_QF",8,0]
["CHINO_2_QF",9,0]
["CHINO_2_QF",10,0]
["CHINO_2_QF",11,0]
["CHINO_2_QF",12,0]
["CHINO_2_SASOLR",1,0]
["CHINO_2_SASOLR",2,0]
["CHINO_2_SASOLR",3,0]
["CHINO_2_SASOLR",4,0]
["CHINO_2_SASOLR",5,0]
["CHINO_2_SASOLR",6,0]
["CHINO_2_SASOLR",7,0]
["CHINO_2_SASOLR",8,0]
["CHINO_2_SASOLR",9,0]
["CHINO_2_SASOLR",10,0]
["CHINO_2_SASOLR",11,0]
["CHINO_2_SASOLR",12,0]
["CHINO_2_SOLAR",1,0]
["CHINO_2_SOLAR",2,0.03]
["CHINO_2_SOLAR",3,0.04]
["CHINO_2_SOLAR",4,0.04]
["CHINO_2_SOLAR",5,0.06]
["CHINO_2_SOLAR",6,0.13]
["CHINO_2_SOLAR",7,0.14000000000000001]
["CHINO_2_SOLAR",8,0.12]
["CHINO_2_SOLAR",9,0.11]
["CHINO_2_SOLAR",10,7.0000000000000007E-2]
["CHINO_2_SOLAR",11,0.06]
["CHINO_2_SOLAR",12,0.04]
["CHINO_2_SOLAR2",1,0]
["CHINO_2_SOLAR2",2,0]
["CHINO_2_SOLAR2",3,0]
["CHINO_2_SOLAR2",4,0]
["CHINO_2_SOLAR2",5,0]
["CHINO_2_SOLAR2",6,0]
["CHINO_2_SOLAR2",7,0]
["CHINO_2_SOLAR2",8,0]
["CHINO_2_SOLAR2",9,0]
["CHINO_2_SOLAR2",10,0]
["CHINO_2_SOLAR2",11,0]
["CHINO_2_SOLAR2",12,0]
["CHINO_6_CIMGEN",1,26]
["CHINO_6_CIMGEN",2,26]
["CHINO_6_CIMGEN",3,26]
["CHINO_6_CIMGEN",4,26]
["CHINO_6_CIMGEN",5,26]
["CHINO_6_CIMGEN",6,26]
["CHINO_6_CIMGEN",7,26]
["CHINO_6_CIMGEN",8,26]
["CHINO_6_CIMGEN",9,26]
["CHINO_6_CIMGEN",10,26]
["CHINO_6_CIMGEN",11,26]
["CHINO_6_CIMGEN",12,26]
["CHWCHL_1_BIOMAS",1,9.67]
["CHWCHL_1_BIOMAS",2,9.8000000000000007]
["CHWCHL_1_BIOMAS",3,9.3800000000000008]
["CHWCHL_1_BIOMAS",4,9.32]
["CHWCHL_1_BIOMAS",5,9.4700000000000006]
["CHWCHL_1_BIOMAS",6,9.76]
["CHWCHL_1_BIOMAS",7,9.6]
["CHWCHL_1_BIOMAS",8,9.39]
["CHWCHL_1_BIOMAS",9,9.61]
["CHWCHL_1_BIOMAS",10,9.4499999999999993]
["CHWCHL_1_BIOMAS",11,9.42]
["CHWCHL_1_BIOMAS",12,9.08]
["CHWCHL_1_UNIT",1,48]
["CHWCHL_1_UNIT",2,48]
["CHWCHL_1_UNIT",3,48]
["CHWCHL_1_UNIT",4,48]
["CHWCHL_1_UNIT",5,48]
["CHWCHL_1_UNIT",6,48]
["CHWCHL_1_UNIT",7,48]
["CHWCHL_1_UNIT",8,48]
["CHWCHL_1_UNIT",9,48]
["CHWCHL_1_UNIT",10,48]
["CHWCHL_1_UNIT",11,48]
["CHWCHL_1_UNIT",12,48]
["CLOVDL_1_SOLAR",1,0.01]
["CLOVDL_1_SOLAR",2,0.05]
["CLOVDL_1_SOLAR",3,0.05]
["CLOVDL_1_SOLAR",4,7.0000000000000007E-2]
["CLOVDL_1_SOLAR",5,0.1]
["CLOVDL_1_SOLAR",6,0.2]
["CLOVDL_1_SOLAR",7,0.22]
["CLOVDL_1_SOLAR",8,0.19]
["CLOVDL_1_SOLAR",9,0.17]
["CLOVDL_1_SOLAR",10,0.11]
["CLOVDL_1_SOLAR",11,0.09]
["CLOVDL_1_SOLAR",12,0.05]
["CLOVER_2_UNIT",1,0.51]
["CLOVER_2_UNIT",2,0.62]
["CLOVER_2_UNIT",3,0.53]
["CLOVER_2_UNIT",4,0.72]
["CLOVER_2_UNIT",5,0.47]
["CLOVER_2_UNIT",6,0.32]
["CLOVER_2_UNIT",7,0.21]
["CLOVER_2_UNIT",8,0.13]
["CLOVER_2_UNIT",9,0.06]
["CLOVER_2_UNIT",10,0.04]
["CLOVER_2_UNIT",11,0.09]
["CLOVER_2_UNIT",12,0.37]
["CLRMTK_1_QF",1,0]
["CLRMTK_1_QF",2,0]
["CLRMTK_1_QF",3,0]
["CLRMTK_1_QF",4,0]
["CLRMTK_1_QF",5,0]
["CLRMTK_1_QF",6,0]
["CLRMTK_1_QF",7,0]
["CLRMTK_1_QF",8,0]
["CLRMTK_1_QF",9,0]
["CLRMTK_1_QF",10,0]
["CLRMTK_1_QF",11,0]
["CLRMTK_1_QF",12,0]
["CNTNLA_2_SOLAR1",1,0.5]
["CNTNLA_2_SOLAR1",2,3.75]
["CNTNLA_2_SOLAR1",3,4.38]
["CNTNLA_2_SOLAR1",4,5.5]
["CNTNLA_2_SOLAR1",5,8]
["CNTNLA_2_SOLAR1",6,16.38]
["CNTNLA_2_SOLAR1",7,18]
["CNTNLA_2_SOLAR1",8,15.5]
["CNTNLA_2_SOLAR1",9,13.88]
["CNTNLA_2_SOLAR1",10,9.25]
["CNTNLA_2_SOLAR1",11,7.13]
["CNTNLA_2_SOLAR1",12,4.38]
["CNTNLA_2_SOLAR2",1,0.18]
["CNTNLA_2_SOLAR2",2,1.37]
["CNTNLA_2_SOLAR2",3,1.6]
["CNTNLA_2_SOLAR2",4,2.0099999999999998]
["CNTNLA_2_SOLAR2",5,2.92]
["CNTNLA_2_SOLAR2",6,5.97]
["CNTNLA_2_SOLAR2",7,6.57]
["CNTNLA_2_SOLAR2",8,5.65]
["CNTNLA_2_SOLAR2",9,5.0599999999999996]
["CNTNLA_2_SOLAR2",10,3.37]
["CNTNLA_2_SOLAR2",11,2.6]
["CNTNLA_2_SOLAR2",12,1.6]
["COCOPP_2_CTG1",1,203.08]
["COCOPP_2_CTG1",2,202.82]
["COCOPP_2_CTG1",3,202.21]
["COCOPP_2_CTG1",4,199.04]
["COCOPP_2_CTG1",5,197.87]
["COCOPP_2_CTG1",6,194.63]
["COCOPP_2_CTG1",7,193.62]
["COCOPP_2_CTG1",8,193.09]
["COCOPP_2_CTG1",9,194.72]
["COCOPP_2_CTG1",10,198.97]
["COCOPP_2_CTG1",11,200.43]
["COCOPP_2_CTG1",12,203.72]
["COCOPP_2_CTG2",1,202.25]
["COCOPP_2_CTG2",2,201.68]
["COCOPP_2_CTG2",3,201.36]
["COCOPP_2_CTG2",4,198.21]
["COCOPP_2_CTG2",5,197.04]
["COCOPP_2_CTG2",6,193.81]
["COCOPP_2_CTG2",7,192.86]
["COCOPP_2_CTG2",8,192.32]
["COCOPP_2_CTG2",9,193.95]
["COCOPP_2_CTG2",10,198.13]
["COCOPP_2_CTG2",11,199.65]
["COCOPP_2_CTG2",12,202.7]
["COCOPP_2_CTG3",1,201.79]
["COCOPP_2_CTG3",2,201.31]
["COCOPP_2_CTG3",3,200.92]
["COCOPP_2_CTG3",4,197.81]
["COCOPP_2_CTG3",5,196.72]
["COCOPP_2_CTG3",6,193.1]
["COCOPP_2_CTG3",7,192.03]
["COCOPP_2_CTG3",8,191.57]
["COCOPP_2_CTG3",9,193.18]
["COCOPP_2_CTG3",10,197.81]
["COCOPP_2_CTG3",11,199.11]
["COCOPP_2_CTG3",12,202.45]
["COCOPP_2_CTG4",1,203.72]
["COCOPP_2_CTG4",2,203.2]
["COCOPP_2_CTG4",3,202.81]
["COCOPP_2_CTG4",4,199.67]
["COCOPP_2_CTG4",5,198.47]
["COCOPP_2_CTG4",6,194.44]
["COCOPP_2_CTG4",7,193.36]
["COCOPP_2_CTG4",8,192.89]
["COCOPP_2_CTG4",9,194.53]
["COCOPP_2_CTG4",10,199.67]
["COCOPP_2_CTG4",11,200.98]
["COCOPP_2_CTG4",12,204.2]
["COCOSB_6_SOLAR",1,0]
["COCOSB_6_SOLAR",2,0]
["COCOSB_6_SOLAR",3,0]
["COCOSB_6_SOLAR",4,0]
["COCOSB_6_SOLAR",5,0]
["COCOSB_6_SOLAR",6,0]
["COCOSB_6_SOLAR",7,0]
["COCOSB_6_SOLAR",8,0]
["COCOSB_6_SOLAR",9,0]
["COCOSB_6_SOLAR",10,0]
["COCOSB_6_SOLAR",11,0]
["COCOSB_6_SOLAR",12,0]
["COGNAT_1_UNIT",1,45]
["COGNAT_1_UNIT",2,45]
["COGNAT_1_UNIT",3,45]
["COGNAT_1_UNIT",4,44.93]
["COGNAT_1_UNIT",5,45]
["COGNAT_1_UNIT",6,45]
["COGNAT_1_UNIT",7,45]
["COGNAT_1_UNIT",8,45]
["COGNAT_1_UNIT",9,45]
["COGNAT_1_UNIT",10,45]
["COGNAT_1_UNIT",11,45]
["COGNAT_1_UNIT",12,45]
["COLEMN_2_UNIT",1,5.07]
["COLEMN_2_UNIT",2,4.93]
["COLEMN_2_UNIT",3,5.94]
["COLEMN_2_UNIT",4,5.96]
["COLEMN_2_UNIT",5,6.14]
["COLEMN_2_UNIT",6,3.57]
["COLEMN_2_UNIT",7,1.84]
["COLEMN_2_UNIT",8,0.28000000000000003]
["COLEMN_2_UNIT",9,2.2799999999999998]
["COLEMN_2_UNIT",10,2.37]
["COLEMN_2_UNIT",11,2.93]
["COLEMN_2_UNIT",12,3.76]
["COLGAT_7_UNIT 1",1,120]
["COLGAT_7_UNIT 1",2,144.80000000000001]
["COLGAT_7_UNIT 1",3,156.4]
["COLGAT_7_UNIT 1",4,131.19999999999999]
["COLGAT_7_UNIT 1",5,162.4]
["COLGAT_7_UNIT 1",6,161.6]
["COLGAT_7_UNIT 1",7,159.19999999999999]
["COLGAT_7_UNIT 1",8,154.4]
["COLGAT_7_UNIT 1",9,153.4]
["COLGAT_7_UNIT 1",10,169.58]
["COLGAT_7_UNIT 1",11,121.6]
["COLGAT_7_UNIT 1",12,121.6]
["COLGAT_7_UNIT 2",1,120]
["COLGAT_7_UNIT 2",2,120]
["COLGAT_7_UNIT 2",3,124.8]
["COLGAT_7_UNIT 2",4,129.6]
["COLGAT_7_UNIT 2",5,132]
["COLGAT_7_UNIT 2",6,161.19999999999999]
["COLGAT_7_UNIT 2",7,157.19999999999999]
["COLGAT_7_UNIT 2",8,156]
["COLGAT_7_UNIT 2",9,154.19999999999999]
["COLGAT_7_UNIT 2",10,153]
["COLGAT_7_UNIT 2",11,124.8]
["COLGAT_7_UNIT 2",12,149.80000000000001]
["COLPIN_6_COLLNS",1,0]
["COLPIN_6_COLLNS",2,0]
["COLPIN_6_COLLNS",3,0]
["COLPIN_6_COLLNS",4,0]
["COLPIN_6_COLLNS",5,0]
["COLPIN_6_COLLNS",6,0]
["COLPIN_6_COLLNS",7,0]
["COLPIN_6_COLLNS",8,0]
["COLPIN_6_COLLNS",9,0]
["COLPIN_6_COLLNS",10,0]
["COLPIN_6_COLLNS",11,0]
["COLPIN_6_COLLNS",12,0]
["COLTON_6_AGUAM1",1,43]
["COLTON_6_AGUAM1",2,43]
["COLTON_6_AGUAM1",3,43]
["COLTON_6_AGUAM1",4,43]
["COLTON_6_AGUAM1",5,43]
["COLTON_6_AGUAM1",6,43]
["COLTON_6_AGUAM1",7,43]
["COLTON_6_AGUAM1",8,43]
["COLTON_6_AGUAM1",9,43]
["COLTON_6_AGUAM1",10,43]
["COLTON_6_AGUAM1",11,43]
["COLTON_6_AGUAM1",12,43]
["COLUSA_2_PL1X3",1,625.22]
["COLUSA_2_PL1X3",2,627.91]
["COLUSA_2_PL1X3",3,623.91]
["COLUSA_2_PL1X3",4,617.80999999999995]
["COLUSA_2_PL1X3",5,617.86]
["COLUSA_2_PL1X3",6,592.96]
["COLUSA_2_PL1X3",7,597.89]
["COLUSA_2_PL1X3",8,594.5]
["COLUSA_2_PL1X3",9,601.37]
["COLUSA_2_PL1X3",10,617.6]
["COLUSA_2_PL1X3",11,622.01]
["COLUSA_2_PL1X3",12,624.58000000000004]
["COLVIL_7_PL1X2",1,246.86]
["COLVIL_7_PL1X2",2,246.86]
["COLVIL_7_PL1X2",3,246.86]
["COLVIL_7_PL1X2",4,246.86]
["COLVIL_7_PL1X2",5,246.86]
["COLVIL_7_PL1X2",6,246.86]
["COLVIL_7_PL1X2",7,246.86]
["COLVIL_7_PL1X2",8,246.86]
["COLVIL_7_PL1X2",9,246.86]
["COLVIL_7_PL1X2",10,246.86]
["COLVIL_7_PL1X2",11,246.86]
["COLVIL_7_PL1X2",12,246.86]
["CONTRL_1_CASAD1",1,7.2]
["CONTRL_1_CASAD1",2,7.2]
["CONTRL_1_CASAD1",3,6.97]
["CONTRL_1_CASAD1",4,6.69]
["CONTRL_1_CASAD1",5,6.54]
["CONTRL_1_CASAD1",6,5.51]
["CONTRL_1_CASAD1",7,5.32]
["CONTRL_1_CASAD1",8,5.44]
["CONTRL_1_CASAD1",9,5.85]
["CONTRL_1_CASAD1",10,6.41]
["CONTRL_1_CASAD1",11,7.18]
["CONTRL_1_CASAD1",12,6.88]
["CONTRL_1_CASAD2",1,10.11]
["CONTRL_1_CASAD2",2,9.9700000000000006]
["CONTRL_1_CASAD2",3,9.4499999999999993]
["CONTRL_1_CASAD2",4,8.35]
["CONTRL_1_CASAD2",5,8.6300000000000008]
["CONTRL_1_CASAD2",6,8.23]
["CONTRL_1_CASAD2",7,9.41]
["CONTRL_1_CASAD2",8,9.2799999999999994]
["CONTRL_1_CASAD2",9,9.17]
["CONTRL_1_CASAD2",10,9.16]
["CONTRL_1_CASAD2",11,9.99]
["CONTRL_1_CASAD2",12,10.199999999999999]
["CONTRL_1_CASAD3",1,12.61]
["CONTRL_1_CASAD3",2,13.07]
["CONTRL_1_CASAD3",3,12.95]
["CONTRL_1_CASAD3",4,11.17]
["CONTRL_1_CASAD3",5,7.49]
["CONTRL_1_CASAD3",6,6.5]
["CONTRL_1_CASAD3",7,8.66]
["CONTRL_1_CASAD3",8,8.84]
["CONTRL_1_CASAD3",9,9.73]
["CONTRL_1_CASAD3",10,10.67]
["CONTRL_1_CASAD3",11,12.67]
["CONTRL_1_CASAD3",12,12.91]
["CONTRL_1_LUNDY",1,0.41]
["CONTRL_1_LUNDY",2,0.39]
["CONTRL_1_LUNDY",3,0.48]
["CONTRL_1_LUNDY",4,0.67]
["CONTRL_1_LUNDY",5,1.48]
["CONTRL_1_LUNDY",6,1.94]
["CONTRL_1_LUNDY",7,1.52]
["CONTRL_1_LUNDY",8,1.1000000000000001]
["CONTRL_1_LUNDY",9,0.78]
["CONTRL_1_LUNDY",10,0.49]
["CONTRL_1_LUNDY",11,0.47]
["CONTRL_1_LUNDY",12,0.35]
["CONTRL_1_OXBOW",1,59.72]
["CONTRL_1_OXBOW",2,57.58]
["CONTRL_1_OXBOW",3,57.37]
["CONTRL_1_OXBOW",4,56.05]
["CONTRL_1_OXBOW",5,55.56]
["CONTRL_1_OXBOW",6,55.56]
["CONTRL_1_OXBOW",7,54.71]
["CONTRL_1_OXBOW",8,54.35]
["CONTRL_1_OXBOW",9,54.36]
["CONTRL_1_OXBOW",10,52.52]
["CONTRL_1_OXBOW",11,59.52]
["CONTRL_1_OXBOW",12,58.84]
["CONTRL_1_POOLE",1,0.9]
["CONTRL_1_POOLE",2,0.98]
["CONTRL_1_POOLE",3,0.65]
["CONTRL_1_POOLE",4,0.72]
["CONTRL_1_POOLE",5,1.81]
["CONTRL_1_POOLE",6,8.9600000000000009]
["CONTRL_1_POOLE",7,7.38]
["CONTRL_1_POOLE",8,4.88]
["CONTRL_1_POOLE",9,10.9]
["CONTRL_1_POOLE",10,0.31]
["CONTRL_1_POOLE",11,0.38]
["CONTRL_1_POOLE",12,0.8]
["CONTRL_1_QF",1,1.21]
["CONTRL_1_QF",2,1.1499999999999999]
["CONTRL_1_QF",3,1.29]
["CONTRL_1_QF",4,1.57]
["CONTRL_1_QF",5,1.43]
["CONTRL_1_QF",6,1.38]
["CONTRL_1_QF",7,1.42]
["CONTRL_1_QF",8,1.25]
["CONTRL_1_QF",9,1.32]
["CONTRL_1_QF",10,1.06]
["CONTRL_1_QF",11,1.07]
["CONTRL_1_QF",12,1.41]
["CONTRL_1_RUSHCK",1,0]
["CONTRL_1_RUSHCK",2,0.8]
["CONTRL_1_RUSHCK",3,5.62]
["CONTRL_1_RUSHCK",4,5.62]
["CONTRL_1_RUSHCK",5,5.6]
["CONTRL_1_RUSHCK",6,4.74]
["CONTRL_1_RUSHCK",7,0.8]
["CONTRL_1_RUSHCK",8,1.3]
["CONTRL_1_RUSHCK",9,11.87]
["CONTRL_1_RUSHCK",10,1.62]
["CONTRL_1_RUSHCK",11,0.66]
["CONTRL_1_RUSHCK",12,0.82]
["COPMT2_2_SOLAR2",1,0.62]
["COPMT2_2_SOLAR2",2,4.6500000000000004]
["COPMT2_2_SOLAR2",3,5.43]
["COPMT2_2_SOLAR2",4,6.82]
["COPMT2_2_SOLAR2",5,9.92]
["COPMT2_2_SOLAR2",6,20.309999999999999]
["COPMT2_2_SOLAR2",7,22.32]
["COPMT2_2_SOLAR2",8,19.22]
["COPMT2_2_SOLAR2",9,17.21]
["COPMT2_2_SOLAR2",10,11.47]
["COPMT2_2_SOLAR2",11,8.84]
["COPMT2_2_SOLAR2",12,5.43]
["COPMT4_2_SOLAR4",1,0.37]
["COPMT4_2_SOLAR4",2,2.76]
["COPMT4_2_SOLAR4",3,3.22]
["COPMT4_2_SOLAR4",4,4.05]
["COPMT4_2_SOLAR4",5,5.89]
["COPMT4_2_SOLAR4",6,12.05]
["COPMT4_2_SOLAR4",7,13.25]
["COPMT4_2_SOLAR4",8,11.41]
["COPMT4_2_SOLAR4",9,10.210000000000001]
["COPMT4_2_SOLAR4",10,6.81]
["COPMT4_2_SOLAR4",11,5.24]
["COPMT4_2_SOLAR4",12,3.22]
["COPMTN_2_CM10",1,0.04]
["COPMTN_2_CM10",2,0.3]
["COPMTN_2_CM10",3,0.35]
["COPMTN_2_CM10",4,0.44]
["COPMTN_2_CM10",5,0.64]
["COPMTN_2_CM10",6,1.31]
["COPMTN_2_CM10",7,1.44]
["COPMTN_2_CM10",8,1.24]
["COPMTN_2_CM10",9,1.1100000000000001]
["COPMTN_2_CM10",10,0.74]
["COPMTN_2_CM10",11,0.56999999999999995]
["COPMTN_2_CM10",12,0.35]
["COPMTN_2_SOLAR1",1,0.19]
["COPMTN_2_SOLAR1",2,1.44]
["COPMTN_2_SOLAR1",3,1.68]
["COPMTN_2_SOLAR1",4,2.11]
["COPMTN_2_SOLAR1",5,3.07]
["COPMTN_2_SOLAR1",6,6.29]
["COPMTN_2_SOLAR1",7,6.91]
["COPMTN_2_SOLAR1",8,5.95]
["COPMTN_2_SOLAR1",9,5.33]
["COPMTN_2_SOLAR1",10,3.55]
["COPMTN_2_SOLAR1",11,2.74]
["COPMTN_2_SOLAR1",12,1.68]
["CORCAN_1_SOLAR1",1,0.08]
["CORCAN_1_SOLAR1",2,0.6]
["CORCAN_1_SOLAR1",3,0.7]
["CORCAN_1_SOLAR1",4,0.88]
["CORCAN_1_SOLAR1",5,1.28]
["CORCAN_1_SOLAR1",6,2.62]
["CORCAN_1_SOLAR1",7,2.88]
["CORCAN_1_SOLAR1",8,2.48]
["CORCAN_1_SOLAR1",9,2.2200000000000002]
["CORCAN_1_SOLAR1",10,1.48]
["CORCAN_1_SOLAR1",11,1.1399999999999999]
["CORCAN_1_SOLAR1",12,0.7]
["CORCAN_1_SOLAR2",1,0.04]
["CORCAN_1_SOLAR2",2,0.33]
["CORCAN_1_SOLAR2",3,0.39]
["CORCAN_1_SOLAR2",4,0.48]
["CORCAN_1_SOLAR2",5,0.7]
["CORCAN_1_SOLAR2",6,1.44]
["CORCAN_1_SOLAR2",7,1.58]
["CORCAN_1_SOLAR2",8,1.36]
["CORCAN_1_SOLAR2",9,1.22]
["CORCAN_1_SOLAR2",10,0.81]
["CORCAN_1_SOLAR2",11,0.63]
["CORCAN_1_SOLAR2",12,0.39]
["CORONS_2_SOLAR",1,0]
["CORONS_2_SOLAR",2,0]
["CORONS_2_SOLAR",3,0]
["CORONS_2_SOLAR",4,0]
["CORONS_2_SOLAR",5,0]
["CORONS_2_SOLAR",6,0]
["CORONS_2_SOLAR",7,0]
["CORONS_2_SOLAR",8,0]
["CORONS_2_SOLAR",9,0]
["CORONS_2_SOLAR",10,0]
["CORONS_2_SOLAR",11,0]
["CORONS_2_SOLAR",12,0]
["CORONS_6_CLRWTR",1,28]
["CORONS_6_CLRWTR",2,28]
["CORONS_6_CLRWTR",3,28]
["CORONS_6_CLRWTR",4,28]
["CORONS_6_CLRWTR",5,28]
["CORONS_6_CLRWTR",6,28]
["CORONS_6_CLRWTR",7,28]
["CORONS_6_CLRWTR",8,28]
["CORONS_6_CLRWTR",9,28]
["CORONS_6_CLRWTR",10,28]
["CORONS_6_CLRWTR",11,28]
["CORONS_6_CLRWTR",12,28]
["CORRAL_6_SJOAQN",1,4.28]
["CORRAL_6_SJOAQN",2,4.21]
["CORRAL_6_SJOAQN",3,4.1900000000000004]
["CORRAL_6_SJOAQN",4,4.3]
["CORRAL_6_SJOAQN",5,4.21]
["CORRAL_6_SJOAQN",6,4.21]
["CORRAL_6_SJOAQN",7,4.22]
["CORRAL_6_SJOAQN",8,4.28]
["CORRAL_6_SJOAQN",9,4.25]
["CORRAL_6_SJOAQN",10,4.28]
["CORRAL_6_SJOAQN",11,4.22]
["CORRAL_6_SJOAQN",12,4.29]
["COTTLE_2_FRNKNH",1,0]
["COTTLE_2_FRNKNH",2,0]
["COTTLE_2_FRNKNH",3,0.31]
["COTTLE_2_FRNKNH",4,1]
["COTTLE_2_FRNKNH",5,0.71]
["COTTLE_2_FRNKNH",6,0.9]
["COTTLE_2_FRNKNH",7,1.05]
["COTTLE_2_FRNKNH",8,1.02]
["COTTLE_2_FRNKNH",9,0.77]
["COTTLE_2_FRNKNH",10,0]
["COTTLE_2_FRNKNH",11,0]
["COTTLE_2_FRNKNH",12,0]
["COVERD_2_HCKHY1",1,1.97]
["COVERD_2_HCKHY1",2,3.05]
["COVERD_2_HCKHY1",3,3.07]
["COVERD_2_HCKHY1",4,3.5]
["COVERD_2_HCKHY1",5,3.01]
["COVERD_2_HCKHY1",6,1.06]
["COVERD_2_HCKHY1",7,7.0000000000000007E-2]
["COVERD_2_HCKHY1",8,0]
["COVERD_2_HCKHY1",9,0]
["COVERD_2_HCKHY1",10,0.14000000000000001]
["COVERD_2_HCKHY1",11,0.09]
["COVERD_2_HCKHY1",12,0.65]
["COVERD_2_MCKHY1",1,1.3]
["COVERD_2_MCKHY1",2,1.35]
["COVERD_2_MCKHY1",3,1.55]
["COVERD_2_MCKHY1",4,1.41]
["COVERD_2_MCKHY1",5,1.07]
["COVERD_2_MCKHY1",6,0.36]
["COVERD_2_MCKHY1",7,0.08]
["COVERD_2_MCKHY1",8,0.01]
["COVERD_2_MCKHY1",9,0]
["COVERD_2_MCKHY1",10,0.08]
["COVERD_2_MCKHY1",11,0]
["COVERD_2_MCKHY1",12,0.74]
["COVERD_2_QFUNTS",1,0.34]
["COVERD_2_QFUNTS",2,2.33]
["COVERD_2_QFUNTS",3,0.57999999999999996]
["COVERD_2_QFUNTS",4,1.28]
["COVERD_2_QFUNTS",5,1.3]
["COVERD_2_QFUNTS",6,0.76]
["COVERD_2_QFUNTS",7,0]
["COVERD_2_QFUNTS",8,0]
["COVERD_2_QFUNTS",9,0]
["COVERD_2_QFUNTS",10,1.2]
["COVERD_2_QFUNTS",11,0.4]
["COVERD_2_QFUNTS",12,0.8]
["COVERD_2_RCKHY1",1,0.88]
["COVERD_2_RCKHY1",2,1.3]
["COVERD_2_RCKHY1",3,0.84]
["COVERD_2_RCKHY1",4,1]
["COVERD_2_RCKHY1",5,0.67]
["COVERD_2_RCKHY1",6,0.45]
["COVERD_2_RCKHY1",7,0.13]
["COVERD_2_RCKHY1",8,0]
["COVERD_2_RCKHY1",9,0]
["COVERD_2_RCKHY1",10,0.04]
["COVERD_2_RCKHY1",11,0.09]
["COVERD_2_RCKHY1",12,0.46]
["COWCRK_2_UNIT",1,0.85]
["COWCRK_2_UNIT",2,0.84]
["COWCRK_2_UNIT",3,0.78]
["COWCRK_2_UNIT",4,0.85]
["COWCRK_2_UNIT",5,0.48]
["COWCRK_2_UNIT",6,0.37]
["COWCRK_2_UNIT",7,0.13]
["COWCRK_2_UNIT",8,0.03]
["COWCRK_2_UNIT",9,0.01]
["COWCRK_2_UNIT",10,0.18]
["COWCRK_2_UNIT",11,0.53]
["COWCRK_2_UNIT",12,0.69]
["CPVERD_2_SOLAR",1,0.56000000000000005]
["CPVERD_2_SOLAR",2,4.17]
["CPVERD_2_SOLAR",3,4.87]
["CPVERD_2_SOLAR",4,6.12]
["CPVERD_2_SOLAR",5,8.9]
["CPVERD_2_SOLAR",6,18.21]
["CPVERD_2_SOLAR",7,20.02]
["CPVERD_2_SOLAR",8,17.239999999999998]
["CPVERD_2_SOLAR",9,15.43]
["CPVERD_2_SOLAR",10,10.29]
["CPVERD_2_SOLAR",11,7.92]
["CPVERD_2_SOLAR",12,4.87]
["CRELMN_6_RAMON1",1,0.01]
["CRELMN_6_RAMON1",2,0.06]
["CRELMN_6_RAMON1",3,7.0000000000000007E-2]
["CRELMN_6_RAMON1",4,0.09]
["CRELMN_6_RAMON1",5,0.13]
["CRELMN_6_RAMON1",6,0.26]
["CRELMN_6_RAMON1",7,0.28999999999999998]
["CRELMN_6_RAMON1",8,0.25]
["CRELMN_6_RAMON1",9,0.22]
["CRELMN_6_RAMON1",10,0.15]
["CRELMN_6_RAMON1",11,0.11]
["CRELMN_6_RAMON1",12,7.0000000000000007E-2]
["CRELMN_6_RAMON2",1,0.02]
["CRELMN_6_RAMON2",2,0.15]
["CRELMN_6_RAMON2",3,0.18]
["CRELMN_6_RAMON2",4,0.22]
["CRELMN_6_RAMON2",5,0.32]
["CRELMN_6_RAMON2",6,0.66]
["CRELMN_6_RAMON2",7,0.72]
["CRELMN_6_RAMON2",8,0.62]
["CRELMN_6_RAMON2",9,0.56000000000000005]
["CRELMN_6_RAMON2",10,0.37]
["CRELMN_6_RAMON2",11,0.28999999999999998]
["CRELMN_6_RAMON2",12,0.18]
["CRELMN_6_RAMSR3",1,0.02]
["CRELMN_6_RAMSR3",2,0.1]
["CRELMN_6_RAMSR3",3,0.12]
["CRELMN_6_RAMSR3",4,0.15]
["CRELMN_6_RAMSR3",5,0.22]
["CRELMN_6_RAMSR3",6,0.46]
["CRELMN_6_RAMSR3",7,0.5]
["CRELMN_6_RAMSR3",8,0.43]
["CRELMN_6_RAMSR3",9,0.38]
["CRELMN_6_RAMSR3",10,0.26]
["CRELMN_6_RAMSR3",11,0.2]
["CRELMN_6_RAMSR3",12,0.12]
["CRESSY_1_PARKER",1,0]
["CRESSY_1_PARKER",2,0]
["CRESSY_1_PARKER",3,0.01]
["CRESSY_1_PARKER",4,0.47]
["CRESSY_1_PARKER",5,1.1599999999999999]
["CRESSY_1_PARKER",6,1.39]
["CRESSY_1_PARKER",7,1.27]
["CRESSY_1_PARKER",8,0.88]
["CRESSY_1_PARKER",9,0.66]
["CRESSY_1_PARKER",10,0.34]
["CRESSY_1_PARKER",11,0]
["CRESSY_1_PARKER",12,0]
["CRESTA_7_PL1X2",1,42]
["CRESTA_7_PL1X2",2,40.520000000000003]
["CRESTA_7_PL1X2",3,50.29]
["CRESTA_7_PL1X2",4,46.8]
["CRESTA_7_PL1X2",5,35.200000000000003]
["CRESTA_7_PL1X2",6,30]
["CRESTA_7_PL1X2",7,40.619999999999997]
["CRESTA_7_PL1X2",8,47.6]
["CRESTA_7_PL1X2",9,44.61]
["CRESTA_7_PL1X2",10,28]
["CRESTA_7_PL1X2",11,19.2]
["CRESTA_7_PL1X2",12,27.2]
["CRIMSN_2_CRMBT1",1,200]
["CRIMSN_2_CRMBT1",2,200]
["CRIMSN_2_CRMBT1",3,200]
["CRIMSN_2_CRMBT1",4,200]
["CRIMSN_2_CRMBT1",5,200]
["CRIMSN_2_CRMBT1",6,200]
["CRIMSN_2_CRMBT1",7,200]
["CRIMSN_2_CRMBT1",8,200]
["CRIMSN_2_CRMBT1",9,200]
["CRIMSN_2_CRMBT1",10,200]
["CRIMSN_2_CRMBT1",11,200]
["CRIMSN_2_CRMBT1",12,200]
["CRIMSN_2_CRMBT2",1,150]
["CRIMSN_2_CRMBT2",2,150]
["CRIMSN_2_CRMBT2",3,150]
["CRIMSN_2_CRMBT2",4,150]
["CRIMSN_2_CRMBT2",5,150]
["CRIMSN_2_CRMBT2",6,150]
["CRIMSN_2_CRMBT2",7,150]
["CRIMSN_2_CRMBT2",8,150]
["CRIMSN_2_CRMBT2",9,150]
["CRIMSN_2_CRMBT2",10,150]
["CRIMSN_2_CRMBT2",11,150]
["CRIMSN_2_CRMBT2",12,150]
["CRNEVL_6_CRNVA",1,0]
["CRNEVL_6_CRNVA",2,0]
["CRNEVL_6_CRNVA",3,0]
["CRNEVL_6_CRNVA",4,0]
["CRNEVL_6_CRNVA",5,0]
["CRNEVL_6_CRNVA",6,0]
["CRNEVL_6_CRNVA",7,0]
["CRNEVL_6_CRNVA",8,0]
["CRNEVL_6_CRNVA",9,0.11]
["CRNEVL_6_CRNVA",10,0.37]
["CRNEVL_6_CRNVA",11,0.26]
["CRNEVL_6_CRNVA",12,0]
["CRNEVL_6_SJQN 2",1,0]
["CRNEVL_6_SJQN 2",2,0]
["CRNEVL_6_SJQN 2",3,0]
["CRNEVL_6_SJQN 2",4,0]
["CRNEVL_6_SJQN 2",5,0]
["CRNEVL_6_SJQN 2",6,0]
["CRNEVL_6_SJQN 2",7,0]
["CRNEVL_6_SJQN 2",8,0]
["CRNEVL_6_SJQN 2",9,0]
["CRNEVL_6_SJQN 2",10,0]
["CRNEVL_6_SJQN 2",11,0]
["CRNEVL_6_SJQN 2",12,0]
["CROKET_7_UNIT",1,222.23]
["CROKET_7_UNIT",2,223.89]
["CROKET_7_UNIT",3,153.69999999999999]
["CROKET_7_UNIT",4,226.85]
["CROKET_7_UNIT",5,228]
["CROKET_7_UNIT",6,229.14]
["CROKET_7_UNIT",7,227.06]
["CROKET_7_UNIT",8,222.84]
["CROKET_7_UNIT",9,215.79]
["CROKET_7_UNIT",10,215.91]
["CROKET_7_UNIT",11,217.86]
["CROKET_7_UNIT",12,220.49]
["CRSTWD_6_KUMYAY",1,8.84]
["CRSTWD_6_KUMYAY",2,9.4]
["CRSTWD_6_KUMYAY",3,8.26]
["CRSTWD_6_KUMYAY",4,7.91]
["CRSTWD_6_KUMYAY",5,8.41]
["CRSTWD_6_KUMYAY",6,7.71]
["CRSTWD_6_KUMYAY",7,7.16]
["CRSTWD_6_KUMYAY",8,5.44]
["CRSTWD_6_KUMYAY",9,5.62]
["CRSTWD_6_KUMYAY",10,5.22]
["CRSTWD_6_KUMYAY",11,7.03]
["CRSTWD_6_KUMYAY",12,8.52]
["CRWCKS_1_SOLAR1",1,0]
["CRWCKS_1_SOLAR1",2,0]
["CRWCKS_1_SOLAR1",3,0]
["CRWCKS_1_SOLAR1",4,0]
["CRWCKS_1_SOLAR1",5,0]
["CRWCKS_1_SOLAR1",6,0]
["CRWCKS_1_SOLAR1",7,0]
["CRWCKS_1_SOLAR1",8,0]
["CRWCKS_1_SOLAR1",9,0]
["CRWCKS_1_SOLAR1",10,0]
["CRWCKS_1_SOLAR1",11,0]
["CRWCKS_1_SOLAR1",12,0]
["CSCCOG_1_UNIT 1",1,6]
["CSCCOG_1_UNIT 1",2,6]
["CSCCOG_1_UNIT 1",3,6]
["CSCCOG_1_UNIT 1",4,6]
["CSCCOG_1_UNIT 1",5,6]
["CSCCOG_1_UNIT 1",6,6]
["CSCCOG_1_UNIT 1",7,6]
["CSCCOG_1_UNIT 1",8,6]
["CSCCOG_1_UNIT 1",9,6]
["CSCCOG_1_UNIT 1",10,6]
["CSCCOG_1_UNIT 1",11,6]
["CSCCOG_1_UNIT 1",12,6]
["CSCGNR_1_UNIT 1",1,24]
["CSCGNR_1_UNIT 1",2,24]
["CSCGNR_1_UNIT 1",3,24]
["CSCGNR_1_UNIT 1",4,24]
["CSCGNR_1_UNIT 1",5,24]
["CSCGNR_1_UNIT 1",6,24]
["CSCGNR_1_UNIT 1",7,24]
["CSCGNR_1_UNIT 1",8,24]
["CSCGNR_1_UNIT 1",9,24]
["CSCGNR_1_UNIT 1",10,24]
["CSCGNR_1_UNIT 1",11,24]
["CSCGNR_1_UNIT 1",12,24]
["CSCGNR_1_UNIT 2",1,24]
["CSCGNR_1_UNIT 2",2,24]
["CSCGNR_1_UNIT 2",3,24]
["CSCGNR_1_UNIT 2",4,24]
["CSCGNR_1_UNIT 2",5,24]
["CSCGNR_1_UNIT 2",6,24]
["CSCGNR_1_UNIT 2",7,24]
["CSCGNR_1_UNIT 2",8,24]
["CSCGNR_1_UNIT 2",9,24]
["CSCGNR_1_UNIT 2",10,24]
["CSCGNR_1_UNIT 2",11,24]
["CSCGNR_1_UNIT 2",12,24]
["CSLR4S_2_SOLAR",1,0.52]
["CSLR4S_2_SOLAR",2,3.9]
["CSLR4S_2_SOLAR",3,4.55]
["CSLR4S_2_SOLAR",4,5.72]
["CSLR4S_2_SOLAR",5,8.32]
["CSLR4S_2_SOLAR",6,17.03]
["CSLR4S_2_SOLAR",7,18.72]
["CSLR4S_2_SOLAR",8,16.12]
["CSLR4S_2_SOLAR",9,14.43]
["CSLR4S_2_SOLAR",10,9.6199999999999992]
["CSLR4S_2_SOLAR",11,7.41]
["CSLR4S_2_SOLAR",12,4.55]
["CSTOGA_6_LNDFIL",1,0]
["CSTOGA_6_LNDFIL",2,0]
["CSTOGA_6_LNDFIL",3,0]
["CSTOGA_6_LNDFIL",4,0]
["CSTOGA_6_LNDFIL",5,0]
["CSTOGA_6_LNDFIL",6,0]
["CSTOGA_6_LNDFIL",7,0]
["CSTOGA_6_LNDFIL",8,0]
["CSTOGA_6_LNDFIL",9,0]
["CSTOGA_6_LNDFIL",10,0]
["CSTOGA_6_LNDFIL",11,0]
["CSTOGA_6_LNDFIL",12,0]
["CSTRVL_7_PL1X2",1,4.13]
["CSTRVL_7_PL1X2",2,3.51]
["CSTRVL_7_PL1X2",3,3.69]
["CSTRVL_7_PL1X2",4,4.01]
["CSTRVL_7_PL1X2",5,3.63]
["CSTRVL_7_PL1X2",6,3.95]
["CSTRVL_7_PL1X2",7,4.16]
["CSTRVL_7_PL1X2",8,4.1399999999999997]
["CSTRVL_7_PL1X2",9,4.17]
["CSTRVL_7_PL1X2",10,3.86]
["CSTRVL_7_PL1X2",11,3.98]
["CSTRVL_7_PL1X2",12,3.73]
["CSTRVL_7_QFUNTS",1,0.05]
["CSTRVL_7_QFUNTS",2,7.0000000000000007E-2]
["CSTRVL_7_QFUNTS",3,0.13]
["CSTRVL_7_QFUNTS",4,0.1]
["CSTRVL_7_QFUNTS",5,7.0000000000000007E-2]
["CSTRVL_7_QFUNTS",6,0.08]
["CSTRVL_7_QFUNTS",7,7.0000000000000007E-2]
["CSTRVL_7_QFUNTS",8,0.06]
["CSTRVL_7_QFUNTS",9,0.05]
["CSTRVL_7_QFUNTS",10,0.05]
["CSTRVL_7_QFUNTS",11,0.05]
["CSTRVL_7_QFUNTS",12,0.05]
["CTNWDP_1_QF",1,0.04]
["CTNWDP_1_QF",2,0.04]
["CTNWDP_1_QF",3,0.04]
["CTNWDP_1_QF",4,0.04]
["CTNWDP_1_QF",5,0.03]
["CTNWDP_1_QF",6,0.03]
["CTNWDP_1_QF",7,0.02]
["CTNWDP_1_QF",8,0.02]
["CTNWDP_1_QF",9,0.02]
["CTNWDP_1_QF",10,0.03]
["CTNWDP_1_QF",11,0.03]
["CTNWDP_1_QF",12,0.04]
["CUMBIA_1_SOLAR",1,0.08]
["CUMBIA_1_SOLAR",2,0.56999999999999995]
["CUMBIA_1_SOLAR",3,0.67]
["CUMBIA_1_SOLAR",4,0.84]
["CUMBIA_1_SOLAR",5,1.22]
["CUMBIA_1_SOLAR",6,2.4900000000000002]
["CUMBIA_1_SOLAR",7,2.74]
["CUMBIA_1_SOLAR",8,2.36]
["CUMBIA_1_SOLAR",9,2.11]
["CUMBIA_1_SOLAR",10,1.41]
["CUMBIA_1_SOLAR",11,1.08]
["CUMBIA_1_SOLAR",12,0.67]
["CUMMNG_6_SUNCT1",1,3.33]
["CUMMNG_6_SUNCT1",2,3.39]
["CUMMNG_6_SUNCT1",3,3.04]
["CUMMNG_6_SUNCT1",4,3.01]
["CUMMNG_6_SUNCT1",5,3.34]
["CUMMNG_6_SUNCT1",6,3.54]
["CUMMNG_6_SUNCT1",7,3.53]
["CUMMNG_6_SUNCT1",8,3.56]
["CUMMNG_6_SUNCT1",9,3.4]
["CUMMNG_6_SUNCT1",10,3.16]
["CUMMNG_6_SUNCT1",11,3.38]
["CUMMNG_6_SUNCT1",12,3.45]
["CURTIS_1_CANLCK",1,0]
["CURTIS_1_CANLCK",2,0]
["CURTIS_1_CANLCK",3,0]
["CURTIS_1_CANLCK",4,0]
["CURTIS_1_CANLCK",5,0]
["CURTIS_1_CANLCK",6,0]
["CURTIS_1_CANLCK",7,0]
["CURTIS_1_CANLCK",8,0]
["CURTIS_1_CANLCK",9,0]
["CURTIS_1_CANLCK",10,0]
["CURTIS_1_CANLCK",11,0]
["CURTIS_1_CANLCK",12,0]
["CURTIS_1_FARFLD",1,0]
["CURTIS_1_FARFLD",2,0]
["CURTIS_1_FARFLD",3,0]
["CURTIS_1_FARFLD",4,0.01]
["CURTIS_1_FARFLD",5,0.26]
["CURTIS_1_FARFLD",6,0.55000000000000004]
["CURTIS_1_FARFLD",7,0.51]
["CURTIS_1_FARFLD",8,0.49]
["CURTIS_1_FARFLD",9,0.15]
["CURTIS_1_FARFLD",10,0]
["CURTIS_1_FARFLD",11,0]
["CURTIS_1_FARFLD",12,0]
["CUYAMS_6_CUYSR1",1,0.16]
["CUYAMS_6_CUYSR1",2,1.2]
["CUYAMS_6_CUYSR1",3,1.4]
["CUYAMS_6_CUYSR1",4,1.76]
["CUYAMS_6_CUYSR1",5,2.56]
["CUYAMS_6_CUYSR1",6,5.24]
["CUYAMS_6_CUYSR1",7,5.76]
["CUYAMS_6_CUYSR1",8,4.96]
["CUYAMS_6_CUYSR1",9,4.4400000000000004]
["CUYAMS_6_CUYSR1",10,2.96]
["CUYAMS_6_CUYSR1",11,2.2799999999999998]
["CUYAMS_6_CUYSR1",12,1.4]
["DAIRLD_1_MD1SL1",1,0]
["DAIRLD_1_MD1SL1",2,0]
["DAIRLD_1_MD1SL1",3,0]
["DAIRLD_1_MD1SL1",4,0]
["DAIRLD_1_MD1SL1",5,0]
["DAIRLD_1_MD1SL1",6,0]
["DAIRLD_1_MD1SL1",7,0]
["DAIRLD_1_MD1SL1",8,0]
["DAIRLD_1_MD1SL1",9,0]
["DAIRLD_1_MD1SL1",10,0]
["DAIRLD_1_MD1SL1",11,0]
["DAIRLD_1_MD1SL1",12,0]
["DAIRLD_1_MD2BM1",1,0]
["DAIRLD_1_MD2BM1",2,0]
["DAIRLD_1_MD2BM1",3,0]
["DAIRLD_1_MD2BM1",4,0]
["DAIRLD_1_MD2BM1",5,0]
["DAIRLD_1_MD2BM1",6,0]
["DAIRLD_1_MD2BM1",7,0]
["DAIRLD_1_MD2BM1",8,0]
["DAIRLD_1_MD2BM1",9,0]
["DAIRLD_1_MD2BM1",10,0]
["DAIRLD_1_MD2BM1",11,0]
["DAIRLD_1_MD2BM1",12,0]
["DAVIS_1_SOLAR1",1,0]
["DAVIS_1_SOLAR1",2,0]
["DAVIS_1_SOLAR1",3,0]
["DAVIS_1_SOLAR1",4,0]
["DAVIS_1_SOLAR1",5,0]
["DAVIS_1_SOLAR1",6,0]
["DAVIS_1_SOLAR1",7,0]
["DAVIS_1_SOLAR1",8,0]
["DAVIS_1_SOLAR1",9,0]
["DAVIS_1_SOLAR1",10,0]
["DAVIS_1_SOLAR1",11,0]
["DAVIS_1_SOLAR1",12,0]
["DAVIS_1_SOLAR2",1,0]
["DAVIS_1_SOLAR2",2,0]
["DAVIS_1_SOLAR2",3,0]
["DAVIS_1_SOLAR2",4,0]
["DAVIS_1_SOLAR2",5,0]
["DAVIS_1_SOLAR2",6,0]
["DAVIS_1_SOLAR2",7,0]
["DAVIS_1_SOLAR2",8,0]
["DAVIS_1_SOLAR2",9,0]
["DAVIS_1_SOLAR2",10,0]
["DAVIS_1_SOLAR2",11,0]
["DAVIS_1_SOLAR2",12,0]
["DAVIS_7_MNMETH",1,2.5]
["DAVIS_7_MNMETH",2,2.4900000000000002]
["DAVIS_7_MNMETH",3,2.5]
["DAVIS_7_MNMETH",4,2.5]
["DAVIS_7_MNMETH",5,1.96]
["DAVIS_7_MNMETH",6,2.06]
["DAVIS_7_MNMETH",7,2.0699999999999998]
["DAVIS_7_MNMETH",8,2.33]
["DAVIS_7_MNMETH",9,2.4]
["DAVIS_7_MNMETH",10,2.2599999999999998]
["DAVIS_7_MNMETH",11,2.1800000000000002]
["DAVIS_7_MNMETH",12,2.1800000000000002]
["DEADCK_1_UNIT",1,0.28000000000000003]
["DEADCK_1_UNIT",2,0.46]
["DEADCK_1_UNIT",3,0.69]
["DEADCK_1_UNIT",4,0.64]
["DEADCK_1_UNIT",5,0.13]
["DEADCK_1_UNIT",6,0.27]
["DEADCK_1_UNIT",7,0.1]
["DEADCK_1_UNIT",8,0.02]
["DEADCK_1_UNIT",9,0]
["DEADCK_1_UNIT",10,0]
["DEADCK_1_UNIT",11,0]
["DEADCK_1_UNIT",12,0.06]
["DEERCR_6_UNIT 1",1,1.38]
["DEERCR_6_UNIT 1",2,1.07]
["DEERCR_6_UNIT 1",3,0.89]
["DEERCR_6_UNIT 1",4,0.46]
["DEERCR_6_UNIT 1",5,2.72]
["DEERCR_6_UNIT 1",6,3.12]
["DEERCR_6_UNIT 1",7,3.26]
["DEERCR_6_UNIT 1",8,3.14]
["DEERCR_6_UNIT 1",9,2.87]
["DEERCR_6_UNIT 1",10,2.14]
["DEERCR_6_UNIT 1",11,1.57]
["DEERCR_6_UNIT 1",12,1.38]
["DELAMO_2_SOLAR1",1,0.01]
["DELAMO_2_SOLAR1",2,0.05]
["DELAMO_2_SOLAR1",3,0.05]
["DELAMO_2_SOLAR1",4,7.0000000000000007E-2]
["DELAMO_2_SOLAR1",5,0.1]
["DELAMO_2_SOLAR1",6,0.2]
["DELAMO_2_SOLAR1",7,0.22]
["DELAMO_2_SOLAR1",8,0.19]
["DELAMO_2_SOLAR1",9,0.17]
["DELAMO_2_SOLAR1",10,0.11]
["DELAMO_2_SOLAR1",11,0.09]
["DELAMO_2_SOLAR1",12,0.05]
["DELAMO_2_SOLAR2",1,0.01]
["DELAMO_2_SOLAR2",2,0.05]
["DELAMO_2_SOLAR2",3,0.06]
["DELAMO_2_SOLAR2",4,0.08]
["DELAMO_2_SOLAR2",5,0.11]
["DELAMO_2_SOLAR2",6,0.23]
["DELAMO_2_SOLAR2",7,0.25]
["DELAMO_2_SOLAR2",8,0.22]
["DELAMO_2_SOLAR2",9,0.19]
["DELAMO_2_SOLAR2",10,0.13]
["DELAMO_2_SOLAR2",11,0.1]
["DELAMO_2_SOLAR2",12,0.06]
["DELAMO_2_SOLAR3",1,0.01]
["DELAMO_2_SOLAR3",2,0.04]
["DELAMO_2_SOLAR3",3,0.04]
["DELAMO_2_SOLAR3",4,0.06]
["DELAMO_2_SOLAR3",5,0.08]
["DELAMO_2_SOLAR3",6,0.16]
["DELAMO_2_SOLAR3",7,0.18]
["DELAMO_2_SOLAR3",8,0.16]
["DELAMO_2_SOLAR3",9,0.14000000000000001]
["DELAMO_2_SOLAR3",10,0.09]
["DELAMO_2_SOLAR3",11,7.0000000000000007E-2]
["DELAMO_2_SOLAR3",12,0.04]
["DELAMO_2_SOLAR4",1,0.01]
["DELAMO_2_SOLAR4",2,0.04]
["DELAMO_2_SOLAR4",3,0.05]
["DELAMO_2_SOLAR4",4,0.06]
["DELAMO_2_SOLAR4",5,0.08]
["DELAMO_2_SOLAR4",6,0.17]
["DELAMO_2_SOLAR4",7,0.19]
["DELAMO_2_SOLAR4",8,0.16]
["DELAMO_2_SOLAR4",9,0.14000000000000001]
["DELAMO_2_SOLAR4",10,0.1]
["DELAMO_2_SOLAR4",11,7.0000000000000007E-2]
["DELAMO_2_SOLAR4",12,0.05]
["DELAMO_2_SOLAR5",1,0]
["DELAMO_2_SOLAR5",2,0.03]
["DELAMO_2_SOLAR5",3,0.04]
["DELAMO_2_SOLAR5",4,0.04]
["DELAMO_2_SOLAR5",5,0.06]
["DELAMO_2_SOLAR5",6,0.13]
["DELAMO_2_SOLAR5",7,0.14000000000000001]
["DELAMO_2_SOLAR5",8,0.12]
["DELAMO_2_SOLAR5",9,0.11]
["DELAMO_2_SOLAR5",10,7.0000000000000007E-2]
["DELAMO_2_SOLAR5",11,0.06]
["DELAMO_2_SOLAR5",12,0.04]
["DELAMO_2_SOLAR6",1,0.01]
["DELAMO_2_SOLAR6",2,0.06]
["DELAMO_2_SOLAR6",3,7.0000000000000007E-2]
["DELAMO_2_SOLAR6",4,0.09]
["DELAMO_2_SOLAR6",5,0.13]
["DELAMO_2_SOLAR6",6,0.26]
["DELAMO_2_SOLAR6",7,0.28999999999999998]
["DELAMO_2_SOLAR6",8,0.25]
["DELAMO_2_SOLAR6",9,0.22]
["DELAMO_2_SOLAR6",10,0.15]
["DELAMO_2_SOLAR6",11,0.11]
["DELAMO_2_SOLAR6",12,7.0000000000000007E-2]
["DELAMO_2_SOLRC1",1,0]
["DELAMO_2_SOLRC1",2,0]
["DELAMO_2_SOLRC1",3,0]
["DELAMO_2_SOLRC1",4,0]
["DELAMO_2_SOLRC1",5,0]
["DELAMO_2_SOLRC1",6,0]
["DELAMO_2_SOLRC1",7,0]
["DELAMO_2_SOLRC1",8,0]
["DELAMO_2_SOLRC1",9,0]
["DELAMO_2_SOLRC1",10,0]
["DELAMO_2_SOLRC1",11,0]
["DELAMO_2_SOLRC1",12,0]
["DELAMO_2_SOLRD",1,0]
["DELAMO_2_SOLRD",2,0]
["DELAMO_2_SOLRD",3,0]
["DELAMO_2_SOLRD",4,0]
["DELAMO_2_SOLRD",5,0]
["DELAMO_2_SOLRD",6,0]
["DELAMO_2_SOLRD",7,0]
["DELAMO_2_SOLRD",8,0]
["DELAMO_2_SOLRD",9,0]
["DELAMO_2_SOLRD",10,0]
["DELAMO_2_SOLRD",11,0]
["DELAMO_2_SOLRD",12,0]
["DELSUR_6_BSOLAR",1,0.01]
["DELSUR_6_BSOLAR",2,0.09]
["DELSUR_6_BSOLAR",3,0.11]
["DELSUR_6_BSOLAR",4,0.13]
["DELSUR_6_BSOLAR",5,0.19]
["DELSUR_6_BSOLAR",6,0.39]
["DELSUR_6_BSOLAR",7,0.43]
["DELSUR_6_BSOLAR",8,0.37]
["DELSUR_6_BSOLAR",9,0.33]
["DELSUR_6_BSOLAR",10,0.22]
["DELSUR_6_BSOLAR",11,0.17]
["DELSUR_6_BSOLAR",12,0.11]
["DELSUR_6_CREST",1,0]
["DELSUR_6_CREST",2,0]
["DELSUR_6_CREST",3,0]
["DELSUR_6_CREST",4,0]
["DELSUR_6_CREST",5,0]
["DELSUR_6_CREST",6,0]
["DELSUR_6_CREST",7,0]
["DELSUR_6_CREST",8,0]
["DELSUR_6_CREST",9,0]
["DELSUR_6_CREST",10,0]
["DELSUR_6_CREST",11,0]
["DELSUR_6_CREST",12,0]
["DELSUR_6_DRYFRB",1,0.02]
["DELSUR_6_DRYFRB",2,0.15]
["DELSUR_6_DRYFRB",3,0.18]
["DELSUR_6_DRYFRB",4,0.22]
["DELSUR_6_DRYFRB",5,0.32]
["DELSUR_6_DRYFRB",6,0.66]
["DELSUR_6_DRYFRB",7,0.72]
["DELSUR_6_DRYFRB",8,0.62]
["DELSUR_6_DRYFRB",9,0.56000000000000005]
["DELSUR_6_DRYFRB",10,0.37]
["DELSUR_6_DRYFRB",11,0.28999999999999998]
["DELSUR_6_DRYFRB",12,0.18]
["DELSUR_6_SOLAR1",1,0.03]
["DELSUR_6_SOLAR1",2,0.2]
["DELSUR_6_SOLAR1",3,0.23]
["DELSUR_6_SOLAR1",4,0.28999999999999998]
["DELSUR_6_SOLAR1",5,0.42]
["DELSUR_6_SOLAR1",6,0.85]
["DELSUR_6_SOLAR1",7,0.94]
["DELSUR_6_SOLAR1",8,0.81]
["DELSUR_6_SOLAR1",9,0.72]
["DELSUR_6_SOLAR1",10,0.48]
["DELSUR_6_SOLAR1",11,0.37]
["DELSUR_6_SOLAR1",12,0.23]
["DELSUR_6_SOLAR4",1,0]
["DELSUR_6_SOLAR4",2,0]
["DELSUR_6_SOLAR4",3,0]
["DELSUR_6_SOLAR4",4,0]
["DELSUR_6_SOLAR4",5,0]
["DELSUR_6_SOLAR4",6,0]
["DELSUR_6_SOLAR4",7,0]
["DELSUR_6_SOLAR4",8,0]
["DELSUR_6_SOLAR4",9,0]
["DELSUR_6_SOLAR4",10,0]
["DELSUR_6_SOLAR4",11,0]
["DELSUR_6_SOLAR4",12,0]
["DELSUR_6_SOLAR5",1,0]
["DELSUR_6_SOLAR5",2,0]
["DELSUR_6_SOLAR5",3,0]
["DELSUR_6_SOLAR5",4,0]
["DELSUR_6_SOLAR5",5,0]
["DELSUR_6_SOLAR5",6,0]
["DELSUR_6_SOLAR5",7,0]
["DELSUR_6_SOLAR5",8,0]
["DELSUR_6_SOLAR5",9,0]
["DELSUR_6_SOLAR5",10,0]
["DELSUR_6_SOLAR5",11,0]
["DELSUR_6_SOLAR5",12,0]
["DELTA_2_PL1X4",1,880]
["DELTA_2_PL1X4",2,880]
["DELTA_2_PL1X4",3,880]
["DELTA_2_PL1X4",4,875]
["DELTA_2_PL1X4",5,865]
["DELTA_2_PL1X4",6,855]
["DELTA_2_PL1X4",7,848]
["DELTA_2_PL1X4",8,848]
["DELTA_2_PL1X4",9,848]
["DELTA_2_PL1X4",10,865]
["DELTA_2_PL1X4",11,880]
["DELTA_2_PL1X4",12,880]
["DEVERS_1_SEPV05",1,0]
["DEVERS_1_SEPV05",2,0]
["DEVERS_1_SEPV05",3,0]
["DEVERS_1_SEPV05",4,0]
["DEVERS_1_SEPV05",5,0]
["DEVERS_1_SEPV05",6,0]
["DEVERS_1_SEPV05",7,0]
["DEVERS_1_SEPV05",8,0]
["DEVERS_1_SEPV05",9,0]
["DEVERS_1_SEPV05",10,0]
["DEVERS_1_SEPV05",11,0]
["DEVERS_1_SEPV05",12,0]
["DEVERS_1_SOLAR",1,0]
["DEVERS_1_SOLAR",2,0]
["DEVERS_1_SOLAR",3,0]
["DEVERS_1_SOLAR",4,0]
["DEVERS_1_SOLAR",5,0]
["DEVERS_1_SOLAR",6,0]
["DEVERS_1_SOLAR",7,0]
["DEVERS_1_SOLAR",8,0]
["DEVERS_1_SOLAR",9,0]
["DEVERS_1_SOLAR",10,0]
["DEVERS_1_SOLAR",11,0]
["DEVERS_1_SOLAR",12,0]
["DEVERS_1_SOLAR1",1,0]
["DEVERS_1_SOLAR1",2,0]
["DEVERS_1_SOLAR1",3,0]
["DEVERS_1_SOLAR1",4,0]
["DEVERS_1_SOLAR1",5,0]
["DEVERS_1_SOLAR1",6,0]
["DEVERS_1_SOLAR1",7,0]
["DEVERS_1_SOLAR1",8,0]
["DEVERS_1_SOLAR1",9,0]
["DEVERS_1_SOLAR1",10,0]
["DEVERS_1_SOLAR1",11,0]
["DEVERS_1_SOLAR1",12,0]
["DEVERS_1_SOLAR2",1,0]
["DEVERS_1_SOLAR2",2,0]
["DEVERS_1_SOLAR2",3,0]
["DEVERS_1_SOLAR2",4,0]
["DEVERS_1_SOLAR2",5,0]
["DEVERS_1_SOLAR2",6,0]
["DEVERS_1_SOLAR2",7,0]
["DEVERS_1_SOLAR2",8,0]
["DEVERS_1_SOLAR2",9,0]
["DEVERS_1_SOLAR2",10,0]
["DEVERS_1_SOLAR2",11,0]
["DEVERS_1_SOLAR2",12,0]
["DEVERS_2_CS2SR4",1,0]
["DEVERS_2_CS2SR4",2,0]
["DEVERS_2_CS2SR4",3,0]
["DEVERS_2_CS2SR4",4,0]
["DEVERS_2_CS2SR4",5,0]
["DEVERS_2_CS2SR4",6,0]
["DEVERS_2_CS2SR4",7,0]
["DEVERS_2_CS2SR4",8,0]
["DEVERS_2_CS2SR4",9,0]
["DEVERS_2_CS2SR4",10,0]
["DEVERS_2_CS2SR4",11,0]
["DEVERS_2_CS2SR4",12,0]
["DEVERS_2_DHSPG2",1,0]
["DEVERS_2_DHSPG2",2,0]
["DEVERS_2_DHSPG2",3,0]
["DEVERS_2_DHSPG2",4,0]
["DEVERS_2_DHSPG2",5,0]
["DEVERS_2_DHSPG2",6,0]
["DEVERS_2_DHSPG2",7,0]
["DEVERS_2_DHSPG2",8,0]
["DEVERS_2_DHSPG2",9,0]
["DEVERS_2_DHSPG2",10,0]
["DEVERS_2_DHSPG2",11,0]
["DEVERS_2_DHSPG2",12,0]
["DEXZEL_1_UNIT",1,17.45]
["DEXZEL_1_UNIT",2,17.45]
["DEXZEL_1_UNIT",3,17.45]
["DEXZEL_1_UNIT",4,17.03]
["DEXZEL_1_UNIT",5,17.45]
["DEXZEL_1_UNIT",6,17.45]
["DEXZEL_1_UNIT",7,16.28]
["DEXZEL_1_UNIT",8,16.100000000000001]
["DEXZEL_1_UNIT",9,16.93]
["DEXZEL_1_UNIT",10,16.059999999999999]
["DEXZEL_1_UNIT",11,15.35]
["DEXZEL_1_UNIT",12,15.33]
["DIABLO_7_UNIT 1",1,1140]
["DIABLO_7_UNIT 1",2,1140]
["DIABLO_7_UNIT 1",3,1140]
["DIABLO_7_UNIT 1",4,1140]
["DIABLO_7_UNIT 1",5,1140]
["DIABLO_7_UNIT 1",6,1140]
["DIABLO_7_UNIT 1",7,1140]
["DIABLO_7_UNIT 1",8,1140]
["DIABLO_7_UNIT 1",9,1140]
["DIABLO_7_UNIT 1",10,1140]
["DIABLO_7_UNIT 1",11,1140]
["DIABLO_7_UNIT 1",12,1140]
["DIABLO_7_UNIT 2",1,1140]
["DIABLO_7_UNIT 2",2,1140]
["DIABLO_7_UNIT 2",3,1140]
["DIABLO_7_UNIT 2",4,1140]
["DIABLO_7_UNIT 2",5,1140]
["DIABLO_7_UNIT 2",6,1140]
["DIABLO_7_UNIT 2",7,1140]
["DIABLO_7_UNIT 2",8,1140]
["DIABLO_7_UNIT 2",9,1140]
["DIABLO_7_UNIT 2",10,1140]
["DIABLO_7_UNIT 2",11,1140]
["DIABLO_7_UNIT 2",12,1140]
["DISCOV_1_CHEVRN",1,4.38]
["DISCOV_1_CHEVRN",2,7.18]
["DISCOV_1_CHEVRN",3,4.99]
["DISCOV_1_CHEVRN",4,5]
["DISCOV_1_CHEVRN",5,5.87]
["DISCOV_1_CHEVRN",6,6.41]
["DISCOV_1_CHEVRN",7,6.76]
["DISCOV_1_CHEVRN",8,7.23]
["DISCOV_1_CHEVRN",9,6.26]
["DISCOV_1_CHEVRN",10,5.4]
["DISCOV_1_CHEVRN",11,5]
["DISCOV_1_CHEVRN",12,4.26]
["DIXNLD_1_LNDFL",1,0.8]
["DIXNLD_1_LNDFL",2,0.8]
["DIXNLD_1_LNDFL",3,0.87]
["DIXNLD_1_LNDFL",4,0.93]
["DIXNLD_1_LNDFL",5,0.88]
["DIXNLD_1_LNDFL",6,0.92]
["DIXNLD_1_LNDFL",7,0.87]
["DIXNLD_1_LNDFL",8,0.87]
["DIXNLD_1_LNDFL",9,0.82]
["DIXNLD_1_LNDFL",10,0.84]
["DIXNLD_1_LNDFL",11,0.8]
["DIXNLD_1_LNDFL",12,0.77]
["DMDVLY_1_UNITS",1,1.6]
["DMDVLY_1_UNITS",2,3.95]
["DMDVLY_1_UNITS",3,0.72]
["DMDVLY_1_UNITS",4,0.88]
["DMDVLY_1_UNITS",5,3.05]
["DMDVLY_1_UNITS",6,2.63]
["DMDVLY_1_UNITS",7,0.31]
["DMDVLY_1_UNITS",8,3.09]
["DMDVLY_1_UNITS",9,1.04]
["DMDVLY_1_UNITS",10,0.74]
["DMDVLY_1_UNITS",11,1.62]
["DMDVLY_1_UNITS",12,0]
["DONNLS_7_UNIT",1,65.95]
["DONNLS_7_UNIT",2,66.319999999999993]
["DONNLS_7_UNIT",3,67.86]
["DONNLS_7_UNIT",4,65.209999999999994]
["DONNLS_7_UNIT",5,70.099999999999994]
["DONNLS_7_UNIT",6,72]
["DONNLS_7_UNIT",7,72]
["DONNLS_7_UNIT",8,72]
["DONNLS_7_UNIT",9,72]
["DONNLS_7_UNIT",10,70.02]
["DONNLS_7_UNIT",11,67.92]
["DONNLS_7_UNIT",12,66.81]
["DOSMGO_2_NSPIN",1,16]
["DOSMGO_2_NSPIN",2,15.97]
["DOSMGO_2_NSPIN",3,16]
["DOSMGO_2_NSPIN",4,15.46]
["DOSMGO_2_NSPIN",5,16]
["DOSMGO_2_NSPIN",6,15.99]
["DOSMGO_2_NSPIN",7,16]
["DOSMGO_2_NSPIN",8,16]
["DOSMGO_2_NSPIN",9,15.99]
["DOSMGO_2_NSPIN",10,13.64]
["DOSMGO_2_NSPIN",11,15.99]
["DOSMGO_2_NSPIN",12,16]
["DOUBLC_1_UNITS",1,52.23]
["DOUBLC_1_UNITS",2,52.23]
["DOUBLC_1_UNITS",3,52.23]
["DOUBLC_1_UNITS",4,52.23]
["DOUBLC_1_UNITS",5,52.23]
["DOUBLC_1_UNITS",6,52.23]
["DOUBLC_1_UNITS",7,52.23]
["DOUBLC_1_UNITS",8,52.23]
["DOUBLC_1_UNITS",9,52.23]
["DOUBLC_1_UNITS",10,52.23]
["DOUBLC_1_UNITS",11,52.23]
["DOUBLC_1_UNITS",12,52.23]
["DRACKR_2_D4SR4B",1,0.25]
["DRACKR_2_D4SR4B",2,1.88]
["DRACKR_2_D4SR4B",3,2.19]
["DRACKR_2_D4SR4B",4,2.75]
["DRACKR_2_D4SR4B",5,4]
["DRACKR_2_D4SR4B",6,8.19]
["DRACKR_2_D4SR4B",7,9]
["DRACKR_2_D4SR4B",8,7.75]
["DRACKR_2_D4SR4B",9,6.94]
["DRACKR_2_D4SR4B",10,4.63]
["DRACKR_2_D4SR4B",11,3.56]
["DRACKR_2_D4SR4B",12,2.19]
["DRACKR_2_DS3SR3",1,0]
["DRACKR_2_DS3SR3",2,0]
["DRACKR_2_DS3SR3",3,0]
["DRACKR_2_DS3SR3",4,0]
["DRACKR_2_DS3SR3",5,0]
["DRACKR_2_DS3SR3",6,0]
["DRACKR_2_DS3SR3",7,0]
["DRACKR_2_DS3SR3",8,0]
["DRACKR_2_DS3SR3",9,0]
["DRACKR_2_DS3SR3",10,0]
["DRACKR_2_DS3SR3",11,0]
["DRACKR_2_DS3SR3",12,0]
["DRACKR_2_DS4SR4",1,0.08]
["DRACKR_2_DS4SR4",2,0.91]
["DRACKR_2_DS4SR4",3,1.06]
["DRACKR_2_DS4SR4",4,1.77]
["DRACKR_2_DS4SR4",5,2.7]
["DRACKR_2_DS4SR4",6,5.54]
["DRACKR_2_DS4SR4",7,6.01]
["DRACKR_2_DS4SR4",8,5.09]
["DRACKR_2_DS4SR4",9,4.41]
["DRACKR_2_DS4SR4",10,2.66]
["DRACKR_2_DS4SR4",11,1.6]
["DRACKR_2_DS4SR4",12,0.47]
["DRACKR_2_DSUBT1",1,63]
["DRACKR_2_DSUBT1",2,63]
["DRACKR_2_DSUBT1",3,63]
["DRACKR_2_DSUBT1",4,63]
["DRACKR_2_DSUBT1",5,63]
["DRACKR_2_DSUBT1",6,63]
["DRACKR_2_DSUBT1",7,63]
["DRACKR_2_DSUBT1",8,63]
["DRACKR_2_DSUBT1",9,63]
["DRACKR_2_DSUBT1",10,63]
["DRACKR_2_DSUBT1",11,63]
["DRACKR_2_DSUBT1",12,63]
["DRACKR_2_DSUBT2",1,115]
["DRACKR_2_DSUBT2",2,115]
["DRACKR_2_DSUBT2",3,115]
["DRACKR_2_DSUBT2",4,115]
["DRACKR_2_DSUBT2",5,115]
["DRACKR_2_DSUBT2",6,115]
["DRACKR_2_DSUBT2",7,115]
["DRACKR_2_DSUBT2",8,115]
["DRACKR_2_DSUBT2",9,115]
["DRACKR_2_DSUBT2",10,115]
["DRACKR_2_DSUBT2",11,115]
["DRACKR_2_DSUBT2",12,115]
["DRACKR_2_DSUBT3",1,115]
["DRACKR_2_DSUBT3",2,115]
["DRACKR_2_DSUBT3",3,115]
["DRACKR_2_DSUBT3",4,115]
["DRACKR_2_DSUBT3",5,115]
["DRACKR_2_DSUBT3",6,115]
["DRACKR_2_DSUBT3",7,115]
["DRACKR_2_DSUBT3",8,115]
["DRACKR_2_DSUBT3",9,115]
["DRACKR_2_DSUBT3",10,115]
["DRACKR_2_DSUBT3",11,115]
["DRACKR_2_DSUBT3",12,97.86]
["DRACKR_2_DSUBT4",1,47]
["DRACKR_2_DSUBT4",2,47]
["DRACKR_2_DSUBT4",3,47]
["DRACKR_2_DSUBT4",4,47]
["DRACKR_2_DSUBT4",5,47]
["DRACKR_2_DSUBT4",6,47]
["DRACKR_2_DSUBT4",7,47]
["DRACKR_2_DSUBT4",8,47]
["DRACKR_2_DSUBT4",9,47]
["DRACKR_2_DSUBT4",10,47]
["DRACKR_2_DSUBT4",11,47]
["DRACKR_2_DSUBT4",12,47]
["DRACKR_2_SOLAR1",1,0.22]
["DRACKR_2_SOLAR1",2,1.91]
["DRACKR_2_SOLAR1",3,2.58]
["DRACKR_2_SOLAR1",4,3.61]
["DRACKR_2_SOLAR1",5,5.47]
["DRACKR_2_SOLAR1",6,11.2]
["DRACKR_2_SOLAR1",7,11.97]
["DRACKR_2_SOLAR1",8,10.15]
["DRACKR_2_SOLAR1",9,8.6199999999999992]
["DRACKR_2_SOLAR1",10,5.49]
["DRACKR_2_SOLAR1",11,3.35]
["DRACKR_2_SOLAR1",12,1.47]
["DRACKR_2_SOLAR2",1,0]
["DRACKR_2_SOLAR2",2,0]
["DRACKR_2_SOLAR2",3,0]
["DRACKR_2_SOLAR2",4,0]
["DRACKR_2_SOLAR2",5,0]
["DRACKR_2_SOLAR2",6,0]
["DRACKR_2_SOLAR2",7,0]
["DRACKR_2_SOLAR2",8,0]
["DRACKR_2_SOLAR2",9,0]
["DRACKR_2_SOLAR2",10,0]
["DRACKR_2_SOLAR2",11,0]
["DRACKR_2_SOLAR2",12,0]
["DREWS_6_PL1X4",1,40]
["DREWS_6_PL1X4",2,40]
["DREWS_6_PL1X4",3,40]
["DREWS_6_PL1X4",4,40]
["DREWS_6_PL1X4",5,40]
["DREWS_6_PL1X4",6,40]
["DREWS_6_PL1X4",7,40]
["DREWS_6_PL1X4",8,40]
["DREWS_6_PL1X4",9,40]
["DREWS_6_PL1X4",10,40]
["DREWS_6_PL1X4",11,40]
["DREWS_6_PL1X4",12,40]
["DRUM_7_PL1X2",1,0]
["DRUM_7_PL1X2",2,0]
["DRUM_7_PL1X2",3,0]
["DRUM_7_PL1X2",4,0]
["DRUM_7_PL1X2",5,0]
["DRUM_7_PL1X2",6,0]
["DRUM_7_PL1X2",7,0]
["DRUM_7_PL1X2",8,10.4]
["DRUM_7_PL1X2",9,0]
["DRUM_7_PL1X2",10,0]
["DRUM_7_PL1X2",11,0]
["DRUM_7_PL1X2",12,9.6]
["DRUM_7_PL3X4",1,12.8]
["DRUM_7_PL3X4",2,0]
["DRUM_7_PL3X4",3,0]
["DRUM_7_PL3X4",4,0]
["DRUM_7_PL3X4",5,12.8]
["DRUM_7_PL3X4",6,12.8]
["DRUM_7_PL3X4",7,12.8]
["DRUM_7_PL3X4",8,9.6]
["DRUM_7_PL3X4",9,0]
["DRUM_7_PL3X4",10,0]
["DRUM_7_PL3X4",11,12.8]
["DRUM_7_PL3X4",12,12.8]
["DRUM_7_UNIT 5",1,39.6]
["DRUM_7_UNIT 5",2,44.6]
["DRUM_7_UNIT 5",3,43.6]
["DRUM_7_UNIT 5",4,39.6]
["DRUM_7_UNIT 5",5,41.74]
["DRUM_7_UNIT 5",6,39.6]
["DRUM_7_UNIT 5",7,48.1]
["DRUM_7_UNIT 5",8,47.74]
["DRUM_7_UNIT 5",9,25.6]
["DRUM_7_UNIT 5",10,0]
["DRUM_7_UNIT 5",11,34.479999999999997]
["DRUM_7_UNIT 5",12,39.200000000000003]
["DSABLA_7_UNIT",1,6.43]
["DSABLA_7_UNIT",2,4.8499999999999996]
["DSABLA_7_UNIT",3,3.64]
["DSABLA_7_UNIT",4,1.56]
["DSABLA_7_UNIT",5,7.28]
["DSABLA_7_UNIT",6,7.06]
["DSABLA_7_UNIT",7,9.06]
["DSABLA_7_UNIT",8,6.06]
["DSABLA_7_UNIT",9,4.3499999999999996]
["DSABLA_7_UNIT",10,2.74]
["DSABLA_7_UNIT",11,2.5099999999999998]
["DSABLA_7_UNIT",12,4.1100000000000003]
["DSFLWR_2_WS2SR1",1,0.4]
["DSFLWR_2_WS2SR1",2,3]
["DSFLWR_2_WS2SR1",3,3.5]
["DSFLWR_2_WS2SR1",4,4.4000000000000004]
["DSFLWR_2_WS2SR1",5,6.4]
["DSFLWR_2_WS2SR1",6,13.1]
["DSFLWR_2_WS2SR1",7,14.4]
["DSFLWR_2_WS2SR1",8,12.4]
["DSFLWR_2_WS2SR1",9,11.1]
["DSFLWR_2_WS2SR1",10,7.4]
["DSFLWR_2_WS2SR1",11,5.7]
["DSFLWR_2_WS2SR1",12,3.5]
["DSFLWR_2_W9CSB1",5,0]
["DSFLWR_2_W9CSB1",6,13.35]
["DSFLWR_2_W9CSB1",7,14.67]
["DSFLWR_2_W9CSB1",8,12.64]
["DSFLWR_2_W9CSB1",9,11.31]
["DSFLWR_2_W9CSB1",10,7.54]
["DSFLWR_2_W9CSB1",11,5.81]
["DSFLWR_2_W9CSB1",12,3.57]
["DSFLWR_2_W9CSB2",5,0]
["DSFLWR_2_W9CSB2",6,9.42]
["DSFLWR_2_W9CSB2",7,10.35]
["DSFLWR_2_W9CSB2",8,8.92]
["DSFLWR_2_W9CSB2",9,7.98]
["DSFLWR_2_W9CSB2",10,5.32]
["DSFLWR_2_W9CSB2",11,4.0999999999999996]
["DSFLWR_2_W9CSB2",12,2.52]
["DSRTHV_2_DH1SR1",1,0.32]
["DSRTHV_2_DH1SR1",2,2.4]
["DSRTHV_2_DH1SR1",3,2.8]
["DSRTHV_2_DH1SR1",4,3.52]
["DSRTHV_2_DH1SR1",5,5.12]
["DSRTHV_2_DH1SR1",6,10.48]
["DSRTHV_2_DH1SR1",7,11.52]
["DSRTHV_2_DH1SR1",8,9.92]
["DSRTHV_2_DH1SR1",9,8.8800000000000008]
["DSRTHV_2_DH1SR1",10,5.92]
["DSRTHV_2_DH1SR1",11,4.5599999999999996]
["DSRTHV_2_DH1SR1",12,2.8]
["DSRTHV_2_DH2BT1",1,35]
["DSRTHV_2_DH2BT1",2,35]
["DSRTHV_2_DH2BT1",3,35]
["DSRTHV_2_DH2BT1",4,35]
["DSRTHV_2_DH2BT1",5,35]
["DSRTHV_2_DH2BT1",6,35]
["DSRTHV_2_DH2BT1",7,35]
["DSRTHV_2_DH2BT1",8,35]
["DSRTHV_2_DH2BT1",9,35]
["DSRTHV_2_DH2BT1",10,35]
["DSRTHV_2_DH2BT1",11,35]
["DSRTHV_2_DH2BT1",12,35]
["DSRTHV_2_DH2SR2",1,0.08]
["DSRTHV_2_DH2SR2",2,0.69]
["DSRTHV_2_DH2SR2",3,0.82]
["DSRTHV_2_DH2SR2",4,1.1599999999999999]
["DSRTHV_2_DH2SR2",5,1.72]
["DSRTHV_2_DH2SR2",6,3.55]
["DSRTHV_2_DH2SR2",7,3.92]
["DSRTHV_2_DH2SR2",8,3.32]
["DSRTHV_2_DH2SR2",9,2.86]
["DSRTHV_2_DH2SR2",10,1.8]
["DSRTHV_2_DH2SR2",11,1.21]
["DSRTHV_2_DH2SR2",12,0.59]
["DSRTSL_2_SOLAR1",1,1.18]
["DSRTSL_2_SOLAR1",2,8.89]
["DSRTSL_2_SOLAR1",3,10.37]
["DSRTSL_2_SOLAR1",4,13.03]
["DSRTSL_2_SOLAR1",5,18.96]
["DSRTSL_2_SOLAR1",6,38.799999999999997]
["DSRTSL_2_SOLAR1",7,42.65]
["DSRTSL_2_SOLAR1",8,36.729999999999997]
["DSRTSL_2_SOLAR1",9,32.880000000000003]
["DSRTSL_2_SOLAR1",10,21.92]
["DSRTSL_2_SOLAR1",11,16.88]
["DSRTSL_2_SOLAR1",12,10.37]
["DSRTSN_2_DS2X2",1,230]
["DSRTSN_2_DS2X2",2,230]
["DSRTSN_2_DS2X2",3,230]
["DSRTSN_2_DS2X2",4,230]
["DSRTSN_2_DS2X2",5,230]
["DSRTSN_2_DS2X2",6,230]
["DSRTSN_2_DS2X2",7,230]
["DSRTSN_2_DS2X2",8,230]
["DSRTSN_2_DS2X2",9,230]
["DSRTSN_2_DS2X2",10,230]
["DSRTSN_2_DS2X2",11,230]
["DSRTSN_2_DS2X2",12,214.29]
["DSRTSN_2_SOLAR1",1,1.2]
["DSRTSN_2_SOLAR1",2,9]
["DSRTSN_2_SOLAR1",3,10.5]
["DSRTSN_2_SOLAR1",4,13.2]
["DSRTSN_2_SOLAR1",5,19.2]
["DSRTSN_2_SOLAR1",6,39.299999999999997]
["DSRTSN_2_SOLAR1",7,43.2]
["DSRTSN_2_SOLAR1",8,37.200000000000003]
["DSRTSN_2_SOLAR1",9,33.299999999999997]
["DSRTSN_2_SOLAR1",10,22.2]
["DSRTSN_2_SOLAR1",11,17.100000000000001]
["DSRTSN_2_SOLAR1",12,10.5]
["DSRTSN_2_SOLAR2",1,0.12]
["DSRTSN_2_SOLAR2",2,2.4700000000000002]
["DSRTSN_2_SOLAR2",3,3.51]
["DSRTSN_2_SOLAR2",4,5.73]
["DSRTSN_2_SOLAR2",5,8.89]
["DSRTSN_2_SOLAR2",6,19.2]
["DSRTSN_2_SOLAR2",7,21.02]
["DSRTSN_2_SOLAR2",8,17.21]
["DSRTSN_2_SOLAR2",9,13.47]
["DSRTSN_2_SOLAR2",10,7.49]
["DSRTSN_2_SOLAR2",11,3.27]
["DSRTSN_2_SOLAR2",12,0]
["DTCHWD_2_BT3WND",1,0.8]
["DTCHWD_2_BT3WND",2,0.85]
["DTCHWD_2_BT3WND",3,0.74]
["DTCHWD_2_BT3WND",4,0.71]
["DTCHWD_2_BT3WND",5,0.76]
["DTCHWD_2_BT3WND",6,0.69]
["DTCHWD_2_BT3WND",7,0.64]
["DTCHWD_2_BT3WND",8,0.49]
["DTCHWD_2_BT3WND",9,0.51]
["DTCHWD_2_BT3WND",10,0.47]
["DTCHWD_2_BT3WND",11,0.63]
["DTCHWD_2_BT3WND",12,0.77]
["DTCHWD_2_BT4WND",1,1.1499999999999999]
["DTCHWD_2_BT4WND",2,1.23]
["DTCHWD_2_BT4WND",3,1.08]
["DTCHWD_2_BT4WND",4,1.03]
["DTCHWD_2_BT4WND",5,1.1000000000000001]
["DTCHWD_2_BT4WND",6,1.01]
["DTCHWD_2_BT4WND",7,0.93]
["DTCHWD_2_BT4WND",8,0.71]
["DTCHWD_2_BT4WND",9,0.73]
["DTCHWD_2_BT4WND",10,0.68]
["DTCHWD_2_BT4WND",11,0.92]
["DTCHWD_2_BT4WND",12,1.1100000000000001]
["DUANE_1_PL1X3",1,147.80000000000001]
["DUANE_1_PL1X3",2,147.80000000000001]
["DUANE_1_PL1X3",3,147.80000000000001]
["DUANE_1_PL1X3",4,147.80000000000001]
["DUANE_1_PL1X3",5,143.5]
["DUANE_1_PL1X3",6,143.5]
["DUANE_1_PL1X3",7,143.5]
["DUANE_1_PL1X3",8,143.5]
["DUANE_1_PL1X3",9,143.5]
["DUANE_1_PL1X3",10,147.80000000000001]
["DUANE_1_PL1X3",11,147.80000000000001]
["DUANE_1_PL1X3",12,147.80000000000001]
["DUTCH1_7_UNIT 1",1,17.600000000000001]
["DUTCH1_7_UNIT 1",2,12.8]
["DUTCH1_7_UNIT 1",3,9.36]
["DUTCH1_7_UNIT 1",4,16]
["DUTCH1_7_UNIT 1",5,17.399999999999999]
["DUTCH1_7_UNIT 1",6,18.8]
["DUTCH1_7_UNIT 1",7,18.8]
["DUTCH1_7_UNIT 1",8,19]
["DUTCH1_7_UNIT 1",9,16.8]
["DUTCH1_7_UNIT 1",10,6.4]
["DUTCH1_7_UNIT 1",11,15.3]
["DUTCH1_7_UNIT 1",12,18.64]
["DUTCH2_7_UNIT 1",1,0]
["DUTCH2_7_UNIT 1",2,5.16]
["DUTCH2_7_UNIT 1",3,17.52]
["DUTCH2_7_UNIT 1",4,5.6]
["DUTCH2_7_UNIT 1",5,15.2]
["DUTCH2_7_UNIT 1",6,5.6]
["DUTCH2_7_UNIT 1",7,15.6]
["DUTCH2_7_UNIT 1",8,16.760000000000002]
["DUTCH2_7_UNIT 1",9,0]
["DUTCH2_7_UNIT 1",10,0]
["DUTCH2_7_UNIT 1",11,0]
["DUTCH2_7_UNIT 1",12,15.28]
["DVLCYN_1_UNITS",1,24.74]
["DVLCYN_1_UNITS",2,29.27]
["DVLCYN_1_UNITS",3,29.13]
["DVLCYN_1_UNITS",4,94.77]
["DVLCYN_1_UNITS",5,87.34]
["DVLCYN_1_UNITS",6,96.31]
["DVLCYN_1_UNITS",7,153.15]
["DVLCYN_1_UNITS",8,148.13]
["DVLCYN_1_UNITS",9,144.96]
["DVLCYN_1_UNITS",10,156.44]
["DVLCYN_1_UNITS",11,154.81]
["DVLCYN_1_UNITS",12,132.56]
["DYERSM_6_DSWWD1",1,14.71]
["DYERSM_6_DSWWD1",2,15.78]
["DYERSM_6_DSWWD1",3,14.08]
["DYERSM_6_DSWWD1",4,14.87]
["DYERSM_6_DSWWD1",5,15.39]
["DYERSM_6_DSWWD1",6,11.35]
["DYERSM_6_DSWWD1",7,10.09]
["DYERSM_6_DSWWD1",8,9.48]
["DYERSM_6_DSWWD1",9,9.73]
["DYERSM_6_DSWWD1",10,8.16]
["DYERSM_6_DSWWD1",11,10.3]
["DYERSM_6_DSWWD1",12,13.17]
["EASTWD_7_UNIT",1,199]
["EASTWD_7_UNIT",2,199]
["EASTWD_7_UNIT",3,199]
["EASTWD_7_UNIT",4,199]
["EASTWD_7_UNIT",5,199]
["EASTWD_7_UNIT",6,199]
["EASTWD_7_UNIT",7,199]
["EASTWD_7_UNIT",8,199]
["EASTWD_7_UNIT",9,199]
["EASTWD_7_UNIT",10,199]
["EASTWD_7_UNIT",11,199]
["EASTWD_7_UNIT",12,199]
["EDMONS_2_NSPIN",1,236]
["EDMONS_2_NSPIN",2,236]
["EDMONS_2_NSPIN",3,236]
["EDMONS_2_NSPIN",4,236]
["EDMONS_2_NSPIN",5,236]
["EDMONS_2_NSPIN",6,236]
["EDMONS_2_NSPIN",7,236]
["EDMONS_2_NSPIN",8,236]
["EDMONS_2_NSPIN",9,236]
["EDMONS_2_NSPIN",10,236]
["EDMONS_2_NSPIN",11,236]
["EDMONS_2_NSPIN",12,236]
["EDWARD_2_E21SB1",1,71.25]
["EDWARD_2_E21SB1",2,73.349999999999994]
["EDWARD_2_E21SB1",3,73.930000000000007]
["EDWARD_2_E21SB1",4,75.09]
["EDWARD_2_E21SB1",5,77.12]
["EDWARD_2_E21SB1",6,83.85]
["EDWARD_2_E21SB1",7,85.1]
["EDWARD_2_E21SB1",8,82.86]
["EDWARD_2_E21SB1",9,81.02]
["EDWARD_2_E21SB1",10,77.22]
["EDWARD_2_E21SB1",11,75.02]
["EDWARD_2_E21SB1",12,72.650000000000006]
["EDWARD_2_E23SB1",1,6.07]
["EDWARD_2_E23SB1",2,6.59]
["EDWARD_2_E23SB1",3,6.7]
["EDWARD_2_E23SB1",4,6.92]
["EDWARD_2_E23SB1",5,7.35]
["EDWARD_2_E23SB1",6,8.7899999999999991]
["EDWARD_2_E23SB1",7,9.07]
["EDWARD_2_E23SB1",8,8.6199999999999992]
["EDWARD_2_E23SB1",9,8.2899999999999991]
["EDWARD_2_E23SB1",10,7.49]
["EDWARD_2_E23SB1",11,7.08]
["EDWARD_2_E23SB1",12,6.6]
["EDWARD_2_ES2BT3",1,66.22]
["EDWARD_2_ES2BT3",2,68.099999999999994]
["EDWARD_2_ES2BT3",3,68.63]
["EDWARD_2_ES2BT3",4,69.680000000000007]
["EDWARD_2_ES2BT3",5,71.510000000000005]
["EDWARD_2_ES2BT3",6,77.569999999999993]
["EDWARD_2_ES2BT3",7,78.69]
["EDWARD_2_ES2BT3",8,76.67]
["EDWARD_2_ES2BT3",9,75]
["EDWARD_2_ES2BT3",10,71.569999999999993]
["EDWARD_2_ES2BT3",11,69.58]
["EDWARD_2_ES2BT3",12,67.44]
["EDWARD_2_ESSSB1",1,0]
["EDWARD_2_ESSSB1",2,0]
["EDWARD_2_ESSSB1",3,0]
["EDWARD_2_ESSSB1",4,0]
["EDWARD_2_ESSSB1",5,0]
["EDWARD_2_ESSSB1",6,0]
["EDWARD_2_ESSSB1",7,0]
["EDWARD_2_ESSSB1",8,0]
["EDWARD_2_ESSSB1",9,0]
["EDWARD_2_ESSSB1",10,0]
["EDWARD_2_ESSSB1",11,0]
["EDWARD_2_ESSSB1",12,0]
["EDWARD_2_ESSSB2",1,0]
["EDWARD_2_ESSSB2",2,0]
["EDWARD_2_ESSSB2",3,0]
["EDWARD_2_ESSSB2",4,0]
["EDWARD_2_ESSSB2",5,0]
["EDWARD_2_ESSSB2",6,0]
["EDWARD_2_ESSSB2",7,0]
["EDWARD_2_ESSSB2",8,0]
["EDWARD_2_ESSSB2",9,0]
["EDWARD_2_ESSSB2",10,0]
["EDWARD_2_ESSSB2",11,0]
["EDWARD_2_ESSSB2",12,0]
["EEKTMN_6_SOLAR1",1,0]
["EEKTMN_6_SOLAR1",2,0]
["EEKTMN_6_SOLAR1",3,0]
["EEKTMN_6_SOLAR1",4,0]
["EEKTMN_6_SOLAR1",5,0]
["EEKTMN_6_SOLAR1",6,0]
["EEKTMN_6_SOLAR1",7,0]
["EEKTMN_6_SOLAR1",8,0]
["EEKTMN_6_SOLAR1",9,0]
["EEKTMN_6_SOLAR1",10,0]
["EEKTMN_6_SOLAR1",11,0]
["EEKTMN_6_SOLAR1",12,0]
["ELCAJN_6_EB1BT1",1,7.5]
["ELCAJN_6_EB1BT1",2,7.5]
["ELCAJN_6_EB1BT1",3,7.5]
["ELCAJN_6_EB1BT1",4,7.5]
["ELCAJN_6_EB1BT1",5,7.5]
["ELCAJN_6_EB1BT1",6,7.5]
["ELCAJN_6_EB1BT1",7,7.5]
["ELCAJN_6_EB1BT1",8,7.5]
["ELCAJN_6_EB1BT1",9,7.5]
["ELCAJN_6_EB1BT1",10,7.5]
["ELCAJN_6_EB1BT1",11,7.5]
["ELCAJN_6_EB1BT1",12,7.5]
["ELCAJN_6_LM6K",1,48.1]
["ELCAJN_6_LM6K",2,48.1]
["ELCAJN_6_LM6K",3,48.1]
["ELCAJN_6_LM6K",4,48.1]
["ELCAJN_6_LM6K",5,48.1]
["ELCAJN_6_LM6K",6,48.1]
["ELCAJN_6_LM6K",7,48.1]
["ELCAJN_6_LM6K",8,48.1]
["ELCAJN_6_LM6K",9,48.1]
["ELCAJN_6_LM6K",10,48.1]
["ELCAJN_6_LM6K",11,48.1]
["ELCAJN_6_LM6K",12,48.1]
["ELCAJN_6_UNITA1",1,45.42]
["ELCAJN_6_UNITA1",2,45.42]
["ELCAJN_6_UNITA1",3,45.42]
["ELCAJN_6_UNITA1",4,45.42]
["ELCAJN_6_UNITA1",5,45.42]
["ELCAJN_6_UNITA1",6,45.42]
["ELCAJN_6_UNITA1",7,45.42]
["ELCAJN_6_UNITA1",8,45.42]
["ELCAJN_6_UNITA1",9,45.42]
["ELCAJN_6_UNITA1",10,45.42]
["ELCAJN_6_UNITA1",11,45.42]
["ELCAJN_6_UNITA1",12,45.42]
["ELCAP_1_SOLAR",1,0]
["ELCAP_1_SOLAR",2,0]
["ELCAP_1_SOLAR",3,0]
["ELCAP_1_SOLAR",4,0]
["ELCAP_1_SOLAR",5,0]
["ELCAP_1_SOLAR",6,0]
["ELCAP_1_SOLAR",7,0]
["ELCAP_1_SOLAR",8,0]
["ELCAP_1_SOLAR",9,0]
["ELCAP_1_SOLAR",10,0]
["ELCAP_1_SOLAR",11,0]
["ELCAP_1_SOLAR",12,0]
["ELDORO_7_UNIT 1",1,4.49]
["ELDORO_7_UNIT 1",2,3.83]
["ELDORO_7_UNIT 1",3,5.44]
["ELDORO_7_UNIT 1",4,8.35]
["ELDORO_7_UNIT 1",5,8.5]
["ELDORO_7_UNIT 1",6,6.39]
["ELDORO_7_UNIT 1",7,5.1100000000000003]
["ELDORO_7_UNIT 1",8,2.5299999999999998]
["ELDORO_7_UNIT 1",9,3.6]
["ELDORO_7_UNIT 1",10,0]
["ELDORO_7_UNIT 1",11,0]
["ELDORO_7_UNIT 1",12,1.05]
["ELDORO_7_UNIT 2",1,7]
["ELDORO_7_UNIT 2",2,4.09]
["ELDORO_7_UNIT 2",3,4]
["ELDORO_7_UNIT 2",4,8.0500000000000007]
["ELDORO_7_UNIT 2",5,8.81]
["ELDORO_7_UNIT 2",6,6.44]
["ELDORO_7_UNIT 2",7,4.24]
["ELDORO_7_UNIT 2",8,5.18]
["ELDORO_7_UNIT 2",9,3.18]
["ELDORO_7_UNIT 2",10,0]
["ELDORO_7_UNIT 2",11,0]
["ELDORO_7_UNIT 2",12,0.68]
["ELECTR_7_PL1X3",1,49.36]
["ELECTR_7_PL1X3",2,33.74]
["ELECTR_7_PL1X3",3,51]
["ELECTR_7_PL1X3",4,25.4]
["ELECTR_7_PL1X3",5,48.6]
["ELECTR_7_PL1X3",6,53.88]
["ELECTR_7_PL1X3",7,50.6]
["ELECTR_7_PL1X3",8,54.6]
["ELECTR_7_PL1X3",9,61.28]
["ELECTR_7_PL1X3",10,48.64]
["ELECTR_7_PL1X3",11,50.76]
["ELECTR_7_PL1X3",12,55.6]
["ELKCRK_6_STONYG",1,1.8]
["ELKCRK_6_STONYG",2,2.4]
["ELKCRK_6_STONYG",3,2.7]
["ELKCRK_6_STONYG",4,2.2000000000000002]
["ELKCRK_6_STONYG",5,1.6]
["ELKCRK_6_STONYG",6,1.7]
["ELKCRK_6_STONYG",7,2.2000000000000002]
["ELKCRK_6_STONYG",8,2]
["ELKCRK_6_STONYG",9,1.4]
["ELKCRK_6_STONYG",10,0.4]
["ELKCRK_6_STONYG",11,0.1]
["ELKCRK_6_STONYG",12,0.9]
["ELKHIL_2_PL1X3",1,380]
["ELKHIL_2_PL1X3",2,380]
["ELKHIL_2_PL1X3",3,380]
["ELKHIL_2_PL1X3",4,380]
["ELKHIL_2_PL1X3",5,380]
["ELKHIL_2_PL1X3",6,380]
["ELKHIL_2_PL1X3",7,380]
["ELKHIL_2_PL1X3",8,380]
["ELKHIL_2_PL1X3",9,380]
["ELKHIL_2_PL1X3",10,380]
["ELKHIL_2_PL1X3",11,380]
["ELKHIL_2_PL1X3",12,380]
["ELKHRN_1_EESX3",1,182.5]
["ELKHRN_1_EESX3",2,182.5]
["ELKHRN_1_EESX3",3,182.5]
["ELKHRN_1_EESX3",4,182.5]
["ELKHRN_1_EESX3",5,182.5]
["ELKHRN_1_EESX3",6,182.5]
["ELKHRN_1_EESX3",7,182.5]
["ELKHRN_1_EESX3",8,182.5]
["ELKHRN_1_EESX3",9,182.5]
["ELKHRN_1_EESX3",10,182.5]
["ELKHRN_1_EESX3",11,182.5]
["ELKHRN_1_EESX3",12,182.5]
["ELLIS_2_QF",1,0.24]
["ELLIS_2_QF",2,0.33]
["ELLIS_2_QF",3,7.0000000000000007E-2]
["ELLIS_2_QF",4,0.05]
["ELLIS_2_QF",5,0.06]
["ELLIS_2_QF",6,0.11]
["ELLIS_2_QF",7,0.2]
["ELLIS_2_QF",8,0.55000000000000004]
["ELLIS_2_QF",9,1]
["ELLIS_2_QF",10,1]
["ELLIS_2_QF",11,1]
["ELLIS_2_QF",12,0.98]
["ELNIDP_6_BIOMAS",1,8.89]
["ELNIDP_6_BIOMAS",2,9.2200000000000006]
["ELNIDP_6_BIOMAS",3,9.31]
["ELNIDP_6_BIOMAS",4,8.81]
["ELNIDP_6_BIOMAS",5,8.6300000000000008]
["ELNIDP_6_BIOMAS",6,9.48]
["ELNIDP_6_BIOMAS",7,8.99]
["ELNIDP_6_BIOMAS",8,9.24]
["ELNIDP_6_BIOMAS",9,9.17]
["ELNIDP_6_BIOMAS",10,6.97]
["ELNIDP_6_BIOMAS",11,5.57]
["ELNIDP_6_BIOMAS",12,6.38]
["ELSEGN_2_UN1011",1,274.31]
["ELSEGN_2_UN1011",2,274.31]
["ELSEGN_2_UN1011",3,274.31]
["ELSEGN_2_UN1011",4,274.31]
["ELSEGN_2_UN1011",5,274.31]
["ELSEGN_2_UN1011",6,274.31]
["ELSEGN_2_UN1011",7,274.31]
["ELSEGN_2_UN1011",8,274.31]
["ELSEGN_2_UN1011",9,274.31]
["ELSEGN_2_UN1011",10,274.31]
["ELSEGN_2_UN1011",11,274.31]
["ELSEGN_2_UN1011",12,274.31]
["ELSEGN_2_UN2021",1,271.74]
["ELSEGN_2_UN2021",2,271.74]
["ELSEGN_2_UN2021",3,271.74]
["ELSEGN_2_UN2021",4,271.74]
["ELSEGN_2_UN2021",5,271.74]
["ELSEGN_2_UN2021",6,271.74]
["ELSEGN_2_UN2021",7,271.74]
["ELSEGN_2_UN2021",8,271.74]
["ELSEGN_2_UN2021",9,271.74]
["ELSEGN_2_UN2021",10,271.74]
["ELSEGN_2_UN2021",11,271.74]
["ELSEGN_2_UN2021",12,271.74]
["ENERSJ_2_WIND",1,26.68]
["ENERSJ_2_WIND",2,28.38]
["ENERSJ_2_WIND",3,24.93]
["ENERSJ_2_WIND",4,23.89]
["ENERSJ_2_WIND",5,25.4]
["ENERSJ_2_WIND",6,23.28]
["ENERSJ_2_WIND",7,21.63]
["ENERSJ_2_WIND",8,16.440000000000001]
["ENERSJ_2_WIND",9,16.98]
["ENERSJ_2_WIND",10,15.75]
["ENERSJ_2_WIND",11,21.23]
["ENERSJ_2_WIND",12,25.72]
["ENERSJ_5_ESJWD2",1,18.55]
["ENERSJ_5_ESJWD2",2,19.73]
["ENERSJ_5_ESJWD2",3,17.34]
["ENERSJ_5_ESJWD2",4,16.61]
["ENERSJ_5_ESJWD2",5,17.66]
["ENERSJ_5_ESJWD2",6,16.190000000000001]
["ENERSJ_5_ESJWD2",7,15.04]
["ENERSJ_5_ESJWD2",8,11.43]
["ENERSJ_5_ESJWD2",9,11.81]
["ENERSJ_5_ESJWD2",10,10.95]
["ENERSJ_5_ESJWD2",11,14.76]
["ENERSJ_5_ESJWD2",12,17.88]
["ENWIND_2_WIND1",1,8.32]
["ENWIND_2_WIND1",2,8.85]
["ENWIND_2_WIND1",3,7.78]
["ENWIND_2_WIND1",4,7.45]
["ENWIND_2_WIND1",5,7.92]
["ENWIND_2_WIND1",6,7.26]
["ENWIND_2_WIND1",7,6.75]
["ENWIND_2_WIND1",8,5.13]
["ENWIND_2_WIND1",9,5.3]
["ENWIND_2_WIND1",10,4.91]
["ENWIND_2_WIND1",11,6.62]
["ENWIND_2_WIND1",12,8.02]
["ENWIND_2_WIND2",1,6.76]
["ENWIND_2_WIND2",2,7.19]
["ENWIND_2_WIND2",3,6.31]
["ENWIND_2_WIND2",4,6.05]
["ENWIND_2_WIND2",5,6.43]
["ENWIND_2_WIND2",6,5.9]
["ENWIND_2_WIND2",7,5.48]
["ENWIND_2_WIND2",8,4.16]
["ENWIND_2_WIND2",9,4.3]
["ENWIND_2_WIND2",10,3.99]
["ENWIND_2_WIND2",11,5.38]
["ENWIND_2_WIND2",12,6.51]
["ESCNDO_6_EB1BT1",1,10]
["ESCNDO_6_EB1BT1",2,10]
["ESCNDO_6_EB1BT1",3,10]
["ESCNDO_6_EB1BT1",4,10]
["ESCNDO_6_EB1BT1",5,10]
["ESCNDO_6_EB1BT1",6,10]
["ESCNDO_6_EB1BT1",7,10]
["ESCNDO_6_EB1BT1",8,10]
["ESCNDO_6_EB1BT1",9,10]
["ESCNDO_6_EB1BT1",10,10]
["ESCNDO_6_EB1BT1",11,10]
["ESCNDO_6_EB1BT1",12,10]
["ESCNDO_6_EB2BT2",1,10]
["ESCNDO_6_EB2BT2",2,10]
["ESCNDO_6_EB2BT2",3,10]
["ESCNDO_6_EB2BT2",4,10]
["ESCNDO_6_EB2BT2",5,10]
["ESCNDO_6_EB2BT2",6,10]
["ESCNDO_6_EB2BT2",7,10]
["ESCNDO_6_EB2BT2",8,10]
["ESCNDO_6_EB2BT2",9,10]
["ESCNDO_6_EB2BT2",10,10]
["ESCNDO_6_EB2BT2",11,10]
["ESCNDO_6_EB2BT2",12,10]
["ESCNDO_6_EB3BT3",1,10]
["ESCNDO_6_EB3BT3",2,10]
["ESCNDO_6_EB3BT3",3,10]
["ESCNDO_6_EB3BT3",4,10]
["ESCNDO_6_EB3BT3",5,10]
["ESCNDO_6_EB3BT3",6,10]
["ESCNDO_6_EB3BT3",7,10]
["ESCNDO_6_EB3BT3",8,10]
["ESCNDO_6_EB3BT3",9,10]
["ESCNDO_6_EB3BT3",10,10]
["ESCNDO_6_EB3BT3",11,10]
["ESCNDO_6_EB3BT3",12,10]
["ESCNDO_6_PL1X2",1,48.71]
["ESCNDO_6_PL1X2",2,48.71]
["ESCNDO_6_PL1X2",3,48.71]
["ESCNDO_6_PL1X2",4,48.71]
["ESCNDO_6_PL1X2",5,48.71]
["ESCNDO_6_PL1X2",6,48.71]
["ESCNDO_6_PL1X2",7,48.71]
["ESCNDO_6_PL1X2",8,48.71]
["ESCNDO_6_PL1X2",9,48.71]
["ESCNDO_6_PL1X2",10,48.71]
["ESCNDO_6_PL1X2",11,48.71]
["ESCNDO_6_PL1X2",12,48.71]
["ESCNDO_6_UNITB1",1,48.04]
["ESCNDO_6_UNITB1",2,48.04]
["ESCNDO_6_UNITB1",3,48.04]
["ESCNDO_6_UNITB1",4,48.04]
["ESCNDO_6_UNITB1",5,48.04]
["ESCNDO_6_UNITB1",6,48.04]
["ESCNDO_6_UNITB1",7,48.04]
["ESCNDO_6_UNITB1",8,48.04]
["ESCNDO_6_UNITB1",9,48.04]
["ESCNDO_6_UNITB1",10,48.04]
["ESCNDO_6_UNITB1",11,48.04]
["ESCNDO_6_UNITB1",12,48.04]
["ESCO_6_GLMQF",1,49.9]
["ESCO_6_GLMQF",2,49.9]
["ESCO_6_GLMQF",3,49.9]
["ESCO_6_GLMQF",4,49.9]
["ESCO_6_GLMQF",5,49.9]
["ESCO_6_GLMQF",6,49.9]
["ESCO_6_GLMQF",7,49.9]
["ESCO_6_GLMQF",8,49.9]
["ESCO_6_GLMQF",9,49.9]
["ESCO_6_GLMQF",10,49.9]
["ESCO_6_GLMQF",11,49.9]
["ESCO_6_GLMQF",12,49.9]
["ESNHWR_2_WC1BT1",1,1.5]
["ESNHWR_2_WC1BT1",2,1.5]
["ESNHWR_2_WC1BT1",3,1.5]
["ESNHWR_2_WC1BT1",4,1.5]
["ESNHWR_2_WC1BT1",5,1.5]
["ESNHWR_2_WC1BT1",6,1.5]
["ESNHWR_2_WC1BT1",7,1.5]
["ESNHWR_2_WC1BT1",8,1.5]
["ESNHWR_2_WC1BT1",9,1.5]
["ESNHWR_2_WC1BT1",10,1.5]
["ESNHWR_2_WC1BT1",11,1.5]
["ESNHWR_2_WC1BT1",12,1.5]
["ESQUON_6_LNDFIL",1,0]
["ESQUON_6_LNDFIL",2,0]
["ESQUON_6_LNDFIL",3,0]
["ESQUON_6_LNDFIL",4,0]
["ESQUON_6_LNDFIL",5,0]
["ESQUON_6_LNDFIL",6,0]
["ESQUON_6_LNDFIL",7,0]
["ESQUON_6_LNDFIL",8,0]
["ESQUON_6_LNDFIL",9,0]
["ESQUON_6_LNDFIL",10,0]
["ESQUON_6_LNDFIL",11,0]
["ESQUON_6_LNDFIL",12,0]
["ESTWND_2_OPPWD1",1,10.1]
["ESTWND_2_OPPWD1",2,10.74]
["ESTWND_2_OPPWD1",3,9.44]
["ESTWND_2_OPPWD1",4,9.0399999999999991]
["ESTWND_2_OPPWD1",5,9.61]
["ESTWND_2_OPPWD1",6,8.81]
["ESTWND_2_OPPWD1",7,8.19]
["ESTWND_2_OPPWD1",8,6.22]
["ESTWND_2_OPPWD1",9,6.43]
["ESTWND_2_OPPWD1",10,5.96]
["ESTWND_2_OPPWD1",11,8.0299999999999994]
["ESTWND_2_OPPWD1",12,9.73]
["ETIWND_2_CHMPNE",1,0]
["ETIWND_2_CHMPNE",2,0]
["ETIWND_2_CHMPNE",3,0]
["ETIWND_2_CHMPNE",4,0]
["ETIWND_2_CHMPNE",5,0]
["ETIWND_2_CHMPNE",6,0]
["ETIWND_2_CHMPNE",7,0]
["ETIWND_2_CHMPNE",8,0]
["ETIWND_2_CHMPNE",9,0]
["ETIWND_2_CHMPNE",10,0]
["ETIWND_2_CHMPNE",11,0]
["ETIWND_2_CHMPNE",12,0]
["ETIWND_2_FONTNA",1,0.91]
["ETIWND_2_FONTNA",2,0.9]
["ETIWND_2_FONTNA",3,0.55000000000000004]
["ETIWND_2_FONTNA",4,0.92]
["ETIWND_2_FONTNA",5,0.94]
["ETIWND_2_FONTNA",6,0.72]
["ETIWND_2_FONTNA",7,0.75]
["ETIWND_2_FONTNA",8,0.65]
["ETIWND_2_FONTNA",9,0.71]
["ETIWND_2_FONTNA",10,0.6]
["ETIWND_2_FONTNA",11,0.81]
["ETIWND_2_FONTNA",12,0.74]
["ETIWND_2_RTS010",1,0.01]
["ETIWND_2_RTS010",2,0.05]
["ETIWND_2_RTS010",3,0.05]
["ETIWND_2_RTS010",4,7.0000000000000007E-2]
["ETIWND_2_RTS010",5,0.1]
["ETIWND_2_RTS010",6,0.2]
["ETIWND_2_RTS010",7,0.22]
["ETIWND_2_RTS010",8,0.19]
["ETIWND_2_RTS010",9,0.17]
["ETIWND_2_RTS010",10,0.11]
["ETIWND_2_RTS010",11,0.09]
["ETIWND_2_RTS010",12,0.05]
["ETIWND_2_RTS015",1,0.01]
["ETIWND_2_RTS015",2,0.09]
["ETIWND_2_RTS015",3,0.11]
["ETIWND_2_RTS015",4,0.13]
["ETIWND_2_RTS015",5,0.19]
["ETIWND_2_RTS015",6,0.39]
["ETIWND_2_RTS015",7,0.43]
["ETIWND_2_RTS015",8,0.37]
["ETIWND_2_RTS015",9,0.33]
["ETIWND_2_RTS015",10,0.22]
["ETIWND_2_RTS015",11,0.17]
["ETIWND_2_RTS015",12,0.11]
["ETIWND_2_RTS017",1,0.01]
["ETIWND_2_RTS017",2,0.11]
["ETIWND_2_RTS017",3,0.12]
["ETIWND_2_RTS017",4,0.15]
["ETIWND_2_RTS017",5,0.22]
["ETIWND_2_RTS017",6,0.46]
["ETIWND_2_RTS017",7,0.5]
["ETIWND_2_RTS017",8,0.43]
["ETIWND_2_RTS017",9,0.39]
["ETIWND_2_RTS017",10,0.26]
["ETIWND_2_RTS017",11,0.2]
["ETIWND_2_RTS017",12,0.12]
["ETIWND_2_RTS018",1,0.01]
["ETIWND_2_RTS018",2,0.05]
["ETIWND_2_RTS018",3,0.05]
["ETIWND_2_RTS018",4,7.0000000000000007E-2]
["ETIWND_2_RTS018",5,0.1]
["ETIWND_2_RTS018",6,0.2]
["ETIWND_2_RTS018",7,0.22]
["ETIWND_2_RTS018",8,0.19]
["ETIWND_2_RTS018",9,0.17]
["ETIWND_2_RTS018",10,0.11]
["ETIWND_2_RTS018",11,0.09]
["ETIWND_2_RTS018",12,0.05]
["ETIWND_2_RTS023",1,0.01]
["ETIWND_2_RTS023",2,0.08]
["ETIWND_2_RTS023",3,0.09]
["ETIWND_2_RTS023",4,0.11]
["ETIWND_2_RTS023",5,0.16]
["ETIWND_2_RTS023",6,0.33]
["ETIWND_2_RTS023",7,0.36]
["ETIWND_2_RTS023",8,0.31]
["ETIWND_2_RTS023",9,0.28000000000000003]
["ETIWND_2_RTS023",10,0.19]
["ETIWND_2_RTS023",11,0.14000000000000001]
["ETIWND_2_RTS023",12,0.09]
["ETIWND_2_RTS026",1,0.02]
["ETIWND_2_RTS026",2,0.18]
["ETIWND_2_RTS026",3,0.21]
["ETIWND_2_RTS026",4,0.26]
["ETIWND_2_RTS026",5,0.38]
["ETIWND_2_RTS026",6,0.79]
["ETIWND_2_RTS026",7,0.86]
["ETIWND_2_RTS026",8,0.74]
["ETIWND_2_RTS026",9,0.67]
["ETIWND_2_RTS026",10,0.44]
["ETIWND_2_RTS026",11,0.34]
["ETIWND_2_RTS026",12,0.21]
["ETIWND_2_RTS027",1,0.01]
["ETIWND_2_RTS027",2,0.06]
["ETIWND_2_RTS027",3,7.0000000000000007E-2]
["ETIWND_2_RTS027",4,0.09]
["ETIWND_2_RTS027",5,0.13]
["ETIWND_2_RTS027",6,0.26]
["ETIWND_2_RTS027",7,0.28999999999999998]
["ETIWND_2_RTS027",8,0.25]
["ETIWND_2_RTS027",9,0.22]
["ETIWND_2_RTS027",10,0.15]
["ETIWND_2_RTS027",11,0.11]
["ETIWND_2_RTS027",12,7.0000000000000007E-2]
["ETIWND_2_SOLAR1",1,0]
["ETIWND_2_SOLAR1",2,0.03]
["ETIWND_2_SOLAR1",3,0.04]
["ETIWND_2_SOLAR1",4,0.04]
["ETIWND_2_SOLAR1",5,0.06]
["ETIWND_2_SOLAR1",6,0.13]
["ETIWND_2_SOLAR1",7,0.14000000000000001]
["ETIWND_2_SOLAR1",8,0.12]
["ETIWND_2_SOLAR1",9,0.11]
["ETIWND_2_SOLAR1",10,7.0000000000000007E-2]
["ETIWND_2_SOLAR1",11,0.06]
["ETIWND_2_SOLAR1",12,0.04]
["ETIWND_2_SOLAR2",1,0]
["ETIWND_2_SOLAR2",2,0]
["ETIWND_2_SOLAR2",3,0]
["ETIWND_2_SOLAR2",4,0]
["ETIWND_2_SOLAR2",5,0]
["ETIWND_2_SOLAR2",6,0]
["ETIWND_2_SOLAR2",7,0]
["ETIWND_2_SOLAR2",8,0]
["ETIWND_2_SOLAR2",9,0]
["ETIWND_2_SOLAR2",10,0]
["ETIWND_2_SOLAR2",11,0]
["ETIWND_2_SOLAR2",12,0]
["ETIWND_2_SOLAR5",1,0]
["ETIWND_2_SOLAR5",2,0]
["ETIWND_2_SOLAR5",3,0]
["ETIWND_2_SOLAR5",4,0]
["ETIWND_2_SOLAR5",5,0]
["ETIWND_2_SOLAR5",6,0]
["ETIWND_2_SOLAR5",7,0]
["ETIWND_2_SOLAR5",8,0]
["ETIWND_2_SOLAR5",9,0]
["ETIWND_2_SOLAR5",10,0]
["ETIWND_2_SOLAR5",11,0]
["ETIWND_2_SOLAR5",12,0]
["ETIWND_2_UNIT1",1,33.6]
["ETIWND_2_UNIT1",2,33.6]
["ETIWND_2_UNIT1",3,33.6]
["ETIWND_2_UNIT1",4,33.6]
["ETIWND_2_UNIT1",5,33.6]
["ETIWND_2_UNIT1",6,33.6]
["ETIWND_2_UNIT1",7,33.6]
["ETIWND_2_UNIT1",8,33.6]
["ETIWND_2_UNIT1",9,33.6]
["ETIWND_2_UNIT1",10,33.6]
["ETIWND_2_UNIT1",11,33.6]
["ETIWND_2_UNIT1",12,33.6]
["ETIWND_6_GRPLND",1,45.64]
["ETIWND_6_GRPLND",2,45.64]
["ETIWND_6_GRPLND",3,45.64]
["ETIWND_6_GRPLND",4,45.64]
["ETIWND_6_GRPLND",5,45.64]
["ETIWND_6_GRPLND",6,45.64]
["ETIWND_6_GRPLND",7,45.64]
["ETIWND_6_GRPLND",8,45.64]
["ETIWND_6_GRPLND",9,45.64]
["ETIWND_6_GRPLND",10,45.64]
["ETIWND_6_GRPLND",11,45.64]
["ETIWND_6_GRPLND",12,45.64]
["ETIWND_6_MWDETI",1,1.26]
["ETIWND_6_MWDETI",2,2.98]
["ETIWND_6_MWDETI",3,0]
["ETIWND_6_MWDETI",4,3.5]
["ETIWND_6_MWDETI",5,4.04]
["ETIWND_6_MWDETI",6,1.85]
["ETIWND_6_MWDETI",7,3.18]
["ETIWND_6_MWDETI",8,2.4500000000000002]
["ETIWND_6_MWDETI",9,2.35]
["ETIWND_6_MWDETI",10,2.4]
["ETIWND_6_MWDETI",11,4.91]
["ETIWND_6_MWDETI",12,5.39]
["EXCHEC_7_UNIT 1",1,91.89]
["EXCHEC_7_UNIT 1",2,91.89]
["EXCHEC_7_UNIT 1",3,91.89]
["EXCHEC_7_UNIT 1",4,91.89]
["EXCHEC_7_UNIT 1",5,91.89]
["EXCHEC_7_UNIT 1",6,91.89]
["EXCHEC_7_UNIT 1",7,91.89]
["EXCHEC_7_UNIT 1",8,91.89]
["EXCHEC_7_UNIT 1",9,91.89]
["EXCHEC_7_UNIT 1",10,91.89]
["EXCHEC_7_UNIT 1",11,91.89]
["EXCHEC_7_UNIT 1",12,91.89]
["EXCLSG_1_SOLAR",1,0.24]
["EXCLSG_1_SOLAR",2,1.8]
["EXCLSG_1_SOLAR",3,2.1]
["EXCLSG_1_SOLAR",4,2.64]
["EXCLSG_1_SOLAR",5,3.84]
["EXCLSG_1_SOLAR",6,7.86]
["EXCLSG_1_SOLAR",7,8.64]
["EXCLSG_1_SOLAR",8,7.44]
["EXCLSG_1_SOLAR",9,6.66]
["EXCLSG_1_SOLAR",10,4.4400000000000004]
["EXCLSG_1_SOLAR",11,3.42]
["EXCLSG_1_SOLAR",12,2.1]
["FALBRK_6_FESBT1",6,40]
["FALBRK_6_FESBT1",7,40]
["FALBRK_6_FESBT1",8,40]
["FALBRK_6_FESBT1",9,40]
["FALBRK_6_FESBT1",10,40]
["FALBRK_6_FESBT1",11,40]
["FALBRK_6_FESBT1",12,40]
["FELLOW_7_QFUNTS",1,2.15]
["FELLOW_7_QFUNTS",2,2.0499999999999998]
["FELLOW_7_QFUNTS",3,2.09]
["FELLOW_7_QFUNTS",4,2.17]
["FELLOW_7_QFUNTS",5,2.41]
["FELLOW_7_QFUNTS",6,2.37]
["FELLOW_7_QFUNTS",7,2.2999999999999998]
["FELLOW_7_QFUNTS",8,2.2999999999999998]
["FELLOW_7_QFUNTS",9,2.4900000000000002]
["FELLOW_7_QFUNTS",10,2.56]
["FELLOW_7_QFUNTS",11,2.5]
["FELLOW_7_QFUNTS",12,2.4700000000000002]
["FIFTHS_2_FSSBT",7,137]
["FIFTHS_2_FSSBT",8,137]
["FIFTHS_2_FSSBT",9,137]
["FIFTHS_2_FSSBT",10,137]
["FIFTHS_2_FSSBT",11,137]
["FIFTHS_2_FSSBT",12,137]
["FLOWD2_2_FPLWND",1,5.91]
["FLOWD2_2_FPLWND",2,6.34]
["FLOWD2_2_FPLWND",3,5.66]
["FLOWD2_2_FPLWND",4,5.98]
["FLOWD2_2_FPLWND",5,6.18]
["FLOWD2_2_FPLWND",6,4.5599999999999996]
["FLOWD2_2_FPLWND",7,4.0599999999999996]
["FLOWD2_2_FPLWND",8,3.81]
["FLOWD2_2_FPLWND",9,3.91]
["FLOWD2_2_FPLWND",10,3.28]
["FLOWD2_2_FPLWND",11,4.1399999999999997]
["FLOWD2_2_FPLWND",12,5.29]
["FLOWD_2_RT2WD2",1,4.84]
["FLOWD_2_RT2WD2",2,5.15]
["FLOWD_2_RT2WD2",3,4.5199999999999996]
["FLOWD_2_RT2WD2",4,4.33]
["FLOWD_2_RT2WD2",5,4.6100000000000003]
["FLOWD_2_RT2WD2",6,4.22]
["FLOWD_2_RT2WD2",7,3.92]
["FLOWD_2_RT2WD2",8,2.98]
["FLOWD_2_RT2WD2",9,3.08]
["FLOWD_2_RT2WD2",10,2.86]
["FLOWD_2_RT2WD2",11,3.85]
["FLOWD_2_RT2WD2",12,4.66]
["FLOWD_2_WIND1",1,2.1]
["FLOWD_2_WIND1",2,2.2400000000000002]
["FLOWD_2_WIND1",3,1.97]
["FLOWD_2_WIND1",4,1.88]
["FLOWD_2_WIND1",5,2]
["FLOWD_2_WIND1",6,1.83]
["FLOWD_2_WIND1",7,1.7]
["FLOWD_2_WIND1",8,1.3]
["FLOWD_2_WIND1",9,1.34]
["FLOWD_2_WIND1",10,1.24]
["FLOWD_2_WIND1",11,1.67]
["FLOWD_2_WIND1",12,2.0299999999999998]
["FMEADO_6_HELLHL",1,0.17]
["FMEADO_6_HELLHL",2,0.16]
["FMEADO_6_HELLHL",3,0.17]
["FMEADO_6_HELLHL",4,0.2]
["FMEADO_6_HELLHL",5,0.11]
["FMEADO_6_HELLHL",6,0.34]
["FMEADO_6_HELLHL",7,0.44]
["FMEADO_6_HELLHL",8,0.41]
["FMEADO_6_HELLHL",9,0.33]
["FMEADO_6_HELLHL",10,0.35]
["FMEADO_6_HELLHL",11,0.3]
["FMEADO_6_HELLHL",12,0.27]
["FMEADO_7_UNIT",1,16]
["FMEADO_7_UNIT",2,16]
["FMEADO_7_UNIT",3,16]
["FMEADO_7_UNIT",4,16]
["FMEADO_7_UNIT",5,16]
["FMEADO_7_UNIT",6,16]
["FMEADO_7_UNIT",7,16]
["FMEADO_7_UNIT",8,16]
["FMEADO_7_UNIT",9,16]
["FMEADO_7_UNIT",10,16]
["FMEADO_7_UNIT",11,16]
["FMEADO_7_UNIT",12,16]
["FORBST_7_UNIT 1",1,37.5]
["FORBST_7_UNIT 1",2,37.5]
["FORBST_7_UNIT 1",3,37.5]
["FORBST_7_UNIT 1",4,37.5]
["FORBST_7_UNIT 1",5,37.5]
["FORBST_7_UNIT 1",6,37.5]
["FORBST_7_UNIT 1",7,37.5]
["FORBST_7_UNIT 1",8,37.5]
["FORBST_7_UNIT 1",9,37.5]
["FORBST_7_UNIT 1",10,37.5]
["FORBST_7_UNIT 1",11,37.5]
["FORBST_7_UNIT 1",12,37.5]
["FRESHW_1_SOLAR1",1,0]
["FRESHW_1_SOLAR1",2,0]
["FRESHW_1_SOLAR1",3,0]
["FRESHW_1_SOLAR1",4,0]
["FRESHW_1_SOLAR1",5,0]
["FRESHW_1_SOLAR1",6,0]
["FRESHW_1_SOLAR1",7,0]
["FRESHW_1_SOLAR1",8,0]
["FRESHW_1_SOLAR1",9,0]
["FRESHW_1_SOLAR1",10,0]
["FRESHW_1_SOLAR1",11,0]
["FRESHW_1_SOLAR1",12,0]
["FRIANT_6_UNITS",1,1.2]
["FRIANT_6_UNITS",2,5.05]
["FRIANT_6_UNITS",3,6.22]
["FRIANT_6_UNITS",4,4.67]
["FRIANT_6_UNITS",5,8.81]
["FRIANT_6_UNITS",6,15.33]
["FRIANT_6_UNITS",7,15.5]
["FRIANT_6_UNITS",8,10.48]
["FRIANT_6_UNITS",9,6.54]
["FRIANT_6_UNITS",10,4.5999999999999996]
["FRIANT_6_UNITS",11,1.86]
["FRIANT_6_UNITS",12,1.96]
["FRITO_1_LAY",1,0.14000000000000001]
["FRITO_1_LAY",2,0.19]
["FRITO_1_LAY",3,0.13]
["FRITO_1_LAY",4,0.09]
["FRITO_1_LAY",5,7.0000000000000007E-2]
["FRITO_1_LAY",6,0.08]
["FRITO_1_LAY",7,0.06]
["FRITO_1_LAY",8,7.0000000000000007E-2]
["FRITO_1_LAY",9,0.09]
["FRITO_1_LAY",10,7.0000000000000007E-2]
["FRITO_1_LAY",11,0.1]
["FRITO_1_LAY",12,0.19]
["FRNTBW_6_SOLAR1",1,0.08]
["FRNTBW_6_SOLAR1",2,0.6]
["FRNTBW_6_SOLAR1",3,0.7]
["FRNTBW_6_SOLAR1",4,0.88]
["FRNTBW_6_SOLAR1",5,1.28]
["FRNTBW_6_SOLAR1",6,2.62]
["FRNTBW_6_SOLAR1",7,2.88]
["FRNTBW_6_SOLAR1",8,2.48]
["FRNTBW_6_SOLAR1",9,2.2200000000000002]
["FRNTBW_6_SOLAR1",10,1.48]
["FRNTBW_6_SOLAR1",11,1.1399999999999999]
["FRNTBW_6_SOLAR1",12,0.7]
["FROGTN_1_UTICAA",1,0.73]
["FROGTN_1_UTICAA",2,0.85]
["FROGTN_1_UTICAA",3,0.89]
["FROGTN_1_UTICAA",4,0.78]
["FROGTN_1_UTICAA",5,0.61]
["FROGTN_1_UTICAA",6,0.52]
["FROGTN_1_UTICAA",7,0.45]
["FROGTN_1_UTICAA",8,0.37]
["FROGTN_1_UTICAA",9,0.47]
["FROGTN_1_UTICAA",10,0.48]
["FROGTN_1_UTICAA",11,0.06]
["FROGTN_1_UTICAA",12,0.81]
["FROGTN_1_UTICAM",1,1.53]
["FROGTN_1_UTICAM",2,1.77]
["FROGTN_1_UTICAM",3,2.04]
["FROGTN_1_UTICAM",4,1.75]
["FROGTN_1_UTICAM",5,1.71]
["FROGTN_1_UTICAM",6,1.7]
["FROGTN_1_UTICAM",7,1.49]
["FROGTN_1_UTICAM",8,1.51]
["FROGTN_1_UTICAM",9,1.5]
["FROGTN_1_UTICAM",10,1.24]
["FROGTN_1_UTICAM",11,0.09]
["FROGTN_1_UTICAM",12,1.65]
["FTSWRD_6_TRFORK",1,0.59]
["FTSWRD_6_TRFORK",2,0.67]
["FTSWRD_6_TRFORK",3,0.57999999999999996]
["FTSWRD_6_TRFORK",4,0.67]
["FTSWRD_6_TRFORK",5,0.56999999999999995]
["FTSWRD_6_TRFORK",6,0.37]
["FTSWRD_6_TRFORK",7,0.27]
["FTSWRD_6_TRFORK",8,0.1]
["FTSWRD_6_TRFORK",9,0.19]
["FTSWRD_6_TRFORK",10,0.1]
["FTSWRD_6_TRFORK",11,0.12]
["FTSWRD_6_TRFORK",12,0.16]
["FTSWRD_7_QFUNTS",1,0]
["FTSWRD_7_QFUNTS",2,0]
["FTSWRD_7_QFUNTS",3,0]
["FTSWRD_7_QFUNTS",4,0]
["FTSWRD_7_QFUNTS",5,0]
["FTSWRD_7_QFUNTS",6,0]
["FTSWRD_7_QFUNTS",7,0]
["FTSWRD_7_QFUNTS",8,0]
["FTSWRD_7_QFUNTS",9,0]
["FTSWRD_7_QFUNTS",10,0]
["FTSWRD_7_QFUNTS",11,0]
["FTSWRD_7_QFUNTS",12,0]
["FULTON_1_QF",1,0.13]
["FULTON_1_QF",2,0.12]
["FULTON_1_QF",3,0.11]
["FULTON_1_QF",4,0.14000000000000001]
["FULTON_1_QF",5,0.13]
["FULTON_1_QF",6,0.1]
["FULTON_1_QF",7,7.0000000000000007E-2]
["FULTON_1_QF",8,0.04]
["FULTON_1_QF",9,0.05]
["FULTON_1_QF",10,0.06]
["FULTON_1_QF",11,7.0000000000000007E-2]
["FULTON_1_QF",12,0.1]
["GALE_1_SR3SR3",1,0.06]
["GALE_1_SR3SR3",2,0.41]
["GALE_1_SR3SR3",3,0.48]
["GALE_1_SR3SR3",4,0.61]
["GALE_1_SR3SR3",5,0.88]
["GALE_1_SR3SR3",6,1.81]
["GALE_1_SR3SR3",7,1.99]
["GALE_1_SR3SR3",8,1.71]
["GALE_1_SR3SR3",9,1.53]
["GALE_1_SR3SR3",10,1.02]
["GALE_1_SR3SR3",11,0.79]
["GALE_1_SR3SR3",12,0.48]
["GANSO_1_WSTBM1",1,0]
["GANSO_1_WSTBM1",2,0]
["GANSO_1_WSTBM1",3,0]
["GANSO_1_WSTBM1",4,0]
["GANSO_1_WSTBM1",5,0]
["GANSO_1_WSTBM1",6,0]
["GANSO_1_WSTBM1",7,0]
["GANSO_1_WSTBM1",8,0]
["GANSO_1_WSTBM1",9,0]
["GANSO_1_WSTBM1",10,0]
["GANSO_1_WSTBM1",11,0]
["GANSO_1_WSTBM1",12,0]
["GARLND_2_GARBT1",1,88]
["GARLND_2_GARBT1",2,88]
["GARLND_2_GARBT1",3,88]
["GARLND_2_GARBT1",4,88]
["GARLND_2_GARBT1",5,88]
["GARLND_2_GARBT1",6,88]
["GARLND_2_GARBT1",7,88]
["GARLND_2_GARBT1",8,88]
["GARLND_2_GARBT1",9,88]
["GARLND_2_GARBT1",10,88]
["GARLND_2_GARBT1",11,88]
["GARLND_2_GARBT1",12,88]
["GARLND_2_GASLR",1,0.38]
["GARLND_2_GASLR",2,3.26]
["GARLND_2_GASLR",3,3.89]
["GARLND_2_GASLR",4,5.09]
["GARLND_2_GASLR",5,7.65]
["GARLND_2_GASLR",6,16.82]
["GARLND_2_GASLR",7,18.7]
["GARLND_2_GASLR",8,15.85]
["GARLND_2_GASLR",9,13.56]
["GARLND_2_GASLR",10,8.39]
["GARLND_2_GASLR",11,5.79]
["GARLND_2_GASLR",12,2.92]
["GARLND_2_GASLRA",1,0.08]
["GARLND_2_GASLRA",2,0.6]
["GARLND_2_GASLRA",3,0.7]
["GARLND_2_GASLRA",4,0.88]
["GARLND_2_GASLRA",5,1.28]
["GARLND_2_GASLRA",6,2.62]
["GARLND_2_GASLRA",7,2.88]
["GARLND_2_GASLRA",8,2.48]
["GARLND_2_GASLRA",9,2.2200000000000002]
["GARLND_2_GASLRA",10,1.48]
["GARLND_2_GASLRA",11,1.1399999999999999]
["GARLND_2_GASLRA",12,0.7]
["GARNET_1_SOLAR",1,0]
["GARNET_1_SOLAR",2,0]
["GARNET_1_SOLAR",3,0]
["GARNET_1_SOLAR",4,0]
["GARNET_1_SOLAR",5,0]
["GARNET_1_SOLAR",6,0]
["GARNET_1_SOLAR",7,0]
["GARNET_1_SOLAR",8,0]
["GARNET_1_SOLAR",9,0]
["GARNET_1_SOLAR",10,0]
["GARNET_1_SOLAR",11,0]
["GARNET_1_SOLAR",12,0]
["GARNET_1_SOLAR2",1,0.02]
["GARNET_1_SOLAR2",2,0.12]
["GARNET_1_SOLAR2",3,0.14000000000000001]
["GARNET_1_SOLAR2",4,0.18]
["GARNET_1_SOLAR2",5,0.26]
["GARNET_1_SOLAR2",6,0.52]
["GARNET_1_SOLAR2",7,0.57999999999999996]
["GARNET_1_SOLAR2",8,0.5]
["GARNET_1_SOLAR2",9,0.44]
["GARNET_1_SOLAR2",10,0.3]
["GARNET_1_SOLAR2",11,0.23]
["GARNET_1_SOLAR2",12,0.14000000000000001]
["GARNET_1_WIND",1,1.1499999999999999]
["GARNET_1_WIND",2,1.22]
["GARNET_1_WIND",3,1.07]
["GARNET_1_WIND",4,1.03]
["GARNET_1_WIND",5,1.0900000000000001]
["GARNET_1_WIND",6,1]
["GARNET_1_WIND",7,0.93]
["GARNET_1_WIND",8,0.71]
["GARNET_1_WIND",9,0.73]
["GARNET_1_WIND",10,0.68]
["GARNET_1_WIND",11,0.91]
["GARNET_1_WIND",12,1.1100000000000001]
["GARNET_1_WINDS",1,3.98]
["GARNET_1_WINDS",2,4.2300000000000004]
["GARNET_1_WINDS",3,3.72]
["GARNET_1_WINDS",4,3.56]
["GARNET_1_WINDS",5,3.79]
["GARNET_1_WINDS",6,3.47]
["GARNET_1_WINDS",7,3.22]
["GARNET_1_WINDS",8,2.4500000000000002]
["GARNET_1_WINDS",9,2.5299999999999998]
["GARNET_1_WINDS",10,2.35]
["GARNET_1_WINDS",11,3.16]
["GARNET_1_WINDS",12,3.83]
["GARNET_1_WT3WND",1,0]
["GARNET_1_WT3WND",2,0]
["GARNET_1_WT3WND",3,0]
["GARNET_1_WT3WND",4,0]
["GARNET_1_WT3WND",5,0]
["GARNET_1_WT3WND",6,0]
["GARNET_1_WT3WND",7,0]
["GARNET_1_WT3WND",8,0]
["GARNET_1_WT3WND",9,0]
["GARNET_1_WT3WND",10,0]
["GARNET_1_WT3WND",11,0]
["GARNET_1_WT3WND",12,0]
["GARNET_2_COAWD2",1,1.91]
["GARNET_2_COAWD2",2,2.0299999999999998]
["GARNET_2_COAWD2",3,1.78]
["GARNET_2_COAWD2",4,1.71]
["GARNET_2_COAWD2",5,1.82]
["GARNET_2_COAWD2",6,1.67]
["GARNET_2_COAWD2",7,1.55]
["GARNET_2_COAWD2",8,1.18]
["GARNET_2_COAWD2",9,1.21]
["GARNET_2_COAWD2",10,1.1299999999999999]
["GARNET_2_COAWD2",11,1.52]
["GARNET_2_COAWD2",12,1.84]
["GARNET_2_HYDRO",1,0.09]
["GARNET_2_HYDRO",2,0]
["GARNET_2_HYDRO",3,0]
["GARNET_2_HYDRO",4,0.15]
["GARNET_2_HYDRO",5,0.28999999999999998]
["GARNET_2_HYDRO",6,0.27]
["GARNET_2_HYDRO",7,0.31]
["GARNET_2_HYDRO",8,0.3]
["GARNET_2_HYDRO",9,0.31]
["GARNET_2_HYDRO",10,0.46]
["GARNET_2_HYDRO",11,0.24]
["GARNET_2_HYDRO",12,0.42]
["GARNET_2_WIND1",1,1.98]
["GARNET_2_WIND1",2,2.1]
["GARNET_2_WIND1",3,1.85]
["GARNET_2_WIND1",4,1.77]
["GARNET_2_WIND1",5,1.88]
["GARNET_2_WIND1",6,1.73]
["GARNET_2_WIND1",7,1.6]
["GARNET_2_WIND1",8,1.22]
["GARNET_2_WIND1",9,1.26]
["GARNET_2_WIND1",10,1.17]
["GARNET_2_WIND1",11,1.57]
["GARNET_2_WIND1",12,1.91]
["GARNET_2_WIND2",1,2.0699999999999998]
["GARNET_2_WIND2",2,2.2000000000000002]
["GARNET_2_WIND2",3,1.93]
["GARNET_2_WIND2",4,1.85]
["GARNET_2_WIND2",5,1.97]
["GARNET_2_WIND2",6,1.8]
["GARNET_2_WIND2",7,1.68]
["GARNET_2_WIND2",8,1.27]
["GARNET_2_WIND2",9,1.32]
["GARNET_2_WIND2",10,1.22]
["GARNET_2_WIND2",11,1.64]
["GARNET_2_WIND2",12,1.99]
["GARNET_2_WIND3",1,2.23]
["GARNET_2_WIND3",2,2.37]
["GARNET_2_WIND3",3,2.08]
["GARNET_2_WIND3",4,1.99]
["GARNET_2_WIND3",5,2.12]
["GARNET_2_WIND3",6,1.94]
["GARNET_2_WIND3",7,1.81]
["GARNET_2_WIND3",8,1.37]
["GARNET_2_WIND3",9,1.42]
["GARNET_2_WIND3",10,1.31]
["GARNET_2_WIND3",11,1.77]
["GARNET_2_WIND3",12,2.15]
["GARNET_2_WIND4",1,1.73]
["GARNET_2_WIND4",2,1.84]
["GARNET_2_WIND4",3,1.62]
["GARNET_2_WIND4",4,1.55]
["GARNET_2_WIND4",5,1.65]
["GARNET_2_WIND4",6,1.51]
["GARNET_2_WIND4",7,1.4]
["GARNET_2_WIND4",8,1.07]
["GARNET_2_WIND4",9,1.1000000000000001]
["GARNET_2_WIND4",10,1.02]
["GARNET_2_WIND4",11,1.38]
["GARNET_2_WIND4",12,1.67]
["GARNET_2_WIND5",1,0.53]
["GARNET_2_WIND5",2,0.56000000000000005]
["GARNET_2_WIND5",3,0.5]
["GARNET_2_WIND5",4,0.47]
["GARNET_2_WIND5",5,0.5]
["GARNET_2_WIND5",6,0.46]
["GARNET_2_WIND5",7,0.43]
["GARNET_2_WIND5",8,0.33]
["GARNET_2_WIND5",9,0.34]
["GARNET_2_WIND5",10,0.31]
["GARNET_2_WIND5",11,0.42]
["GARNET_2_WIND5",12,0.51]
["GASKW1_2_GW1SR1",1,0.08]
["GASKW1_2_GW1SR1",2,0.6]
["GASKW1_2_GW1SR1",3,0.7]
["GASKW1_2_GW1SR1",4,0.88]
["GASKW1_2_GW1SR1",5,1.28]
["GASKW1_2_GW1SR1",6,2.62]
["GASKW1_2_GW1SR1",7,2.88]
["GASKW1_2_GW1SR1",8,2.48]
["GASKW1_2_GW1SR1",9,2.2200000000000002]
["GASKW1_2_GW1SR1",10,1.48]
["GASKW1_2_GW1SR1",11,1.1399999999999999]
["GASKW1_2_GW1SR1",12,0.7]
["GASKW1_2_GW2SR1",7,2.2999999999999998]
["GASKW1_2_GW2SR1",8,1.98]
["GASKW1_2_GW2SR1",9,1.78]
["GASKW1_2_GW2SR1",10,1.18]
["GASKW1_2_GW2SR1",11,0.91]
["GASKW1_2_GW2SR1",12,0.56000000000000005]
["GASKW1_2_GW2SR2",7,4.0999999999999996]
["GASKW1_2_GW2SR2",8,3.5]
["GASKW1_2_GW2SR2",9,3.2]
["GASKW1_2_GW2SR2",10,2.1]
["GASKW1_2_GW2SR2",11,1.6]
["GASKW1_2_GW2SR2",12,1.01]
["GASKW1_2_GW3SR1",6,2.62]
["GASKW1_2_GW3SR1",7,2.88]
["GASKW1_2_GW3SR1",8,2.48]
["GASKW1_2_GW3SR1",9,2.2200000000000002]
["GASKW1_2_GW3SR1",10,1.48]
["GASKW1_2_GW3SR1",11,1.1399999999999999]
["GASKW1_2_GW3SR1",12,0.7]
["GASKW1_2_GW4SR1",6,2.62]
["GASKW1_2_GW4SR1",7,2.88]
["GASKW1_2_GW4SR1",8,2.48]
["GASKW1_2_GW4SR1",9,2.2200000000000002]
["GASKW1_2_GW4SR1",10,1.48]
["GASKW1_2_GW4SR1",11,1.1399999999999999]
["GASKW1_2_GW4SR1",12,0.7]
["GASKW1_2_GW5SR1",6,2.62]
["GASKW1_2_GW5SR1",7,2.88]
["GASKW1_2_GW5SR1",8,2.48]
["GASKW1_2_GW5SR1",9,2.2200000000000002]
["GASKW1_2_GW5SR1",10,1.48]
["GASKW1_2_GW5SR1",11,1.1399999999999999]
["GASKW1_2_GW5SR1",12,0.7]
["GATES_2_SOLAR",1,0.08]
["GATES_2_SOLAR",2,0.6]
["GATES_2_SOLAR",3,0.7]
["GATES_2_SOLAR",4,0.88]
["GATES_2_SOLAR",5,1.28]
["GATES_2_SOLAR",6,2.62]
["GATES_2_SOLAR",7,2.88]
["GATES_2_SOLAR",8,2.48]
["GATES_2_SOLAR",9,2.2200000000000002]
["GATES_2_SOLAR",10,1.48]
["GATES_2_SOLAR",11,1.1399999999999999]
["GATES_2_SOLAR",12,0.7]
["GATES_2_WSOLAR",1,0.04]
["GATES_2_WSOLAR",2,0.3]
["GATES_2_WSOLAR",3,0.35]
["GATES_2_WSOLAR",4,0.44]
["GATES_2_WSOLAR",5,0.64]
["GATES_2_WSOLAR",6,1.31]
["GATES_2_WSOLAR",7,1.44]
["GATES_2_WSOLAR",8,1.24]
["GATES_2_WSOLAR",9,1.1100000000000001]
["GATES_2_WSOLAR",10,0.74]
["GATES_2_WSOLAR",11,0.56999999999999995]
["GATES_2_WSOLAR",12,0.35]
["GATEWY_2_GESBT1",1,175]
["GATEWY_2_GESBT1",2,175]
["GATEWY_2_GESBT1",3,175]
["GATEWY_2_GESBT1",4,175]
["GATEWY_2_GESBT1",5,175]
["GATEWY_2_GESBT1",6,175]
["GATEWY_2_GESBT1",7,175]
["GATEWY_2_GESBT1",8,175]
["GATEWY_2_GESBT1",9,175]
["GATEWY_2_GESBT1",10,175]
["GATEWY_2_GESBT1",11,175]
["GATEWY_2_GESBT1",12,175]
["GATWAY_2_PL1X3",1,551.36]
["GATWAY_2_PL1X3",2,552.25]
["GATWAY_2_PL1X3",3,547.69000000000005]
["GATWAY_2_PL1X3",4,570.70000000000005]
["GATWAY_2_PL1X3",5,542.96]
["GATWAY_2_PL1X3",6,517.12]
["GATWAY_2_PL1X3",7,511.3]
["GATWAY_2_PL1X3",8,508.85]
["GATWAY_2_PL1X3",9,511.61]
["GATWAY_2_PL1X3",10,527.41]
["GATWAY_2_PL1X3",11,536.72]
["GATWAY_2_PL1X3",12,546.73]
["GENESI_2_STG",1,0.27]
["GENESI_2_STG",2,3.93]
["GENESI_2_STG",3,5.84]
["GENESI_2_STG",4,8.4700000000000006]
["GENESI_2_STG",5,12.72]
["GENESI_2_STG",6,26.43]
["GENESI_2_STG",7,28.91]
["GENESI_2_STG",8,24.59]
["GENESI_2_STG",9,20.65]
["GENESI_2_STG",10,12.94]
["GENESI_2_STG",11,7.54]
["GENESI_2_STG",12,0.79]
["GEYS11_7_UNIT11",1,68]
["GEYS11_7_UNIT11",2,68]
["GEYS11_7_UNIT11",3,68]
["GEYS11_7_UNIT11",4,68]
["GEYS11_7_UNIT11",5,68]
["GEYS11_7_UNIT11",6,68]
["GEYS11_7_UNIT11",7,68]
["GEYS11_7_UNIT11",8,68]
["GEYS11_7_UNIT11",9,68]
["GEYS11_7_UNIT11",10,68]
["GEYS11_7_UNIT11",11,68]
["GEYS11_7_UNIT11",12,68]
["GEYS12_7_UNIT12",1,50]
["GEYS12_7_UNIT12",2,50]
["GEYS12_7_UNIT12",3,50]
["GEYS12_7_UNIT12",4,50]
["GEYS12_7_UNIT12",5,50]
["GEYS12_7_UNIT12",6,50]
["GEYS12_7_UNIT12",7,50]
["GEYS12_7_UNIT12",8,50]
["GEYS12_7_UNIT12",9,50]
["GEYS12_7_UNIT12",10,50]
["GEYS12_7_UNIT12",11,50]
["GEYS12_7_UNIT12",12,50]
["GEYS13_7_UNIT13",1,56]
["GEYS13_7_UNIT13",2,56]
["GEYS13_7_UNIT13",3,56]
["GEYS13_7_UNIT13",4,56]
["GEYS13_7_UNIT13",5,56]
["GEYS13_7_UNIT13",6,56]
["GEYS13_7_UNIT13",7,56]
["GEYS13_7_UNIT13",8,56]
["GEYS13_7_UNIT13",9,56]
["GEYS13_7_UNIT13",10,56]
["GEYS13_7_UNIT13",11,56]
["GEYS13_7_UNIT13",12,56]
["GEYS14_7_UNIT14",1,70]
["GEYS14_7_UNIT14",2,70]
["GEYS14_7_UNIT14",3,70]
["GEYS14_7_UNIT14",4,70]
["GEYS14_7_UNIT14",5,70]
["GEYS14_7_UNIT14",6,70]
["GEYS14_7_UNIT14",7,70]
["GEYS14_7_UNIT14",8,70]
["GEYS14_7_UNIT14",9,70]
["GEYS14_7_UNIT14",10,70]
["GEYS14_7_UNIT14",11,70]
["GEYS14_7_UNIT14",12,70]
["GEYS16_7_UNIT16",1,63]
["GEYS16_7_UNIT16",2,63]
["GEYS16_7_UNIT16",3,63]
["GEYS16_7_UNIT16",4,63]
["GEYS16_7_UNIT16",5,63]
["GEYS16_7_UNIT16",6,63]
["GEYS16_7_UNIT16",7,63]
["GEYS16_7_UNIT16",8,63]
["GEYS16_7_UNIT16",9,63]
["GEYS16_7_UNIT16",10,63]
["GEYS16_7_UNIT16",11,63]
["GEYS16_7_UNIT16",12,63]
["GEYS17_7_UNIT17",1,75.5]
["GEYS17_7_UNIT17",2,75.5]
["GEYS17_7_UNIT17",3,75.5]
["GEYS17_7_UNIT17",4,75.5]
["GEYS17_7_UNIT17",5,75.5]
["GEYS17_7_UNIT17",6,75.5]
["GEYS17_7_UNIT17",7,75.5]
["GEYS17_7_UNIT17",8,75.5]
["GEYS17_7_UNIT17",9,75.5]
["GEYS17_7_UNIT17",10,75.5]
["GEYS17_7_UNIT17",11,75.5]
["GEYS17_7_UNIT17",12,75.5]
["GEYS18_7_UNIT18",1,72]
["GEYS18_7_UNIT18",2,72]
["GEYS18_7_UNIT18",3,72]
["GEYS18_7_UNIT18",4,72]
["GEYS18_7_UNIT18",5,72]
["GEYS18_7_UNIT18",6,72]
["GEYS18_7_UNIT18",7,72]
["GEYS18_7_UNIT18",8,72]
["GEYS18_7_UNIT18",9,72]
["GEYS18_7_UNIT18",10,72]
["GEYS18_7_UNIT18",11,72]
["GEYS18_7_UNIT18",12,72]
["GEYS20_7_UNIT20",1,50]
["GEYS20_7_UNIT20",2,50]
["GEYS20_7_UNIT20",3,50]
["GEYS20_7_UNIT20",4,50]
["GEYS20_7_UNIT20",5,50]
["GEYS20_7_UNIT20",6,50]
["GEYS20_7_UNIT20",7,50]
["GEYS20_7_UNIT20",8,50]
["GEYS20_7_UNIT20",9,50]
["GEYS20_7_UNIT20",10,50]
["GEYS20_7_UNIT20",11,50]
["GEYS20_7_UNIT20",12,50]
["GIFENS_6_BUGSL1",1,0.08]
["GIFENS_6_BUGSL1",2,0.6]
["GIFENS_6_BUGSL1",3,0.7]
["GIFENS_6_BUGSL1",4,0.88]
["GIFENS_6_BUGSL1",5,1.28]
["GIFENS_6_BUGSL1",6,2.62]
["GIFENS_6_BUGSL1",7,2.88]
["GIFENS_6_BUGSL1",8,2.48]
["GIFENS_6_BUGSL1",9,2.2200000000000002]
["GIFENS_6_BUGSL1",10,1.48]
["GIFENS_6_BUGSL1",11,1.1399999999999999]
["GIFENS_6_BUGSL1",12,0.7]
["GIFFEN_6_SOLAR",1,0.04]
["GIFFEN_6_SOLAR",2,0.3]
["GIFFEN_6_SOLAR",3,0.35]
["GIFFEN_6_SOLAR",4,0.44]
["GIFFEN_6_SOLAR",5,0.64]
["GIFFEN_6_SOLAR",6,1.31]
["GIFFEN_6_SOLAR",7,1.44]
["GIFFEN_6_SOLAR",8,1.24]
["GIFFEN_6_SOLAR",9,1.1100000000000001]
["GIFFEN_6_SOLAR",10,0.74]
["GIFFEN_6_SOLAR",11,0.56999999999999995]
["GIFFEN_6_SOLAR",12,0.35]
["GIFFEN_6_SOLAR1",1,0]
["GIFFEN_6_SOLAR1",2,0]
["GIFFEN_6_SOLAR1",3,0]
["GIFFEN_6_SOLAR1",4,0]
["GIFFEN_6_SOLAR1",5,0]
["GIFFEN_6_SOLAR1",6,0]
["GIFFEN_6_SOLAR1",7,0]
["GIFFEN_6_SOLAR1",8,0]
["GIFFEN_6_SOLAR1",9,0]
["GIFFEN_6_SOLAR1",10,0]
["GIFFEN_6_SOLAR1",11,0]
["GIFFEN_6_SOLAR1",12,0]
["GILROY_1_UNIT",1,120]
["GILROY_1_UNIT",2,120]
["GILROY_1_UNIT",3,120]
["GILROY_1_UNIT",4,120]
["GILROY_1_UNIT",5,115]
["GILROY_1_UNIT",6,115]
["GILROY_1_UNIT",7,115]
["GILROY_1_UNIT",8,115]
["GILROY_1_UNIT",9,115]
["GILROY_1_UNIT",10,120]
["GILROY_1_UNIT",11,120]
["GILROY_1_UNIT",12,120]
["GILRPP_1_PL1X2",1,95.2]
["GILRPP_1_PL1X2",2,95.2]
["GILRPP_1_PL1X2",3,95.2]
["GILRPP_1_PL1X2",4,95.2]
["GILRPP_1_PL1X2",5,95.2]
["GILRPP_1_PL1X2",6,95.2]
["GILRPP_1_PL1X2",7,95.2]
["GILRPP_1_PL1X2",8,95.2]
["GILRPP_1_PL1X2",9,95.2]
["GILRPP_1_PL1X2",10,95.2]
["GILRPP_1_PL1X2",11,95.2]
["GILRPP_1_PL1X2",12,95.2]
["GILRPP_1_PL3X4",1,46.2]
["GILRPP_1_PL3X4",2,46.2]
["GILRPP_1_PL3X4",3,46.2]
["GILRPP_1_PL3X4",4,46.2]
["GILRPP_1_PL3X4",5,46.2]
["GILRPP_1_PL3X4",6,46.2]
["GILRPP_1_PL3X4",7,46.2]
["GILRPP_1_PL3X4",8,46.2]
["GILRPP_1_PL3X4",9,46.2]
["GILRPP_1_PL3X4",10,46.2]
["GILRPP_1_PL3X4",11,46.2]
["GILRPP_1_PL3X4",12,46.2]
["GLDFGR_6_SOLAR1",1,0.08]
["GLDFGR_6_SOLAR1",2,0.6]
["GLDFGR_6_SOLAR1",3,0.7]
["GLDFGR_6_SOLAR1",4,0.88]
["GLDFGR_6_SOLAR1",5,1.28]
["GLDFGR_6_SOLAR1",6,2.62]
["GLDFGR_6_SOLAR1",7,2.88]
["GLDFGR_6_SOLAR1",8,2.48]
["GLDFGR_6_SOLAR1",9,2.2200000000000002]
["GLDFGR_6_SOLAR1",10,1.48]
["GLDFGR_6_SOLAR1",11,1.1399999999999999]
["GLDFGR_6_SOLAR1",12,0.7]
["GLDFGR_6_SOLAR2",1,0.05]
["GLDFGR_6_SOLAR2",2,0.34]
["GLDFGR_6_SOLAR2",3,0.4]
["GLDFGR_6_SOLAR2",4,0.5]
["GLDFGR_6_SOLAR2",5,0.73]
["GLDFGR_6_SOLAR2",6,1.49]
["GLDFGR_6_SOLAR2",7,1.64]
["GLDFGR_6_SOLAR2",8,1.41]
["GLDFGR_6_SOLAR2",9,1.27]
["GLDFGR_6_SOLAR2",10,0.84]
["GLDFGR_6_SOLAR2",11,0.65]
["GLDFGR_6_SOLAR2",12,0.4]
["GLDTWN_6_COLUM3",1,0.04]
["GLDTWN_6_COLUM3",2,0.3]
["GLDTWN_6_COLUM3",3,0.35]
["GLDTWN_6_COLUM3",4,0.44]
["GLDTWN_6_COLUM3",5,0.64]
["GLDTWN_6_COLUM3",6,1.31]
["GLDTWN_6_COLUM3",7,1.44]
["GLDTWN_6_COLUM3",8,1.24]
["GLDTWN_6_COLUM3",9,1.1100000000000001]
["GLDTWN_6_COLUM3",10,0.74]
["GLDTWN_6_COLUM3",11,0.56999999999999995]
["GLDTWN_6_COLUM3",12,0.35]
["GLDTWN_6_SOLAR",1,0.02]
["GLDTWN_6_SOLAR",2,0.15]
["GLDTWN_6_SOLAR",3,0.18]
["GLDTWN_6_SOLAR",4,0.22]
["GLDTWN_6_SOLAR",5,0.32]
["GLDTWN_6_SOLAR",6,0.66]
["GLDTWN_6_SOLAR",7,0.72]
["GLDTWN_6_SOLAR",8,0.62]
["GLDTWN_6_SOLAR",9,0.56000000000000005]
["GLDTWN_6_SOLAR",10,0.37]
["GLDTWN_6_SOLAR",11,0.28999999999999998]
["GLDTWN_6_SOLAR",12,0.18]
["GLNARM_2_UNIT 5",1,65]
["GLNARM_2_UNIT 5",2,65]
["GLNARM_2_UNIT 5",3,65]
["GLNARM_2_UNIT 5",4,65]
["GLNARM_2_UNIT 5",5,65]
["GLNARM_2_UNIT 5",6,65]
["GLNARM_2_UNIT 5",7,65]
["GLNARM_2_UNIT 5",8,65]
["GLNARM_2_UNIT 5",9,65]
["GLNARM_2_UNIT 5",10,65]
["GLNARM_2_UNIT 5",11,65]
["GLNARM_2_UNIT 5",12,65]
["GLNARM_7_UNIT 1",1,22.13]
["GLNARM_7_UNIT 1",2,22.13]
["GLNARM_7_UNIT 1",3,22.13]
["GLNARM_7_UNIT 1",4,22.13]
["GLNARM_7_UNIT 1",5,22.13]
["GLNARM_7_UNIT 1",6,22.13]
["GLNARM_7_UNIT 1",7,22.13]
["GLNARM_7_UNIT 1",8,22.13]
["GLNARM_7_UNIT 1",9,22.13]
["GLNARM_7_UNIT 1",10,22.13]
["GLNARM_7_UNIT 1",11,22.13]
["GLNARM_7_UNIT 1",12,22.13]
["GLNARM_7_UNIT 2",1,22.38]
["GLNARM_7_UNIT 2",2,22.38]
["GLNARM_7_UNIT 2",3,22.38]
["GLNARM_7_UNIT 2",4,22.38]
["GLNARM_7_UNIT 2",5,22.38]
["GLNARM_7_UNIT 2",6,22.38]
["GLNARM_7_UNIT 2",7,22.38]
["GLNARM_7_UNIT 2",8,22.38]
["GLNARM_7_UNIT 2",9,22.38]
["GLNARM_7_UNIT 2",10,22.38]
["GLNARM_7_UNIT 2",11,22.38]
["GLNARM_7_UNIT 2",12,22.38]
["GLNARM_7_UNIT 3",1,44.83]
["GLNARM_7_UNIT 3",2,44.83]
["GLNARM_7_UNIT 3",3,44.83]
["GLNARM_7_UNIT 3",4,44.83]
["GLNARM_7_UNIT 3",5,44.83]
["GLNARM_7_UNIT 3",6,44.83]
["GLNARM_7_UNIT 3",7,44.83]
["GLNARM_7_UNIT 3",8,44.83]
["GLNARM_7_UNIT 3",9,44.83]
["GLNARM_7_UNIT 3",10,44.83]
["GLNARM_7_UNIT 3",11,44.83]
["GLNARM_7_UNIT 3",12,44.83]
["GLNARM_7_UNIT 4",1,42.42]
["GLNARM_7_UNIT 4",2,42.42]
["GLNARM_7_UNIT 4",3,42.42]
["GLNARM_7_UNIT 4",4,42.42]
["GLNARM_7_UNIT 4",5,42.42]
["GLNARM_7_UNIT 4",6,42.42]
["GLNARM_7_UNIT 4",7,42.42]
["GLNARM_7_UNIT 4",8,42.42]
["GLNARM_7_UNIT 4",9,42.42]
["GLNARM_7_UNIT 4",10,42.42]
["GLNARM_7_UNIT 4",11,42.42]
["GLNARM_7_UNIT 4",12,42.42]
["GLOW_6_SOLAR",1,0]
["GLOW_6_SOLAR",2,0]
["GLOW_6_SOLAR",3,0]
["GLOW_6_SOLAR",4,0]
["GLOW_6_SOLAR",5,0]
["GLOW_6_SOLAR",6,0]
["GLOW_6_SOLAR",7,0]
["GLOW_6_SOLAR",8,0]
["GLOW_6_SOLAR",9,0]
["GLOW_6_SOLAR",10,0]
["GLOW_6_SOLAR",11,0]
["GLOW_6_SOLAR",12,0]
["GOLETA_2_QF",1,0.03]
["GOLETA_2_QF",2,0.03]
["GOLETA_2_QF",3,0.02]
["GOLETA_2_QF",4,0.05]
["GOLETA_2_QF",5,0.06]
["GOLETA_2_QF",6,0.08]
["GOLETA_2_QF",7,0.1]
["GOLETA_2_QF",8,0.1]
["GOLETA_2_QF",9,0.12]
["GOLETA_2_QF",10,0.1]
["GOLETA_2_QF",11,0.05]
["GOLETA_2_QF",12,0.04]
["GOLETA_2_VALBT1",1,10]
["GOLETA_2_VALBT1",2,10]
["GOLETA_2_VALBT1",3,10]
["GOLETA_2_VALBT1",4,10]
["GOLETA_2_VALBT1",5,10]
["GOLETA_2_VALBT1",6,10]
["GOLETA_2_VALBT1",7,10]
["GOLETA_2_VALBT1",8,10]
["GOLETA_2_VALBT1",9,10]
["GOLETA_2_VALBT1",10,10]
["GOLETA_2_VALBT1",11,10]
["GOLETA_2_VALBT1",12,10]
["GOLETA_6_ELLWOD",1,54]
["GOLETA_6_ELLWOD",2,54]
["GOLETA_6_ELLWOD",3,54]
["GOLETA_6_ELLWOD",4,54]
["GOLETA_6_ELLWOD",5,54]
["GOLETA_6_ELLWOD",6,54]
["GOLETA_6_ELLWOD",7,54]
["GOLETA_6_ELLWOD",8,54]
["GOLETA_6_ELLWOD",9,54]
["GOLETA_6_ELLWOD",10,54]
["GOLETA_6_ELLWOD",11,54]
["GOLETA_6_ELLWOD",12,54]
["GOLETA_6_EXGEN",1,0]
["GOLETA_6_EXGEN",2,0]
["GOLETA_6_EXGEN",3,0]
["GOLETA_6_EXGEN",4,0]
["GOLETA_6_EXGEN",5,0]
["GOLETA_6_EXGEN",6,0]
["GOLETA_6_EXGEN",7,0]
["GOLETA_6_EXGEN",8,0]
["GOLETA_6_EXGEN",9,0]
["GOLETA_6_EXGEN",10,0]
["GOLETA_6_EXGEN",11,0]
["GOLETA_6_EXGEN",12,0]
["GONZLS_6_UNIT",1,1.42]
["GONZLS_6_UNIT",2,1.41]
["GONZLS_6_UNIT",3,1.42]
["GONZLS_6_UNIT",4,1.35]
["GONZLS_6_UNIT",5,1.37]
["GONZLS_6_UNIT",6,1.41]
["GONZLS_6_UNIT",7,1.41]
["GONZLS_6_UNIT",8,1.42]
["GONZLS_6_UNIT",9,1.34]
["GONZLS_6_UNIT",10,1.42]
["GONZLS_6_UNIT",11,1.42]
["GONZLS_6_UNIT",12,1.4]
["GOOSLK_1_SOLAR1",1,0.05]
["GOOSLK_1_SOLAR1",2,0.36]
["GOOSLK_1_SOLAR1",3,0.42]
["GOOSLK_1_SOLAR1",4,0.53]
["GOOSLK_1_SOLAR1",5,0.77]
["GOOSLK_1_SOLAR1",6,1.57]
["GOOSLK_1_SOLAR1",7,1.73]
["GOOSLK_1_SOLAR1",8,1.49]
["GOOSLK_1_SOLAR1",9,1.33]
["GOOSLK_1_SOLAR1",10,0.89]
["GOOSLK_1_SOLAR1",11,0.68]
["GOOSLK_1_SOLAR1",12,0.42]
["GRIDLY_6_SOLAR",1,0]
["GRIDLY_6_SOLAR",2,0]
["GRIDLY_6_SOLAR",3,0]
["GRIDLY_6_SOLAR",4,0]
["GRIDLY_6_SOLAR",5,0]
["GRIDLY_6_SOLAR",6,0]
["GRIDLY_6_SOLAR",7,0]
["GRIDLY_6_SOLAR",8,0]
["GRIDLY_6_SOLAR",9,0]
["GRIDLY_6_SOLAR",10,0]
["GRIDLY_6_SOLAR",11,0]
["GRIDLY_6_SOLAR",12,0]
["GRIZLY_1_UNIT 1",1,20]
["GRIZLY_1_UNIT 1",2,20]
["GRIZLY_1_UNIT 1",3,20]
["GRIZLY_1_UNIT 1",4,20]
["GRIZLY_1_UNIT 1",5,20]
["GRIZLY_1_UNIT 1",6,20]
["GRIZLY_1_UNIT 1",7,20]
["GRIZLY_1_UNIT 1",8,20]
["GRIZLY_1_UNIT 1",9,20]
["GRIZLY_1_UNIT 1",10,20]
["GRIZLY_1_UNIT 1",11,20]
["GRIZLY_1_UNIT 1",12,20]
["GRNLF2_1_UNIT",1,49.2]
["GRNLF2_1_UNIT",2,49.2]
["GRNLF2_1_UNIT",3,49.2]
["GRNLF2_1_UNIT",4,49.2]
["GRNLF2_1_UNIT",5,49.2]
["GRNLF2_1_UNIT",6,49.2]
["GRNLF2_1_UNIT",7,49.2]
["GRNLF2_1_UNIT",8,49.2]
["GRNLF2_1_UNIT",9,49.2]
["GRNLF2_1_UNIT",10,49.2]
["GRNLF2_1_UNIT",11,49.2]
["GRNLF2_1_UNIT",12,49.2]
["GRNVLY_7_SCLAND",1,2.92]
["GRNVLY_7_SCLAND",2,2.59]
["GRNVLY_7_SCLAND",3,2.92]
["GRNVLY_7_SCLAND",4,2.94]
["GRNVLY_7_SCLAND",5,2.97]
["GRNVLY_7_SCLAND",6,2.99]
["GRNVLY_7_SCLAND",7,2.69]
["GRNVLY_7_SCLAND",8,2.91]
["GRNVLY_7_SCLAND",9,2.92]
["GRNVLY_7_SCLAND",10,2.93]
["GRNVLY_7_SCLAND",11,3]
["GRNVLY_7_SCLAND",12,3.01]
["GRSCRK_6_BGCKWW",1,1.03]
["GRSCRK_6_BGCKWW",2,1.45]
["GRSCRK_6_BGCKWW",3,1.57]
["GRSCRK_6_BGCKWW",4,1.85]
["GRSCRK_6_BGCKWW",5,1.21]
["GRSCRK_6_BGCKWW",6,0.23]
["GRSCRK_6_BGCKWW",7,0]
["GRSCRK_6_BGCKWW",8,0]
["GRSCRK_6_BGCKWW",9,0]
["GRSCRK_6_BGCKWW",10,0]
["GRSCRK_6_BGCKWW",11,0]
["GRSCRK_6_BGCKWW",12,0]
["GRZZLY_1_BERKLY",1,0.43]
["GRZZLY_1_BERKLY",2,7.78]
["GRZZLY_1_BERKLY",3,0.23]
["GRZZLY_1_BERKLY",4,2.97]
["GRZZLY_1_BERKLY",5,0.91]
["GRZZLY_1_BERKLY",6,0.66]
["GRZZLY_1_BERKLY",7,0.55000000000000004]
["GRZZLY_1_BERKLY",8,0.5]
["GRZZLY_1_BERKLY",9,0.14000000000000001]
["GRZZLY_1_BERKLY",10,0.16]
["GRZZLY_1_BERKLY",11,0.26]
["GRZZLY_1_BERKLY",12,0.2]
["GUERNS_6_HD3BM3",1,0]
["GUERNS_6_HD3BM3",2,0]
["GUERNS_6_HD3BM3",3,0]
["GUERNS_6_HD3BM3",4,0]
["GUERNS_6_HD3BM3",5,0]
["GUERNS_6_HD3BM3",6,0]
["GUERNS_6_HD3BM3",7,0]
["GUERNS_6_HD3BM3",8,0]
["GUERNS_6_HD3BM3",9,0]
["GUERNS_6_HD3BM3",10,0]
["GUERNS_6_HD3BM3",11,0]
["GUERNS_6_HD3BM3",12,0]
["GUERNS_6_SOLAR",1,0.08]
["GUERNS_6_SOLAR",2,0.6]
["GUERNS_6_SOLAR",3,0.7]
["GUERNS_6_SOLAR",4,0.88]
["GUERNS_6_SOLAR",5,1.28]
["GUERNS_6_SOLAR",6,2.62]
["GUERNS_6_SOLAR",7,2.88]
["GUERNS_6_SOLAR",8,2.48]
["GUERNS_6_SOLAR",9,2.2200000000000002]
["GUERNS_6_SOLAR",10,1.48]
["GUERNS_6_SOLAR",11,1.1399999999999999]
["GUERNS_6_SOLAR",12,0.7]
["GUERNS_6_VH2BM1",1,0]
["GUERNS_6_VH2BM1",2,0]
["GUERNS_6_VH2BM1",3,0]
["GUERNS_6_VH2BM1",4,0]
["GUERNS_6_VH2BM1",5,0]
["GUERNS_6_VH2BM1",6,0]
["GUERNS_6_VH2BM1",7,0]
["GUERNS_6_VH2BM1",8,0]
["GUERNS_6_VH2BM1",9,0]
["GUERNS_6_VH2BM1",10,0]
["GUERNS_6_VH2BM1",11,0]
["GUERNS_6_VH2BM1",12,0]
["GWFPWR_1_UNITS",1,98.46]
["GWFPWR_1_UNITS",2,98.46]
["GWFPWR_1_UNITS",3,98.46]
["GWFPWR_1_UNITS",4,98.46]
["GWFPWR_1_UNITS",5,98.46]
["GWFPWR_1_UNITS",6,98.46]
["GWFPWR_1_UNITS",7,98.46]
["GWFPWR_1_UNITS",8,98.46]
["GWFPWR_1_UNITS",9,98.46]
["GWFPWR_1_UNITS",10,98.46]
["GWFPWR_1_UNITS",11,98.46]
["GWFPWR_1_UNITS",12,98.46]
["GYS5X6_7_UNITS",1,85]
["GYS5X6_7_UNITS",2,85]
["GYS5X6_7_UNITS",3,85]
["GYS5X6_7_UNITS",4,85]
["GYS5X6_7_UNITS",5,85]
["GYS5X6_7_UNITS",6,85]
["GYS5X6_7_UNITS",7,85]
["GYS5X6_7_UNITS",8,85]
["GYS5X6_7_UNITS",9,85]
["GYS5X6_7_UNITS",10,85]
["GYS5X6_7_UNITS",11,85]
["GYS5X6_7_UNITS",12,85]
["GYS7X8_7_UNITS",1,95.8]
["GYS7X8_7_UNITS",2,95.8]
["GYS7X8_7_UNITS",3,95.8]
["GYS7X8_7_UNITS",4,95.8]
["GYS7X8_7_UNITS",5,95.8]
["GYS7X8_7_UNITS",6,95.8]
["GYS7X8_7_UNITS",7,95.8]
["GYS7X8_7_UNITS",8,95.8]
["GYS7X8_7_UNITS",9,95.8]
["GYS7X8_7_UNITS",10,95.8]
["GYS7X8_7_UNITS",11,95.8]
["GYS7X8_7_UNITS",12,95.8]
["GYSRVL_7_WSPRNG",1,0]
["GYSRVL_7_WSPRNG",2,0]
["GYSRVL_7_WSPRNG",3,0]
["GYSRVL_7_WSPRNG",4,0]
["GYSRVL_7_WSPRNG",5,0]
["GYSRVL_7_WSPRNG",6,0]
["GYSRVL_7_WSPRNG",7,0]
["GYSRVL_7_WSPRNG",8,0]
["GYSRVL_7_WSPRNG",9,0]
["GYSRVL_7_WSPRNG",10,0]
["GYSRVL_7_WSPRNG",11,0]
["GYSRVL_7_WSPRNG",12,0]
["HAASPH_7_PL1X2",1,115.2]
["HAASPH_7_PL1X2",2,115.2]
["HAASPH_7_PL1X2",3,115.2]
["HAASPH_7_PL1X2",4,115.2]
["HAASPH_7_PL1X2",5,115.2]
["HAASPH_7_PL1X2",6,139.19999999999999]
["HAASPH_7_PL1X2",7,144]
["HAASPH_7_PL1X2",8,144]
["HAASPH_7_PL1X2",9,129.6]
["HAASPH_7_PL1X2",10,129.6]
["HAASPH_7_PL1X2",11,115.2]
["HAASPH_7_PL1X2",12,115.2]
["HALSEY_6_UNIT",1,1.95]
["HALSEY_6_UNIT",2,2.78]
["HALSEY_6_UNIT",3,2.75]
["HALSEY_6_UNIT",4,3.96]
["HALSEY_6_UNIT",5,4.9400000000000004]
["HALSEY_6_UNIT",6,4.54]
["HALSEY_6_UNIT",7,6]
["HALSEY_6_UNIT",8,5.22]
["HALSEY_6_UNIT",9,4.3099999999999996]
["HALSEY_6_UNIT",10,0]
["HALSEY_6_UNIT",11,0]
["HALSEY_6_UNIT",12,1.8]
["HARBGN_7_UNITS",1,100]
["HARBGN_7_UNITS",2,100]
["HARBGN_7_UNITS",3,100]
["HARBGN_7_UNITS",4,100]
["HARBGN_7_UNITS",5,100]
["HARBGN_7_UNITS",6,100]
["HARBGN_7_UNITS",7,100]
["HARBGN_7_UNITS",8,100]
["HARBGN_7_UNITS",9,100]
["HARBGN_7_UNITS",10,100]
["HARBGN_7_UNITS",11,100]
["HARBGN_7_UNITS",12,100]
["HARDWK_6_STWBM1",1,0]
["HARDWK_6_STWBM1",2,0]
["HARDWK_6_STWBM1",3,0]
["HARDWK_6_STWBM1",4,0]
["HARDWK_6_STWBM1",5,0]
["HARDWK_6_STWBM1",6,0]
["HARDWK_6_STWBM1",7,0]
["HARDWK_6_STWBM1",8,0]
["HARDWK_6_STWBM1",9,0]
["HARDWK_6_STWBM1",10,0]
["HARDWK_6_STWBM1",11,0]
["HARDWK_6_STWBM1",12,0]
["HATCR1_7_UNIT",1,4.3099999999999996]
["HATCR1_7_UNIT",2,4.17]
["HATCR1_7_UNIT",3,4.29]
["HATCR1_7_UNIT",4,3.69]
["HATCR1_7_UNIT",5,3.21]
["HATCR1_7_UNIT",6,3.66]
["HATCR1_7_UNIT",7,3.43]
["HATCR1_7_UNIT",8,3.17]
["HATCR1_7_UNIT",9,2.88]
["HATCR1_7_UNIT",10,2.37]
["HATCR1_7_UNIT",11,3.7]
["HATCR1_7_UNIT",12,4.24]
["HATCR2_7_UNIT",1,4.43]
["HATCR2_7_UNIT",2,5.18]
["HATCR2_7_UNIT",3,4.6100000000000003]
["HATCR2_7_UNIT",4,3.23]
["HATCR2_7_UNIT",5,2.96]
["HATCR2_7_UNIT",6,3.31]
["HATCR2_7_UNIT",7,3.1]
["HATCR2_7_UNIT",8,3.62]
["HATCR2_7_UNIT",9,4.0599999999999996]
["HATCR2_7_UNIT",10,4.2]
["HATCR2_7_UNIT",11,3.18]
["HATCR2_7_UNIT",12,2.74]
["HATLOS_6_BWDHY1",1,1.4]
["HATLOS_6_BWDHY1",2,1.42]
["HATLOS_6_BWDHY1",3,1.46]
["HATLOS_6_BWDHY1",4,1.44]
["HATLOS_6_BWDHY1",5,0.97]
["HATLOS_6_BWDHY1",6,0.8]
["HATLOS_6_BWDHY1",7,0.89]
["HATLOS_6_BWDHY1",8,0.87]
["HATLOS_6_BWDHY1",9,1.04]
["HATLOS_6_BWDHY1",10,1.29]
["HATLOS_6_BWDHY1",11,1.38]
["HATLOS_6_BWDHY1",12,1.35]
["HATLOS_6_LSCRK",1,1.02]
["HATLOS_6_LSCRK",2,1.02]
["HATLOS_6_LSCRK",3,1.0900000000000001]
["HATLOS_6_LSCRK",4,1.0900000000000001]
["HATLOS_6_LSCRK",5,1]
["HATLOS_6_LSCRK",6,0.92]
["HATLOS_6_LSCRK",7,0.97]
["HATLOS_6_LSCRK",8,0.95]
["HATLOS_6_LSCRK",9,0.96]
["HATLOS_6_LSCRK",10,0.96]
["HATLOS_6_LSCRK",11,0.98]
["HATLOS_6_LSCRK",12,0.94]
["HATRDG_2_WIND",1,33.49]
["HATRDG_2_WIND",2,35.94]
["HATRDG_2_WIND",3,32.049999999999997]
["HATRDG_2_WIND",4,33.86]
["HATRDG_2_WIND",5,35.03]
["HATRDG_2_WIND",6,25.84]
["HATRDG_2_WIND",7,22.98]
["HATRDG_2_WIND",8,21.58]
["HATRDG_2_WIND",9,22.16]
["HATRDG_2_WIND",10,18.57]
["HATRDG_2_WIND",11,23.46]
["HATRDG_2_WIND",12,29.99]
["HAYPRS_6_HAYHD1",1,3.29]
["HAYPRS_6_HAYHD1",2,3.1]
["HAYPRS_6_HAYHD1",3,2.37]
["HAYPRS_6_HAYHD1",4,2.75]
["HAYPRS_6_HAYHD1",5,2.91]
["HAYPRS_6_HAYHD1",6,2.69]
["HAYPRS_6_HAYHD1",7,2.79]
["HAYPRS_6_HAYHD1",8,2.5]
["HAYPRS_6_HAYHD1",9,2.46]
["HAYPRS_6_HAYHD1",10,1.93]
["HAYPRS_6_HAYHD1",11,1.98]
["HAYPRS_6_HAYHD1",12,2.2200000000000002]
["HAYPRS_6_HAYHD2",1,3.8]
["HAYPRS_6_HAYHD2",2,3.58]
["HAYPRS_6_HAYHD2",3,4.1100000000000003]
["HAYPRS_6_HAYHD2",4,3.45]
["HAYPRS_6_HAYHD2",5,3.45]
["HAYPRS_6_HAYHD2",6,3.11]
["HAYPRS_6_HAYHD2",7,3.23]
["HAYPRS_6_HAYHD2",8,2.89]
["HAYPRS_6_HAYHD2",9,2.85]
["HAYPRS_6_HAYHD2",10,2.23]
["HAYPRS_6_HAYHD2",11,2.27]
["HAYPRS_6_HAYHD2",12,2.56]
["HELMPG_7_UNIT 1",1,407]
["HELMPG_7_UNIT 1",2,407]
["HELMPG_7_UNIT 1",3,407]
["HELMPG_7_UNIT 1",4,407]
["HELMPG_7_UNIT 1",5,407]
["HELMPG_7_UNIT 1",6,407]
["HELMPG_7_UNIT 1",7,407]
["HELMPG_7_UNIT 1",8,407]
["HELMPG_7_UNIT 1",9,407]
["HELMPG_7_UNIT 1",10,407]
["HELMPG_7_UNIT 1",11,407]
["HELMPG_7_UNIT 1",12,407]
["HELMPG_7_UNIT 2",1,407]
["HELMPG_7_UNIT 2",2,407]
["HELMPG_7_UNIT 2",3,407]
["HELMPG_7_UNIT 2",4,407]
["HELMPG_7_UNIT 2",5,407]
["HELMPG_7_UNIT 2",6,407]
["HELMPG_7_UNIT 2",7,407]
["HELMPG_7_UNIT 2",8,407]
["HELMPG_7_UNIT 2",9,407]
["HELMPG_7_UNIT 2",10,407]
["HELMPG_7_UNIT 2",11,407]
["HELMPG_7_UNIT 2",12,407]
["HELMPG_7_UNIT 3",1,404]
["HELMPG_7_UNIT 3",2,404]
["HELMPG_7_UNIT 3",3,404]
["HELMPG_7_UNIT 3",4,404]
["HELMPG_7_UNIT 3",5,404]
["HELMPG_7_UNIT 3",6,404]
["HELMPG_7_UNIT 3",7,404]
["HELMPG_7_UNIT 3",8,404]
["HELMPG_7_UNIT 3",9,404]
["HELMPG_7_UNIT 3",10,404]
["HELMPG_7_UNIT 3",11,404]
["HELMPG_7_UNIT 3",12,404]
["HENRTA_6_HDEBT1",1,10]
["HENRTA_6_HDEBT1",2,10]
["HENRTA_6_HDEBT1",3,10]
["HENRTA_6_HDEBT1",4,10]
["HENRTA_6_HDEBT1",5,10]
["HENRTA_6_HDEBT1",6,10]
["HENRTA_6_HDEBT1",7,10]
["HENRTA_6_HDEBT1",8,10]
["HENRTA_6_HDEBT1",9,10]
["HENRTA_6_HDEBT1",10,10]
["HENRTA_6_HDEBT1",11,10]
["HENRTA_6_HDEBT1",12,10]
["HENRTA_6_SOLAR1",1,0.01]
["HENRTA_6_SOLAR1",2,0.05]
["HENRTA_6_SOLAR1",3,0.05]
["HENRTA_6_SOLAR1",4,7.0000000000000007E-2]
["HENRTA_6_SOLAR1",5,0.1]
["HENRTA_6_SOLAR1",6,0.2]
["HENRTA_6_SOLAR1",7,0.22]
["HENRTA_6_SOLAR1",8,0.19]
["HENRTA_6_SOLAR1",9,0.17]
["HENRTA_6_SOLAR1",10,0.11]
["HENRTA_6_SOLAR1",11,0.09]
["HENRTA_6_SOLAR1",12,0.05]
["HENRTA_6_SOLAR2",1,0]
["HENRTA_6_SOLAR2",2,0]
["HENRTA_6_SOLAR2",3,0]
["HENRTA_6_SOLAR2",4,0]
["HENRTA_6_SOLAR2",5,0]
["HENRTA_6_SOLAR2",6,0]
["HENRTA_6_SOLAR2",7,0]
["HENRTA_6_SOLAR2",8,0]
["HENRTA_6_SOLAR2",9,0]
["HENRTA_6_SOLAR2",10,0]
["HENRTA_6_SOLAR2",11,0]
["HENRTA_6_SOLAR2",12,0]
["HENRTA_6_UNITA1",1,49.98]
["HENRTA_6_UNITA1",2,49.98]
["HENRTA_6_UNITA1",3,49.98]
["HENRTA_6_UNITA1",4,49.98]
["HENRTA_6_UNITA1",5,49.98]
["HENRTA_6_UNITA1",6,49.98]
["HENRTA_6_UNITA1",7,49.98]
["HENRTA_6_UNITA1",8,49.98]
["HENRTA_6_UNITA1",9,49.98]
["HENRTA_6_UNITA1",10,49.98]
["HENRTA_6_UNITA1",11,49.98]
["HENRTA_6_UNITA1",12,49.98]
["HENRTA_6_UNITA2",1,49.42]
["HENRTA_6_UNITA2",2,49.42]
["HENRTA_6_UNITA2",3,49.42]
["HENRTA_6_UNITA2",4,49.42]
["HENRTA_6_UNITA2",5,49.42]
["HENRTA_6_UNITA2",6,49.42]
["HENRTA_6_UNITA2",7,49.42]
["HENRTA_6_UNITA2",8,49.42]
["HENRTA_6_UNITA2",9,49.42]
["HENRTA_6_UNITA2",10,49.42]
["HENRTA_6_UNITA2",11,49.42]
["HENRTA_6_UNITA2",12,49.42]
["HENRTS_1_SOLAR",1,0.4]
["HENRTS_1_SOLAR",2,3]
["HENRTS_1_SOLAR",3,3.5]
["HENRTS_1_SOLAR",4,4.4000000000000004]
["HENRTS_1_SOLAR",5,6.4]
["HENRTS_1_SOLAR",6,13.1]
["HENRTS_1_SOLAR",7,14.4]
["HENRTS_1_SOLAR",8,12.4]
["HENRTS_1_SOLAR",9,11.1]
["HENRTS_1_SOLAR",10,7.4]
["HENRTS_1_SOLAR",11,5.7]
["HENRTS_1_SOLAR",12,3.5]
["HERDLN_6_BYHSR1",1,0]
["HERDLN_6_BYHSR1",2,0]
["HERDLN_6_BYHSR1",3,0]
["HERDLN_6_BYHSR1",4,0]
["HERDLN_6_BYHSR1",5,0]
["HERDLN_6_BYHSR1",6,0]
["HERDLN_6_BYHSR1",7,0]
["HERDLN_6_BYHSR1",8,0]
["HERDLN_6_BYHSR1",9,0]
["HERDLN_6_BYHSR1",10,0]
["HERDLN_6_BYHSR1",11,0]
["HERDLN_6_BYHSR1",12,0]
["HIDSRT_2_UNITS",1,830]
["HIDSRT_2_UNITS",2,830]
["HIDSRT_2_UNITS",3,830]
["HIDSRT_2_UNITS",4,830]
["HIDSRT_2_UNITS",5,830]
["HIDSRT_2_UNITS",6,830]
["HIDSRT_2_UNITS",7,830]
["HIDSRT_2_UNITS",8,830]
["HIDSRT_2_UNITS",9,830]
["HIDSRT_2_UNITS",10,830]
["HIDSRT_2_UNITS",11,830]
["HIDSRT_2_UNITS",12,830]
["HIGGNS_1_COMBIE",1,0.72]
["HIGGNS_1_COMBIE",2,0.76]
["HIGGNS_1_COMBIE",3,0.79]
["HIGGNS_1_COMBIE",4,0.7]
["HIGGNS_1_COMBIE",5,0.79]
["HIGGNS_1_COMBIE",6,0.53]
["HIGGNS_1_COMBIE",7,0.44]
["HIGGNS_1_COMBIE",8,0.33]
["HIGGNS_1_COMBIE",9,0.32]
["HIGGNS_1_COMBIE",10,0.28999999999999998]
["HIGGNS_1_COMBIE",11,0.92]
["HIGGNS_1_COMBIE",12,0.7]
["HIGGNS_7_QFUNTS",1,0.06]
["HIGGNS_7_QFUNTS",2,0.11]
["HIGGNS_7_QFUNTS",3,0.12]
["HIGGNS_7_QFUNTS",4,0.16]
["HIGGNS_7_QFUNTS",5,0.24]
["HIGGNS_7_QFUNTS",6,0.25]
["HIGGNS_7_QFUNTS",7,0.24]
["HIGGNS_7_QFUNTS",8,0.24]
["HIGGNS_7_QFUNTS",9,0.24]
["HIGGNS_7_QFUNTS",10,0.1]
["HIGGNS_7_QFUNTS",11,0.05]
["HIGGNS_7_QFUNTS",12,0.11]
["HIGHDS_2_H5SBT1",1,50]
["HIGHDS_2_H5SBT1",2,50]
["HIGHDS_2_H5SBT1",3,50]
["HIGHDS_2_H5SBT1",4,50]
["HIGHDS_2_H5SBT1",5,50]
["HIGHDS_2_H5SBT1",6,50]
["HIGHDS_2_H5SBT1",7,50]
["HIGHDS_2_H5SBT1",8,50]
["HIGHDS_2_H5SBT1",9,50]
["HIGHDS_2_H5SBT1",10,50]
["HIGHDS_2_H5SBT1",11,50]
["HIGHDS_2_H5SBT1",12,50]
["HIGHDS_2_H5SSR1",1,0.21]
["HIGHDS_2_H5SSR1",2,1.91]
["HIGHDS_2_H5SSR1",3,2.36]
["HIGHDS_2_H5SSR1",4,3.25]
["HIGHDS_2_H5SSR1",5,4.8499999999999996]
["HIGHDS_2_H5SSR1",6,10.15]
["HIGHDS_2_H5SSR1",7,11.14]
["HIGHDS_2_H5SSR1",8,9.41]
["HIGHDS_2_H5SSR1",9,8.06]
["HIGHDS_2_H5SSR1",10,5.13]
["HIGHDS_2_H5SSR1",11,3.54]
["HIGHDS_2_H5SSR1",12,1.6]
["HILAND_7_YOLOWD",1,0]
["HILAND_7_YOLOWD",2,0]
["HILAND_7_YOLOWD",3,0]
["HILAND_7_YOLOWD",4,0]
["HILAND_7_YOLOWD",5,0]
["HILAND_7_YOLOWD",6,0]
["HILAND_7_YOLOWD",7,0]
["HILAND_7_YOLOWD",8,0]
["HILAND_7_YOLOWD",9,0]
["HILAND_7_YOLOWD",10,0]
["HILAND_7_YOLOWD",11,0]
["HILAND_7_YOLOWD",12,0]
["HINSON_6_LBECH1",1,63]
["HINSON_6_LBECH1",2,63]
["HINSON_6_LBECH1",3,63]
["HINSON_6_LBECH1",4,63]
["HINSON_6_LBECH1",5,63]
["HINSON_6_LBECH1",6,63]
["HINSON_6_LBECH1",7,63]
["HINSON_6_LBECH1",8,63]
["HINSON_6_LBECH1",9,63]
["HINSON_6_LBECH1",10,63]
["HINSON_6_LBECH1",11,63]
["HINSON_6_LBECH1",12,63]
["HINSON_6_LBECH2",1,63]
["HINSON_6_LBECH2",2,63]
["HINSON_6_LBECH2",3,63]
["HINSON_6_LBECH2",4,63]
["HINSON_6_LBECH2",5,63]
["HINSON_6_LBECH2",6,63]
["HINSON_6_LBECH2",7,63]
["HINSON_6_LBECH2",8,63]
["HINSON_6_LBECH2",9,63]
["HINSON_6_LBECH2",10,63]
["HINSON_6_LBECH2",11,63]
["HINSON_6_LBECH2",12,63]
["HINSON_6_LBECH3",1,63]
["HINSON_6_LBECH3",2,63]
["HINSON_6_LBECH3",3,63]
["HINSON_6_LBECH3",4,63]
["HINSON_6_LBECH3",5,63]
["HINSON_6_LBECH3",6,63]
["HINSON_6_LBECH3",7,63]
["HINSON_6_LBECH3",8,63]
["HINSON_6_LBECH3",9,63]
["HINSON_6_LBECH3",10,63]
["HINSON_6_LBECH3",11,63]
["HINSON_6_LBECH3",12,63]
["HINSON_6_LBECH4",1,63]
["HINSON_6_LBECH4",2,63]
["HINSON_6_LBECH4",3,63]
["HINSON_6_LBECH4",4,63]
["HINSON_6_LBECH4",5,63]
["HINSON_6_LBECH4",6,63]
["HINSON_6_LBECH4",7,63]
["HINSON_6_LBECH4",8,63]
["HINSON_6_LBECH4",9,63]
["HINSON_6_LBECH4",10,63]
["HINSON_6_LBECH4",11,63]
["HINSON_6_LBECH4",12,63]
["HINSON_6_SERRGN",1,34]
["HINSON_6_SERRGN",2,34]
["HINSON_6_SERRGN",3,34]
["HINSON_6_SERRGN",4,34]
["HINSON_6_SERRGN",5,34]
["HINSON_6_SERRGN",6,34]
["HINSON_6_SERRGN",7,34]
["HINSON_6_SERRGN",8,34]
["HINSON_6_SERRGN",9,34]
["HINSON_6_SERRGN",10,34]
["HINSON_6_SERRGN",11,34]
["HINSON_6_SERRGN",12,34]
["HNTGBH_2_PL1X3",1,673.8]
["HNTGBH_2_PL1X3",2,673.8]
["HNTGBH_2_PL1X3",3,673.8]
["HNTGBH_2_PL1X3",4,673.8]
["HNTGBH_2_PL1X3",5,673.8]
["HNTGBH_2_PL1X3",6,673.8]
["HNTGBH_2_PL1X3",7,673.8]
["HNTGBH_2_PL1X3",8,673.8]
["HNTGBH_2_PL1X3",9,673.8]
["HNTGBH_2_PL1X3",10,673.8]
["HNTGBH_2_PL1X3",11,673.8]
["HNTGBH_2_PL1X3",12,673.8]
["HNTGBH_7_UNIT 2",1,226.84]
["HNTGBH_7_UNIT 2",2,226.84]
["HNTGBH_7_UNIT 2",3,226.84]
["HNTGBH_7_UNIT 2",4,226.84]
["HNTGBH_7_UNIT 2",5,226.84]
["HNTGBH_7_UNIT 2",6,226.84]
["HNTGBH_7_UNIT 2",7,226.84]
["HNTGBH_7_UNIT 2",8,226.84]
["HNTGBH_7_UNIT 2",9,226.84]
["HNTGBH_7_UNIT 2",10,226.84]
["HNTGBH_7_UNIT 2",11,226.84]
["HNTGBH_7_UNIT 2",12,226.84]
["HOLGAT_1_BORAX",1,17.170000000000002]
["HOLGAT_1_BORAX",2,15.12]
["HOLGAT_1_BORAX",3,13.09]
["HOLGAT_1_BORAX",4,4.87]
["HOLGAT_1_BORAX",5,7.33]
["HOLGAT_1_BORAX",6,13.88]
["HOLGAT_1_BORAX",7,12.08]
["HOLGAT_1_BORAX",8,11.68]
["HOLGAT_1_BORAX",9,13.9]
["HOLGAT_1_BORAX",10,14.74]
["HOLGAT_1_BORAX",11,15.84]
["HOLGAT_1_BORAX",12,14.94]
["HOLSTR_1_SOLAR",1,0]
["HOLSTR_1_SOLAR",2,0]
["HOLSTR_1_SOLAR",3,0]
["HOLSTR_1_SOLAR",4,0]
["HOLSTR_1_SOLAR",5,0]
["HOLSTR_1_SOLAR",6,0]
["HOLSTR_1_SOLAR",7,0]
["HOLSTR_1_SOLAR",8,0]
["HOLSTR_1_SOLAR",9,0]
["HOLSTR_1_SOLAR",10,0]
["HOLSTR_1_SOLAR",11,0]
["HOLSTR_1_SOLAR",12,0]
["HOLSTR_1_SOLAR2",1,0.01]
["HOLSTR_1_SOLAR2",2,0.05]
["HOLSTR_1_SOLAR2",3,0.05]
["HOLSTR_1_SOLAR2",4,7.0000000000000007E-2]
["HOLSTR_1_SOLAR2",5,0.1]
["HOLSTR_1_SOLAR2",6,0.2]
["HOLSTR_1_SOLAR2",7,0.22]
["HOLSTR_1_SOLAR2",8,0.19]
["HOLSTR_1_SOLAR2",9,0.17]
["HOLSTR_1_SOLAR2",10,0.11]
["HOLSTR_1_SOLAR2",11,0.09]
["HOLSTR_1_SOLAR2",12,0.05]
["HUMBPP_1_UNITS3",1,65.08]
["HUMBPP_1_UNITS3",2,65.08]
["HUMBPP_1_UNITS3",3,65.08]
["HUMBPP_1_UNITS3",4,65.08]
["HUMBPP_1_UNITS3",5,65.08]
["HUMBPP_1_UNITS3",6,65.08]
["HUMBPP_1_UNITS3",7,65.08]
["HUMBPP_1_UNITS3",8,65.08]
["HUMBPP_1_UNITS3",9,65.08]
["HUMBPP_1_UNITS3",10,65.08]
["HUMBPP_1_UNITS3",11,65.08]
["HUMBPP_1_UNITS3",12,65.08]
["HUMBPP_6_UNITS",1,97.62]
["HUMBPP_6_UNITS",2,97.62]
["HUMBPP_6_UNITS",3,97.62]
["HUMBPP_6_UNITS",4,97.62]
["HUMBPP_6_UNITS",5,97.62]
["HUMBPP_6_UNITS",6,97.62]
["HUMBPP_6_UNITS",7,97.62]
["HUMBPP_6_UNITS",8,97.62]
["HUMBPP_6_UNITS",9,97.62]
["HUMBPP_6_UNITS",10,97.62]
["HUMBPP_6_UNITS",11,97.62]
["HUMBPP_6_UNITS",12,97.62]
["HURON_6_SOLAR",1,0.08]
["HURON_6_SOLAR",2,0.6]
["HURON_6_SOLAR",3,0.7]
["HURON_6_SOLAR",4,0.88]
["HURON_6_SOLAR",5,1.28]
["HURON_6_SOLAR",6,2.62]
["HURON_6_SOLAR",7,2.88]
["HURON_6_SOLAR",8,2.48]
["HURON_6_SOLAR",9,2.2200000000000002]
["HURON_6_SOLAR",10,1.48]
["HURON_6_SOLAR",11,1.1399999999999999]
["HURON_6_SOLAR",12,0.7]
["HYTTHM_2_UNITS",1,109.25]
["HYTTHM_2_UNITS",2,69.52]
["HYTTHM_2_UNITS",3,61.54]
["HYTTHM_2_UNITS",4,135.74]
["HYTTHM_2_UNITS",5,240.32]
["HYTTHM_2_UNITS",6,484.32]
["HYTTHM_2_UNITS",7,654.27]
["HYTTHM_2_UNITS",8,558.82000000000005]
["HYTTHM_2_UNITS",9,336.74]
["HYTTHM_2_UNITS",10,141.44]
["HYTTHM_2_UNITS",11,172.84]
["HYTTHM_2_UNITS",12,145.94]
["IGNACO_1_QF",1,0.01]
["IGNACO_1_QF",2,0.01]
["IGNACO_1_QF",3,0.01]
["IGNACO_1_QF",4,0.01]
["IGNACO_1_QF",5,0.02]
["IGNACO_1_QF",6,0.02]
["IGNACO_1_QF",7,0.02]
["IGNACO_1_QF",8,0.01]
["IGNACO_1_QF",9,0.01]
["IGNACO_1_QF",10,0.01]
["IGNACO_1_QF",11,0.01]
["IGNACO_1_QF",12,0.01]
["INDIGO_1_UNIT 1",1,45.3]
["INDIGO_1_UNIT 1",2,45.3]
["INDIGO_1_UNIT 1",3,45.3]
["INDIGO_1_UNIT 1",4,45.3]
["INDIGO_1_UNIT 1",5,45.3]
["INDIGO_1_UNIT 1",6,45.3]
["INDIGO_1_UNIT 1",7,45.3]
["INDIGO_1_UNIT 1",8,45.3]
["INDIGO_1_UNIT 1",9,45.3]
["INDIGO_1_UNIT 1",10,45.3]
["INDIGO_1_UNIT 1",11,45.3]
["INDIGO_1_UNIT 1",12,45.3]
["INDIGO_1_UNIT 2",1,45.3]
["INDIGO_1_UNIT 2",2,45.3]
["INDIGO_1_UNIT 2",3,45.3]
["INDIGO_1_UNIT 2",4,45.3]
["INDIGO_1_UNIT 2",5,45.3]
["INDIGO_1_UNIT 2",6,45.3]
["INDIGO_1_UNIT 2",7,45.3]
["INDIGO_1_UNIT 2",8,45.3]
["INDIGO_1_UNIT 2",9,45.3]
["INDIGO_1_UNIT 2",10,45.3]
["INDIGO_1_UNIT 2",11,45.3]
["INDIGO_1_UNIT 2",12,45.3]
["INDIGO_1_UNIT 3",1,45.3]
["INDIGO_1_UNIT 3",2,45.3]
["INDIGO_1_UNIT 3",3,45.3]
["INDIGO_1_UNIT 3",4,45.3]
["INDIGO_1_UNIT 3",5,45.3]
["INDIGO_1_UNIT 3",6,45.3]
["INDIGO_1_UNIT 3",7,45.3]
["INDIGO_1_UNIT 3",8,45.3]
["INDIGO_1_UNIT 3",9,45.3]
["INDIGO_1_UNIT 3",10,45.3]
["INDIGO_1_UNIT 3",11,45.3]
["INDIGO_1_UNIT 3",12,45.3]
["INDVLY_1_UNITS",1,0]
["INDVLY_1_UNITS",2,0]
["INDVLY_1_UNITS",3,0.53]
["INDVLY_1_UNITS",4,1.03]
["INDVLY_1_UNITS",5,1.01]
["INDVLY_1_UNITS",6,1.62]
["INDVLY_1_UNITS",7,1.61]
["INDVLY_1_UNITS",8,1.59]
["INDVLY_1_UNITS",9,1.33]
["INDVLY_1_UNITS",10,0.15]
["INDVLY_1_UNITS",11,0]
["INDVLY_1_UNITS",12,0]
["INTKEP_2_UNITS",1,307]
["INTKEP_2_UNITS",2,307]
["INTKEP_2_UNITS",3,307]
["INTKEP_2_UNITS",4,307]
["INTKEP_2_UNITS",5,307]
["INTKEP_2_UNITS",6,307]
["INTKEP_2_UNITS",7,307]
["INTKEP_2_UNITS",8,307]
["INTKEP_2_UNITS",9,307]
["INTKEP_2_UNITS",10,307]
["INTKEP_2_UNITS",11,307]
["INTKEP_2_UNITS",12,307]
["INTTRB_6_UNIT",1,6.04]
["INTTRB_6_UNIT",2,6.48]
["INTTRB_6_UNIT",3,5.78]
["INTTRB_6_UNIT",4,6.11]
["INTTRB_6_UNIT",5,6.32]
["INTTRB_6_UNIT",6,4.66]
["INTTRB_6_UNIT",7,4.1500000000000004]
["INTTRB_6_UNIT",8,3.89]
["INTTRB_6_UNIT",9,4]
["INTTRB_6_UNIT",10,3.35]
["INTTRB_6_UNIT",11,4.2300000000000004]
["INTTRB_6_UNIT",12,5.41]
["IVANPA_1_UNIT1",1,0.5]
["IVANPA_1_UNIT1",2,3.78]
["IVANPA_1_UNIT1",3,4.41]
["IVANPA_1_UNIT1",4,5.54]
["IVANPA_1_UNIT1",5,8.06]
["IVANPA_1_UNIT1",6,16.510000000000002]
["IVANPA_1_UNIT1",7,18.14]
["IVANPA_1_UNIT1",8,15.62]
["IVANPA_1_UNIT1",9,13.99]
["IVANPA_1_UNIT1",10,9.32]
["IVANPA_1_UNIT1",11,7.18]
["IVANPA_1_UNIT1",12,4.41]
["IVANPA_1_UNIT2",1,0.53]
["IVANPA_1_UNIT2",2,3.99]
["IVANPA_1_UNIT2",3,4.66]
["IVANPA_1_UNIT2",4,5.85]
["IVANPA_1_UNIT2",5,8.51]
["IVANPA_1_UNIT2",6,17.420000000000002]
["IVANPA_1_UNIT2",7,19.149999999999999]
["IVANPA_1_UNIT2",8,16.489999999999998]
["IVANPA_1_UNIT2",9,14.76]
["IVANPA_1_UNIT2",10,9.84]
["IVANPA_1_UNIT2",11,7.58]
["IVANPA_1_UNIT2",12,4.66]
["IVANPA_1_UNIT3",1,0.53]
["IVANPA_1_UNIT3",2,3.99]
["IVANPA_1_UNIT3",3,4.66]
["IVANPA_1_UNIT3",4,5.85]
["IVANPA_1_UNIT3",5,8.51]
["IVANPA_1_UNIT3",6,17.420000000000002]
["IVANPA_1_UNIT3",7,19.149999999999999]
["IVANPA_1_UNIT3",8,16.489999999999998]
["IVANPA_1_UNIT3",9,14.76]
["IVANPA_1_UNIT3",10,9.84]
["IVANPA_1_UNIT3",11,7.58]
["IVANPA_1_UNIT3",12,4.66]
["IVSLR2_2_SM2SR1",1,0.6]
["IVSLR2_2_SM2SR1",2,4.5]
["IVSLR2_2_SM2SR1",3,5.25]
["IVSLR2_2_SM2SR1",4,6.6]
["IVSLR2_2_SM2SR1",5,9.6]
["IVSLR2_2_SM2SR1",6,19.649999999999999]
["IVSLR2_2_SM2SR1",7,21.6]
["IVSLR2_2_SM2SR1",8,18.600000000000001]
["IVSLR2_2_SM2SR1",9,16.649999999999999]
["IVSLR2_2_SM2SR1",10,11.1]
["IVSLR2_2_SM2SR1",11,8.5500000000000007]
["IVSLR2_2_SM2SR1",12,5.25]
["IVSLRP_2_SOLAR1",1,0.8]
["IVSLRP_2_SOLAR1",2,6]
["IVSLRP_2_SOLAR1",3,7]
["IVSLRP_2_SOLAR1",4,8.8000000000000007]
["IVSLRP_2_SOLAR1",5,12.8]
["IVSLRP_2_SOLAR1",6,26.2]
["IVSLRP_2_SOLAR1",7,28.8]
["IVSLRP_2_SOLAR1",8,24.8]
["IVSLRP_2_SOLAR1",9,22.2]
["IVSLRP_2_SOLAR1",10,14.8]
["IVSLRP_2_SOLAR1",11,11.4]
["IVSLRP_2_SOLAR1",12,7]
["IVWEST_2_SOLAR1",1,0.6]
["IVWEST_2_SOLAR1",2,4.5]
["IVWEST_2_SOLAR1",3,5.25]
["IVWEST_2_SOLAR1",4,6.6]
["IVWEST_2_SOLAR1",5,9.6]
["IVWEST_2_SOLAR1",6,19.649999999999999]
["IVWEST_2_SOLAR1",7,21.6]
["IVWEST_2_SOLAR1",8,18.600000000000001]
["IVWEST_2_SOLAR1",9,16.649999999999999]
["IVWEST_2_SOLAR1",10,11.1]
["IVWEST_2_SOLAR1",11,8.5500000000000007]
["IVWEST_2_SOLAR1",12,5.25]
["JACMSR_1_JACSR1",1,0.08]
["JACMSR_1_JACSR1",2,0.6]
["JACMSR_1_JACSR1",3,0.7]
["JACMSR_1_JACSR1",4,0.88]
["JACMSR_1_JACSR1",5,1.28]
["JACMSR_1_JACSR1",6,2.62]
["JACMSR_1_JACSR1",7,2.88]
["JACMSR_1_JACSR1",8,2.48]
["JACMSR_1_JACSR1",9,2.2200000000000002]
["JACMSR_1_JACSR1",10,1.48]
["JACMSR_1_JACSR1",11,1.1399999999999999]
["JACMSR_1_JACSR1",12,0.7]
["JAVASR_1_JAVSR1",3,0.47]
["JAVASR_1_JAVSR1",4,0.59]
["JAVASR_1_JAVSR1",5,0.86]
["JAVASR_1_JAVSR1",6,1.76]
["JAVASR_1_JAVSR1",7,1.94]
["JAVASR_1_JAVSR1",8,1.67]
["JAVASR_1_JAVSR1",9,1.49]
["JAVASR_1_JAVSR1",10,0.99]
["JAVASR_1_JAVSR1",11,0.76]
["JAVASR_1_JAVSR1",12,0.47]
["JAWBNE_2_NSRWND",1,28.27]
["JAWBNE_2_NSRWND",2,30.07]
["JAWBNE_2_NSRWND",3,26.42]
["JAWBNE_2_NSRWND",4,25.31]
["JAWBNE_2_NSRWND",5,26.92]
["JAWBNE_2_NSRWND",6,24.67]
["JAWBNE_2_NSRWND",7,22.92]
["JAWBNE_2_NSRWND",8,17.420000000000002]
["JAWBNE_2_NSRWND",9,17.989999999999998]
["JAWBNE_2_NSRWND",10,16.690000000000001]
["JAWBNE_2_NSRWND",11,22.5]
["JAWBNE_2_NSRWND",12,27.25]
["JAWBNE_2_SRWND",1,5.3]
["JAWBNE_2_SRWND",2,5.64]
["JAWBNE_2_SRWND",3,4.95]
["JAWBNE_2_SRWND",4,4.75]
["JAWBNE_2_SRWND",5,5.05]
["JAWBNE_2_SRWND",6,4.63]
["JAWBNE_2_SRWND",7,4.3]
["JAWBNE_2_SRWND",8,3.27]
["JAWBNE_2_SRWND",9,3.37]
["JAWBNE_2_SRWND",10,3.13]
["JAWBNE_2_SRWND",11,4.22]
["JAWBNE_2_SRWND",12,5.1100000000000003]
["JAWBNE_2_SRWWD2",1,5.34]
["JAWBNE_2_SRWWD2",2,5.68]
["JAWBNE_2_SRWWD2",3,4.99]
["JAWBNE_2_SRWWD2",4,4.78]
["JAWBNE_2_SRWWD2",5,5.08]
["JAWBNE_2_SRWWD2",6,4.66]
["JAWBNE_2_SRWWD2",7,4.33]
["JAWBNE_2_SRWWD2",8,3.29]
["JAWBNE_2_SRWWD2",9,3.4]
["JAWBNE_2_SRWWD2",10,3.15]
["JAWBNE_2_SRWWD2",11,4.25]
["JAWBNE_2_SRWWD2",12,5.14]
["JAYNE_6_WLSLR",1,0]
["JAYNE_6_WLSLR",2,0]
["JAYNE_6_WLSLR",3,0]
["JAYNE_6_WLSLR",4,0]
["JAYNE_6_WLSLR",5,0]
["JAYNE_6_WLSLR",6,0]
["JAYNE_6_WLSLR",7,0]
["JAYNE_6_WLSLR",8,0]
["JAYNE_6_WLSLR",9,0]
["JAYNE_6_WLSLR",10,0]
["JAYNE_6_WLSLR",11,0]
["JAYNE_6_WLSLR",12,0]
["JOANEC_2_ST3BT3",7,40]
["JOANEC_2_ST3BT3",8,40]
["JOANEC_2_ST3BT3",9,40]
["JOANEC_2_ST3BT3",10,40]
["JOANEC_2_ST3BT3",11,40]
["JOANEC_2_ST3BT3",12,40]
["JOANEC_2_STABT1",1,20]
["JOANEC_2_STABT1",2,20]
["JOANEC_2_STABT1",3,20]
["JOANEC_2_STABT1",4,20]
["JOANEC_2_STABT1",5,20]
["JOANEC_2_STABT1",6,20]
["JOANEC_2_STABT1",7,20]
["JOANEC_2_STABT1",8,20]
["JOANEC_2_STABT1",9,20]
["JOANEC_2_STABT1",10,20]
["JOANEC_2_STABT1",11,20]
["JOANEC_2_STABT1",12,20]
["JOANEC_2_STABT2",1,20]
["JOANEC_2_STABT2",2,20]
["JOANEC_2_STABT2",3,20]
["JOANEC_2_STABT2",4,20]
["JOANEC_2_STABT2",5,20]
["JOANEC_2_STABT2",6,20]
["JOANEC_2_STABT2",7,20]
["JOANEC_2_STABT2",8,20]
["JOANEC_2_STABT2",9,20]
["JOANEC_2_STABT2",10,20]
["JOANEC_2_STABT2",11,20]
["JOANEC_2_STABT2",12,20]
["JOHANN_2_JOSBT1",1,10]
["JOHANN_2_JOSBT1",2,10]
["JOHANN_2_JOSBT1",3,10]
["JOHANN_2_JOSBT1",4,10]
["JOHANN_2_JOSBT1",5,10]
["JOHANN_2_JOSBT1",6,10]
["JOHANN_2_JOSBT1",7,10]
["JOHANN_2_JOSBT1",8,10]
["JOHANN_2_JOSBT1",9,10]
["JOHANN_2_JOSBT1",10,10]
["JOHANN_2_JOSBT1",11,10]
["JOHANN_2_JOSBT1",12,10]
["JOHANN_2_JOSBT2",1,10]
["JOHANN_2_JOSBT2",2,10]
["JOHANN_2_JOSBT2",3,10]
["JOHANN_2_JOSBT2",4,10]
["JOHANN_2_JOSBT2",5,10]
["JOHANN_2_JOSBT2",6,10]
["JOHANN_2_JOSBT2",7,10]
["JOHANN_2_JOSBT2",8,10]
["JOHANN_2_JOSBT2",9,10]
["JOHANN_2_JOSBT2",10,10]
["JOHANN_2_JOSBT2",11,10]
["JOHANN_2_JOSBT2",12,10]
["JOHANN_2_OCEBT2",1,9]
["JOHANN_2_OCEBT2",2,9]
["JOHANN_2_OCEBT2",3,9]
["JOHANN_2_OCEBT2",4,9]
["JOHANN_2_OCEBT2",5,9]
["JOHANN_2_OCEBT2",6,9]
["JOHANN_2_OCEBT2",7,9]
["JOHANN_2_OCEBT2",8,9]
["JOHANN_2_OCEBT2",9,9]
["JOHANN_2_OCEBT2",10,9]
["JOHANN_2_OCEBT2",11,9]
["JOHANN_2_OCEBT2",12,9]
["JOHANN_2_OCEBT3",1,6]
["JOHANN_2_OCEBT3",2,6]
["JOHANN_2_OCEBT3",3,6]
["JOHANN_2_OCEBT3",4,6]
["JOHANN_2_OCEBT3",5,6]
["JOHANN_2_OCEBT3",6,6]
["JOHANN_2_OCEBT3",7,6]
["JOHANN_2_OCEBT3",8,6]
["JOHANN_2_OCEBT3",9,6]
["JOHANN_2_OCEBT3",10,6]
["JOHANN_2_OCEBT3",11,6]
["JOHANN_2_OCEBT3",12,6]
["KANSAS_6_SOLAR",1,0]
["KANSAS_6_SOLAR",2,0]
["KANSAS_6_SOLAR",3,0]
["KANSAS_6_SOLAR",4,0]
["KANSAS_6_SOLAR",5,0]
["KANSAS_6_SOLAR",6,0]
["KANSAS_6_SOLAR",7,0]
["KANSAS_6_SOLAR",8,0]
["KANSAS_6_SOLAR",9,0]
["KANSAS_6_SOLAR",10,0]
["KANSAS_6_SOLAR",11,0]
["KANSAS_6_SOLAR",12,0]
["KEARNY_6_NESBT1",1,10]
["KEARNY_6_NESBT1",2,10]
["KEARNY_6_NESBT1",3,10]
["KEARNY_6_NESBT1",4,10]
["KEARNY_6_NESBT1",5,10]
["KEARNY_6_NESBT1",6,10]
["KEARNY_6_NESBT1",7,10]
["KEARNY_6_NESBT1",8,10]
["KEARNY_6_NESBT1",9,10]
["KEARNY_6_NESBT1",10,10]
["KEARNY_6_NESBT1",11,10]
["KEARNY_6_NESBT1",12,10]
["KEARNY_6_SESBT2",1,10]
["KEARNY_6_SESBT2",2,10]
["KEARNY_6_SESBT2",3,10]
["KEARNY_6_SESBT2",4,10]
["KEARNY_6_SESBT2",5,10]
["KEARNY_6_SESBT2",6,10]
["KEARNY_6_SESBT2",7,10]
["KEARNY_6_SESBT2",8,10]
["KEARNY_6_SESBT2",9,10]
["KEARNY_6_SESBT2",10,10]
["KEARNY_6_SESBT2",11,10]
["KEARNY_6_SESBT2",12,10]
["KEKAWK_6_UNIT",1,0]
["KEKAWK_6_UNIT",2,0]
["KEKAWK_6_UNIT",3,0]
["KEKAWK_6_UNIT",4,0]
["KEKAWK_6_UNIT",5,0]
["KEKAWK_6_UNIT",6,0]
["KEKAWK_6_UNIT",7,0]
["KEKAWK_6_UNIT",8,0]
["KEKAWK_6_UNIT",9,0]
["KEKAWK_6_UNIT",10,0]
["KEKAWK_6_UNIT",11,0]
["KEKAWK_6_UNIT",12,0]
["KELSO_2_UNITS",1,198.03]
["KELSO_2_UNITS",2,198.03]
["KELSO_2_UNITS",3,198.03]
["KELSO_2_UNITS",4,198.03]
["KELSO_2_UNITS",5,198.03]
["KELSO_2_UNITS",6,198.03]
["KELSO_2_UNITS",7,198.03]
["KELSO_2_UNITS",8,198.03]
["KELSO_2_UNITS",9,198.03]
["KELSO_2_UNITS",10,198.03]
["KELSO_2_UNITS",11,198.03]
["KELSO_2_UNITS",12,198.03]
["KELYRG_6_UNIT",1,11]
["KELYRG_6_UNIT",2,11]
["KELYRG_6_UNIT",3,11]
["KELYRG_6_UNIT",4,11]
["KELYRG_6_UNIT",5,11]
["KELYRG_6_UNIT",6,11]
["KELYRG_6_UNIT",7,11]
["KELYRG_6_UNIT",8,11]
["KELYRG_6_UNIT",9,11]
["KELYRG_6_UNIT",10,11]
["KELYRG_6_UNIT",11,11]
["KELYRG_6_UNIT",12,11]
["KERKH2_7_UNIT 1",1,16]
["KERKH2_7_UNIT 1",2,32]
["KERKH2_7_UNIT 1",3,32]
["KERKH2_7_UNIT 1",4,36]
["KERKH2_7_UNIT 1",5,96]
["KERKH2_7_UNIT 1",6,74.8]
["KERKH2_7_UNIT 1",7,75]
["KERKH2_7_UNIT 1",8,75.599999999999994]
["KERKH2_7_UNIT 1",9,75]
["KERKH2_7_UNIT 1",10,0]
["KERKH2_7_UNIT 1",11,0]
["KERKH2_7_UNIT 1",12,4]
["KERMAN_6_SOLAR1",1,0]
["KERMAN_6_SOLAR1",2,0]
["KERMAN_6_SOLAR1",3,0]
["KERMAN_6_SOLAR1",4,0]
["KERMAN_6_SOLAR1",5,0]
["KERMAN_6_SOLAR1",6,0]
["KERMAN_6_SOLAR1",7,0]
["KERMAN_6_SOLAR1",8,0]
["KERMAN_6_SOLAR1",9,0]
["KERMAN_6_SOLAR1",10,0]
["KERMAN_6_SOLAR1",11,0]
["KERMAN_6_SOLAR1",12,0]
["KERMAN_6_SOLAR2",1,0]
["KERMAN_6_SOLAR2",2,0]
["KERMAN_6_SOLAR2",3,0]
["KERMAN_6_SOLAR2",4,0]
["KERMAN_6_SOLAR2",5,0]
["KERMAN_6_SOLAR2",6,0]
["KERMAN_6_SOLAR2",7,0]
["KERMAN_6_SOLAR2",8,0]
["KERMAN_6_SOLAR2",9,0]
["KERMAN_6_SOLAR2",10,0]
["KERMAN_6_SOLAR2",11,0]
["KERMAN_6_SOLAR2",12,0]
["KERNFT_1_UNITS",1,52.4]
["KERNFT_1_UNITS",2,52.4]
["KERNFT_1_UNITS",3,52.4]
["KERNFT_1_UNITS",4,52.4]
["KERNFT_1_UNITS",5,52.4]
["KERNFT_1_UNITS",6,52.4]
["KERNFT_1_UNITS",7,52.4]
["KERNFT_1_UNITS",8,52.4]
["KERNFT_1_UNITS",9,52.4]
["KERNFT_1_UNITS",10,52.4]
["KERNFT_1_UNITS",11,52.4]
["KERNFT_1_UNITS",12,52.4]
["KERNRG_1_UNITS",1,0.87]
["KERNRG_1_UNITS",2,0.44]
["KERNRG_1_UNITS",3,0.21]
["KERNRG_1_UNITS",4,0.87]
["KERNRG_1_UNITS",5,0.79]
["KERNRG_1_UNITS",6,0.79]
["KERNRG_1_UNITS",7,0.68]
["KERNRG_1_UNITS",8,0.62]
["KERNRG_1_UNITS",9,0.46]
["KERNRG_1_UNITS",10,0.46]
["KERNRG_1_UNITS",11,0.84]
["KERNRG_1_UNITS",12,0.98]
["KERRGN_1_UNIT 1",1,14.64]
["KERRGN_1_UNIT 1",2,10.77]
["KERRGN_1_UNIT 1",3,18.66]
["KERRGN_1_UNIT 1",4,23.74]
["KERRGN_1_UNIT 1",5,24.06]
["KERRGN_1_UNIT 1",6,23.87]
["KERRGN_1_UNIT 1",7,21.7]
["KERRGN_1_UNIT 1",8,18.38]
["KERRGN_1_UNIT 1",9,13.57]
["KERRGN_1_UNIT 1",10,11.48]
["KERRGN_1_UNIT 1",11,12.31]
["KERRGN_1_UNIT 1",12,13.84]
["KINGCO_1_KINGBR",1,34.5]
["KINGCO_1_KINGBR",2,34.5]
["KINGCO_1_KINGBR",3,34.5]
["KINGCO_1_KINGBR",4,34.5]
["KINGCO_1_KINGBR",5,34.5]
["KINGCO_1_KINGBR",6,34.5]
["KINGCO_1_KINGBR",7,34.5]
["KINGCO_1_KINGBR",8,34.5]
["KINGCO_1_KINGBR",9,34.5]
["KINGCO_1_KINGBR",10,34.5]
["KINGCO_1_KINGBR",11,34.5]
["KINGCO_1_KINGBR",12,34.5]
["KINGRV_7_UNIT 1",1,32]
["KINGRV_7_UNIT 1",2,32]
["KINGRV_7_UNIT 1",3,11.2]
["KINGRV_7_UNIT 1",4,11.2]
["KINGRV_7_UNIT 1",5,11.2]
["KINGRV_7_UNIT 1",6,32]
["KINGRV_7_UNIT 1",7,38.4]
["KINGRV_7_UNIT 1",8,39.36]
["KINGRV_7_UNIT 1",9,40.799999999999997]
["KINGRV_7_UNIT 1",10,40.799999999999997]
["KINGRV_7_UNIT 1",11,40.799999999999997]
["KINGRV_7_UNIT 1",12,40.96]
["KIRKER_7_KELCYN",1,3.56]
["KIRKER_7_KELCYN",2,3.53]
["KIRKER_7_KELCYN",3,3.56]
["KIRKER_7_KELCYN",4,3.44]
["KIRKER_7_KELCYN",5,3.56]
["KIRKER_7_KELCYN",6,3.35]
["KIRKER_7_KELCYN",7,3.56]
["KIRKER_7_KELCYN",8,3.44]
["KIRKER_7_KELCYN",9,3.56]
["KIRKER_7_KELCYN",10,3.56]
["KIRKER_7_KELCYN",11,3.56]
["KIRKER_7_KELCYN",12,3.56]
["KNGBRD_2_SOLAR1",1,0.08]
["KNGBRD_2_SOLAR1",2,0.6]
["KNGBRD_2_SOLAR1",3,0.7]
["KNGBRD_2_SOLAR1",4,0.88]
["KNGBRD_2_SOLAR1",5,1.28]
["KNGBRD_2_SOLAR1",6,2.62]
["KNGBRD_2_SOLAR1",7,2.88]
["KNGBRD_2_SOLAR1",8,2.48]
["KNGBRD_2_SOLAR1",9,2.2200000000000002]
["KNGBRD_2_SOLAR1",10,1.48]
["KNGBRD_2_SOLAR1",11,1.1399999999999999]
["KNGBRD_2_SOLAR1",12,0.7]
["KNGBRD_2_SOLAR2",1,0.08]
["KNGBRD_2_SOLAR2",2,0.6]
["KNGBRD_2_SOLAR2",3,0.7]
["KNGBRD_2_SOLAR2",4,0.88]
["KNGBRD_2_SOLAR2",5,1.28]
["KNGBRD_2_SOLAR2",6,2.62]
["KNGBRD_2_SOLAR2",7,2.88]
["KNGBRD_2_SOLAR2",8,2.48]
["KNGBRD_2_SOLAR2",9,2.2200000000000002]
["KNGBRD_2_SOLAR2",10,1.48]
["KNGBRD_2_SOLAR2",11,1.1399999999999999]
["KNGBRD_2_SOLAR2",12,0.7]
["KNGBRG_1_KBSLR1",1,0]
["KNGBRG_1_KBSLR1",2,0]
["KNGBRG_1_KBSLR1",3,0]
["KNGBRG_1_KBSLR1",4,0]
["KNGBRG_1_KBSLR1",5,0]
["KNGBRG_1_KBSLR1",6,0]
["KNGBRG_1_KBSLR1",7,0]
["KNGBRG_1_KBSLR1",8,0]
["KNGBRG_1_KBSLR1",9,0]
["KNGBRG_1_KBSLR1",10,0]
["KNGBRG_1_KBSLR1",11,0]
["KNGBRG_1_KBSLR1",12,0]
["KNGBRG_1_KBSLR2",1,0]
["KNGBRG_1_KBSLR2",2,0]
["KNGBRG_1_KBSLR2",3,0]
["KNGBRG_1_KBSLR2",4,0]
["KNGBRG_1_KBSLR2",5,0]
["KNGBRG_1_KBSLR2",6,0]
["KNGBRG_1_KBSLR2",7,0]
["KNGBRG_1_KBSLR2",8,0]
["KNGBRG_1_KBSLR2",9,0]
["KNGBRG_1_KBSLR2",10,0]
["KNGBRG_1_KBSLR2",11,0]
["KNGBRG_1_KBSLR2",12,0]
["KNGCTY_6_UNITA1",1,44.6]
["KNGCTY_6_UNITA1",2,44.6]
["KNGCTY_6_UNITA1",3,44.6]
["KNGCTY_6_UNITA1",4,44.6]
["KNGCTY_6_UNITA1",5,44.6]
["KNGCTY_6_UNITA1",6,44.6]
["KNGCTY_6_UNITA1",7,44.6]
["KNGCTY_6_UNITA1",8,44.6]
["KNGCTY_6_UNITA1",9,44.6]
["KNGCTY_6_UNITA1",10,44.6]
["KNGCTY_6_UNITA1",11,44.6]
["KNGCTY_6_UNITA1",12,44.6]
["KNTSTH_6_SOLAR",1,0]
["KNTSTH_6_SOLAR",2,0]
["KNTSTH_6_SOLAR",3,0]
["KNTSTH_6_SOLAR",4,0]
["KNTSTH_6_SOLAR",5,0]
["KNTSTH_6_SOLAR",6,0]
["KNTSTH_6_SOLAR",7,0]
["KNTSTH_6_SOLAR",8,0]
["KNTSTH_6_SOLAR",9,0]
["KNTSTH_6_SOLAR",10,0]
["KNTSTH_6_SOLAR",11,0]
["KNTSTH_6_SOLAR",12,0]
["KRAMER_2_SEGS 9",1,0.32]
["KRAMER_2_SEGS 9",2,2.4]
["KRAMER_2_SEGS 9",3,2.8]
["KRAMER_2_SEGS 9",4,3.52]
["KRAMER_2_SEGS 9",5,5.12]
["KRAMER_2_SEGS 9",6,10.48]
["KRAMER_2_SEGS 9",7,11.52]
["KRAMER_2_SEGS 9",8,9.92]
["KRAMER_2_SEGS 9",9,8.8800000000000008]
["KRAMER_2_SEGS 9",10,5.92]
["KRAMER_2_SEGS 9",11,4.5599999999999996]
["KRAMER_2_SEGS 9",12,2.8]
["KRNCNY_6_UNIT",1,6.02]
["KRNCNY_6_UNIT",2,5.66]
["KRNCNY_6_UNIT",3,6.5]
["KRNCNY_6_UNIT",4,7.34]
["KRNCNY_6_UNIT",5,7.49]
["KRNCNY_6_UNIT",6,6.53]
["KRNCNY_6_UNIT",7,6.02]
["KRNCNY_6_UNIT",8,4.6399999999999997]
["KRNCNY_6_UNIT",9,4.5]
["KRNCNY_6_UNIT",10,3.53]
["KRNCNY_6_UNIT",11,3.6]
["KRNCNY_6_UNIT",12,4.05]
["KYCORA_6_KMSBT1",1,0]
["KYCORA_6_KMSBT1",2,0]
["KYCORA_6_KMSBT1",3,0]
["KYCORA_6_KMSBT1",4,0]
["KYCORA_6_KMSBT1",5,0]
["KYCORA_6_KMSBT1",6,0]
["KYCORA_6_KMSBT1",7,0]
["KYCORA_6_KMSBT1",8,0]
["KYCORA_6_KMSBT1",9,0]
["KYCORA_6_KMSBT1",10,0]
["KYCORA_6_KMSBT1",11,0]
["KYCORA_6_KMSBT1",12,0]
["LACIEN_2_VENICE",1,0]
["LACIEN_2_VENICE",2,0]
["LACIEN_2_VENICE",3,0]
["LACIEN_2_VENICE",4,0]
["LACIEN_2_VENICE",5,0]
["LACIEN_2_VENICE",6,0]
["LACIEN_2_VENICE",7,0]
["LACIEN_2_VENICE",8,0]
["LACIEN_2_VENICE",9,0]
["LACIEN_2_VENICE",10,0]
["LACIEN_2_VENICE",11,0]
["LACIEN_2_VENICE",12,0]
["LAKHDG_6_UNIT 1",1,20]
["LAKHDG_6_UNIT 1",2,20]
["LAKHDG_6_UNIT 1",3,20]
["LAKHDG_6_UNIT 1",4,20]
["LAKHDG_6_UNIT 1",5,20]
["LAKHDG_6_UNIT 1",6,20]
["LAKHDG_6_UNIT 1",7,20]
["LAKHDG_6_UNIT 1",8,20]
["LAKHDG_6_UNIT 1",9,20]
["LAKHDG_6_UNIT 1",10,20]
["LAKHDG_6_UNIT 1",11,20]
["LAKHDG_6_UNIT 1",12,20]
["LAKHDG_6_UNIT 2",1,20]
["LAKHDG_6_UNIT 2",2,20]
["LAKHDG_6_UNIT 2",3,20]
["LAKHDG_6_UNIT 2",4,20]
["LAKHDG_6_UNIT 2",5,20]
["LAKHDG_6_UNIT 2",6,20]
["LAKHDG_6_UNIT 2",7,20]
["LAKHDG_6_UNIT 2",8,20]
["LAKHDG_6_UNIT 2",9,20]
["LAKHDG_6_UNIT 2",10,20]
["LAKHDG_6_UNIT 2",11,20]
["LAKHDG_6_UNIT 2",12,20]
["LAMONT_1_SOLAR1",1,0.24]
["LAMONT_1_SOLAR1",2,1.8]
["LAMONT_1_SOLAR1",3,2.1]
["LAMONT_1_SOLAR1",4,2.64]
["LAMONT_1_SOLAR1",5,3.84]
["LAMONT_1_SOLAR1",6,7.86]
["LAMONT_1_SOLAR1",7,8.64]
["LAMONT_1_SOLAR1",8,7.44]
["LAMONT_1_SOLAR1",9,6.66]
["LAMONT_1_SOLAR1",10,4.4400000000000004]
["LAMONT_1_SOLAR1",11,3.42]
["LAMONT_1_SOLAR1",12,2.1]
["LAMONT_1_SOLAR2",1,0.08]
["LAMONT_1_SOLAR2",2,0.6]
["LAMONT_1_SOLAR2",3,0.7]
["LAMONT_1_SOLAR2",4,0.88]
["LAMONT_1_SOLAR2",5,1.28]
["LAMONT_1_SOLAR2",6,2.62]
["LAMONT_1_SOLAR2",7,2.88]
["LAMONT_1_SOLAR2",8,2.48]
["LAMONT_1_SOLAR2",9,2.2200000000000002]
["LAMONT_1_SOLAR2",10,1.48]
["LAMONT_1_SOLAR2",11,1.1399999999999999]
["LAMONT_1_SOLAR2",12,0.7]
["LAMONT_1_SOLAR3",1,0.06]
["LAMONT_1_SOLAR3",2,0.45]
["LAMONT_1_SOLAR3",3,0.52]
["LAMONT_1_SOLAR3",4,0.66]
["LAMONT_1_SOLAR3",5,0.96]
["LAMONT_1_SOLAR3",6,1.96]
["LAMONT_1_SOLAR3",7,2.16]
["LAMONT_1_SOLAR3",8,1.86]
["LAMONT_1_SOLAR3",9,1.66]
["LAMONT_1_SOLAR3",10,1.1100000000000001]
["LAMONT_1_SOLAR3",11,0.85]
["LAMONT_1_SOLAR3",12,0.52]
["LAMONT_1_SOLAR4",1,0.11]
["LAMONT_1_SOLAR4",2,0.8]
["LAMONT_1_SOLAR4",3,0.93]
["LAMONT_1_SOLAR4",4,1.17]
["LAMONT_1_SOLAR4",5,1.71]
["LAMONT_1_SOLAR4",6,3.49]
["LAMONT_1_SOLAR4",7,3.84]
["LAMONT_1_SOLAR4",8,3.31]
["LAMONT_1_SOLAR4",9,2.96]
["LAMONT_1_SOLAR4",10,1.97]
["LAMONT_1_SOLAR4",11,1.52]
["LAMONT_1_SOLAR4",12,0.93]
["LAMONT_1_SOLAR5",1,7.0000000000000007E-2]
["LAMONT_1_SOLAR5",2,0.5]
["LAMONT_1_SOLAR5",3,0.57999999999999996]
["LAMONT_1_SOLAR5",4,0.73]
["LAMONT_1_SOLAR5",5,1.07]
["LAMONT_1_SOLAR5",6,2.1800000000000002]
["LAMONT_1_SOLAR5",7,2.4]
["LAMONT_1_SOLAR5",8,2.0699999999999998]
["LAMONT_1_SOLAR5",9,1.85]
["LAMONT_1_SOLAR5",10,1.23]
["LAMONT_1_SOLAR5",11,0.95]
["LAMONT_1_SOLAR5",12,0.57999999999999996]
["LAPLMA_2_UNIT 1",1,267]
["LAPLMA_2_UNIT 1",2,267]
["LAPLMA_2_UNIT 1",3,267]
["LAPLMA_2_UNIT 1",4,267]
["LAPLMA_2_UNIT 1",5,267]
["LAPLMA_2_UNIT 1",6,267]
["LAPLMA_2_UNIT 1",7,267]
["LAPLMA_2_UNIT 1",8,267]
["LAPLMA_2_UNIT 1",9,267]
["LAPLMA_2_UNIT 1",10,267]
["LAPLMA_2_UNIT 1",11,267]
["LAPLMA_2_UNIT 1",12,267]
["LAPLMA_2_UNIT 2",1,266]
["LAPLMA_2_UNIT 2",2,266]
["LAPLMA_2_UNIT 2",3,266]
["LAPLMA_2_UNIT 2",4,266]
["LAPLMA_2_UNIT 2",5,266]
["LAPLMA_2_UNIT 2",6,266]
["LAPLMA_2_UNIT 2",7,266]
["LAPLMA_2_UNIT 2",8,266]
["LAPLMA_2_UNIT 2",9,266]
["LAPLMA_2_UNIT 2",10,266]
["LAPLMA_2_UNIT 2",11,266]
["LAPLMA_2_UNIT 2",12,266]
["LAPLMA_2_UNIT 3",1,266]
["LAPLMA_2_UNIT 3",2,266]
["LAPLMA_2_UNIT 3",3,266]
["LAPLMA_2_UNIT 3",4,266]
["LAPLMA_2_UNIT 3",5,266]
["LAPLMA_2_UNIT 3",6,266]
["LAPLMA_2_UNIT 3",7,266]
["LAPLMA_2_UNIT 3",8,266]
["LAPLMA_2_UNIT 3",9,266]
["LAPLMA_2_UNIT 3",10,266]
["LAPLMA_2_UNIT 3",11,266]
["LAPLMA_2_UNIT 3",12,266]
["LAPLMA_2_UNIT 4",1,267]
["LAPLMA_2_UNIT 4",2,267]
["LAPLMA_2_UNIT 4",3,267]
["LAPLMA_2_UNIT 4",4,267]
["LAPLMA_2_UNIT 4",5,267]
["LAPLMA_2_UNIT 4",6,267]
["LAPLMA_2_UNIT 4",7,267]
["LAPLMA_2_UNIT 4",8,267]
["LAPLMA_2_UNIT 4",9,267]
["LAPLMA_2_UNIT 4",10,267]
["LAPLMA_2_UNIT 4",11,267]
["LAPLMA_2_UNIT 4",12,267]
["LARKSP_6_UNIT 1",1,49]
["LARKSP_6_UNIT 1",2,49]
["LARKSP_6_UNIT 1",3,49]
["LARKSP_6_UNIT 1",4,49]
["LARKSP_6_UNIT 1",5,49]
["LARKSP_6_UNIT 1",6,49]
["LARKSP_6_UNIT 1",7,49]
["LARKSP_6_UNIT 1",8,49]
["LARKSP_6_UNIT 1",9,49]
["LARKSP_6_UNIT 1",10,49]
["LARKSP_6_UNIT 1",11,49]
["LARKSP_6_UNIT 1",12,49]
["LARKSP_6_UNIT 2",1,49]
["LARKSP_6_UNIT 2",2,49]
["LARKSP_6_UNIT 2",3,49]
["LARKSP_6_UNIT 2",4,49]
["LARKSP_6_UNIT 2",5,49]
["LARKSP_6_UNIT 2",6,49]
["LARKSP_6_UNIT 2",7,49]
["LARKSP_6_UNIT 2",8,49]
["LARKSP_6_UNIT 2",9,49]
["LARKSP_6_UNIT 2",10,49]
["LARKSP_6_UNIT 2",11,49]
["LARKSP_6_UNIT 2",12,49]
["LAROA2_2_UNITA1",1,322]
["LAROA2_2_UNITA1",2,322]
["LAROA2_2_UNITA1",3,322]
["LAROA2_2_UNITA1",4,322]
["LAROA2_2_UNITA1",5,322]
["LAROA2_2_UNITA1",6,322]
["LAROA2_2_UNITA1",7,322]
["LAROA2_2_UNITA1",8,322]
["LAROA2_2_UNITA1",9,322]
["LAROA2_2_UNITA1",10,322]
["LAROA2_2_UNITA1",11,322]
["LAROA2_2_UNITA1",12,322]
["LASSEN_6_UNITS",1,30]
["LASSEN_6_UNITS",2,30]
["LASSEN_6_UNITS",3,30]
["LASSEN_6_UNITS",4,30]
["LASSEN_6_UNITS",5,30]
["LASSEN_6_UNITS",6,30]
["LASSEN_6_UNITS",7,30]
["LASSEN_6_UNITS",8,30]
["LASSEN_6_UNITS",9,30]
["LASSEN_6_UNITS",10,30]
["LASSEN_6_UNITS",11,30]
["LASSEN_6_UNITS",12,30]
["LAWRNC_7_SUNYVL",1,0.11]
["LAWRNC_7_SUNYVL",2,0.04]
["LAWRNC_7_SUNYVL",3,7.0000000000000007E-2]
["LAWRNC_7_SUNYVL",4,0.14000000000000001]
["LAWRNC_7_SUNYVL",5,0.16]
["LAWRNC_7_SUNYVL",6,0.13]
["LAWRNC_7_SUNYVL",7,0.12]
["LAWRNC_7_SUNYVL",8,0.15]
["LAWRNC_7_SUNYVL",9,0.13]
["LAWRNC_7_SUNYVL",10,7.0000000000000007E-2]
["LAWRNC_7_SUNYVL",11,0.09]
["LAWRNC_7_SUNYVL",12,0.18]
["LEBECS_2_UNITS",1,799.47]
["LEBECS_2_UNITS",2,799.47]
["LEBECS_2_UNITS",3,795]
["LEBECS_2_UNITS",4,785]
["LEBECS_2_UNITS",5,775]
["LEBECS_2_UNITS",6,775]
["LEBECS_2_UNITS",7,775]
["LEBECS_2_UNITS",8,775]
["LEBECS_2_UNITS",9,775]
["LEBECS_2_UNITS",10,785]
["LEBECS_2_UNITS",11,799.47]
["LEBECS_2_UNITS",12,799.47]
["LECEF_1_UNITS",1,304]
["LECEF_1_UNITS",2,304]
["LECEF_1_UNITS",3,304]
["LECEF_1_UNITS",4,303]
["LECEF_1_UNITS",5,303]
["LECEF_1_UNITS",6,302]
["LECEF_1_UNITS",7,302]
["LECEF_1_UNITS",8,299]
["LECEF_1_UNITS",9,302]
["LECEF_1_UNITS",10,303]
["LECEF_1_UNITS",11,303]
["LECEF_1_UNITS",12,303]
["LECONT_2_LESBT1",1,40]
["LECONT_2_LESBT1",2,40]
["LECONT_2_LESBT1",3,40]
["LECONT_2_LESBT1",4,40]
["LECONT_2_LESBT1",5,40]
["LECONT_2_LESBT1",6,40]
["LECONT_2_LESBT1",7,40]
["LECONT_2_LESBT1",8,40]
["LECONT_2_LESBT1",9,40]
["LECONT_2_LESBT1",10,40]
["LECONT_2_LESBT1",11,40]
["LECONT_2_LESBT1",12,40]
["LEPRFD_1_KANSAS",1,0.08]
["LEPRFD_1_KANSAS",2,0.6]
["LEPRFD_1_KANSAS",3,0.7]
["LEPRFD_1_KANSAS",4,0.88]
["LEPRFD_1_KANSAS",5,1.28]
["LEPRFD_1_KANSAS",6,2.62]
["LEPRFD_1_KANSAS",7,2.88]
["LEPRFD_1_KANSAS",8,2.48]
["LEPRFD_1_KANSAS",9,2.2200000000000002]
["LEPRFD_1_KANSAS",10,1.48]
["LEPRFD_1_KANSAS",11,1.1399999999999999]
["LEPRFD_1_KANSAS",12,0.7]
["LGHTHP_6_ICEGEN",1,48]
["LGHTHP_6_ICEGEN",2,48]
["LGHTHP_6_ICEGEN",3,48]
["LGHTHP_6_ICEGEN",4,48]
["LGHTHP_6_ICEGEN",5,48]
["LGHTHP_6_ICEGEN",6,48]
["LGHTHP_6_ICEGEN",7,48]
["LGHTHP_6_ICEGEN",8,48]
["LGHTHP_6_ICEGEN",9,48]
["LGHTHP_6_ICEGEN",10,48]
["LGHTHP_6_ICEGEN",11,48]
["LGHTHP_6_ICEGEN",12,48]
["LHILLS_6_SOLAR1",1,0.08]
["LHILLS_6_SOLAR1",2,0.6]
["LHILLS_6_SOLAR1",3,0.7]
["LHILLS_6_SOLAR1",4,0.88]
["LHILLS_6_SOLAR1",5,1.28]
["LHILLS_6_SOLAR1",6,2.62]
["LHILLS_6_SOLAR1",7,2.88]
["LHILLS_6_SOLAR1",8,2.48]
["LHILLS_6_SOLAR1",9,2.2200000000000002]
["LHILLS_6_SOLAR1",10,1.48]
["LHILLS_6_SOLAR1",11,1.1399999999999999]
["LHILLS_6_SOLAR1",12,0.7]
["LILIAC_6_SOLAR",1,0.01]
["LILIAC_6_SOLAR",2,0.09]
["LILIAC_6_SOLAR",3,0.11]
["LILIAC_6_SOLAR",4,0.13]
["LILIAC_6_SOLAR",5,0.19]
["LILIAC_6_SOLAR",6,0.39]
["LILIAC_6_SOLAR",7,0.43]
["LILIAC_6_SOLAR",8,0.37]
["LILIAC_6_SOLAR",9,0.33]
["LILIAC_6_SOLAR",10,0.22]
["LILIAC_6_SOLAR",11,0.17]
["LILIAC_6_SOLAR",12,0.11]
["LITLRK_6_GBCSR1",1,0.01]
["LITLRK_6_GBCSR1",2,0.09]
["LITLRK_6_GBCSR1",3,0.11]
["LITLRK_6_GBCSR1",4,0.13]
["LITLRK_6_GBCSR1",5,0.19]
["LITLRK_6_GBCSR1",6,0.39]
["LITLRK_6_GBCSR1",7,0.43]
["LITLRK_6_GBCSR1",8,0.37]
["LITLRK_6_GBCSR1",9,0.33]
["LITLRK_6_GBCSR1",10,0.22]
["LITLRK_6_GBCSR1",11,0.17]
["LITLRK_6_GBCSR1",12,0.11]
["LITLRK_6_SEPV01",1,0]
["LITLRK_6_SEPV01",2,0]
["LITLRK_6_SEPV01",3,0]
["LITLRK_6_SEPV01",4,0]
["LITLRK_6_SEPV01",5,0]
["LITLRK_6_SEPV01",6,0]
["LITLRK_6_SEPV01",7,0]
["LITLRK_6_SEPV01",8,0]
["LITLRK_6_SEPV01",9,0]
["LITLRK_6_SEPV01",10,0]
["LITLRK_6_SEPV01",11,0]
["LITLRK_6_SEPV01",12,0]
["LITLRK_6_SOLAR1",1,0.02]
["LITLRK_6_SOLAR1",2,0.15]
["LITLRK_6_SOLAR1",3,0.18]
["LITLRK_6_SOLAR1",4,0.22]
["LITLRK_6_SOLAR1",5,0.32]
["LITLRK_6_SOLAR1",6,0.66]
["LITLRK_6_SOLAR1",7,0.72]
["LITLRK_6_SOLAR1",8,0.62]
["LITLRK_6_SOLAR1",9,0.56000000000000005]
["LITLRK_6_SOLAR1",10,0.37]
["LITLRK_6_SOLAR1",11,0.28999999999999998]
["LITLRK_6_SOLAR1",12,0.18]
["LITLRK_6_SOLAR2",1,0.01]
["LITLRK_6_SOLAR2",2,0.06]
["LITLRK_6_SOLAR2",3,7.0000000000000007E-2]
["LITLRK_6_SOLAR2",4,0.09]
["LITLRK_6_SOLAR2",5,0.13]
["LITLRK_6_SOLAR2",6,0.26]
["LITLRK_6_SOLAR2",7,0.28999999999999998]
["LITLRK_6_SOLAR2",8,0.25]
["LITLRK_6_SOLAR2",9,0.22]
["LITLRK_6_SOLAR2",10,0.15]
["LITLRK_6_SOLAR2",11,0.11]
["LITLRK_6_SOLAR2",12,7.0000000000000007E-2]
["LITLRK_6_SOLAR3",1,0.01]
["LITLRK_6_SOLAR3",2,0.06]
["LITLRK_6_SOLAR3",3,7.0000000000000007E-2]
["LITLRK_6_SOLAR3",4,0.09]
["LITLRK_6_SOLAR3",5,0.13]
["LITLRK_6_SOLAR3",6,0.26]
["LITLRK_6_SOLAR3",7,0.28999999999999998]
["LITLRK_6_SOLAR3",8,0.25]
["LITLRK_6_SOLAR3",9,0.22]
["LITLRK_6_SOLAR3",10,0.15]
["LITLRK_6_SOLAR3",11,0.11]
["LITLRK_6_SOLAR3",12,7.0000000000000007E-2]
["LITLRK_6_SOLAR4",1,0.01]
["LITLRK_6_SOLAR4",2,0.09]
["LITLRK_6_SOLAR4",3,0.11]
["LITLRK_6_SOLAR4",4,0.13]
["LITLRK_6_SOLAR4",5,0.19]
["LITLRK_6_SOLAR4",6,0.39]
["LITLRK_6_SOLAR4",7,0.43]
["LITLRK_6_SOLAR4",8,0.37]
["LITLRK_6_SOLAR4",9,0.33]
["LITLRK_6_SOLAR4",10,0.22]
["LITLRK_6_SOLAR4",11,0.17]
["LITLRK_6_SOLAR4",12,0.11]
["LIVEOK_6_SOLAR",1,0]
["LIVEOK_6_SOLAR",2,0.02]
["LIVEOK_6_SOLAR",3,0.02]
["LIVEOK_6_SOLAR",4,0.02]
["LIVEOK_6_SOLAR",5,0.03]
["LIVEOK_6_SOLAR",6,0.06]
["LIVEOK_6_SOLAR",7,7.0000000000000007E-2]
["LIVEOK_6_SOLAR",8,0.06]
["LIVEOK_6_SOLAR",9,0.06]
["LIVEOK_6_SOLAR",10,0.04]
["LIVEOK_6_SOLAR",11,0.03]
["LIVEOK_6_SOLAR",12,0.02]
["LIVOAK_1_UNIT 1",1,49.7]
["LIVOAK_1_UNIT 1",2,49.7]
["LIVOAK_1_UNIT 1",3,49.7]
["LIVOAK_1_UNIT 1",4,49.7]
["LIVOAK_1_UNIT 1",5,49.7]
["LIVOAK_1_UNIT 1",6,49.7]
["LIVOAK_1_UNIT 1",7,49.7]
["LIVOAK_1_UNIT 1",8,49.7]
["LIVOAK_1_UNIT 1",9,49.7]
["LIVOAK_1_UNIT 1",10,49.7]
["LIVOAK_1_UNIT 1",11,49.7]
["LIVOAK_1_UNIT 1",12,49.7]
["LMBEPK_2_UNITA1",1,47.5]
["LMBEPK_2_UNITA1",2,47.5]
["LMBEPK_2_UNITA1",3,47.5]
["LMBEPK_2_UNITA1",4,47.5]
["LMBEPK_2_UNITA1",5,47.5]
["LMBEPK_2_UNITA1",6,47.5]
["LMBEPK_2_UNITA1",7,47.5]
["LMBEPK_2_UNITA1",8,47.5]
["LMBEPK_2_UNITA1",9,47.5]
["LMBEPK_2_UNITA1",10,47.5]
["LMBEPK_2_UNITA1",11,47.5]
["LMBEPK_2_UNITA1",12,47.5]
["LMBEPK_2_UNITA2",1,47.6]
["LMBEPK_2_UNITA2",2,47.6]
["LMBEPK_2_UNITA2",3,47.6]
["LMBEPK_2_UNITA2",4,47.6]
["LMBEPK_2_UNITA2",5,47.6]
["LMBEPK_2_UNITA2",6,47.6]
["LMBEPK_2_UNITA2",7,47.6]
["LMBEPK_2_UNITA2",8,47.6]
["LMBEPK_2_UNITA2",9,47.6]
["LMBEPK_2_UNITA2",10,47.6]
["LMBEPK_2_UNITA2",11,47.6]
["LMBEPK_2_UNITA2",12,47.6]
["LMBEPK_2_UNITA3",1,47.75]
["LMBEPK_2_UNITA3",2,47.75]
["LMBEPK_2_UNITA3",3,47.75]
["LMBEPK_2_UNITA3",4,47.75]
["LMBEPK_2_UNITA3",5,47.75]
["LMBEPK_2_UNITA3",6,47.75]
["LMBEPK_2_UNITA3",7,47.75]
["LMBEPK_2_UNITA3",8,47.75]
["LMBEPK_2_UNITA3",9,47.75]
["LMBEPK_2_UNITA3",10,47.75]
["LMBEPK_2_UNITA3",11,47.75]
["LMBEPK_2_UNITA3",12,47.75]
["LMEC_1_PL1X3",1,580]
["LMEC_1_PL1X3",2,580]
["LMEC_1_PL1X3",3,580]
["LMEC_1_PL1X3",4,580]
["LMEC_1_PL1X3",5,580]
["LMEC_1_PL1X3",6,580]
["LMEC_1_PL1X3",7,580]
["LMEC_1_PL1X3",8,580]
["LMEC_1_PL1X3",9,580]
["LMEC_1_PL1X3",10,580]
["LMEC_1_PL1X3",11,580]
["LMEC_1_PL1X3",12,580]
["LNCSTR_6_CREST",1,0]
["LNCSTR_6_CREST",2,0]
["LNCSTR_6_CREST",3,0]
["LNCSTR_6_CREST",4,0]
["LNCSTR_6_CREST",5,0]
["LNCSTR_6_CREST",6,0]
["LNCSTR_6_CREST",7,0]
["LNCSTR_6_CREST",8,0]
["LNCSTR_6_CREST",9,0]
["LNCSTR_6_CREST",10,0]
["LNCSTR_6_CREST",11,0]
["LNCSTR_6_CREST",12,0]
["LNCSTR_6_SOLAR2",1,3.13]
["LNCSTR_6_SOLAR2",2,4.1100000000000003]
["LNCSTR_6_SOLAR2",3,4.6100000000000003]
["LNCSTR_6_SOLAR2",4,5.26]
["LNCSTR_6_SOLAR2",5,5.28]
["LNCSTR_6_SOLAR2",6,5.33]
["LNCSTR_6_SOLAR2",7,5.34]
["LNCSTR_6_SOLAR2",8,5.31]
["LNCSTR_6_SOLAR2",9,5.26]
["LNCSTR_6_SOLAR2",10,4.6399999999999997]
["LNCSTR_6_SOLAR2",11,3.58]
["LNCSTR_6_SOLAR2",12,2.57]
["LOCKFD_1_BEARCK",1,0.01]
["LOCKFD_1_BEARCK",2,0.05]
["LOCKFD_1_BEARCK",3,0.05]
["LOCKFD_1_BEARCK",4,7.0000000000000007E-2]
["LOCKFD_1_BEARCK",5,0.1]
["LOCKFD_1_BEARCK",6,0.2]
["LOCKFD_1_BEARCK",7,0.22]
["LOCKFD_1_BEARCK",8,0.19]
["LOCKFD_1_BEARCK",9,0.17]
["LOCKFD_1_BEARCK",10,0.11]
["LOCKFD_1_BEARCK",11,0.09]
["LOCKFD_1_BEARCK",12,0.05]
["LOCKFD_1_KSOLAR",1,0]
["LOCKFD_1_KSOLAR",2,0.03]
["LOCKFD_1_KSOLAR",3,0.04]
["LOCKFD_1_KSOLAR",4,0.04]
["LOCKFD_1_KSOLAR",5,0.06]
["LOCKFD_1_KSOLAR",6,0.13]
["LOCKFD_1_KSOLAR",7,0.14000000000000001]
["LOCKFD_1_KSOLAR",8,0.12]
["LOCKFD_1_KSOLAR",9,0.11]
["LOCKFD_1_KSOLAR",10,7.0000000000000007E-2]
["LOCKFD_1_KSOLAR",11,0.06]
["LOCKFD_1_KSOLAR",12,0.04]
["LODI25_2_UNIT 1",1,23.8]
["LODI25_2_UNIT 1",2,23.8]
["LODI25_2_UNIT 1",3,23.8]
["LODI25_2_UNIT 1",4,23.8]
["LODI25_2_UNIT 1",5,23.8]
["LODI25_2_UNIT 1",6,23.8]
["LODI25_2_UNIT 1",7,23.8]
["LODI25_2_UNIT 1",8,23.8]
["LODI25_2_UNIT 1",9,23.8]
["LODI25_2_UNIT 1",10,23.8]
["LODI25_2_UNIT 1",11,23.8]
["LODI25_2_UNIT 1",12,23.8]
["LODIEC_2_PL1X2",1,302.58]
["LODIEC_2_PL1X2",2,302.58]
["LODIEC_2_PL1X2",3,302.58]
["LODIEC_2_PL1X2",4,302.58]
["LODIEC_2_PL1X2",5,302.58]
["LODIEC_2_PL1X2",6,302.58]
["LODIEC_2_PL1X2",7,302.58]
["LODIEC_2_PL1X2",8,302.58]
["LODIEC_2_PL1X2",9,302.58]
["LODIEC_2_PL1X2",10,302.58]
["LODIEC_2_PL1X2",11,302.58]
["LODIEC_2_PL1X2",12,302.58]
["LOTUS_6_LSFSR1",1,0.2]
["LOTUS_6_LSFSR1",2,1.5]
["LOTUS_6_LSFSR1",3,1.75]
["LOTUS_6_LSFSR1",4,2.2000000000000002]
["LOTUS_6_LSFSR1",5,3.2]
["LOTUS_6_LSFSR1",6,6.55]
["LOTUS_6_LSFSR1",7,7.2]
["LOTUS_6_LSFSR1",8,6.2]
["LOTUS_6_LSFSR1",9,5.55]
["LOTUS_6_LSFSR1",10,3.7]
["LOTUS_6_LSFSR1",11,2.85]
["LOTUS_6_LSFSR1",12,1.75]
["LOWGAP_1_SUPHR",1,0.42]
["LOWGAP_1_SUPHR",2,0.44]
["LOWGAP_1_SUPHR",3,0.42]
["LOWGAP_1_SUPHR",4,0.28000000000000003]
["LOWGAP_1_SUPHR",5,0.18]
["LOWGAP_1_SUPHR",6,0]
["LOWGAP_1_SUPHR",7,0]
["LOWGAP_1_SUPHR",8,0]
["LOWGAP_1_SUPHR",9,0]
["LOWGAP_1_SUPHR",10,0.05]
["LOWGAP_1_SUPHR",11,0.04]
["LOWGAP_1_SUPHR",12,0.09]
["LOWGAP_7_QFUNTS",1,0.59]
["LOWGAP_7_QFUNTS",2,1.08]
["LOWGAP_7_QFUNTS",3,0.97]
["LOWGAP_7_QFUNTS",4,0.83]
["LOWGAP_7_QFUNTS",5,0.65]
["LOWGAP_7_QFUNTS",6,0.38]
["LOWGAP_7_QFUNTS",7,0.19]
["LOWGAP_7_QFUNTS",8,0.15]
["LOWGAP_7_QFUNTS",9,0.24]
["LOWGAP_7_QFUNTS",10,0.26]
["LOWGAP_7_QFUNTS",11,0.7]
["LOWGAP_7_QFUNTS",12,0.43]
["LTBEAR_1_LB3SR3",1,0.08]
["LTBEAR_1_LB3SR3",2,0.6]
["LTBEAR_1_LB3SR3",3,0.7]
["LTBEAR_1_LB3SR3",4,0.88]
["LTBEAR_1_LB3SR3",5,1.28]
["LTBEAR_1_LB3SR3",6,2.62]
["LTBEAR_1_LB3SR3",7,2.88]
["LTBEAR_1_LB3SR3",8,2.48]
["LTBEAR_1_LB3SR3",9,2.2200000000000002]
["LTBEAR_1_LB3SR3",10,1.48]
["LTBEAR_1_LB3SR3",11,1.1399999999999999]
["LTBEAR_1_LB3SR3",12,0.7]
["LTBEAR_1_LB4SR4",1,0.2]
["LTBEAR_1_LB4SR4",2,1.5]
["LTBEAR_1_LB4SR4",3,1.75]
["LTBEAR_1_LB4SR4",4,2.2000000000000002]
["LTBEAR_1_LB4SR4",5,3.2]
["LTBEAR_1_LB4SR4",6,6.55]
["LTBEAR_1_LB4SR4",7,7.2]
["LTBEAR_1_LB4SR4",8,6.2]
["LTBEAR_1_LB4SR4",9,5.55]
["LTBEAR_1_LB4SR4",10,3.7]
["LTBEAR_1_LB4SR4",11,2.85]
["LTBEAR_1_LB4SR4",12,1.75]
["LTBEAR_1_LB4SR5",1,0.2]
["LTBEAR_1_LB4SR5",2,1.5]
["LTBEAR_1_LB4SR5",3,1.75]
["LTBEAR_1_LB4SR5",4,2.2000000000000002]
["LTBEAR_1_LB4SR5",5,3.2]
["LTBEAR_1_LB4SR5",6,6.55]
["LTBEAR_1_LB4SR5",7,7.2]
["LTBEAR_1_LB4SR5",8,6.2]
["LTBEAR_1_LB4SR5",9,5.55]
["LTBEAR_1_LB4SR5",10,3.7]
["LTBEAR_1_LB4SR5",11,2.85]
["LTBEAR_1_LB4SR5",12,1.75]
["LTBERA_1_LB1SR1",1,0.16]
["LTBERA_1_LB1SR1",2,1.2]
["LTBERA_1_LB1SR1",3,1.4]
["LTBERA_1_LB1SR1",4,1.76]
["LTBERA_1_LB1SR1",5,2.56]
["LTBERA_1_LB1SR1",6,5.24]
["LTBERA_1_LB1SR1",7,5.76]
["LTBERA_1_LB1SR1",8,4.96]
["LTBERA_1_LB1SR1",9,4.4400000000000004]
["LTBERA_1_LB1SR1",10,2.96]
["LTBERA_1_LB1SR1",11,2.2799999999999998]
["LTBERA_1_LB1SR1",12,1.4]
["MAGUND_1_BKISR1",1,0]
["MAGUND_1_BKISR1",2,0.03]
["MAGUND_1_BKISR1",3,0.04]
["MAGUND_1_BKISR1",4,0.04]
["MAGUND_1_BKISR1",5,0.06]
["MAGUND_1_BKISR1",6,0.13]
["MAGUND_1_BKISR1",7,0.14000000000000001]
["MAGUND_1_BKISR1",8,0.12]
["MAGUND_1_BKISR1",9,0.11]
["MAGUND_1_BKISR1",10,7.0000000000000007E-2]
["MAGUND_1_BKISR1",11,0.06]
["MAGUND_1_BKISR1",12,0.04]
["MAGUND_1_BKSSR2",1,0.02]
["MAGUND_1_BKSSR2",2,0.16]
["MAGUND_1_BKSSR2",3,0.18]
["MAGUND_1_BKSSR2",4,0.23]
["MAGUND_1_BKSSR2",5,0.34]
["MAGUND_1_BKSSR2",6,0.69]
["MAGUND_1_BKSSR2",7,0.76]
["MAGUND_1_BKSSR2",8,0.65]
["MAGUND_1_BKSSR2",9,0.57999999999999996]
["MAGUND_1_BKSSR2",10,0.39]
["MAGUND_1_BKSSR2",11,0.3]
["MAGUND_1_BKSSR2",12,0.18]
["MALAGA_1_PL1X2",1,96]
["MALAGA_1_PL1X2",2,96]
["MALAGA_1_PL1X2",3,96]
["MALAGA_1_PL1X2",4,96]
["MALAGA_1_PL1X2",5,96]
["MALAGA_1_PL1X2",6,96]
["MALAGA_1_PL1X2",7,96]
["MALAGA_1_PL1X2",8,96]
["MALAGA_1_PL1X2",9,96]
["MALAGA_1_PL1X2",10,96]
["MALAGA_1_PL1X2",11,96]
["MALAGA_1_PL1X2",12,96]
["MALCHQ_7_UNIT 1",1,3.87]
["MALCHQ_7_UNIT 1",2,17.11]
["MALCHQ_7_UNIT 1",3,12.79]
["MALCHQ_7_UNIT 1",4,14.25]
["MALCHQ_7_UNIT 1",5,7.95]
["MALCHQ_7_UNIT 1",6,5.3]
["MALCHQ_7_UNIT 1",7,2.13]
["MALCHQ_7_UNIT 1",8,0.14000000000000001]
["MALCHQ_7_UNIT 1",9,0]
["MALCHQ_7_UNIT 1",10,0.26]
["MALCHQ_7_UNIT 1",11,0.67]
["MALCHQ_7_UNIT 1",12,0.99]
["MANTEC_1_ML1SR1",1,0]
["MANTEC_1_ML1SR1",2,0]
["MANTEC_1_ML1SR1",3,0]
["MANTEC_1_ML1SR1",4,0]
["MANTEC_1_ML1SR1",5,0]
["MANTEC_1_ML1SR1",6,0]
["MANTEC_1_ML1SR1",7,0]
["MANTEC_1_ML1SR1",8,0]
["MANTEC_1_ML1SR1",9,0]
["MANTEC_1_ML1SR1",10,0]
["MANTEC_1_ML1SR1",11,0]
["MANTEC_1_ML1SR1",12,0]
["MANZNA_2_WIND",1,33.4]
["MANZNA_2_WIND",2,35.520000000000003]
["MANZNA_2_WIND",3,31.21]
["MANZNA_2_WIND",4,29.9]
["MANZNA_2_WIND",5,31.8]
["MANZNA_2_WIND",6,29.14]
["MANZNA_2_WIND",7,27.08]
["MANZNA_2_WIND",8,20.57]
["MANZNA_2_WIND",9,21.25]
["MANZNA_2_WIND",10,19.72]
["MANZNA_2_WIND",11,26.57]
["MANZNA_2_WIND",12,32.19]
["MARCPW_6_SOLAR1",1,0.08]
["MARCPW_6_SOLAR1",2,0.6]
["MARCPW_6_SOLAR1",3,0.7]
["MARCPW_6_SOLAR1",4,0.88]
["MARCPW_6_SOLAR1",5,1.28]
["MARCPW_6_SOLAR1",6,2.62]
["MARCPW_6_SOLAR1",7,2.88]
["MARCPW_6_SOLAR1",8,2.48]
["MARCPW_6_SOLAR1",9,2.2200000000000002]
["MARCPW_6_SOLAR1",10,1.48]
["MARCPW_6_SOLAR1",11,1.1399999999999999]
["MARCPW_6_SOLAR1",12,0.7]
["MARTIN_1_SUNSET",1,0.02]
["MARTIN_1_SUNSET",2,0.14000000000000001]
["MARTIN_1_SUNSET",3,0.16]
["MARTIN_1_SUNSET",4,0.2]
["MARTIN_1_SUNSET",5,0.28999999999999998]
["MARTIN_1_SUNSET",6,0.59]
["MARTIN_1_SUNSET",7,0.65]
["MARTIN_1_SUNSET",8,0.56000000000000005]
["MARTIN_1_SUNSET",9,0.5]
["MARTIN_1_SUNSET",10,0.33]
["MARTIN_1_SUNSET",11,0.26]
["MARTIN_1_SUNSET",12,0.16]
["MCARTH_6_FRIVRB",1,0.01]
["MCARTH_6_FRIVRB",2,0.05]
["MCARTH_6_FRIVRB",3,0.05]
["MCARTH_6_FRIVRB",4,7.0000000000000007E-2]
["MCARTH_6_FRIVRB",5,0.1]
["MCARTH_6_FRIVRB",6,0.2]
["MCARTH_6_FRIVRB",7,0.22]
["MCARTH_6_FRIVRB",8,0.19]
["MCARTH_6_FRIVRB",9,0.17]
["MCARTH_6_FRIVRB",10,0.11]
["MCARTH_6_FRIVRB",11,0.09]
["MCARTH_6_FRIVRB",12,0.05]
["MCCALL_1_QF",1,0.35]
["MCCALL_1_QF",2,0.45]
["MCCALL_1_QF",3,0.36]
["MCCALL_1_QF",4,0.28000000000000003]
["MCCALL_1_QF",5,0.36]
["MCCALL_1_QF",6,0.33]
["MCCALL_1_QF",7,0.32]
["MCCALL_1_QF",8,0.24]
["MCCALL_1_QF",9,0.36]
["MCCALL_1_QF",10,0.45]
["MCCALL_1_QF",11,0.35]
["MCCALL_1_QF",12,0.2]
["MCSWAN_6_UNITS",1,8.73]
["MCSWAN_6_UNITS",2,8.73]
["MCSWAN_6_UNITS",3,8.73]
["MCSWAN_6_UNITS",4,8.73]
["MCSWAN_6_UNITS",5,8.73]
["MCSWAN_6_UNITS",6,8.73]
["MCSWAN_6_UNITS",7,8.73]
["MCSWAN_6_UNITS",8,8.73]
["MCSWAN_6_UNITS",9,8.73]
["MCSWAN_6_UNITS",10,8.73]
["MCSWAN_6_UNITS",11,8.73]
["MCSWAN_6_UNITS",12,8.73]
["MDFKRL_2_PROJCT",1,210]
["MDFKRL_2_PROJCT",2,210]
["MDFKRL_2_PROJCT",3,210]
["MDFKRL_2_PROJCT",4,210]
["MDFKRL_2_PROJCT",5,210]
["MDFKRL_2_PROJCT",6,210]
["MDFKRL_2_PROJCT",7,210]
["MDFKRL_2_PROJCT",8,210]
["MDFKRL_2_PROJCT",9,210]
["MDFKRL_2_PROJCT",10,210]
["MDFKRL_2_PROJCT",11,210]
["MDFKRL_2_PROJCT",12,210]
["MENBIO_6_RENEW1",1,0.02]
["MENBIO_6_RENEW1",2,0.15]
["MENBIO_6_RENEW1",3,0.18]
["MENBIO_6_RENEW1",4,0.22]
["MENBIO_6_RENEW1",5,0.32]
["MENBIO_6_RENEW1",6,0.66]
["MENBIO_6_RENEW1",7,0.72]
["MENBIO_6_RENEW1",8,0.62]
["MENBIO_6_RENEW1",9,0.56000000000000005]
["MENBIO_6_RENEW1",10,0.37]
["MENBIO_6_RENEW1",11,0.28999999999999998]
["MENBIO_6_RENEW1",12,0.18]
["MERCED_1_SOLAR1",1,0]
["MERCED_1_SOLAR1",2,0]
["MERCED_1_SOLAR1",3,0]
["MERCED_1_SOLAR1",4,0]
["MERCED_1_SOLAR1",5,0]
["MERCED_1_SOLAR1",6,0]
["MERCED_1_SOLAR1",7,0]
["MERCED_1_SOLAR1",8,0]
["MERCED_1_SOLAR1",9,0]
["MERCED_1_SOLAR1",10,0]
["MERCED_1_SOLAR1",11,0]
["MERCED_1_SOLAR1",12,0]
["MERCED_1_SOLAR2",1,0]
["MERCED_1_SOLAR2",2,0]
["MERCED_1_SOLAR2",3,0]
["MERCED_1_SOLAR2",4,0]
["MERCED_1_SOLAR2",5,0]
["MERCED_1_SOLAR2",6,0]
["MERCED_1_SOLAR2",7,0]
["MERCED_1_SOLAR2",8,0]
["MERCED_1_SOLAR2",9,0]
["MERCED_1_SOLAR2",10,0]
["MERCED_1_SOLAR2",11,0]
["MERCED_1_SOLAR2",12,0]
["MERCFL_6_UNIT",1,3.26]
["MERCFL_6_UNIT",2,3.26]
["MERCFL_6_UNIT",3,3.26]
["MERCFL_6_UNIT",4,3.26]
["MERCFL_6_UNIT",5,3.26]
["MERCFL_6_UNIT",6,3.26]
["MERCFL_6_UNIT",7,3.26]
["MERCFL_6_UNIT",8,3.26]
["MERCFL_6_UNIT",9,3.26]
["MERCFL_6_UNIT",10,3.26]
["MERCFL_6_UNIT",11,3.26]
["MERCFL_6_UNIT",12,3.26]
["MESAP_1_QF",1,0]
["MESAP_1_QF",2,0]
["MESAP_1_QF",3,0]
["MESAP_1_QF",4,0]
["MESAP_1_QF",5,0]
["MESAP_1_QF",6,0]
["MESAP_1_QF",7,0]
["MESAP_1_QF",8,0]
["MESAP_1_QF",9,0]
["MESAP_1_QF",10,0]
["MESAP_1_QF",11,0]
["MESAP_1_QF",12,0]
["METEC_2_PL1X3",1,597.04999999999995]
["METEC_2_PL1X3",2,597.04999999999995]
["METEC_2_PL1X3",3,597.04999999999995]
["METEC_2_PL1X3",4,597.04999999999995]
["METEC_2_PL1X3",5,597.04999999999995]
["METEC_2_PL1X3",6,597.04999999999995]
["METEC_2_PL1X3",7,597.04999999999995]
["METEC_2_PL1X3",8,597.04999999999995]
["METEC_2_PL1X3",9,597.04999999999995]
["METEC_2_PL1X3",10,597.04999999999995]
["METEC_2_PL1X3",11,597.04999999999995]
["METEC_2_PL1X3",12,597.04999999999995]
["MIDWD_2_WIND2",1,0.53]
["MIDWD_2_WIND2",2,0.56000000000000005]
["MIDWD_2_WIND2",3,0.5]
["MIDWD_2_WIND2",4,0.47]
["MIDWD_2_WIND2",5,0.5]
["MIDWD_2_WIND2",6,0.46]
["MIDWD_2_WIND2",7,0.43]
["MIDWD_2_WIND2",8,0.33]
["MIDWD_2_WIND2",9,0.34]
["MIDWD_2_WIND2",10,0.31]
["MIDWD_2_WIND2",11,0.42]
["MIDWD_2_WIND2",12,0.51]
["MIDWD_7_CORAMB",1,1.33]
["MIDWD_7_CORAMB",2,1.41]
["MIDWD_7_CORAMB",3,1.24]
["MIDWD_7_CORAMB",4,1.19]
["MIDWD_7_CORAMB",5,1.26]
["MIDWD_7_CORAMB",6,1.1599999999999999]
["MIDWD_7_CORAMB",7,1.07]
["MIDWD_7_CORAMB",8,0.82]
["MIDWD_7_CORAMB",9,0.84]
["MIDWD_7_CORAMB",10,0.78]
["MIDWD_7_CORAMB",11,1.05]
["MIDWD_7_CORAMB",12,1.28]
["MIRLOM_2_CORONA",1,2]
["MIRLOM_2_CORONA",2,0.54]
["MIRLOM_2_CORONA",3,0.22]
["MIRLOM_2_CORONA",4,0.25]
["MIRLOM_2_CORONA",5,1.1299999999999999]
["MIRLOM_2_CORONA",6,1.33]
["MIRLOM_2_CORONA",7,0.33]
["MIRLOM_2_CORONA",8,0.64]
["MIRLOM_2_CORONA",9,1.18]
["MIRLOM_2_CORONA",10,1.42]
["MIRLOM_2_CORONA",11,0.87]
["MIRLOM_2_CORONA",12,1.24]
["MIRLOM_2_CREST",1,0]
["MIRLOM_2_CREST",2,0]
["MIRLOM_2_CREST",3,0]
["MIRLOM_2_CREST",4,0]
["MIRLOM_2_CREST",5,0]
["MIRLOM_2_CREST",6,0]
["MIRLOM_2_CREST",7,0]
["MIRLOM_2_CREST",8,0]
["MIRLOM_2_CREST",9,0]
["MIRLOM_2_CREST",10,0]
["MIRLOM_2_CREST",11,0]
["MIRLOM_2_CREST",12,0]
["MIRLOM_2_LNDFL",1,0.01]
["MIRLOM_2_LNDFL",2,0.09]
["MIRLOM_2_LNDFL",3,0.11]
["MIRLOM_2_LNDFL",4,0.13]
["MIRLOM_2_LNDFL",5,0.19]
["MIRLOM_2_LNDFL",6,0.39]
["MIRLOM_2_LNDFL",7,0.43]
["MIRLOM_2_LNDFL",8,0.37]
["MIRLOM_2_LNDFL",9,0.33]
["MIRLOM_2_LNDFL",10,0.22]
["MIRLOM_2_LNDFL",11,0.17]
["MIRLOM_2_LNDFL",12,0.11]
["MIRLOM_2_MLBBTA",1,10]
["MIRLOM_2_MLBBTA",2,10]
["MIRLOM_2_MLBBTA",3,10]
["MIRLOM_2_MLBBTA",4,10]
["MIRLOM_2_MLBBTA",5,10]
["MIRLOM_2_MLBBTA",6,10]
["MIRLOM_2_MLBBTA",7,10]
["MIRLOM_2_MLBBTA",8,10]
["MIRLOM_2_MLBBTA",9,10]
["MIRLOM_2_MLBBTA",10,10]
["MIRLOM_2_MLBBTA",11,10]
["MIRLOM_2_MLBBTA",12,10]
["MIRLOM_2_MLBBTB",1,10]
["MIRLOM_2_MLBBTB",2,10]
["MIRLOM_2_MLBBTB",3,10]
["MIRLOM_2_MLBBTB",4,10]
["MIRLOM_2_MLBBTB",5,10]
["MIRLOM_2_MLBBTB",6,10]
["MIRLOM_2_MLBBTB",7,10]
["MIRLOM_2_MLBBTB",8,10]
["MIRLOM_2_MLBBTB",9,10]
["MIRLOM_2_MLBBTB",10,10]
["MIRLOM_2_MLBBTB",11,10]
["MIRLOM_2_MLBBTB",12,10]
["MIRLOM_2_ONTARO",1,0.02]
["MIRLOM_2_ONTARO",2,0.17]
["MIRLOM_2_ONTARO",3,0.19]
["MIRLOM_2_ONTARO",4,0.24]
["MIRLOM_2_ONTARO",5,0.35]
["MIRLOM_2_ONTARO",6,0.72]
["MIRLOM_2_ONTARO",7,0.79]
["MIRLOM_2_ONTARO",8,0.68]
["MIRLOM_2_ONTARO",9,0.61]
["MIRLOM_2_ONTARO",10,0.41]
["MIRLOM_2_ONTARO",11,0.31]
["MIRLOM_2_ONTARO",12,0.19]
["MIRLOM_2_RTS032",1,0.01]
["MIRLOM_2_RTS032",2,0.05]
["MIRLOM_2_RTS032",3,0.05]
["MIRLOM_2_RTS032",4,7.0000000000000007E-2]
["MIRLOM_2_RTS032",5,0.1]
["MIRLOM_2_RTS032",6,0.2]
["MIRLOM_2_RTS032",7,0.22]
["MIRLOM_2_RTS032",8,0.19]
["MIRLOM_2_RTS032",9,0.17]
["MIRLOM_2_RTS032",10,0.11]
["MIRLOM_2_RTS032",11,0.09]
["MIRLOM_2_RTS032",12,0.05]
["MIRLOM_2_RTS033",1,0]
["MIRLOM_2_RTS033",2,0.03]
["MIRLOM_2_RTS033",3,0.04]
["MIRLOM_2_RTS033",4,0.04]
["MIRLOM_2_RTS033",5,0.06]
["MIRLOM_2_RTS033",6,0.13]
["MIRLOM_2_RTS033",7,0.14000000000000001]
["MIRLOM_2_RTS033",8,0.12]
["MIRLOM_2_RTS033",9,0.11]
["MIRLOM_2_RTS033",10,7.0000000000000007E-2]
["MIRLOM_2_RTS033",11,0.06]
["MIRLOM_2_RTS033",12,0.04]
["MIRLOM_2_TEMESC",1,2]
["MIRLOM_2_TEMESC",2,0.69]
["MIRLOM_2_TEMESC",3,0.28999999999999998]
["MIRLOM_2_TEMESC",4,0.91]
["MIRLOM_2_TEMESC",5,0.89]
["MIRLOM_2_TEMESC",6,0.82]
["MIRLOM_2_TEMESC",7,0.06]
["MIRLOM_2_TEMESC",8,0.77]
["MIRLOM_2_TEMESC",9,0.56000000000000005]
["MIRLOM_2_TEMESC",10,0.73]
["MIRLOM_2_TEMESC",11,0.85]
["MIRLOM_2_TEMESC",12,1.43]
["MIRLOM_6_PEAKER",1,47.18]
["MIRLOM_6_PEAKER",2,47.18]
["MIRLOM_6_PEAKER",3,47.18]
["MIRLOM_6_PEAKER",4,47.18]
["MIRLOM_6_PEAKER",5,47.18]
["MIRLOM_6_PEAKER",6,47.18]
["MIRLOM_6_PEAKER",7,47.18]
["MIRLOM_6_PEAKER",8,47.18]
["MIRLOM_6_PEAKER",9,47.18]
["MIRLOM_6_PEAKER",10,47.18]
["MIRLOM_6_PEAKER",11,47.18]
["MIRLOM_6_PEAKER",12,47.18]
["MIRLOM_7_MWDLKM",1,4]
["MIRLOM_7_MWDLKM",2,0]
["MIRLOM_7_MWDLKM",3,0]
["MIRLOM_7_MWDLKM",4,2.4]
["MIRLOM_7_MWDLKM",5,3]
["MIRLOM_7_MWDLKM",6,3.8]
["MIRLOM_7_MWDLKM",7,4]
["MIRLOM_7_MWDLKM",8,3.9]
["MIRLOM_7_MWDLKM",9,3.7]
["MIRLOM_7_MWDLKM",10,3.4]
["MIRLOM_7_MWDLKM",11,3]
["MIRLOM_7_MWDLKM",12,2.8]
["MISSIX_1_QF",1,0.01]
["MISSIX_1_QF",2,0.01]
["MISSIX_1_QF",3,0.01]
["MISSIX_1_QF",4,0.01]
["MISSIX_1_QF",5,0.01]
["MISSIX_1_QF",6,0.01]
["MISSIX_1_QF",7,0.01]
["MISSIX_1_QF",8,0.01]
["MISSIX_1_QF",9,0.01]
["MISSIX_1_QF",10,0.01]
["MISSIX_1_QF",11,0.01]
["MISSIX_1_QF",12,0.01]
["MKTRCK_1_UNIT 1",1,47.49]
["MKTRCK_1_UNIT 1",2,47.49]
["MKTRCK_1_UNIT 1",3,47.49]
["MKTRCK_1_UNIT 1",4,47.49]
["MKTRCK_1_UNIT 1",5,47.49]
["MKTRCK_1_UNIT 1",6,47.49]
["MKTRCK_1_UNIT 1",7,47.49]
["MKTRCK_1_UNIT 1",8,47.49]
["MKTRCK_1_UNIT 1",9,47.49]
["MKTRCK_1_UNIT 1",10,47.49]
["MKTRCK_1_UNIT 1",11,47.49]
["MKTRCK_1_UNIT 1",12,47.49]
["MLPTAS_7_QFUNTS",1,0]
["MLPTAS_7_QFUNTS",2,0]
["MLPTAS_7_QFUNTS",3,0]
["MLPTAS_7_QFUNTS",4,0]
["MLPTAS_7_QFUNTS",5,0]
["MLPTAS_7_QFUNTS",6,0]
["MLPTAS_7_QFUNTS",7,0]
["MLPTAS_7_QFUNTS",8,0]
["MLPTAS_7_QFUNTS",9,0]
["MLPTAS_7_QFUNTS",10,0]
["MLPTAS_7_QFUNTS",11,0]
["MLPTAS_7_QFUNTS",12,0]
["MNDALY_6_MCGRTH",1,48.56]
["MNDALY_6_MCGRTH",2,48.56]
["MNDALY_6_MCGRTH",3,48.56]
["MNDALY_6_MCGRTH",4,48.56]
["MNDALY_6_MCGRTH",5,48.56]
["MNDALY_6_MCGRTH",6,48.56]
["MNDALY_6_MCGRTH",7,48.56]
["MNDALY_6_MCGRTH",8,48.56]
["MNDALY_6_MCGRTH",9,48.56]
["MNDALY_6_MCGRTH",10,48.56]
["MNDALY_6_MCGRTH",11,48.56]
["MNDALY_6_MCGRTH",12,48.56]
["MNDOTA_1_SOLAR1",1,0.24]
["MNDOTA_1_SOLAR1",2,1.8]
["MNDOTA_1_SOLAR1",3,2.1]
["MNDOTA_1_SOLAR1",4,2.64]
["MNDOTA_1_SOLAR1",5,3.84]
["MNDOTA_1_SOLAR1",6,7.86]
["MNDOTA_1_SOLAR1",7,8.64]
["MNDOTA_1_SOLAR1",8,7.44]
["MNDOTA_1_SOLAR1",9,6.66]
["MNDOTA_1_SOLAR1",10,4.4400000000000004]
["MNDOTA_1_SOLAR1",11,3.42]
["MNDOTA_1_SOLAR1",12,2.1]
["MNDOTA_1_SOLAR2",1,0]
["MNDOTA_1_SOLAR2",2,0]
["MNDOTA_1_SOLAR2",3,0]
["MNDOTA_1_SOLAR2",4,0]
["MNDOTA_1_SOLAR2",5,0]
["MNDOTA_1_SOLAR2",6,0]
["MNDOTA_1_SOLAR2",7,0]
["MNDOTA_1_SOLAR2",8,0]
["MNDOTA_1_SOLAR2",9,0]
["MNDOTA_1_SOLAR2",10,0]
["MNDOTA_1_SOLAR2",11,0]
["MNDOTA_1_SOLAR2",12,0]
["MOJAVE_1_SIPHON",1,1.22]
["MOJAVE_1_SIPHON",2,1.01]
["MOJAVE_1_SIPHON",3,1.21]
["MOJAVE_1_SIPHON",4,6.55]
["MOJAVE_1_SIPHON",5,6.12]
["MOJAVE_1_SIPHON",6,6.58]
["MOJAVE_1_SIPHON",7,12.32]
["MOJAVE_1_SIPHON",8,10.75]
["MOJAVE_1_SIPHON",9,10.9]
["MOJAVE_1_SIPHON",10,11.55]
["MOJAVE_1_SIPHON",11,11.99]
["MOJAVE_1_SIPHON",12,9.6]
["MOJAVW_2_SOLAR",1,0.08]
["MOJAVW_2_SOLAR",2,0.6]
["MOJAVW_2_SOLAR",3,0.7]
["MOJAVW_2_SOLAR",4,0.88]
["MOJAVW_2_SOLAR",5,1.28]
["MOJAVW_2_SOLAR",6,2.62]
["MOJAVW_2_SOLAR",7,2.88]
["MOJAVW_2_SOLAR",8,2.48]
["MOJAVW_2_SOLAR",9,2.2200000000000002]
["MOJAVW_2_SOLAR",10,1.48]
["MOJAVW_2_SOLAR",11,1.1399999999999999]
["MOJAVW_2_SOLAR",12,0.7]
["MONTPH_7_UNITS",1,0.52]
["MONTPH_7_UNITS",2,0.91]
["MONTPH_7_UNITS",3,5.98]
["MONTPH_7_UNITS",4,7.42]
["MONTPH_7_UNITS",5,6.28]
["MONTPH_7_UNITS",6,8.6199999999999992]
["MONTPH_7_UNITS",7,8.7100000000000009]
["MONTPH_7_UNITS",8,7.09]
["MONTPH_7_UNITS",9,5.66]
["MONTPH_7_UNITS",10,1.36]
["MONTPH_7_UNITS",11,0.46]
["MONTPH_7_UNITS",12,0.43]
["MOORPK_2_ACOBT1",1,1]
["MOORPK_2_ACOBT1",2,1]
["MOORPK_2_ACOBT1",3,1]
["MOORPK_2_ACOBT1",4,1]
["MOORPK_2_ACOBT1",5,1]
["MOORPK_2_ACOBT1",6,1]
["MOORPK_2_ACOBT1",7,1]
["MOORPK_2_ACOBT1",8,1]
["MOORPK_2_ACOBT1",9,1]
["MOORPK_2_ACOBT1",10,1]
["MOORPK_2_ACOBT1",11,1]
["MOORPK_2_ACOBT1",12,1]
["MOORPK_2_CALABS",1,4.74]
["MOORPK_2_CALABS",2,4.5999999999999996]
["MOORPK_2_CALABS",3,4.2]
["MOORPK_2_CALABS",4,4.2699999999999996]
["MOORPK_2_CALABS",5,4.54]
["MOORPK_2_CALABS",6,4.49]
["MOORPK_2_CALABS",7,4.32]
["MOORPK_2_CALABS",8,3.98]
["MOORPK_2_CALABS",9,4.01]
["MOORPK_2_CALABS",10,4.47]
["MOORPK_2_CALABS",11,4.3899999999999997]
["MOORPK_2_CALABS",12,4.4000000000000004]
["MOORPK_6_QF",1,0.04]
["MOORPK_6_QF",2,0.05]
["MOORPK_6_QF",3,0.02]
["MOORPK_6_QF",4,0.01]
["MOORPK_6_QF",5,0]
["MOORPK_6_QF",6,0.06]
["MOORPK_6_QF",7,0.09]
["MOORPK_6_QF",8,0.32]
["MOORPK_6_QF",9,0.4]
["MOORPK_6_QF",10,0.4]
["MOORPK_6_QF",11,0.4]
["MOORPK_6_QF",12,0.39]
["MORWD_6_QF",1,6.74]
["MORWD_6_QF",2,7.17]
["MORWD_6_QF",3,6.3]
["MORWD_6_QF",4,6.04]
["MORWD_6_QF",5,6.42]
["MORWD_6_QF",6,5.88]
["MORWD_6_QF",7,5.47]
["MORWD_6_QF",8,4.1500000000000004]
["MORWD_6_QF",9,4.29]
["MORWD_6_QF",10,3.98]
["MORWD_6_QF",11,5.37]
["MORWD_6_QF",12,6.5]
["MOSSLD_1_QF",1,0.05]
["MOSSLD_1_QF",2,0.04]
["MOSSLD_1_QF",3,0.03]
["MOSSLD_1_QF",4,0.03]
["MOSSLD_1_QF",5,0.03]
["MOSSLD_1_QF",6,0.03]
["MOSSLD_1_QF",7,0.03]
["MOSSLD_1_QF",8,0.04]
["MOSSLD_1_QF",9,0.05]
["MOSSLD_1_QF",10,0.04]
["MOSSLD_1_QF",11,0.05]
["MOSSLD_1_QF",12,7.0000000000000007E-2]
["MOSSLD_2_PSP1",1,510]
["MOSSLD_2_PSP1",2,510]
["MOSSLD_2_PSP1",3,510]
["MOSSLD_2_PSP1",4,510]
["MOSSLD_2_PSP1",5,510]
["MOSSLD_2_PSP1",6,510]
["MOSSLD_2_PSP1",7,510]
["MOSSLD_2_PSP1",8,510]
["MOSSLD_2_PSP1",9,510]
["MOSSLD_2_PSP1",10,510]
["MOSSLD_2_PSP1",11,510]
["MOSSLD_2_PSP1",12,510]
["MOSSLD_2_PSP2",1,510]
["MOSSLD_2_PSP2",2,510]
["MOSSLD_2_PSP2",3,510]
["MOSSLD_2_PSP2",4,510]
["MOSSLD_2_PSP2",5,510]
["MOSSLD_2_PSP2",6,510]
["MOSSLD_2_PSP2",7,510]
["MOSSLD_2_PSP2",8,510]
["MOSSLD_2_PSP2",9,510]
["MOSSLD_2_PSP2",10,510]
["MOSSLD_2_PSP2",11,510]
["MOSSLD_2_PSP2",12,510]
["MRCHNT_2_PL1X3",1,419.25]
["MRCHNT_2_PL1X3",2,419.25]
["MRCHNT_2_PL1X3",3,419.25]
["MRCHNT_2_PL1X3",4,419.25]
["MRCHNT_2_PL1X3",5,419.25]
["MRCHNT_2_PL1X3",6,419.25]
["MRCHNT_2_PL1X3",7,419.25]
["MRCHNT_2_PL1X3",8,419.25]
["MRCHNT_2_PL1X3",9,419.25]
["MRCHNT_2_PL1X3",10,419.25]
["MRCHNT_2_PL1X3",11,419.25]
["MRCHNT_2_PL1X3",12,419.25]
["MRGT_6_MEF2",1,44]
["MRGT_6_MEF2",2,44]
["MRGT_6_MEF2",3,44]
["MRGT_6_MEF2",4,44]
["MRGT_6_MEF2",5,44]
["MRGT_6_MEF2",6,44]
["MRGT_6_MEF2",7,44]
["MRGT_6_MEF2",8,44]
["MRGT_6_MEF2",9,44]
["MRGT_6_MEF2",10,44]
["MRGT_6_MEF2",11,44]
["MRGT_6_MEF2",12,44]
["MRGT_6_MMAREF",1,45]
["MRGT_6_MMAREF",2,45]
["MRGT_6_MMAREF",3,45]
["MRGT_6_MMAREF",4,45]
["MRGT_6_MMAREF",5,45]
["MRGT_6_MMAREF",6,45]
["MRGT_6_MMAREF",7,45]
["MRGT_6_MMAREF",8,45]
["MRGT_6_MMAREF",9,45]
["MRGT_6_MMAREF",10,45]
["MRGT_6_MMAREF",11,45]
["MRGT_6_MMAREF",12,45]
["MRGT_6_TGEBT1",1,30]
["MRGT_6_TGEBT1",2,30]
["MRGT_6_TGEBT1",3,30]
["MRGT_6_TGEBT1",4,30]
["MRGT_6_TGEBT1",5,30]
["MRGT_6_TGEBT1",6,30]
["MRGT_6_TGEBT1",7,30]
["MRGT_6_TGEBT1",8,30]
["MRGT_6_TGEBT1",9,30]
["MRGT_6_TGEBT1",10,30]
["MRGT_6_TGEBT1",11,30]
["MRGT_6_TGEBT1",12,30]
["MRLSDS_6_SOLAR1",1,0.06]
["MRLSDS_6_SOLAR1",2,0.45]
["MRLSDS_6_SOLAR1",3,0.53]
["MRLSDS_6_SOLAR1",4,0.66]
["MRLSDS_6_SOLAR1",5,0.96]
["MRLSDS_6_SOLAR1",6,1.97]
["MRLSDS_6_SOLAR1",7,2.16]
["MRLSDS_6_SOLAR1",8,1.86]
["MRLSDS_6_SOLAR1",9,1.67]
["MRLSDS_6_SOLAR1",10,1.1100000000000001]
["MRLSDS_6_SOLAR1",11,0.86]
["MRLSDS_6_SOLAR1",12,0.53]
["MSHGTS_6_MMARLF",1,3.78]
["MSHGTS_6_MMARLF",2,3.63]
["MSHGTS_6_MMARLF",3,3.48]
["MSHGTS_6_MMARLF",4,3.95]
["MSHGTS_6_MMARLF",5,3.89]
["MSHGTS_6_MMARLF",6,3.87]
["MSHGTS_6_MMARLF",7,3.94]
["MSHGTS_6_MMARLF",8,3.7]
["MSHGTS_6_MMARLF",9,3.89]
["MSHGTS_6_MMARLF",10,3.87]
["MSHGTS_6_MMARLF",11,3.89]
["MSHGTS_6_MMARLF",12,3.61]
["MSOLAR_2_SOLAR1",1,0.66]
["MSOLAR_2_SOLAR1",2,4.95]
["MSOLAR_2_SOLAR1",3,5.78]
["MSOLAR_2_SOLAR1",4,7.26]
["MSOLAR_2_SOLAR1",5,10.56]
["MSOLAR_2_SOLAR1",6,21.62]
["MSOLAR_2_SOLAR1",7,23.76]
["MSOLAR_2_SOLAR1",8,20.46]
["MSOLAR_2_SOLAR1",9,18.32]
["MSOLAR_2_SOLAR1",10,12.21]
["MSOLAR_2_SOLAR1",11,9.41]
["MSOLAR_2_SOLAR1",12,5.78]
["MSOLAR_2_SOLAR2",1,0.4]
["MSOLAR_2_SOLAR2",2,3.02]
["MSOLAR_2_SOLAR2",3,3.53]
["MSOLAR_2_SOLAR2",4,4.4400000000000004]
["MSOLAR_2_SOLAR2",5,6.45]
["MSOLAR_2_SOLAR2",6,13.21]
["MSOLAR_2_SOLAR2",7,14.52]
["MSOLAR_2_SOLAR2",8,12.5]
["MSOLAR_2_SOLAR2",9,11.19]
["MSOLAR_2_SOLAR2",10,7.46]
["MSOLAR_2_SOLAR2",11,5.75]
["MSOLAR_2_SOLAR2",12,3.53]
["MSOLAR_2_SOLAR3",1,0.61]
["MSOLAR_2_SOLAR3",2,4.5599999999999996]
["MSOLAR_2_SOLAR3",3,5.32]
["MSOLAR_2_SOLAR3",4,6.69]
["MSOLAR_2_SOLAR3",5,9.73]
["MSOLAR_2_SOLAR3",6,19.91]
["MSOLAR_2_SOLAR3",7,21.89]
["MSOLAR_2_SOLAR3",8,18.850000000000001]
["MSOLAR_2_SOLAR3",9,16.87]
["MSOLAR_2_SOLAR3",10,11.25]
["MSOLAR_2_SOLAR3",11,8.66]
["MSOLAR_2_SOLAR3",12,5.32]
["MSSION_2_QF",1,0.15]
["MSSION_2_QF",2,0.15]
["MSSION_2_QF",3,0.15]
["MSSION_2_QF",4,0.19]
["MSSION_2_QF",5,0.28999999999999998]
["MSSION_2_QF",6,0.33]
["MSSION_2_QF",7,0.3]
["MSSION_2_QF",8,0.32]
["MSSION_2_QF",9,0.32]
["MSSION_2_QF",10,0.28000000000000003]
["MSSION_2_QF",11,0.26]
["MSSION_2_QF",12,0.16]
["MSTANG_2_MTGBT1",1,75]
["MSTANG_2_MTGBT1",2,75]
["MSTANG_2_MTGBT1",3,75]
["MSTANG_2_MTGBT1",4,75]
["MSTANG_2_MTGBT1",5,75]
["MSTANG_2_MTGBT1",6,75]
["MSTANG_2_MTGBT1",7,75]
["MSTANG_2_MTGBT1",8,75]
["MSTANG_2_MTGBT1",9,75]
["MSTANG_2_MTGBT1",10,75]
["MSTANG_2_MTGBT1",11,75]
["MSTANG_2_MTGBT1",12,75]
["MSTANG_2_SOLAR",1,0]
["MSTANG_2_SOLAR",2,0]
["MSTANG_2_SOLAR",3,0]
["MSTANG_2_SOLAR",4,0]
["MSTANG_2_SOLAR",5,0]
["MSTANG_2_SOLAR",6,0]
["MSTANG_2_SOLAR",7,0]
["MSTANG_2_SOLAR",8,0]
["MSTANG_2_SOLAR",9,0]
["MSTANG_2_SOLAR",10,0]
["MSTANG_2_SOLAR",11,0]
["MSTANG_2_SOLAR",12,0]
["MSTANG_2_SOLAR3",1,0.06]
["MSTANG_2_SOLAR3",2,0.45]
["MSTANG_2_SOLAR3",3,0.52]
["MSTANG_2_SOLAR3",4,0.66]
["MSTANG_2_SOLAR3",5,0.96]
["MSTANG_2_SOLAR3",6,1.96]
["MSTANG_2_SOLAR3",7,2.15]
["MSTANG_2_SOLAR3",8,1.85]
["MSTANG_2_SOLAR3",9,1.66]
["MSTANG_2_SOLAR3",10,1.1100000000000001]
["MSTANG_2_SOLAR3",11,0.85]
["MSTANG_2_SOLAR3",12,0.52]
["MSTANG_2_SOLAR4",1,0.12]
["MSTANG_2_SOLAR4",2,0.9]
["MSTANG_2_SOLAR4",3,1.05]
["MSTANG_2_SOLAR4",4,1.32]
["MSTANG_2_SOLAR4",5,1.92]
["MSTANG_2_SOLAR4",6,3.93]
["MSTANG_2_SOLAR4",7,4.32]
["MSTANG_2_SOLAR4",8,3.72]
["MSTANG_2_SOLAR4",9,3.33]
["MSTANG_2_SOLAR4",10,2.2200000000000002]
["MSTANG_2_SOLAR4",11,1.71]
["MSTANG_2_SOLAR4",12,1.05]
["MTNPOS_1_UNIT",1,43.37]
["MTNPOS_1_UNIT",2,40.619999999999997]
["MTNPOS_1_UNIT",3,31.39]
["MTNPOS_1_UNIT",4,43.55]
["MTNPOS_1_UNIT",5,43.34]
["MTNPOS_1_UNIT",6,42.44]
["MTNPOS_1_UNIT",7,42.48]
["MTNPOS_1_UNIT",8,41.48]
["MTNPOS_1_UNIT",9,40.6]
["MTNPOS_1_UNIT",10,40.450000000000003]
["MTNPOS_1_UNIT",11,38.979999999999997]
["MTNPOS_1_UNIT",12,29.01]
["MTWIND_1_MVPWD1",1,11.77]
["MTWIND_1_MVPWD1",2,12.52]
["MTWIND_1_MVPWD1",3,11]
["MTWIND_1_MVPWD1",4,10.54]
["MTWIND_1_MVPWD1",5,11.2]
["MTWIND_1_MVPWD1",6,10.27]
["MTWIND_1_MVPWD1",7,9.5399999999999991]
["MTWIND_1_MVPWD1",8,7.25]
["MTWIND_1_MVPWD1",9,7.49]
["MTWIND_1_MVPWD1",10,6.95]
["MTWIND_1_MVPWD1",11,9.36]
["MTWIND_1_MVPWD1",12,11.34]
["MTWIND_1_UNIT 3",1,3.97]
["MTWIND_1_UNIT 3",2,4.22]
["MTWIND_1_UNIT 3",3,3.71]
["MTWIND_1_UNIT 3",4,3.55]
["MTWIND_1_UNIT 3",5,3.78]
["MTWIND_1_UNIT 3",6,3.46]
["MTWIND_1_UNIT 3",7,3.21]
["MTWIND_1_UNIT 3",8,2.44]
["MTWIND_1_UNIT 3",9,2.52]
["MTWIND_1_UNIT 3",10,2.34]
["MTWIND_1_UNIT 3",11,3.15]
["MTWIND_1_UNIT 3",12,3.82]
["MURRAY_6_UNIT",1,0]
["MURRAY_6_UNIT",2,0]
["MURRAY_6_UNIT",3,0]
["MURRAY_6_UNIT",4,0]
["MURRAY_6_UNIT",5,0]
["MURRAY_6_UNIT",6,0]
["MURRAY_6_UNIT",7,0]
["MURRAY_6_UNIT",8,0]
["MURRAY_6_UNIT",9,0]
["MURRAY_6_UNIT",10,0]
["MURRAY_6_UNIT",11,0]
["MURRAY_6_UNIT",12,0]
["NAROW1_2_UNIT",1,6.05]
["NAROW1_2_UNIT",2,6.66]
["NAROW1_2_UNIT",3,9.41]
["NAROW1_2_UNIT",4,8.81]
["NAROW1_2_UNIT",5,8.93]
["NAROW1_2_UNIT",6,9.32]
["NAROW1_2_UNIT",7,9.02]
["NAROW1_2_UNIT",8,8.5]
["NAROW1_2_UNIT",9,7.71]
["NAROW1_2_UNIT",10,8.11]
["NAROW1_2_UNIT",11,6.41]
["NAROW1_2_UNIT",12,7]
["NAROW2_2_UNIT",1,8.24]
["NAROW2_2_UNIT",2,8.9600000000000009]
["NAROW2_2_UNIT",3,41.6]
["NAROW2_2_UNIT",4,39.659999999999997]
["NAROW2_2_UNIT",5,30.86]
["NAROW2_2_UNIT",6,27.4]
["NAROW2_2_UNIT",7,25.22]
["NAROW2_2_UNIT",8,20]
["NAROW2_2_UNIT",9,10]
["NAROW2_2_UNIT",10,10.8]
["NAROW2_2_UNIT",11,11.2]
["NAROW2_2_UNIT",12,11.52]
["NAVYII_2_UNITS",1,55]
["NAVYII_2_UNITS",2,55]
["NAVYII_2_UNITS",3,55]
["NAVYII_2_UNITS",4,55]
["NAVYII_2_UNITS",5,55]
["NAVYII_2_UNITS",6,55]
["NAVYII_2_UNITS",7,55]
["NAVYII_2_UNITS",8,55]
["NAVYII_2_UNITS",9,55]
["NAVYII_2_UNITS",10,55]
["NAVYII_2_UNITS",11,55]
["NAVYII_2_UNITS",12,55]
["NCPA_7_GP1UN1",1,38.85]
["NCPA_7_GP1UN1",2,38.85]
["NCPA_7_GP1UN1",3,38.85]
["NCPA_7_GP1UN1",4,38.85]
["NCPA_7_GP1UN1",5,38.85]
["NCPA_7_GP1UN1",6,38.85]
["NCPA_7_GP1UN1",7,38.85]
["NCPA_7_GP1UN1",8,38.85]
["NCPA_7_GP1UN1",9,38.85]
["NCPA_7_GP1UN1",10,38.85]
["NCPA_7_GP1UN1",11,38.85]
["NCPA_7_GP1UN1",12,38.85]
["NCPA_7_GP1UN2",1,39.94]
["NCPA_7_GP1UN2",2,39.94]
["NCPA_7_GP1UN2",3,39.94]
["NCPA_7_GP1UN2",4,39.94]
["NCPA_7_GP1UN2",5,39.94]
["NCPA_7_GP1UN2",6,39.94]
["NCPA_7_GP1UN2",7,39.94]
["NCPA_7_GP1UN2",8,39.94]
["NCPA_7_GP1UN2",9,39.94]
["NCPA_7_GP1UN2",10,39.94]
["NCPA_7_GP1UN2",11,39.94]
["NCPA_7_GP1UN2",12,39.94]
["NCPA_7_GP2UN3",1,0]
["NCPA_7_GP2UN3",2,0]
["NCPA_7_GP2UN3",3,0]
["NCPA_7_GP2UN3",4,0]
["NCPA_7_GP2UN3",5,0]
["NCPA_7_GP2UN3",6,0]
["NCPA_7_GP2UN3",7,0]
["NCPA_7_GP2UN3",8,0]
["NCPA_7_GP2UN3",9,0]
["NCPA_7_GP2UN3",10,0]
["NCPA_7_GP2UN3",11,0]
["NCPA_7_GP2UN3",12,0]
["NCPA_7_GP2UN4",1,52.73]
["NCPA_7_GP2UN4",2,52.73]
["NCPA_7_GP2UN4",3,52.73]
["NCPA_7_GP2UN4",4,52.73]
["NCPA_7_GP2UN4",5,52.73]
["NCPA_7_GP2UN4",6,52.73]
["NCPA_7_GP2UN4",7,52.73]
["NCPA_7_GP2UN4",8,52.73]
["NCPA_7_GP2UN4",9,52.73]
["NCPA_7_GP2UN4",10,52.73]
["NCPA_7_GP2UN4",11,52.73]
["NCPA_7_GP2UN4",12,52.73]
["NEENCH_6_SOLAR",1,0.26]
["NEENCH_6_SOLAR",2,1.98]
["NEENCH_6_SOLAR",3,2.31]
["NEENCH_6_SOLAR",4,2.9]
["NEENCH_6_SOLAR",5,4.22]
["NEENCH_6_SOLAR",6,8.65]
["NEENCH_6_SOLAR",7,9.5]
["NEENCH_6_SOLAR",8,8.18]
["NEENCH_6_SOLAR",9,7.33]
["NEENCH_6_SOLAR",10,4.88]
["NEENCH_6_SOLAR",11,3.76]
["NEENCH_6_SOLAR",12,2.31]
["NEWARK_1_QF",1,0.04]
["NEWARK_1_QF",2,0.03]
["NEWARK_1_QF",3,0.03]
["NEWARK_1_QF",4,0.03]
["NEWARK_1_QF",5,0.03]
["NEWARK_1_QF",6,0.03]
["NEWARK_1_QF",7,0.03]
["NEWARK_1_QF",8,0.03]
["NEWARK_1_QF",9,0.03]
["NEWARK_1_QF",10,0.03]
["NEWARK_1_QF",11,0.03]
["NEWARK_1_QF",12,0.03]
["NHOGAN_6_UNITS",1,0.19]
["NHOGAN_6_UNITS",2,0.61]
["NHOGAN_6_UNITS",3,0.32]
["NHOGAN_6_UNITS",4,0.54]
["NHOGAN_6_UNITS",5,1.44]
["NHOGAN_6_UNITS",6,1.1599999999999999]
["NHOGAN_6_UNITS",7,1.89]
["NHOGAN_6_UNITS",8,1.41]
["NHOGAN_6_UNITS",9,0.94]
["NHOGAN_6_UNITS",10,0.12]
["NHOGAN_6_UNITS",11,0.02]
["NHOGAN_6_UNITS",12,0.15]
["NOVATO_6_LNDFL",1,3.69]
["NOVATO_6_LNDFL",2,3.72]
["NOVATO_6_LNDFL",3,3.68]
["NOVATO_6_LNDFL",4,3.66]
["NOVATO_6_LNDFL",5,3.64]
["NOVATO_6_LNDFL",6,3.53]
["NOVATO_6_LNDFL",7,3.27]
["NOVATO_6_LNDFL",8,3.45]
["NOVATO_6_LNDFL",9,3.39]
["NOVATO_6_LNDFL",10,3.16]
["NOVATO_6_LNDFL",11,3.6]
["NOVATO_6_LNDFL",12,3.45]
["NWCSTL_7_UNIT 1",1,1.67]
["NWCSTL_7_UNIT 1",2,3.36]
["NWCSTL_7_UNIT 1",3,3.55]
["NWCSTL_7_UNIT 1",4,2.58]
["NWCSTL_7_UNIT 1",5,1.57]
["NWCSTL_7_UNIT 1",6,0.69]
["NWCSTL_7_UNIT 1",7,0.99]
["NWCSTL_7_UNIT 1",8,0.18]
["NWCSTL_7_UNIT 1",9,0]
["NWCSTL_7_UNIT 1",10,0]
["NWCSTL_7_UNIT 1",11,0]
["NWCSTL_7_UNIT 1",12,1.21]
["NZWIND_2_WDSTR5",1,1.1100000000000001]
["NZWIND_2_WDSTR5",2,1.19]
["NZWIND_2_WDSTR5",3,1.04]
["NZWIND_2_WDSTR5",4,1]
["NZWIND_2_WDSTR5",5,1.06]
["NZWIND_2_WDSTR5",6,0.97]
["NZWIND_2_WDSTR5",7,0.9]
["NZWIND_2_WDSTR5",8,0.69]
["NZWIND_2_WDSTR5",9,0.71]
["NZWIND_2_WDSTR5",10,0.66]
["NZWIND_2_WDSTR5",11,0.89]
["NZWIND_2_WDSTR5",12,1.07]
["NZWIND_6_CALWND",1,1.59]
["NZWIND_6_CALWND",2,1.69]
["NZWIND_6_CALWND",3,1.49]
["NZWIND_6_CALWND",4,1.42]
["NZWIND_6_CALWND",5,1.51]
["NZWIND_6_CALWND",6,1.39]
["NZWIND_6_CALWND",7,1.29]
["NZWIND_6_CALWND",8,0.98]
["NZWIND_6_CALWND",9,1.01]
["NZWIND_6_CALWND",10,0.94]
["NZWIND_6_CALWND",11,1.27]
["NZWIND_6_CALWND",12,1.53]
["NZWIND_6_WDSTR",1,0.59]
["NZWIND_6_WDSTR",2,0.63]
["NZWIND_6_WDSTR",3,0.55000000000000004]
["NZWIND_6_WDSTR",4,0.53]
["NZWIND_6_WDSTR",5,0.56000000000000005]
["NZWIND_6_WDSTR",6,0.52]
["NZWIND_6_WDSTR",7,0.48]
["NZWIND_6_WDSTR",8,0.36]
["NZWIND_6_WDSTR",9,0.38]
["NZWIND_6_WDSTR",10,0.35]
["NZWIND_6_WDSTR",11,0.47]
["NZWIND_6_WDSTR",12,0.56999999999999995]
["NZWIND_6_WDSTR2",1,0.72]
["NZWIND_6_WDSTR2",2,0.76]
["NZWIND_6_WDSTR2",3,0.67]
["NZWIND_6_WDSTR2",4,0.64]
["NZWIND_6_WDSTR2",5,0.68]
["NZWIND_6_WDSTR2",6,0.63]
["NZWIND_6_WDSTR2",7,0.57999999999999996]
["NZWIND_6_WDSTR2",8,0.44]
["NZWIND_6_WDSTR2",9,0.46]
["NZWIND_6_WDSTR2",10,0.42]
["NZWIND_6_WDSTR2",11,0.56999999999999995]
["NZWIND_6_WDSTR2",12,0.69]
["NZWIND_6_WDSTR3",1,0.68]
["NZWIND_6_WDSTR3",2,0.73]
["NZWIND_6_WDSTR3",3,0.64]
["NZWIND_6_WDSTR3",4,0.61]
["NZWIND_6_WDSTR3",5,0.65]
["NZWIND_6_WDSTR3",6,0.6]
["NZWIND_6_WDSTR3",7,0.55000000000000004]
["NZWIND_6_WDSTR3",8,0.42]
["NZWIND_6_WDSTR3",9,0.43]
["NZWIND_6_WDSTR3",10,0.4]
["NZWIND_6_WDSTR3",11,0.54]
["NZWIND_6_WDSTR3",12,0.66]
["NZWIND_6_WDSTR4",1,1.2]
["NZWIND_6_WDSTR4",2,1.27]
["NZWIND_6_WDSTR4",3,1.1200000000000001]
["NZWIND_6_WDSTR4",4,1.07]
["NZWIND_6_WDSTR4",5,1.1399999999999999]
["NZWIND_6_WDSTR4",6,1.04]
["NZWIND_6_WDSTR4",7,0.97]
["NZWIND_6_WDSTR4",8,0.74]
["NZWIND_6_WDSTR4",9,0.76]
["NZWIND_6_WDSTR4",10,0.71]
["NZWIND_6_WDSTR4",11,0.95]
["NZWIND_6_WDSTR4",12,1.1499999999999999]
["OAK C_1_EBMUD",1,0.9]
["OAK C_1_EBMUD",2,1.1299999999999999]
["OAK C_1_EBMUD",3,1.58]
["OAK C_1_EBMUD",4,1.54]
["OAK C_1_EBMUD",5,1.62]
["OAK C_1_EBMUD",6,1.44]
["OAK C_1_EBMUD",7,1.29]
["OAK C_1_EBMUD",8,1.49]
["OAK C_1_EBMUD",9,1.64]
["OAK C_1_EBMUD",10,1.45]
["OAK C_1_EBMUD",11,1.37]
["OAK C_1_EBMUD",12,1.76]
["OAK C_7_UNIT 1",1,55]
["OAK C_7_UNIT 1",2,55]
["OAK C_7_UNIT 1",3,55]
["OAK C_7_UNIT 1",4,55]
["OAK C_7_UNIT 1",5,55]
["OAK C_7_UNIT 1",6,55]
["OAK C_7_UNIT 1",7,55]
["OAK C_7_UNIT 1",8,55]
["OAK C_7_UNIT 1",9,55]
["OAK C_7_UNIT 1",10,55]
["OAK C_7_UNIT 1",11,55]
["OAK C_7_UNIT 1",12,55]
["OAK C_7_UNIT 3",1,55]
["OAK C_7_UNIT 3",2,55]
["OAK C_7_UNIT 3",3,55]
["OAK C_7_UNIT 3",4,55]
["OAK C_7_UNIT 3",5,55]
["OAK C_7_UNIT 3",6,55]
["OAK C_7_UNIT 3",7,55]
["OAK C_7_UNIT 3",8,55]
["OAK C_7_UNIT 3",9,55]
["OAK C_7_UNIT 3",10,55]
["OAK C_7_UNIT 3",11,55]
["OAK C_7_UNIT 3",12,55]
["OAK L_1_GTG1",1,0]
["OAK L_1_GTG1",2,0]
["OAK L_1_GTG1",3,0]
["OAK L_1_GTG1",4,0]
["OAK L_1_GTG1",5,0]
["OAK L_1_GTG1",6,0]
["OAK L_1_GTG1",7,0]
["OAK L_1_GTG1",8,0]
["OAK L_1_GTG1",9,0]
["OAK L_1_GTG1",10,0]
["OAK L_1_GTG1",11,0]
["OAK L_1_GTG1",12,0]
["OAKWD_6_QF",1,4.92]
["OAKWD_6_QF",2,5.24]
["OAKWD_6_QF",3,4.5999999999999996]
["OAKWD_6_QF",4,4.41]
["OAKWD_6_QF",5,4.6900000000000004]
["OAKWD_6_QF",6,4.3]
["OAKWD_6_QF",7,3.99]
["OAKWD_6_QF",8,3.03]
["OAKWD_6_QF",9,3.13]
["OAKWD_6_QF",10,2.91]
["OAKWD_6_QF",11,3.92]
["OAKWD_6_QF",12,4.75]
["OAKWD_6_ZEPHWD",1,0.62]
["OAKWD_6_ZEPHWD",2,0.66]
["OAKWD_6_ZEPHWD",3,0.57999999999999996]
["OAKWD_6_ZEPHWD",4,0.55000000000000004]
["OAKWD_6_ZEPHWD",5,0.59]
["OAKWD_6_ZEPHWD",6,0.54]
["OAKWD_6_ZEPHWD",7,0.5]
["OAKWD_6_ZEPHWD",8,0.38]
["OAKWD_6_ZEPHWD",9,0.39]
["OAKWD_6_ZEPHWD",10,0.37]
["OAKWD_6_ZEPHWD",11,0.49]
["OAKWD_6_ZEPHWD",12,0.6]
["OASIS_6_CREST",1,0]
["OASIS_6_CREST",2,0]
["OASIS_6_CREST",3,0]
["OASIS_6_CREST",4,0]
["OASIS_6_CREST",5,0]
["OASIS_6_CREST",6,0]
["OASIS_6_CREST",7,0]
["OASIS_6_CREST",8,0]
["OASIS_6_CREST",9,0]
["OASIS_6_CREST",10,0]
["OASIS_6_CREST",11,0]
["OASIS_6_CREST",12,0]
["OASIS_6_GBDSR4",1,0.01]
["OASIS_6_GBDSR4",2,0.09]
["OASIS_6_GBDSR4",3,0.11]
["OASIS_6_GBDSR4",4,0.13]
["OASIS_6_GBDSR4",5,0.19]
["OASIS_6_GBDSR4",6,0.39]
["OASIS_6_GBDSR4",7,0.43]
["OASIS_6_GBDSR4",8,0.37]
["OASIS_6_GBDSR4",9,0.33]
["OASIS_6_GBDSR4",10,0.22]
["OASIS_6_GBDSR4",11,0.17]
["OASIS_6_GBDSR4",12,0.11]
["OASIS_6_SOLAR1",1,0]
["OASIS_6_SOLAR1",2,0]
["OASIS_6_SOLAR1",3,0]
["OASIS_6_SOLAR1",4,0]
["OASIS_6_SOLAR1",5,0]
["OASIS_6_SOLAR1",6,0]
["OASIS_6_SOLAR1",7,0]
["OASIS_6_SOLAR1",8,0]
["OASIS_6_SOLAR1",9,0]
["OASIS_6_SOLAR1",10,0]
["OASIS_6_SOLAR1",11,0]
["OASIS_6_SOLAR1",12,0]
["OASIS_6_SOLAR2",1,0.08]
["OASIS_6_SOLAR2",2,0.6]
["OASIS_6_SOLAR2",3,0.7]
["OASIS_6_SOLAR2",4,0.88]
["OASIS_6_SOLAR2",5,1.28]
["OASIS_6_SOLAR2",6,2.62]
["OASIS_6_SOLAR2",7,2.88]
["OASIS_6_SOLAR2",8,2.48]
["OASIS_6_SOLAR2",9,2.2200000000000002]
["OASIS_6_SOLAR2",10,1.48]
["OASIS_6_SOLAR2",11,1.1399999999999999]
["OASIS_6_SOLAR2",12,0.7]
["OASIS_6_SOLAR3",1,0]
["OASIS_6_SOLAR3",2,0]
["OASIS_6_SOLAR3",3,0]
["OASIS_6_SOLAR3",4,0]
["OASIS_6_SOLAR3",5,0]
["OASIS_6_SOLAR3",6,0]
["OASIS_6_SOLAR3",7,0]
["OASIS_6_SOLAR3",8,0]
["OASIS_6_SOLAR3",9,0]
["OASIS_6_SOLAR3",10,0]
["OASIS_6_SOLAR3",11,0]
["OASIS_6_SOLAR3",12,0]
["OCTILO_5_WIND",1,46.83]
["OCTILO_5_WIND",2,49.8]
["OCTILO_5_WIND",3,43.76]
["OCTILO_5_WIND",4,41.92]
["OCTILO_5_WIND",5,44.58]
["OCTILO_5_WIND",6,40.86]
["OCTILO_5_WIND",7,37.97]
["OCTILO_5_WIND",8,28.85]
["OCTILO_5_WIND",9,29.8]
["OCTILO_5_WIND",10,27.65]
["OCTILO_5_WIND",11,37.26]
["OCTILO_5_WIND",12,45.13]
["OGROVE_6_PL1X2",1,96]
["OGROVE_6_PL1X2",2,96]
["OGROVE_6_PL1X2",3,96]
["OGROVE_6_PL1X2",4,96]
["OGROVE_6_PL1X2",5,96]
["OGROVE_6_PL1X2",6,96]
["OGROVE_6_PL1X2",7,96]
["OGROVE_6_PL1X2",8,96]
["OGROVE_6_PL1X2",9,96]
["OGROVE_6_PL1X2",10,96]
["OGROVE_6_PL1X2",11,96]
["OGROVE_6_PL1X2",12,96]
["OILFLD_7_QFUNTS",1,0.08]
["OILFLD_7_QFUNTS",2,0.13]
["OILFLD_7_QFUNTS",3,0.75]
["OILFLD_7_QFUNTS",4,2.1800000000000002]
["OILFLD_7_QFUNTS",5,2.59]
["OILFLD_7_QFUNTS",6,2.19]
["OILFLD_7_QFUNTS",7,2.06]
["OILFLD_7_QFUNTS",8,1.84]
["OILFLD_7_QFUNTS",9,1.08]
["OILFLD_7_QFUNTS",10,0.12]
["OILFLD_7_QFUNTS",11,0.1]
["OILFLD_7_QFUNTS",12,7.0000000000000007E-2]
["OLDRIV_6_BIOGAS",1,1.61]
["OLDRIV_6_BIOGAS",2,1.76]
["OLDRIV_6_BIOGAS",3,1.79]
["OLDRIV_6_BIOGAS",4,1.62]
["OLDRIV_6_BIOGAS",5,1.68]
["OLDRIV_6_BIOGAS",6,1.78]
["OLDRIV_6_BIOGAS",7,1.69]
["OLDRIV_6_BIOGAS",8,1.76]
["OLDRIV_6_BIOGAS",9,1.77]
["OLDRIV_6_BIOGAS",10,1.72]
["OLDRIV_6_BIOGAS",11,1.75]
["OLDRIV_6_BIOGAS",12,1.73]
["OLDRIV_6_CESDBM",1,0.94]
["OLDRIV_6_CESDBM",2,0.97]
["OLDRIV_6_CESDBM",3,0.93]
["OLDRIV_6_CESDBM",4,0.93]
["OLDRIV_6_CESDBM",5,0.95]
["OLDRIV_6_CESDBM",6,0.92]
["OLDRIV_6_CESDBM",7,0.91]
["OLDRIV_6_CESDBM",8,0.92]
["OLDRIV_6_CESDBM",9,0.93]
["OLDRIV_6_CESDBM",10,0.95]
["OLDRIV_6_CESDBM",11,0.97]
["OLDRIV_6_CESDBM",12,0.97]
["OLDRIV_6_LKVBM1",1,0.97]
["OLDRIV_6_LKVBM1",2,0.96]
["OLDRIV_6_LKVBM1",3,0.94]
["OLDRIV_6_LKVBM1",4,0.95]
["OLDRIV_6_LKVBM1",5,0.94]
["OLDRIV_6_LKVBM1",6,0.94]
["OLDRIV_6_LKVBM1",7,0.94]
["OLDRIV_6_LKVBM1",8,0.92]
["OLDRIV_6_LKVBM1",9,0.94]
["OLDRIV_6_LKVBM1",10,0.95]
["OLDRIV_6_LKVBM1",11,0.97]
["OLDRIV_6_LKVBM1",12,0.95]
["OLDRV1_6_SOLAR",1,0.08]
["OLDRV1_6_SOLAR",2,0.6]
["OLDRV1_6_SOLAR",3,0.7]
["OLDRV1_6_SOLAR",4,0.88]
["OLDRV1_6_SOLAR",5,1.28]
["OLDRV1_6_SOLAR",6,2.62]
["OLDRV1_6_SOLAR",7,2.88]
["OLDRV1_6_SOLAR",8,2.48]
["OLDRV1_6_SOLAR",9,2.2200000000000002]
["OLDRV1_6_SOLAR",10,1.48]
["OLDRV1_6_SOLAR",11,1.1399999999999999]
["OLDRV1_6_SOLAR",12,0.7]
["OLINDA_2_COYCRK",1,3.13]
["OLINDA_2_COYCRK",2,3.13]
["OLINDA_2_COYCRK",3,3.13]
["OLINDA_2_COYCRK",4,3.13]
["OLINDA_2_COYCRK",5,3.13]
["OLINDA_2_COYCRK",6,3.13]
["OLINDA_2_COYCRK",7,3.13]
["OLINDA_2_COYCRK",8,3.13]
["OLINDA_2_COYCRK",9,3.13]
["OLINDA_2_COYCRK",10,3.13]
["OLINDA_2_COYCRK",11,3.13]
["OLINDA_2_COYCRK",12,3.13]
["OLINDA_2_LNDFL2",1,25.9]
["OLINDA_2_LNDFL2",2,26.41]
["OLINDA_2_LNDFL2",3,26.2]
["OLINDA_2_LNDFL2",4,22.78]
["OLINDA_2_LNDFL2",5,25.05]
["OLINDA_2_LNDFL2",6,22.34]
["OLINDA_2_LNDFL2",7,24.08]
["OLINDA_2_LNDFL2",8,24.83]
["OLINDA_2_LNDFL2",9,24.91]
["OLINDA_2_LNDFL2",10,24.5]
["OLINDA_2_LNDFL2",11,26.05]
["OLINDA_2_LNDFL2",12,26.19]
["OLINDA_7_BLKSND",1,0.11]
["OLINDA_7_BLKSND",2,0.1]
["OLINDA_7_BLKSND",3,0.15]
["OLINDA_7_BLKSND",4,0.22]
["OLINDA_7_BLKSND",5,0.28999999999999998]
["OLINDA_7_BLKSND",6,0.38]
["OLINDA_7_BLKSND",7,0.36]
["OLINDA_7_BLKSND",8,0.25]
["OLINDA_7_BLKSND",9,0.98]
["OLINDA_7_BLKSND",10,1.28]
["OLINDA_7_BLKSND",11,1.04]
["OLINDA_7_BLKSND",12,1.48]
["OLIVEP_1_SOLAR",1,0.08]
["OLIVEP_1_SOLAR",2,0.6]
["OLIVEP_1_SOLAR",3,0.7]
["OLIVEP_1_SOLAR",4,0.88]
["OLIVEP_1_SOLAR",5,1.28]
["OLIVEP_1_SOLAR",6,2.62]
["OLIVEP_1_SOLAR",7,2.88]
["OLIVEP_1_SOLAR",8,2.48]
["OLIVEP_1_SOLAR",9,2.2200000000000002]
["OLIVEP_1_SOLAR",10,1.48]
["OLIVEP_1_SOLAR",11,1.1399999999999999]
["OLIVEP_1_SOLAR",12,0.7]
["OLIVEP_1_SOLAR2",1,0.08]
["OLIVEP_1_SOLAR2",2,0.59]
["OLIVEP_1_SOLAR2",3,0.69]
["OLIVEP_1_SOLAR2",4,0.87]
["OLIVEP_1_SOLAR2",5,1.26]
["OLIVEP_1_SOLAR2",6,2.59]
["OLIVEP_1_SOLAR2",7,2.84]
["OLIVEP_1_SOLAR2",8,2.4500000000000002]
["OLIVEP_1_SOLAR2",9,2.19]
["OLIVEP_1_SOLAR2",10,1.46]
["OLIVEP_1_SOLAR2",11,1.1299999999999999]
["OLIVEP_1_SOLAR2",12,0.69]
["OLSEN_2_UNIT",1,1.28]
["OLSEN_2_UNIT",2,1.63]
["OLSEN_2_UNIT",3,2.12]
["OLSEN_2_UNIT",4,3.35]
["OLSEN_2_UNIT",5,2.66]
["OLSEN_2_UNIT",6,1.24]
["OLSEN_2_UNIT",7,0.22]
["OLSEN_2_UNIT",8,0.01]
["OLSEN_2_UNIT",9,0]
["OLSEN_2_UNIT",10,0.11]
["OLSEN_2_UNIT",11,0.09]
["OLSEN_2_UNIT",12,0.21]
["OMAR_2_UNIT 1",1,75]
["OMAR_2_UNIT 1",2,75]
["OMAR_2_UNIT 1",3,75]
["OMAR_2_UNIT 1",4,75]
["OMAR_2_UNIT 1",5,74.67]
["OMAR_2_UNIT 1",6,73.67]
["OMAR_2_UNIT 1",7,73]
["OMAR_2_UNIT 1",8,72.67]
["OMAR_2_UNIT 1",9,73.67]
["OMAR_2_UNIT 1",10,74.33]
["OMAR_2_UNIT 1",11,75]
["OMAR_2_UNIT 1",12,75]
["OMAR_2_UNIT 2",1,75]
["OMAR_2_UNIT 2",2,75]
["OMAR_2_UNIT 2",3,75]
["OMAR_2_UNIT 2",4,75]
["OMAR_2_UNIT 2",5,74.67]
["OMAR_2_UNIT 2",6,73.67]
["OMAR_2_UNIT 2",7,73.33]
["OMAR_2_UNIT 2",8,73]
["OMAR_2_UNIT 2",9,73.67]
["OMAR_2_UNIT 2",10,74.67]
["OMAR_2_UNIT 2",11,75]
["OMAR_2_UNIT 2",12,75]
["OMAR_2_UNIT 3",1,75]
["OMAR_2_UNIT 3",2,75]
["OMAR_2_UNIT 3",3,75]
["OMAR_2_UNIT 3",4,75]
["OMAR_2_UNIT 3",5,73.67]
["OMAR_2_UNIT 3",6,73.67]
["OMAR_2_UNIT 3",7,73.33]
["OMAR_2_UNIT 3",8,73]
["OMAR_2_UNIT 3",9,73.67]
["OMAR_2_UNIT 3",10,75]
["OMAR_2_UNIT 3",11,75]
["OMAR_2_UNIT 3",12,75]
["OMAR_2_UNIT 4",1,75]
["OMAR_2_UNIT 4",2,75]
["OMAR_2_UNIT 4",3,75]
["OMAR_2_UNIT 4",4,75]
["OMAR_2_UNIT 4",5,74]
["OMAR_2_UNIT 4",6,73.33]
["OMAR_2_UNIT 4",7,73.67]
["OMAR_2_UNIT 4",8,73.67]
["OMAR_2_UNIT 4",9,74.33]
["OMAR_2_UNIT 4",10,75]
["OMAR_2_UNIT 4",11,75]
["OMAR_2_UNIT 4",12,75]
["ONLLPP_6_UNITS",1,0]
["ONLLPP_6_UNITS",2,0.57999999999999996]
["ONLLPP_6_UNITS",3,7.0000000000000007E-2]
["ONLLPP_6_UNITS",4,0.32]
["ONLLPP_6_UNITS",5,1.71]
["ONLLPP_6_UNITS",6,1.64]
["ONLLPP_6_UNITS",7,1.48]
["ONLLPP_6_UNITS",8,0.64]
["ONLLPP_6_UNITS",9,0.05]
["ONLLPP_6_UNITS",10,0.67]
["ONLLPP_6_UNITS",11,0.42]
["ONLLPP_6_UNITS",12,0]
["ORLND_6_HIGHLI",1,0]
["ORLND_6_HIGHLI",2,0]
["ORLND_6_HIGHLI",3,0]
["ORLND_6_HIGHLI",4,0.06]
["ORLND_6_HIGHLI",5,0.06]
["ORLND_6_HIGHLI",6,0.03]
["ORLND_6_HIGHLI",7,0]
["ORLND_6_HIGHLI",8,0]
["ORLND_6_HIGHLI",9,0]
["ORLND_6_HIGHLI",10,0.04]
["ORLND_6_HIGHLI",11,0]
["ORLND_6_HIGHLI",12,0]
["ORLND_6_SOLAR1",1,0.01]
["ORLND_6_SOLAR1",2,0.05]
["ORLND_6_SOLAR1",3,0.05]
["ORLND_6_SOLAR1",4,7.0000000000000007E-2]
["ORLND_6_SOLAR1",5,0.1]
["ORLND_6_SOLAR1",6,0.2]
["ORLND_6_SOLAR1",7,0.22]
["ORLND_6_SOLAR1",8,0.19]
["ORLND_6_SOLAR1",9,0.17]
["ORLND_6_SOLAR1",10,0.11]
["ORLND_6_SOLAR1",11,0.09]
["ORLND_6_SOLAR1",12,0.05]
["ORMOND_7_UNIT 1",1,741.27]
["ORMOND_7_UNIT 1",2,741.27]
["ORMOND_7_UNIT 1",3,741.27]
["ORMOND_7_UNIT 1",4,741.27]
["ORMOND_7_UNIT 1",5,741.27]
["ORMOND_7_UNIT 1",6,741.27]
["ORMOND_7_UNIT 1",7,741.27]
["ORMOND_7_UNIT 1",8,741.27]
["ORMOND_7_UNIT 1",9,741.27]
["ORMOND_7_UNIT 1",10,741.27]
["ORMOND_7_UNIT 1",11,741.27]
["ORMOND_7_UNIT 1",12,741.27]
["ORMOND_7_UNIT 2",1,750]
["ORMOND_7_UNIT 2",2,750]
["ORMOND_7_UNIT 2",3,750]
["ORMOND_7_UNIT 2",4,750]
["ORMOND_7_UNIT 2",5,750]
["ORMOND_7_UNIT 2",6,750]
["ORMOND_7_UNIT 2",7,750]
["ORMOND_7_UNIT 2",8,750]
["ORMOND_7_UNIT 2",9,750]
["ORMOND_7_UNIT 2",10,750]
["ORMOND_7_UNIT 2",11,750]
["ORMOND_7_UNIT 2",12,750]
["OROLOM_1_SOLAR1",1,0]
["OROLOM_1_SOLAR1",2,0]
["OROLOM_1_SOLAR1",3,0]
["OROLOM_1_SOLAR1",4,0]
["OROLOM_1_SOLAR1",5,0]
["OROLOM_1_SOLAR1",6,0]
["OROLOM_1_SOLAR1",7,0]
["OROLOM_1_SOLAR1",8,0]
["OROLOM_1_SOLAR1",9,0]
["OROLOM_1_SOLAR1",10,0]
["OROLOM_1_SOLAR1",11,0]
["OROLOM_1_SOLAR1",12,0]
["OROLOM_1_SOLAR2",1,0]
["OROLOM_1_SOLAR2",2,0]
["OROLOM_1_SOLAR2",3,0]
["OROLOM_1_SOLAR2",4,0]
["OROLOM_1_SOLAR2",5,0]
["OROLOM_1_SOLAR2",6,0]
["OROLOM_1_SOLAR2",7,0]
["OROLOM_1_SOLAR2",8,0]
["OROLOM_1_SOLAR2",9,0]
["OROLOM_1_SOLAR2",10,0]
["OROLOM_1_SOLAR2",11,0]
["OROLOM_1_SOLAR2",12,0]
["OROVIL_6_UNIT",1,7.5]
["OROVIL_6_UNIT",2,7.5]
["OROVIL_6_UNIT",3,7.5]
["OROVIL_6_UNIT",4,7.5]
["OROVIL_6_UNIT",5,7.5]
["OROVIL_6_UNIT",6,7.5]
["OROVIL_6_UNIT",7,7.5]
["OROVIL_6_UNIT",8,7.5]
["OROVIL_6_UNIT",9,7.5]
["OROVIL_6_UNIT",10,7.5]
["OROVIL_6_UNIT",11,7.5]
["OROVIL_6_UNIT",12,7.5]
["ORTGA_6_ME1SL1",1,0.01]
["ORTGA_6_ME1SL1",2,0.09]
["ORTGA_6_ME1SL1",3,0.11]
["ORTGA_6_ME1SL1",4,0.13]
["ORTGA_6_ME1SL1",5,0.19]
["ORTGA_6_ME1SL1",6,0.39]
["ORTGA_6_ME1SL1",7,0.43]
["ORTGA_6_ME1SL1",8,0.37]
["ORTGA_6_ME1SL1",9,0.33]
["ORTGA_6_ME1SL1",10,0.22]
["ORTGA_6_ME1SL1",11,0.17]
["ORTGA_6_ME1SL1",12,0.11]
["OSO_6_NSPIN",1,18]
["OSO_6_NSPIN",2,18]
["OSO_6_NSPIN",3,18]
["OSO_6_NSPIN",4,18]
["OSO_6_NSPIN",5,18]
["OSO_6_NSPIN",6,18]
["OSO_6_NSPIN",7,18]
["OSO_6_NSPIN",8,18]
["OSO_6_NSPIN",9,18]
["OSO_6_NSPIN",10,18]
["OSO_6_NSPIN",11,18]
["OSO_6_NSPIN",12,18]
["OTAY_6_PL1X2",1,37.200000000000003]
["OTAY_6_PL1X2",2,37.200000000000003]
["OTAY_6_PL1X2",3,37.200000000000003]
["OTAY_6_PL1X2",4,37.200000000000003]
["OTAY_6_PL1X2",5,37.200000000000003]
["OTAY_6_PL1X2",6,37.200000000000003]
["OTAY_6_PL1X2",7,37.200000000000003]
["OTAY_6_PL1X2",8,37.200000000000003]
["OTAY_6_PL1X2",9,37.200000000000003]
["OTAY_6_PL1X2",10,37.200000000000003]
["OTAY_6_PL1X2",11,37.200000000000003]
["OTAY_6_PL1X2",12,37.200000000000003]
["OTMESA_2_PL1X3",1,603.6]
["OTMESA_2_PL1X3",2,603.6]
["OTMESA_2_PL1X3",3,603.6]
["OTMESA_2_PL1X3",4,603.6]
["OTMESA_2_PL1X3",5,603.6]
["OTMESA_2_PL1X3",6,603.6]
["OTMESA_2_PL1X3",7,603.6]
["OTMESA_2_PL1X3",8,603.6]
["OTMESA_2_PL1X3",9,603.6]
["OTMESA_2_PL1X3",10,603.6]
["OTMESA_2_PL1X3",11,603.6]
["OTMESA_2_PL1X3",12,603.6]
["OXBOW_6_DRUM",1,2.38]
["OXBOW_6_DRUM",2,2]
["OXBOW_6_DRUM",3,2.0099999999999998]
["OXBOW_6_DRUM",4,3.71]
["OXBOW_6_DRUM",5,2.83]
["OXBOW_6_DRUM",6,2.57]
["OXBOW_6_DRUM",7,2.6]
["OXBOW_6_DRUM",8,3.22]
["OXBOW_6_DRUM",9,2.99]
["OXBOW_6_DRUM",10,0.02]
["OXBOW_6_DRUM",11,1.48]
["OXBOW_6_DRUM",12,2.71]
["OXMTN_6_LNDFIL",1,10.34]
["OXMTN_6_LNDFIL",2,10.37]
["OXMTN_6_LNDFIL",3,10.62]
["OXMTN_6_LNDFIL",4,10.62]
["OXMTN_6_LNDFIL",5,10.34]
["OXMTN_6_LNDFIL",6,10.39]
["OXMTN_6_LNDFIL",7,10.59]
["OXMTN_6_LNDFIL",8,10.26]
["OXMTN_6_LNDFIL",9,10.39]
["OXMTN_6_LNDFIL",10,10.16]
["OXMTN_6_LNDFIL",11,10.48]
["OXMTN_6_LNDFIL",12,10.62]
["PACLUM_6_UNIT",1,15.1]
["PACLUM_6_UNIT",2,12.4]
["PACLUM_6_UNIT",3,11.73]
["PACLUM_6_UNIT",4,8.93]
["PACLUM_6_UNIT",5,14.21]
["PACLUM_6_UNIT",6,15.71]
["PACLUM_6_UNIT",7,14.8]
["PACLUM_6_UNIT",8,12.89]
["PACLUM_6_UNIT",9,14.53]
["PACLUM_6_UNIT",10,14.53]
["PACLUM_6_UNIT",11,12.81]
["PACLUM_6_UNIT",12,15.07]
["PADUA_2_ONTARO",1,0.7]
["PADUA_2_ONTARO",2,0.61]
["PADUA_2_ONTARO",3,0.78]
["PADUA_2_ONTARO",4,1.1200000000000001]
["PADUA_2_ONTARO",5,1]
["PADUA_2_ONTARO",6,0.85]
["PADUA_2_ONTARO",7,0.85]
["PADUA_2_ONTARO",8,0.82]
["PADUA_2_ONTARO",9,0.74]
["PADUA_2_ONTARO",10,0.62]
["PADUA_2_ONTARO",11,0.49]
["PADUA_2_ONTARO",12,0.64]
["PADUA_2_SOLAR1",1,0]
["PADUA_2_SOLAR1",2,0]
["PADUA_2_SOLAR1",3,0]
["PADUA_2_SOLAR1",4,0]
["PADUA_2_SOLAR1",5,0]
["PADUA_2_SOLAR1",6,0]
["PADUA_2_SOLAR1",7,0]
["PADUA_2_SOLAR1",8,0]
["PADUA_2_SOLAR1",9,0]
["PADUA_2_SOLAR1",10,0]
["PADUA_2_SOLAR1",11,0]
["PADUA_2_SOLAR1",12,0]
["PADUA_6_MWDSDM",1,2.4]
["PADUA_6_MWDSDM",2,2.4]
["PADUA_6_MWDSDM",3,0]
["PADUA_6_MWDSDM",4,2.4]
["PADUA_6_MWDSDM",5,6]
["PADUA_6_MWDSDM",6,0]
["PADUA_6_MWDSDM",7,0]
["PADUA_6_MWDSDM",8,0]
["PADUA_6_MWDSDM",9,0]
["PADUA_6_MWDSDM",10,0]
["PADUA_6_MWDSDM",11,0]
["PADUA_6_MWDSDM",12,0]
["PADUA_6_QF",1,0.2]
["PADUA_6_QF",2,0.28000000000000003]
["PADUA_6_QF",3,0.24]
["PADUA_6_QF",4,0.35]
["PADUA_6_QF",5,0.5]
["PADUA_6_QF",6,0.52]
["PADUA_6_QF",7,0.54]
["PADUA_6_QF",8,0.43]
["PADUA_6_QF",9,0.5]
["PADUA_6_QF",10,0.49]
["PADUA_6_QF",11,0.44]
["PADUA_6_QF",12,0.19]
["PADUA_7_SDIMAS",1,0]
["PADUA_7_SDIMAS",2,0]
["PADUA_7_SDIMAS",3,0]
["PADUA_7_SDIMAS",4,0]
["PADUA_7_SDIMAS",5,1.05]
["PADUA_7_SDIMAS",6,1.05]
["PADUA_7_SDIMAS",7,1.05]
["PADUA_7_SDIMAS",8,1.05]
["PADUA_7_SDIMAS",9,1.05]
["PADUA_7_SDIMAS",10,0]
["PADUA_7_SDIMAS",11,0]
["PADUA_7_SDIMAS",12,0]
["PAIGES_6_SOLAR",1,0]
["PAIGES_6_SOLAR",2,0]
["PAIGES_6_SOLAR",3,0]
["PAIGES_6_SOLAR",4,0]
["PAIGES_6_SOLAR",5,0]
["PAIGES_6_SOLAR",6,0]
["PAIGES_6_SOLAR",7,0]
["PAIGES_6_SOLAR",8,0]
["PAIGES_6_SOLAR",9,0]
["PAIGES_6_SOLAR",10,0]
["PAIGES_6_SOLAR",11,0]
["PAIGES_6_SOLAR",12,0]
["PALALT_7_COBUG",1,0]
["PALALT_7_COBUG",2,0]
["PALALT_7_COBUG",3,0]
["PALALT_7_COBUG",4,0]
["PALALT_7_COBUG",5,0]
["PALALT_7_COBUG",6,0]
["PALALT_7_COBUG",7,0]
["PALALT_7_COBUG",8,0]
["PALALT_7_COBUG",9,0]
["PALALT_7_COBUG",10,0]
["PALALT_7_COBUG",11,0]
["PALALT_7_COBUG",12,0]
["PALOMR_2_PL1X3",1,588.21]
["PALOMR_2_PL1X3",2,588.21]
["PALOMR_2_PL1X3",3,588.21]
["PALOMR_2_PL1X3",4,588.21]
["PALOMR_2_PL1X3",5,588.21]
["PALOMR_2_PL1X3",6,588.21]
["PALOMR_2_PL1X3",7,588.21]
["PALOMR_2_PL1X3",8,588.21]
["PALOMR_2_PL1X3",9,588.21]
["PALOMR_2_PL1X3",10,588.21]
["PALOMR_2_PL1X3",11,588.21]
["PALOMR_2_PL1X3",12,588.21]
["PARDEB_6_UNITS",1,17.7]
["PARDEB_6_UNITS",2,15.62]
["PARDEB_6_UNITS",3,7.7]
["PARDEB_6_UNITS",4,19.940000000000001]
["PARDEB_6_UNITS",5,7.76]
["PARDEB_6_UNITS",6,27.3]
["PARDEB_6_UNITS",7,17.7]
["PARDEB_6_UNITS",8,19.18]
["PARDEB_6_UNITS",9,15.44]
["PARDEB_6_UNITS",10,18.7]
["PARDEB_6_UNITS",11,15.7]
["PARDEB_6_UNITS",12,26.42]
["PBLOSM_2_SOLAR",1,0.04]
["PBLOSM_2_SOLAR",2,0.28999999999999998]
["PBLOSM_2_SOLAR",3,0.33]
["PBLOSM_2_SOLAR",4,0.42]
["PBLOSM_2_SOLAR",5,0.61]
["PBLOSM_2_SOLAR",6,1.24]
["PBLOSM_2_SOLAR",7,1.37]
["PBLOSM_2_SOLAR",8,1.18]
["PBLOSM_2_SOLAR",9,1.05]
["PBLOSM_2_SOLAR",10,0.7]
["PBLOSM_2_SOLAR",11,0.54]
["PBLOSM_2_SOLAR",12,0.33]
["PEABDY_2_LNDFIL",1,1.55]
["PEABDY_2_LNDFIL",2,1.55]
["PEABDY_2_LNDFIL",3,1.5]
["PEABDY_2_LNDFIL",4,1.53]
["PEABDY_2_LNDFIL",5,1.53]
["PEABDY_2_LNDFIL",6,1.52]
["PEABDY_2_LNDFIL",7,1.5]
["PEABDY_2_LNDFIL",8,1.52]
["PEABDY_2_LNDFIL",9,1.52]
["PEABDY_2_LNDFIL",10,1.54]
["PEABDY_2_LNDFIL",11,1.54]
["PEABDY_2_LNDFIL",12,1.53]
["PEABDY_2_LNDFL1",1,7.72]
["PEABDY_2_LNDFL1",2,7.69]
["PEABDY_2_LNDFL1",3,7.55]
["PEABDY_2_LNDFL1",4,7.63]
["PEABDY_2_LNDFL1",5,7.16]
["PEABDY_2_LNDFL1",6,7.44]
["PEABDY_2_LNDFL1",7,7.58]
["PEABDY_2_LNDFL1",8,7.53]
["PEABDY_2_LNDFL1",9,7.55]
["PEABDY_2_LNDFL1",10,7.49]
["PEABDY_2_LNDFL1",11,7.38]
["PEABDY_2_LNDFL1",12,7.24]
["PEARBL_2_NSPIN",1,21]
["PEARBL_2_NSPIN",2,21]
["PEARBL_2_NSPIN",3,21]
["PEARBL_2_NSPIN",4,46]
["PEARBL_2_NSPIN",5,46]
["PEARBL_2_NSPIN",6,46]
["PEARBL_2_NSPIN",7,46]
["PEARBL_2_NSPIN",8,46]
["PEARBL_2_NSPIN",9,46]
["PEARBL_2_NSPIN",10,46]
["PEARBL_2_NSPIN",11,46]
["PEARBL_2_NSPIN",12,46]
["PEASE_1_TBEBT1",1,5]
["PEASE_1_TBEBT1",2,5]
["PEASE_1_TBEBT1",3,5]
["PEASE_1_TBEBT1",4,5]
["PEASE_1_TBEBT1",5,5]
["PEASE_1_TBEBT1",6,5]
["PEASE_1_TBEBT1",7,5]
["PEASE_1_TBEBT1",8,5]
["PEASE_1_TBEBT1",9,5]
["PEASE_1_TBEBT1",10,5]
["PEASE_1_TBEBT1",11,5]
["PEASE_1_TBEBT1",12,5]
["PEORIA_1_SOLAR",1,0.01]
["PEORIA_1_SOLAR",2,0.05]
["PEORIA_1_SOLAR",3,0.05]
["PEORIA_1_SOLAR",4,7.0000000000000007E-2]
["PEORIA_1_SOLAR",5,0.1]
["PEORIA_1_SOLAR",6,0.2]
["PEORIA_1_SOLAR",7,0.22]
["PEORIA_1_SOLAR",8,0.19]
["PEORIA_1_SOLAR",9,0.17]
["PEORIA_1_SOLAR",10,0.11]
["PEORIA_1_SOLAR",11,0.09]
["PEORIA_1_SOLAR",12,0.05]
["PHOENX_1_UNIT",1,0.33]
["PHOENX_1_UNIT",2,0.28000000000000003]
["PHOENX_1_UNIT",3,0.68]
["PHOENX_1_UNIT",4,0.93]
["PHOENX_1_UNIT",5,0.88]
["PHOENX_1_UNIT",6,0.82]
["PHOENX_1_UNIT",7,0.92]
["PHOENX_1_UNIT",8,0.92]
["PHOENX_1_UNIT",9,0.9]
["PHOENX_1_UNIT",10,0.45]
["PHOENX_1_UNIT",11,0.45]
["PHOENX_1_UNIT",12,0.55000000000000004]
["PINFLT_7_UNITS",1,0]
["PINFLT_7_UNITS",2,0]
["PINFLT_7_UNITS",3,0]
["PINFLT_7_UNITS",4,0]
["PINFLT_7_UNITS",5,70.650000000000006]
["PINFLT_7_UNITS",6,129.53]
["PINFLT_7_UNITS",7,138]
["PINFLT_7_UNITS",8,71.55]
["PINFLT_7_UNITS",9,7.3]
["PINFLT_7_UNITS",10,0]
["PINFLT_7_UNITS",11,0]
["PINFLT_7_UNITS",12,0]
["PIOPIC_2_CTG1",1,111.3]
["PIOPIC_2_CTG1",2,111.3]
["PIOPIC_2_CTG1",3,111.3]
["PIOPIC_2_CTG1",4,111.3]
["PIOPIC_2_CTG1",5,111.3]
["PIOPIC_2_CTG1",6,111.3]
["PIOPIC_2_CTG1",7,111.3]
["PIOPIC_2_CTG1",8,111.3]
["PIOPIC_2_CTG1",9,111.3]
["PIOPIC_2_CTG1",10,111.3]
["PIOPIC_2_CTG1",11,111.3]
["PIOPIC_2_CTG1",12,111.3]
["PIOPIC_2_CTG2",1,112.7]
["PIOPIC_2_CTG2",2,112.7]
["PIOPIC_2_CTG2",3,112.7]
["PIOPIC_2_CTG2",4,112.7]
["PIOPIC_2_CTG2",5,112.7]
["PIOPIC_2_CTG2",6,112.7]
["PIOPIC_2_CTG2",7,112.7]
["PIOPIC_2_CTG2",8,112.7]
["PIOPIC_2_CTG2",9,112.7]
["PIOPIC_2_CTG2",10,112.7]
["PIOPIC_2_CTG2",11,112.7]
["PIOPIC_2_CTG2",12,112.7]
["PIOPIC_2_CTG3",1,112]
["PIOPIC_2_CTG3",2,112]
["PIOPIC_2_CTG3",3,112]
["PIOPIC_2_CTG3",4,112]
["PIOPIC_2_CTG3",5,112]
["PIOPIC_2_CTG3",6,112]
["PIOPIC_2_CTG3",7,112]
["PIOPIC_2_CTG3",8,112]
["PIOPIC_2_CTG3",9,112]
["PIOPIC_2_CTG3",10,112]
["PIOPIC_2_CTG3",11,112]
["PIOPIC_2_CTG3",12,112]
["PIT1_6_FRIVRA",1,0.01]
["PIT1_6_FRIVRA",2,0.05]
["PIT1_6_FRIVRA",3,0.05]
["PIT1_6_FRIVRA",4,7.0000000000000007E-2]
["PIT1_6_FRIVRA",5,0.1]
["PIT1_6_FRIVRA",6,0.2]
["PIT1_6_FRIVRA",7,0.22]
["PIT1_6_FRIVRA",8,0.19]
["PIT1_6_FRIVRA",9,0.17]
["PIT1_6_FRIVRA",10,0.11]
["PIT1_6_FRIVRA",11,0.09]
["PIT1_6_FRIVRA",12,0.05]
["PIT1_7_UNIT 1",1,20.399999999999999]
["PIT1_7_UNIT 1",2,17]
["PIT1_7_UNIT 1",3,16.88]
["PIT1_7_UNIT 1",4,17.28]
["PIT1_7_UNIT 1",5,18.399999999999999]
["PIT1_7_UNIT 1",6,16.88]
["PIT1_7_UNIT 1",7,15.6]
["PIT1_7_UNIT 1",8,15.76]
["PIT1_7_UNIT 1",9,16.36]
["PIT1_7_UNIT 1",10,0]
["PIT1_7_UNIT 1",11,0]
["PIT1_7_UNIT 1",12,0]
["PIT1_7_UNIT 2",1,14.4]
["PIT1_7_UNIT 2",2,14.4]
["PIT1_7_UNIT 2",3,14.4]
["PIT1_7_UNIT 2",4,14.4]
["PIT1_7_UNIT 2",5,15.6]
["PIT1_7_UNIT 2",6,9.1999999999999993]
["PIT1_7_UNIT 2",7,8.6]
["PIT1_7_UNIT 2",8,9.1999999999999993]
["PIT1_7_UNIT 2",9,9.1999999999999993]
["PIT1_7_UNIT 2",10,6.24]
["PIT1_7_UNIT 2",11,14.4]
["PIT1_7_UNIT 2",12,14.4]
["PIT3_7_PL1X3",1,36]
["PIT3_7_PL1X3",2,32.799999999999997]
["PIT3_7_PL1X3",3,32]
["PIT3_7_PL1X3",4,35.200000000000003]
["PIT3_7_PL1X3",5,44.8]
["PIT3_7_PL1X3",6,49]
["PIT3_7_PL1X3",7,54.6]
["PIT3_7_PL1X3",8,43]
["PIT3_7_PL1X3",9,30.2]
["PIT3_7_PL1X3",10,28.4]
["PIT3_7_PL1X3",11,28.8]
["PIT3_7_PL1X3",12,36.6]
["PIT4_7_PL1X2",1,50.2]
["PIT4_7_PL1X2",2,45.6]
["PIT4_7_PL1X2",3,44]
["PIT4_7_PL1X2",4,45.68]
["PIT4_7_PL1X2",5,45.2]
["PIT4_7_PL1X2",6,55.6]
["PIT4_7_PL1X2",7,65]
["PIT4_7_PL1X2",8,54]
["PIT4_7_PL1X2",9,39.08]
["PIT4_7_PL1X2",10,39.799999999999997]
["PIT4_7_PL1X2",11,42.4]
["PIT4_7_PL1X2",12,49]
["PIT5_7_PL1X2",1,48.4]
["PIT5_7_PL1X2",2,16.8]
["PIT5_7_PL1X2",3,40]
["PIT5_7_PL1X2",4,30.4]
["PIT5_7_PL1X2",5,43.2]
["PIT5_7_PL1X2",6,41.6]
["PIT5_7_PL1X2",7,42.4]
["PIT5_7_PL1X2",8,33.6]
["PIT5_7_PL1X2",9,33.6]
["PIT5_7_PL1X2",10,18.399999999999999]
["PIT5_7_PL1X2",11,31.2]
["PIT5_7_PL1X2",12,25.8]
["PIT5_7_PL3X4",1,32]
["PIT5_7_PL3X4",2,34.4]
["PIT5_7_PL3X4",3,32]
["PIT5_7_PL3X4",4,32]
["PIT5_7_PL3X4",5,32]
["PIT5_7_PL3X4",6,47.2]
["PIT5_7_PL3X4",7,44]
["PIT5_7_PL3X4",8,37.6]
["PIT5_7_PL3X4",9,35.200000000000003]
["PIT5_7_PL3X4",10,46.4]
["PIT5_7_PL3X4",11,32]
["PIT5_7_PL3X4",12,32]
["PIT5_7_QFUNTS",1,0.17]
["PIT5_7_QFUNTS",2,0.28999999999999998]
["PIT5_7_QFUNTS",3,0.41]
["PIT5_7_QFUNTS",4,0.53]
["PIT5_7_QFUNTS",5,0.34]
["PIT5_7_QFUNTS",6,0.11]
["PIT5_7_QFUNTS",7,0.01]
["PIT5_7_QFUNTS",8,0]
["PIT5_7_QFUNTS",9,0]
["PIT5_7_QFUNTS",10,0.01]
["PIT5_7_QFUNTS",11,0.05]
["PIT5_7_QFUNTS",12,0.04]
["PIT6_7_UNIT 1",1,31.2]
["PIT6_7_UNIT 1",2,31.12]
["PIT6_7_UNIT 1",3,31.2]
["PIT6_7_UNIT 1",4,38.200000000000003]
["PIT6_7_UNIT 1",5,31.2]
["PIT6_7_UNIT 1",6,37]
["PIT6_7_UNIT 1",7,37.200000000000003]
["PIT6_7_UNIT 1",8,36.340000000000003]
["PIT6_7_UNIT 1",9,30.46]
["PIT6_7_UNIT 1",10,30.28]
["PIT6_7_UNIT 1",11,35.51]
["PIT6_7_UNIT 1",12,38]
["PIT6_7_UNIT 2",1,38]
["PIT6_7_UNIT 2",2,38.200000000000003]
["PIT6_7_UNIT 2",3,38.51]
["PIT6_7_UNIT 2",4,37.65]
["PIT6_7_UNIT 2",5,31.15]
["PIT6_7_UNIT 2",6,37.799999999999997]
["PIT6_7_UNIT 2",7,36.78]
["PIT6_7_UNIT 2",8,36.700000000000003]
["PIT6_7_UNIT 2",9,35.72]
["PIT6_7_UNIT 2",10,29.76]
["PIT6_7_UNIT 2",11,36.299999999999997]
["PIT6_7_UNIT 2",12,38.04]
["PIT7_7_UNIT 1",1,52.2]
["PIT7_7_UNIT 1",2,51.08]
["PIT7_7_UNIT 1",3,53.2]
["PIT7_7_UNIT 1",4,53.14]
["PIT7_7_UNIT 1",5,51.64]
["PIT7_7_UNIT 1",6,52]
["PIT7_7_UNIT 1",7,53.2]
["PIT7_7_UNIT 1",8,53.4]
["PIT7_7_UNIT 1",9,53.44]
["PIT7_7_UNIT 1",10,51.36]
["PIT7_7_UNIT 1",11,42.4]
["PIT7_7_UNIT 1",12,53.09]
["PIT7_7_UNIT 2",1,49.76]
["PIT7_7_UNIT 2",2,49.46]
["PIT7_7_UNIT 2",3,52.4]
["PIT7_7_UNIT 2",4,52.6]
["PIT7_7_UNIT 2",5,41.9]
["PIT7_7_UNIT 2",6,50.76]
["PIT7_7_UNIT 2",7,52.2]
["PIT7_7_UNIT 2",8,53.2]
["PIT7_7_UNIT 2",9,53.39]
["PIT7_7_UNIT 2",10,52.8]
["PIT7_7_UNIT 2",11,43.47]
["PIT7_7_UNIT 2",12,42.39]
["PIUTE_6_GNBSR1",1,0.01]
["PIUTE_6_GNBSR1",2,0.09]
["PIUTE_6_GNBSR1",3,0.11]
["PIUTE_6_GNBSR1",4,0.13]
["PIUTE_6_GNBSR1",5,0.19]
["PIUTE_6_GNBSR1",6,0.39]
["PIUTE_6_GNBSR1",7,0.43]
["PIUTE_6_GNBSR1",8,0.37]
["PIUTE_6_GNBSR1",9,0.33]
["PIUTE_6_GNBSR1",10,0.22]
["PIUTE_6_GNBSR1",11,0.17]
["PIUTE_6_GNBSR1",12,0.11]
["PLACVL_1_CHILIB",1,0.76]
["PLACVL_1_CHILIB",2,0.56000000000000005]
["PLACVL_1_CHILIB",3,2.91]
["PLACVL_1_CHILIB",4,4.45]
["PLACVL_1_CHILIB",5,4.2]
["PLACVL_1_CHILIB",6,2.93]
["PLACVL_1_CHILIB",7,2.37]
["PLACVL_1_CHILIB",8,2.89]
["PLACVL_1_CHILIB",9,1.86]
["PLACVL_1_CHILIB",10,1.34]
["PLACVL_1_CHILIB",11,1.01]
["PLACVL_1_CHILIB",12,0.97]
["PLACVL_1_RCKCRE",1,0.11]
["PLACVL_1_RCKCRE",2,0.18]
["PLACVL_1_RCKCRE",3,0.42]
["PLACVL_1_RCKCRE",4,0.28999999999999998]
["PLACVL_1_RCKCRE",5,0.09]
["PLACVL_1_RCKCRE",6,0]
["PLACVL_1_RCKCRE",7,0]
["PLACVL_1_RCKCRE",8,0]
["PLACVL_1_RCKCRE",9,0]
["PLACVL_1_RCKCRE",10,0]
["PLACVL_1_RCKCRE",11,0.01]
["PLACVL_1_RCKCRE",12,0.04]
["PLAINV_6_BSOLAR",1,0]
["PLAINV_6_BSOLAR",2,0]
["PLAINV_6_BSOLAR",3,0]
["PLAINV_6_BSOLAR",4,0]
["PLAINV_6_BSOLAR",5,0]
["PLAINV_6_BSOLAR",6,0]
["PLAINV_6_BSOLAR",7,0]
["PLAINV_6_BSOLAR",8,0]
["PLAINV_6_BSOLAR",9,0]
["PLAINV_6_BSOLAR",10,0]
["PLAINV_6_BSOLAR",11,0]
["PLAINV_6_BSOLAR",12,0]
["PLAINV_6_DSOLAR",1,0.04]
["PLAINV_6_DSOLAR",2,0.3]
["PLAINV_6_DSOLAR",3,0.35]
["PLAINV_6_DSOLAR",4,0.44]
["PLAINV_6_DSOLAR",5,0.64]
["PLAINV_6_DSOLAR",6,1.31]
["PLAINV_6_DSOLAR",7,1.44]
["PLAINV_6_DSOLAR",8,1.24]
["PLAINV_6_DSOLAR",9,1.1100000000000001]
["PLAINV_6_DSOLAR",10,0.74]
["PLAINV_6_DSOLAR",11,0.56999999999999995]
["PLAINV_6_DSOLAR",12,0.35]
["PLAINV_6_NLRSR1",1,0]
["PLAINV_6_NLRSR1",2,0]
["PLAINV_6_NLRSR1",3,0]
["PLAINV_6_NLRSR1",4,0]
["PLAINV_6_NLRSR1",5,0]
["PLAINV_6_NLRSR1",6,0]
["PLAINV_6_NLRSR1",7,0]
["PLAINV_6_NLRSR1",8,0]
["PLAINV_6_NLRSR1",9,0]
["PLAINV_6_NLRSR1",10,0]
["PLAINV_6_NLRSR1",11,0]
["PLAINV_6_NLRSR1",12,0]
["PLAINV_6_SOLAR3",1,0]
["PLAINV_6_SOLAR3",2,0]
["PLAINV_6_SOLAR3",3,0]
["PLAINV_6_SOLAR3",4,0]
["PLAINV_6_SOLAR3",5,0]
["PLAINV_6_SOLAR3",6,0]
["PLAINV_6_SOLAR3",7,0]
["PLAINV_6_SOLAR3",8,0]
["PLAINV_6_SOLAR3",9,0]
["PLAINV_6_SOLAR3",10,0]
["PLAINV_6_SOLAR3",11,0]
["PLAINV_6_SOLAR3",12,0]
["PLAINV_6_SOLARC",1,0]
["PLAINV_6_SOLARC",2,0]
["PLAINV_6_SOLARC",3,0]
["PLAINV_6_SOLARC",4,0]
["PLAINV_6_SOLARC",5,0]
["PLAINV_6_SOLARC",6,0]
["PLAINV_6_SOLARC",7,0]
["PLAINV_6_SOLARC",8,0]
["PLAINV_6_SOLARC",9,0]
["PLAINV_6_SOLARC",10,0]
["PLAINV_6_SOLARC",11,0]
["PLAINV_6_SOLARC",12,0]
["PLMSSR_6_HISIER",1,6]
["PLMSSR_6_HISIER",2,6]
["PLMSSR_6_HISIER",3,6]
["PLMSSR_6_HISIER",4,6]
["PLMSSR_6_HISIER",5,6]
["PLMSSR_6_HISIER",6,6]
["PLMSSR_6_HISIER",7,6]
["PLMSSR_6_HISIER",8,6]
["PLMSSR_6_HISIER",9,6]
["PLMSSR_6_HISIER",10,6]
["PLMSSR_6_HISIER",11,6]
["PLMSSR_6_HISIER",12,6]
["PLSNTG_7_LNCLND",1,3.28]
["PLSNTG_7_LNCLND",2,3.26]
["PLSNTG_7_LNCLND",3,3.22]
["PLSNTG_7_LNCLND",4,3.31]
["PLSNTG_7_LNCLND",5,3.69]
["PLSNTG_7_LNCLND",6,3.63]
["PLSNTG_7_LNCLND",7,3.63]
["PLSNTG_7_LNCLND",8,3.6]
["PLSNTG_7_LNCLND",9,3.64]
["PLSNTG_7_LNCLND",10,3.69]
["PLSNTG_7_LNCLND",11,3.48]
["PLSNTG_7_LNCLND",12,3.66]
["PMDLET_6_SOLAR1",1,0.04]
["PMDLET_6_SOLAR1",2,0.3]
["PMDLET_6_SOLAR1",3,0.35]
["PMDLET_6_SOLAR1",4,0.44]
["PMDLET_6_SOLAR1",5,0.64]
["PMDLET_6_SOLAR1",6,1.31]
["PMDLET_6_SOLAR1",7,1.44]
["PMDLET_6_SOLAR1",8,1.24]
["PMDLET_6_SOLAR1",9,1.1100000000000001]
["PMDLET_6_SOLAR1",10,0.74]
["PMDLET_6_SOLAR1",11,0.56999999999999995]
["PMDLET_6_SOLAR1",12,0.35]
["PMPJCK_1_RB2SLR",1,0.08]
["PMPJCK_1_RB2SLR",2,0.6]
["PMPJCK_1_RB2SLR",3,0.7]
["PMPJCK_1_RB2SLR",4,0.88]
["PMPJCK_1_RB2SLR",5,1.28]
["PMPJCK_1_RB2SLR",6,2.62]
["PMPJCK_1_RB2SLR",7,2.88]
["PMPJCK_1_RB2SLR",8,2.48]
["PMPJCK_1_RB2SLR",9,2.2200000000000002]
["PMPJCK_1_RB2SLR",10,1.48]
["PMPJCK_1_RB2SLR",11,1.1399999999999999]
["PMPJCK_1_RB2SLR",12,0.7]
["PMPJCK_1_SOLAR1",1,0.08]
["PMPJCK_1_SOLAR1",2,0.6]
["PMPJCK_1_SOLAR1",3,0.7]
["PMPJCK_1_SOLAR1",4,0.88]
["PMPJCK_1_SOLAR1",5,1.28]
["PMPJCK_1_SOLAR1",6,2.62]
["PMPJCK_1_SOLAR1",7,2.88]
["PMPJCK_1_SOLAR1",8,2.48]
["PMPJCK_1_SOLAR1",9,2.2200000000000002]
["PMPJCK_1_SOLAR1",10,1.48]
["PMPJCK_1_SOLAR1",11,1.1399999999999999]
["PMPJCK_1_SOLAR1",12,0.7]
["PMPJCK_1_SOLAR2",1,0.08]
["PMPJCK_1_SOLAR2",2,0.6]
["PMPJCK_1_SOLAR2",3,0.7]
["PMPJCK_1_SOLAR2",4,0.88]
["PMPJCK_1_SOLAR2",5,1.28]
["PMPJCK_1_SOLAR2",6,2.62]
["PMPJCK_1_SOLAR2",7,2.88]
["PMPJCK_1_SOLAR2",8,2.48]
["PMPJCK_1_SOLAR2",9,2.2200000000000002]
["PMPJCK_1_SOLAR2",10,1.48]
["PMPJCK_1_SOLAR2",11,1.1399999999999999]
["PMPJCK_1_SOLAR2",12,0.7]
["PNCHEG_2_PL1X4",1,417]
["PNCHEG_2_PL1X4",2,417]
["PNCHEG_2_PL1X4",3,417]
["PNCHEG_2_PL1X4",4,417]
["PNCHEG_2_PL1X4",5,417]
["PNCHEG_2_PL1X4",6,417]
["PNCHEG_2_PL1X4",7,417]
["PNCHEG_2_PL1X4",8,417]
["PNCHEG_2_PL1X4",9,417]
["PNCHEG_2_PL1X4",10,417]
["PNCHEG_2_PL1X4",11,417]
["PNCHEG_2_PL1X4",12,417]
["PNCHPP_1_PL1X2",1,119.91]
["PNCHPP_1_PL1X2",2,119.91]
["PNCHPP_1_PL1X2",3,119]
["PNCHPP_1_PL1X2",4,116]
["PNCHPP_1_PL1X2",5,114]
["PNCHPP_1_PL1X2",6,114.2]
["PNCHPP_1_PL1X2",7,114.2]
["PNCHPP_1_PL1X2",8,111]
["PNCHPP_1_PL1X2",9,109]
["PNCHPP_1_PL1X2",10,114]
["PNCHPP_1_PL1X2",11,118]
["PNCHPP_1_PL1X2",12,119.91]
["PNCHVS_2_SOLAR",1,0.56000000000000005]
["PNCHVS_2_SOLAR",2,4.2]
["PNCHVS_2_SOLAR",3,4.9000000000000004]
["PNCHVS_2_SOLAR",4,6.16]
["PNCHVS_2_SOLAR",5,8.9600000000000009]
["PNCHVS_2_SOLAR",6,18.34]
["PNCHVS_2_SOLAR",7,20.16]
["PNCHVS_2_SOLAR",8,17.36]
["PNCHVS_2_SOLAR",9,15.54]
["PNCHVS_2_SOLAR",10,10.36]
["PNCHVS_2_SOLAR",11,7.98]
["PNCHVS_2_SOLAR",12,4.9000000000000004]
["PNOCHE_1_PL1X2",1,49.97]
["PNOCHE_1_PL1X2",2,49.97]
["PNOCHE_1_PL1X2",3,49.97]
["PNOCHE_1_PL1X2",4,49.97]
["PNOCHE_1_PL1X2",5,49.97]
["PNOCHE_1_PL1X2",6,49.97]
["PNOCHE_1_PL1X2",7,49.97]
["PNOCHE_1_PL1X2",8,49.97]
["PNOCHE_1_PL1X2",9,49.97]
["PNOCHE_1_PL1X2",10,49.97]
["PNOCHE_1_PL1X2",11,49.97]
["PNOCHE_1_PL1X2",12,49.97]
["PNOCHE_1_UNITA1",1,52.01]
["PNOCHE_1_UNITA1",2,52.01]
["PNOCHE_1_UNITA1",3,52.01]
["PNOCHE_1_UNITA1",4,52.01]
["PNOCHE_1_UNITA1",5,52.01]
["PNOCHE_1_UNITA1",6,52.01]
["PNOCHE_1_UNITA1",7,52.01]
["PNOCHE_1_UNITA1",8,52.01]
["PNOCHE_1_UNITA1",9,52.01]
["PNOCHE_1_UNITA1",10,52.01]
["PNOCHE_1_UNITA1",11,52.01]
["PNOCHE_1_UNITA1",12,52.01]
["POEPH_7_UNIT 1",1,43.6]
["POEPH_7_UNIT 1",2,48]
["POEPH_7_UNIT 1",3,48]
["POEPH_7_UNIT 1",4,48]
["POEPH_7_UNIT 1",5,43.6]
["POEPH_7_UNIT 1",6,44.8]
["POEPH_7_UNIT 1",7,45.2]
["POEPH_7_UNIT 1",8,44]
["POEPH_7_UNIT 1",9,40.130000000000003]
["POEPH_7_UNIT 1",10,32.4]
["POEPH_7_UNIT 1",11,18.399999999999999]
["POEPH_7_UNIT 1",12,15.55]
["POEPH_7_UNIT 2",1,44]
["POEPH_7_UNIT 2",2,48]
["POEPH_7_UNIT 2",3,48]
["POEPH_7_UNIT 2",4,48]
["POEPH_7_UNIT 2",5,41.41]
["POEPH_7_UNIT 2",6,20]
["POEPH_7_UNIT 2",7,40]
["POEPH_7_UNIT 2",8,42.64]
["POEPH_7_UNIT 2",9,42.64]
["POEPH_7_UNIT 2",10,20.399999999999999]
["POEPH_7_UNIT 2",11,20]
["POEPH_7_UNIT 2",12,15.38]
["POTTER_6_UNITS",1,1.92]
["POTTER_6_UNITS",2,1.38]
["POTTER_6_UNITS",3,0.85]
["POTTER_6_UNITS",4,1.24]
["POTTER_6_UNITS",5,1.34]
["POTTER_6_UNITS",6,1.34]
["POTTER_6_UNITS",7,1.41]
["POTTER_6_UNITS",8,1.42]
["POTTER_6_UNITS",9,1.18]
["POTTER_6_UNITS",10,1]
["POTTER_6_UNITS",11,1.1499999999999999]
["POTTER_6_UNITS",12,1.55]
["POTTER_7_VECINO",1,0]
["POTTER_7_VECINO",2,0]
["POTTER_7_VECINO",3,0]
["POTTER_7_VECINO",4,0]
["POTTER_7_VECINO",5,0]
["POTTER_7_VECINO",6,0]
["POTTER_7_VECINO",7,0]
["POTTER_7_VECINO",8,0]
["POTTER_7_VECINO",9,0]
["POTTER_7_VECINO",10,0]
["POTTER_7_VECINO",11,0]
["POTTER_7_VECINO",12,0]
["PRCTVY_1_MIGBT1",1,0]
["PRCTVY_1_MIGBT1",2,0]
["PRCTVY_1_MIGBT1",3,0]
["PRCTVY_1_MIGBT1",4,0]
["PRCTVY_1_MIGBT1",5,0]
["PRCTVY_1_MIGBT1",6,0]
["PRCTVY_1_MIGBT1",7,0]
["PRCTVY_1_MIGBT1",8,0]
["PRCTVY_1_MIGBT1",9,0]
["PRCTVY_1_MIGBT1",10,0]
["PRCTVY_1_MIGBT1",11,0]
["PRCTVY_1_MIGBT1",12,0]
["PRIMM_2_SOLAR1",1,1]
["PRIMM_2_SOLAR1",2,7.5]
["PRIMM_2_SOLAR1",3,8.75]
["PRIMM_2_SOLAR1",4,11]
["PRIMM_2_SOLAR1",5,16]
["PRIMM_2_SOLAR1",6,32.75]
["PRIMM_2_SOLAR1",7,36]
["PRIMM_2_SOLAR1",8,31]
["PRIMM_2_SOLAR1",9,27.75]
["PRIMM_2_SOLAR1",10,18.5]
["PRIMM_2_SOLAR1",11,14.25]
["PRIMM_2_SOLAR1",12,8.75]
["PSWEET_1_STCRUZ",1,0]
["PSWEET_1_STCRUZ",2,0]
["PSWEET_1_STCRUZ",3,0]
["PSWEET_1_STCRUZ",4,0]
["PSWEET_1_STCRUZ",5,0]
["PSWEET_1_STCRUZ",6,0]
["PSWEET_1_STCRUZ",7,0]
["PSWEET_1_STCRUZ",8,0]
["PSWEET_1_STCRUZ",9,0]
["PSWEET_1_STCRUZ",10,0]
["PSWEET_1_STCRUZ",11,0]
["PSWEET_1_STCRUZ",12,0]
["PSWEET_7_QFUNTS",1,0]
["PSWEET_7_QFUNTS",2,0]
["PSWEET_7_QFUNTS",3,0]
["PSWEET_7_QFUNTS",4,0]
["PSWEET_7_QFUNTS",5,0]
["PSWEET_7_QFUNTS",6,0]
["PSWEET_7_QFUNTS",7,0]
["PSWEET_7_QFUNTS",8,0]
["PSWEET_7_QFUNTS",9,0]
["PSWEET_7_QFUNTS",10,0]
["PSWEET_7_QFUNTS",11,0]
["PSWEET_7_QFUNTS",12,0]
["PUTHCR_1_PCNSB1",1,3]
["PUTHCR_1_PCNSB1",2,3]
["PUTHCR_1_PCNSB1",3,3]
["PUTHCR_1_PCNSB1",4,3]
["PUTHCR_1_PCNSB1",5,3]
["PUTHCR_1_PCNSB1",6,3]
["PUTHCR_1_PCNSB1",7,3]
["PUTHCR_1_PCNSB1",8,3]
["PUTHCR_1_PCNSB1",9,3]
["PUTHCR_1_PCNSB1",10,3]
["PUTHCR_1_PCNSB1",11,3]
["PUTHCR_1_PCNSB1",12,2.57]
["PUTHCR_1_SOLAR1",1,0.01]
["PUTHCR_1_SOLAR1",2,0.06]
["PUTHCR_1_SOLAR1",3,7.0000000000000007E-2]
["PUTHCR_1_SOLAR1",4,0.09]
["PUTHCR_1_SOLAR1",5,0.13]
["PUTHCR_1_SOLAR1",6,0.26]
["PUTHCR_1_SOLAR1",7,0.28999999999999998]
["PUTHCR_1_SOLAR1",8,0.25]
["PUTHCR_1_SOLAR1",9,0.22]
["PUTHCR_1_SOLAR1",10,0.15]
["PUTHCR_1_SOLAR1",11,0.11]
["PUTHCR_1_SOLAR1",12,7.0000000000000007E-2]
["PWEST_1_UNIT",1,0.37]
["PWEST_1_UNIT",2,0.39]
["PWEST_1_UNIT",3,0.35]
["PWEST_1_UNIT",4,0.33]
["PWEST_1_UNIT",5,0.35]
["PWEST_1_UNIT",6,0.32]
["PWEST_1_UNIT",7,0.3]
["PWEST_1_UNIT",8,0.23]
["PWEST_1_UNIT",9,0.24]
["PWEST_1_UNIT",10,0.22]
["PWEST_1_UNIT",11,0.3]
["PWEST_1_UNIT",12,0.36]
["RATSKE_2_NROSR1",1,0.6]
["RATSKE_2_NROSR1",2,4.5]
["RATSKE_2_NROSR1",3,5.25]
["RATSKE_2_NROSR1",4,6.6]
["RATSKE_2_NROSR1",5,9.6]
["RATSKE_2_NROSR1",6,19.649999999999999]
["RATSKE_2_NROSR1",7,21.6]
["RATSKE_2_NROSR1",8,18.600000000000001]
["RATSKE_2_NROSR1",9,16.649999999999999]
["RATSKE_2_NROSR1",10,11.1]
["RATSKE_2_NROSR1",11,8.5500000000000007]
["RATSKE_2_NROSR1",12,5.25]
["RATSKE_2_RBSSB1",1,7.71]
["RATSKE_2_RBSSB1",2,9.14]
["RATSKE_2_RBSSB1",3,9.43]
["RATSKE_2_RBSSB1",4,9.9700000000000006]
["RATSKE_2_RBSSB1",5,11.11]
["RATSKE_2_RBSSB1",6,14.92]
["RATSKE_2_RBSSB1",7,15.65]
["RATSKE_2_RBSSB1",8,14.49]
["RATSKE_2_RBSSB1",9,13.69]
["RATSKE_2_RBSSB1",10,11.58]
["RATSKE_2_RBSSB1",11,10.56]
["RATSKE_2_RBSSB1",12,9.2899999999999991]
["RATSKE_2_RBSSB2",1,5.14]
["RATSKE_2_RBSSB2",2,6.09]
["RATSKE_2_RBSSB2",3,6.29]
["RATSKE_2_RBSSB2",4,6.65]
["RATSKE_2_RBSSB2",5,7.41]
["RATSKE_2_RBSSB2",6,9.9499999999999993]
["RATSKE_2_RBSSB2",7,10.43]
["RATSKE_2_RBSSB2",8,9.66]
["RATSKE_2_RBSSB2",9,9.1300000000000008]
["RATSKE_2_RBSSB2",10,7.72]
["RATSKE_2_RBSSB2",11,7.04]
["RATSKE_2_RBSSB2",12,6.2]
["RCKCRK_7_UNIT 1",1,33.68]
["RCKCRK_7_UNIT 1",2,20]
["RCKCRK_7_UNIT 1",3,33.4]
["RCKCRK_7_UNIT 1",4,36]
["RCKCRK_7_UNIT 1",5,2.4]
["RCKCRK_7_UNIT 1",6,6.4]
["RCKCRK_7_UNIT 1",7,31.89]
["RCKCRK_7_UNIT 1",8,30]
["RCKCRK_7_UNIT 1",9,24]
["RCKCRK_7_UNIT 1",10,16.399999999999999]
["RCKCRK_7_UNIT 1",11,15.48]
["RCKCRK_7_UNIT 1",12,20]
["RCKCRK_7_UNIT 2",1,24]
["RCKCRK_7_UNIT 2",2,36]
["RCKCRK_7_UNIT 2",3,40]
["RCKCRK_7_UNIT 2",4,16]
["RCKCRK_7_UNIT 2",5,16]
["RCKCRK_7_UNIT 2",6,24.26]
["RCKCRK_7_UNIT 2",7,36]
["RCKCRK_7_UNIT 2",8,40]
["RCKCRK_7_UNIT 2",9,40]
["RCKCRK_7_UNIT 2",10,0]
["RCKCRK_7_UNIT 2",11,0]
["RCKCRK_7_UNIT 2",12,16.100000000000001]
["RDWAY_1_CREST",1,0]
["RDWAY_1_CREST",2,0]
["RDWAY_1_CREST",3,0]
["RDWAY_1_CREST",4,0]
["RDWAY_1_CREST",5,0]
["RDWAY_1_CREST",6,0]
["RDWAY_1_CREST",7,0]
["RDWAY_1_CREST",8,0]
["RDWAY_1_CREST",9,0]
["RDWAY_1_CREST",10,0]
["RDWAY_1_CREST",11,0]
["RDWAY_1_CREST",12,0]
["RECTOR_2_CREST",1,0]
["RECTOR_2_CREST",2,0]
["RECTOR_2_CREST",3,0]
["RECTOR_2_CREST",4,0]
["RECTOR_2_CREST",5,0]
["RECTOR_2_CREST",6,0]
["RECTOR_2_CREST",7,0]
["RECTOR_2_CREST",8,0]
["RECTOR_2_CREST",9,0]
["RECTOR_2_CREST",10,0]
["RECTOR_2_CREST",11,0]
["RECTOR_2_CREST",12,0]
["RECTOR_2_IVANPV",1,0]
["RECTOR_2_IVANPV",2,0]
["RECTOR_2_IVANPV",3,0]
["RECTOR_2_IVANPV",4,0]
["RECTOR_2_IVANPV",5,0]
["RECTOR_2_IVANPV",6,0]
["RECTOR_2_IVANPV",7,0]
["RECTOR_2_IVANPV",8,0]
["RECTOR_2_IVANPV",9,0]
["RECTOR_2_IVANPV",10,0]
["RECTOR_2_IVANPV",11,0]
["RECTOR_2_IVANPV",12,0]
["RECTOR_2_KAWEAH",1,2.16]
["RECTOR_2_KAWEAH",2,2.09]
["RECTOR_2_KAWEAH",3,2.58]
["RECTOR_2_KAWEAH",4,3.41]
["RECTOR_2_KAWEAH",5,3.27]
["RECTOR_2_KAWEAH",6,2.96]
["RECTOR_2_KAWEAH",7,2.19]
["RECTOR_2_KAWEAH",8,1.66]
["RECTOR_2_KAWEAH",9,0.76]
["RECTOR_2_KAWEAH",10,0]
["RECTOR_2_KAWEAH",11,0]
["RECTOR_2_KAWEAH",12,1.1599999999999999]
["RECTOR_2_KAWH 1",1,0]
["RECTOR_2_KAWH 1",2,0]
["RECTOR_2_KAWH 1",3,0]
["RECTOR_2_KAWH 1",4,0]
["RECTOR_2_KAWH 1",5,0]
["RECTOR_2_KAWH 1",6,0]
["RECTOR_2_KAWH 1",7,0]
["RECTOR_2_KAWH 1",8,0]
["RECTOR_2_KAWH 1",9,0]
["RECTOR_2_KAWH 1",10,0]
["RECTOR_2_KAWH 1",11,0]
["RECTOR_2_KAWH 1",12,0]
["RECTOR_2_QF",1,0]
["RECTOR_2_QF",2,0]
["RECTOR_2_QF",3,0]
["RECTOR_2_QF",4,0]
["RECTOR_2_QF",5,5.2]
["RECTOR_2_QF",6,12.74]
["RECTOR_2_QF",7,4.8]
["RECTOR_2_QF",8,0]
["RECTOR_2_QF",9,0]
["RECTOR_2_QF",10,0]
["RECTOR_2_QF",11,0]
["RECTOR_2_QF",12,0]
["RECTOR_2_TFDBM1",1,0]
["RECTOR_2_TFDBM1",2,0]
["RECTOR_2_TFDBM1",3,0]
["RECTOR_2_TFDBM1",4,0]
["RECTOR_2_TFDBM1",5,0]
["RECTOR_2_TFDBM1",6,0]
["RECTOR_2_TFDBM1",7,0]
["RECTOR_2_TFDBM1",8,0]
["RECTOR_2_TFDBM1",9,0]
["RECTOR_2_TFDBM1",10,0]
["RECTOR_2_TFDBM1",11,0]
["RECTOR_2_TFDBM1",12,0]
["RECTOR_7_TULARE",1,0]
["RECTOR_7_TULARE",2,0]
["RECTOR_7_TULARE",3,0]
["RECTOR_7_TULARE",4,0]
["RECTOR_7_TULARE",5,0]
["RECTOR_7_TULARE",6,0]
["RECTOR_7_TULARE",7,0]
["RECTOR_7_TULARE",8,0]
["RECTOR_7_TULARE",9,0]
["RECTOR_7_TULARE",10,0]
["RECTOR_7_TULARE",11,0]
["RECTOR_7_TULARE",12,0]
["REDBLF_6_UNIT",1,44]
["REDBLF_6_UNIT",2,44]
["REDBLF_6_UNIT",3,44]
["REDBLF_6_UNIT",4,44]
["REDBLF_6_UNIT",5,44]
["REDBLF_6_UNIT",6,44]
["REDBLF_6_UNIT",7,44]
["REDBLF_6_UNIT",8,44]
["REDBLF_6_UNIT",9,44]
["REDBLF_6_UNIT",10,44]
["REDBLF_6_UNIT",11,44]
["REDBLF_6_UNIT",12,44]
["REDMAN_2_SOLAR",1,0.02]
["REDMAN_2_SOLAR",2,0.11]
["REDMAN_2_SOLAR",3,0.13]
["REDMAN_2_SOLAR",4,0.17]
["REDMAN_2_SOLAR",5,0.24]
["REDMAN_2_SOLAR",6,0.49]
["REDMAN_2_SOLAR",7,0.54]
["REDMAN_2_SOLAR",8,0.47]
["REDMAN_2_SOLAR",9,0.42]
["REDMAN_2_SOLAR",10,0.28000000000000003]
["REDMAN_2_SOLAR",11,0.21]
["REDMAN_2_SOLAR",12,0.13]
["REDMAN_6_AVSSR1",1,0.01]
["REDMAN_6_AVSSR1",2,0.09]
["REDMAN_6_AVSSR1",3,0.11]
["REDMAN_6_AVSSR1",4,0.13]
["REDMAN_6_AVSSR1",5,0.19]
["REDMAN_6_AVSSR1",6,0.39]
["REDMAN_6_AVSSR1",7,0.43]
["REDMAN_6_AVSSR1",8,0.37]
["REDMAN_6_AVSSR1",9,0.33]
["REDMAN_6_AVSSR1",10,0.22]
["REDMAN_6_AVSSR1",11,0.17]
["REDMAN_6_AVSSR1",12,0.11]
["REDOND_7_UNIT 5",1,178.87]
["REDOND_7_UNIT 5",2,178.87]
["REDOND_7_UNIT 5",3,178.87]
["REDOND_7_UNIT 5",4,178.87]
["REDOND_7_UNIT 5",5,178.87]
["REDOND_7_UNIT 5",6,178.87]
["REDOND_7_UNIT 5",7,178.87]
["REDOND_7_UNIT 5",8,178.87]
["REDOND_7_UNIT 5",9,178.87]
["REDOND_7_UNIT 5",10,178.87]
["REDOND_7_UNIT 5",11,178.87]
["REDOND_7_UNIT 5",12,178.87]
["REDOND_7_UNIT 6",1,174.29]
["REDOND_7_UNIT 6",2,174.29]
["REDOND_7_UNIT 6",3,174.29]
["REDOND_7_UNIT 6",4,174.29]
["REDOND_7_UNIT 6",5,174.29]
["REDOND_7_UNIT 6",6,174.29]
["REDOND_7_UNIT 6",7,174.29]
["REDOND_7_UNIT 6",8,174.29]
["REDOND_7_UNIT 6",9,174.29]
["REDOND_7_UNIT 6",10,174.29]
["REDOND_7_UNIT 6",11,174.29]
["REDOND_7_UNIT 6",12,174.29]
["REDOND_7_UNIT 8",1,480]
["REDOND_7_UNIT 8",2,480]
["REDOND_7_UNIT 8",3,480]
["REDOND_7_UNIT 8",4,480]
["REDOND_7_UNIT 8",5,480]
["REDOND_7_UNIT 8",6,480]
["REDOND_7_UNIT 8",7,480]
["REDOND_7_UNIT 8",8,480]
["REDOND_7_UNIT 8",9,480]
["REDOND_7_UNIT 8",10,480]
["REDOND_7_UNIT 8",11,480]
["REDOND_7_UNIT 8",12,480]
["REEDLY_6_SOLAR",1,0]
["REEDLY_6_SOLAR",2,0]
["REEDLY_6_SOLAR",3,0]
["REEDLY_6_SOLAR",4,0]
["REEDLY_6_SOLAR",5,0]
["REEDLY_6_SOLAR",6,0]
["REEDLY_6_SOLAR",7,0]
["REEDLY_6_SOLAR",8,0]
["REEDLY_6_SOLAR",9,0]
["REEDLY_6_SOLAR",10,0]
["REEDLY_6_SOLAR",11,0]
["REEDLY_6_SOLAR",12,0]
["RENWD_1_QF",1,1.77]
["RENWD_1_QF",2,1.88]
["RENWD_1_QF",3,1.65]
["RENWD_1_QF",4,1.58]
["RENWD_1_QF",5,1.68]
["RENWD_1_QF",6,1.54]
["RENWD_1_QF",7,1.43]
["RENWD_1_QF",8,1.0900000000000001]
["RENWD_1_QF",9,1.1200000000000001]
["RENWD_1_QF",10,1.04]
["RENWD_1_QF",11,1.41]
["RENWD_1_QF",12,1.7]
["RICHMN_1_CHVSR2",1,0.03]
["RICHMN_1_CHVSR2",2,0.26]
["RICHMN_1_CHVSR2",3,0.3]
["RICHMN_1_CHVSR2",4,0.37]
["RICHMN_1_CHVSR2",5,0.54]
["RICHMN_1_CHVSR2",6,1.1100000000000001]
["RICHMN_1_CHVSR2",7,1.22]
["RICHMN_1_CHVSR2",8,1.05]
["RICHMN_1_CHVSR2",9,0.94]
["RICHMN_1_CHVSR2",10,0.63]
["RICHMN_1_CHVSR2",11,0.48]
["RICHMN_1_CHVSR2",12,0.3]
["RICHMN_1_SOLAR",1,0.01]
["RICHMN_1_SOLAR",2,0.06]
["RICHMN_1_SOLAR",3,7.0000000000000007E-2]
["RICHMN_1_SOLAR",4,0.09]
["RICHMN_1_SOLAR",5,0.13]
["RICHMN_1_SOLAR",6,0.26]
["RICHMN_1_SOLAR",7,0.28999999999999998]
["RICHMN_1_SOLAR",8,0.25]
["RICHMN_1_SOLAR",9,0.22]
["RICHMN_1_SOLAR",10,0.15]
["RICHMN_1_SOLAR",11,0.11]
["RICHMN_1_SOLAR",12,7.0000000000000007E-2]
["RICHMN_7_BAYENV",1,0.46]
["RICHMN_7_BAYENV",2,0.45]
["RICHMN_7_BAYENV",3,0.4]
["RICHMN_7_BAYENV",4,0.38]
["RICHMN_7_BAYENV",5,0.35]
["RICHMN_7_BAYENV",6,0.4]
["RICHMN_7_BAYENV",7,0.35]
["RICHMN_7_BAYENV",8,0.41]
["RICHMN_7_BAYENV",9,0.1]
["RICHMN_7_BAYENV",10,0.3]
["RICHMN_7_BAYENV",11,0.39]
["RICHMN_7_BAYENV",12,0.28999999999999998]
["RIOBRV_6_UNIT 1",1,0.14000000000000001]
["RIOBRV_6_UNIT 1",2,0.19]
["RIOBRV_6_UNIT 1",3,0.3]
["RIOBRV_6_UNIT 1",4,4.5999999999999996]
["RIOBRV_6_UNIT 1",5,4.3499999999999996]
["RIOBRV_6_UNIT 1",6,3.37]
["RIOBRV_6_UNIT 1",7,6.23]
["RIOBRV_6_UNIT 1",8,4.72]
["RIOBRV_6_UNIT 1",9,2.9]
["RIOBRV_6_UNIT 1",10,1.66]
["RIOBRV_6_UNIT 1",11,0.28999999999999998]
["RIOBRV_6_UNIT 1",12,0]
["RIOOSO_1_QF",1,0.13]
["RIOOSO_1_QF",2,0.38]
["RIOOSO_1_QF",3,0.39]
["RIOOSO_1_QF",4,0.6]
["RIOOSO_1_QF",5,0.73]
["RIOOSO_1_QF",6,0.6]
["RIOOSO_1_QF",7,0.51]
["RIOOSO_1_QF",8,0.59]
["RIOOSO_1_QF",9,0.53]
["RIOOSO_1_QF",10,0.08]
["RIOOSO_1_QF",11,0.02]
["RIOOSO_1_QF",12,0.05]
["RNDMTN_2_SLSPHY1",1,0.2]
["RNDMTN_2_SLSPHY1",2,0.22]
["RNDMTN_2_SLSPHY1",3,0.28000000000000003]
["RNDMTN_2_SLSPHY1",4,0.28999999999999998]
["RNDMTN_2_SLSPHY1",5,0.26]
["RNDMTN_2_SLSPHY1",6,0.23]
["RNDMTN_2_SLSPHY1",7,0.21]
["RNDMTN_2_SLSPHY1",8,0.2]
["RNDMTN_2_SLSPHY1",9,0.17]
["RNDMTN_2_SLSPHY1",10,0.16]
["RNDMTN_2_SLSPHY1",11,0.17]
["RNDMTN_2_SLSPHY1",12,0.16]
["RNDSBG_1_HZASR1",1,0.01]
["RNDSBG_1_HZASR1",2,0.09]
["RNDSBG_1_HZASR1",3,0.1]
["RNDSBG_1_HZASR1",4,0.13]
["RNDSBG_1_HZASR1",5,0.19]
["RNDSBG_1_HZASR1",6,0.39]
["RNDSBG_1_HZASR1",7,0.43]
["RNDSBG_1_HZASR1",8,0.37]
["RNDSBG_1_HZASR1",9,0.33]
["RNDSBG_1_HZASR1",10,0.22]
["RNDSBG_1_HZASR1",11,0.17]
["RNDSBG_1_HZASR1",12,0.1]
["ROLLIN_6_UNIT",1,5.12]
["ROLLIN_6_UNIT",2,4.08]
["ROLLIN_6_UNIT",3,6.58]
["ROLLIN_6_UNIT",4,10.25]
["ROLLIN_6_UNIT",5,9.86]
["ROLLIN_6_UNIT",6,5.96]
["ROLLIN_6_UNIT",7,6.74]
["ROLLIN_6_UNIT",8,5.94]
["ROLLIN_6_UNIT",9,4.6900000000000004]
["ROLLIN_6_UNIT",10,2.11]
["ROLLIN_6_UNIT",11,1.04]
["ROLLIN_6_UNIT",12,6.62]
["ROSMDW_2_WIND1",1,24.74]
["ROSMDW_2_WIND1",2,26.31]
["ROSMDW_2_WIND1",3,23.12]
["ROSMDW_2_WIND1",4,22.15]
["ROSMDW_2_WIND1",5,23.55]
["ROSMDW_2_WIND1",6,21.59]
["ROSMDW_2_WIND1",7,20.059999999999999]
["ROSMDW_2_WIND1",8,15.24]
["ROSMDW_2_WIND1",9,15.74]
["ROSMDW_2_WIND1",10,14.61]
["ROSMDW_2_WIND1",11,19.68]
["ROSMDW_2_WIND1",12,23.84]
["ROSMND_6_SOLAR",1,0.01]
["ROSMND_6_SOLAR",2,0.09]
["ROSMND_6_SOLAR",3,0.11]
["ROSMND_6_SOLAR",4,0.13]
["ROSMND_6_SOLAR",5,0.19]
["ROSMND_6_SOLAR",6,0.39]
["ROSMND_6_SOLAR",7,0.43]
["ROSMND_6_SOLAR",8,0.37]
["ROSMND_6_SOLAR",9,0.33]
["ROSMND_6_SOLAR",10,0.22]
["ROSMND_6_SOLAR",11,0.17]
["ROSMND_6_SOLAR",12,0.11]
["RSMSLR_6_SOLAR1",1,0.08]
["RSMSLR_6_SOLAR1",2,0.6]
["RSMSLR_6_SOLAR1",3,0.7]
["RSMSLR_6_SOLAR1",4,0.88]
["RSMSLR_6_SOLAR1",5,1.28]
["RSMSLR_6_SOLAR1",6,2.62]
["RSMSLR_6_SOLAR1",7,2.88]
["RSMSLR_6_SOLAR1",8,2.48]
["RSMSLR_6_SOLAR1",9,2.2200000000000002]
["RSMSLR_6_SOLAR1",10,1.48]
["RSMSLR_6_SOLAR1",11,1.1399999999999999]
["RSMSLR_6_SOLAR1",12,0.7]
["RSMSLR_6_SOLAR2",1,0.08]
["RSMSLR_6_SOLAR2",2,0.6]
["RSMSLR_6_SOLAR2",3,0.7]
["RSMSLR_6_SOLAR2",4,0.88]
["RSMSLR_6_SOLAR2",5,1.28]
["RSMSLR_6_SOLAR2",6,2.62]
["RSMSLR_6_SOLAR2",7,2.88]
["RSMSLR_6_SOLAR2",8,2.48]
["RSMSLR_6_SOLAR2",9,2.2200000000000002]
["RSMSLR_6_SOLAR2",10,1.48]
["RSMSLR_6_SOLAR2",11,1.1399999999999999]
["RSMSLR_6_SOLAR2",12,0.7]
["RTEDDY_2_SC1SR3",1,0.16]
["RTEDDY_2_SC1SR3",2,1.2]
["RTEDDY_2_SC1SR3",3,1.4]
["RTEDDY_2_SC1SR3",4,1.76]
["RTEDDY_2_SC1SR3",5,2.56]
["RTEDDY_2_SC1SR3",6,5.24]
["RTEDDY_2_SC1SR3",7,5.76]
["RTEDDY_2_SC1SR3",8,4.96]
["RTEDDY_2_SC1SR3",9,4.4400000000000004]
["RTEDDY_2_SC1SR3",10,2.96]
["RTEDDY_2_SC1SR3",11,2.2799999999999998]
["RTEDDY_2_SC1SR3",12,1.4]
["RTEDDY_2_SEBSR3",1,0.22]
["RTEDDY_2_SEBSR3",2,1.68]
["RTEDDY_2_SEBSR3",3,1.96]
["RTEDDY_2_SEBSR3",4,2.46]
["RTEDDY_2_SEBSR3",5,3.58]
["RTEDDY_2_SEBSR3",6,7.34]
["RTEDDY_2_SEBSR3",7,8.06]
["RTEDDY_2_SEBSR3",8,6.94]
["RTEDDY_2_SEBSR3",9,6.22]
["RTEDDY_2_SEBSR3",10,4.1399999999999997]
["RTEDDY_2_SEBSR3",11,3.19]
["RTEDDY_2_SEBSR3",12,1.96]
["RTEDDY_2_SEBSR4",1,0.22]
["RTEDDY_2_SEBSR4",2,1.68]
["RTEDDY_2_SEBSR4",3,1.96]
["RTEDDY_2_SEBSR4",4,2.46]
["RTEDDY_2_SEBSR4",5,3.58]
["RTEDDY_2_SEBSR4",6,7.34]
["RTEDDY_2_SEBSR4",7,8.06]
["RTEDDY_2_SEBSR4",8,6.94]
["RTEDDY_2_SEBSR4",9,6.22]
["RTEDDY_2_SEBSR4",10,4.1399999999999997]
["RTEDDY_2_SEBSR4",11,3.19]
["RTEDDY_2_SEBSR4",12,1.96]
["RTEDDY_2_SOLAR1",1,0.22]
["RTEDDY_2_SOLAR1",2,1.62]
["RTEDDY_2_SOLAR1",3,1.89]
["RTEDDY_2_SOLAR1",4,2.38]
["RTEDDY_2_SOLAR1",5,3.46]
["RTEDDY_2_SOLAR1",6,7.07]
["RTEDDY_2_SOLAR1",7,7.78]
["RTEDDY_2_SOLAR1",8,6.7]
["RTEDDY_2_SOLAR1",9,5.99]
["RTEDDY_2_SOLAR1",10,4]
["RTEDDY_2_SOLAR1",11,3.08]
["RTEDDY_2_SOLAR1",12,1.89]
["RTEDDY_2_SOLAR2",1,0.22]
["RTEDDY_2_SOLAR2",2,1.62]
["RTEDDY_2_SOLAR2",3,1.89]
["RTEDDY_2_SOLAR2",4,2.38]
["RTEDDY_2_SOLAR2",5,3.46]
["RTEDDY_2_SOLAR2",6,7.07]
["RTEDDY_2_SOLAR2",7,7.78]
["RTEDDY_2_SOLAR2",8,6.7]
["RTEDDY_2_SOLAR2",9,5.99]
["RTEDDY_2_SOLAR2",10,4]
["RTEDDY_2_SOLAR2",11,3.08]
["RTEDDY_2_SOLAR2",12,1.89]
["RTEDDY_2_SPASR4",1,0.1]
["RTEDDY_2_SPASR4",2,0.78]
["RTEDDY_2_SPASR4",3,0.91]
["RTEDDY_2_SPASR4",4,1.1399999999999999]
["RTEDDY_2_SPASR4",5,1.66]
["RTEDDY_2_SPASR4",6,3.41]
["RTEDDY_2_SPASR4",7,3.74]
["RTEDDY_2_SPASR4",8,3.22]
["RTEDDY_2_SPASR4",9,2.89]
["RTEDDY_2_SPASR4",10,1.92]
["RTEDDY_2_SPASR4",11,1.48]
["RTEDDY_2_SPASR4",12,0.91]
["RTEDDY_2_SRXSR4",1,0.05]
["RTEDDY_2_SRXSR4",2,0.41]
["RTEDDY_2_SRXSR4",3,0.48]
["RTEDDY_2_SRXSR4",4,0.6]
["RTEDDY_2_SRXSR4",5,0.87]
["RTEDDY_2_SRXSR4",6,1.78]
["RTEDDY_2_SRXSR4",7,1.96]
["RTEDDY_2_SRXSR4",8,1.69]
["RTEDDY_2_SRXSR4",9,1.51]
["RTEDDY_2_SRXSR4",10,1.01]
["RTEDDY_2_SRXSR4",11,0.78]
["RTEDDY_2_SRXSR4",12,0.48]
["RTREE_2_WIND1",1,13.99]
["RTREE_2_WIND1",2,14.88]
["RTREE_2_WIND1",3,13.08]
["RTREE_2_WIND1",4,12.53]
["RTREE_2_WIND1",5,13.32]
["RTREE_2_WIND1",6,12.21]
["RTREE_2_WIND1",7,11.35]
["RTREE_2_WIND1",8,8.6199999999999992]
["RTREE_2_WIND1",9,8.91]
["RTREE_2_WIND1",10,8.26]
["RTREE_2_WIND1",11,11.14]
["RTREE_2_WIND1",12,13.49]
["RTREE_2_WIND2",1,3.5]
["RTREE_2_WIND2",2,3.72]
["RTREE_2_WIND2",3,3.27]
["RTREE_2_WIND2",4,3.13]
["RTREE_2_WIND2",5,3.33]
["RTREE_2_WIND2",6,3.05]
["RTREE_2_WIND2",7,2.84]
["RTREE_2_WIND2",8,2.16]
["RTREE_2_WIND2",9,2.23]
["RTREE_2_WIND2",10,2.0699999999999998]
["RTREE_2_WIND2",11,2.78]
["RTREE_2_WIND2",12,3.37]
["RTREE_2_WIND3",1,17.489999999999998]
["RTREE_2_WIND3",2,18.61]
["RTREE_2_WIND3",3,16.350000000000001]
["RTREE_2_WIND3",4,15.66]
["RTREE_2_WIND3",5,16.649999999999999]
["RTREE_2_WIND3",6,15.27]
["RTREE_2_WIND3",7,14.18]
["RTREE_2_WIND3",8,10.78]
["RTREE_2_WIND3",9,11.13]
["RTREE_2_WIND3",10,10.33]
["RTREE_2_WIND3",11,13.92]
["RTREE_2_WIND3",12,16.86]
["RUSCTY_2_UNITS",1,615.17999999999995]
["RUSCTY_2_UNITS",2,615.17999999999995]
["RUSCTY_2_UNITS",3,615.17999999999995]
["RUSCTY_2_UNITS",4,612.70000000000005]
["RUSCTY_2_UNITS",5,607.70000000000005]
["RUSCTY_2_UNITS",6,601]
["RUSCTY_2_UNITS",7,597.4]
["RUSCTY_2_UNITS",8,597.4]
["RUSCTY_2_UNITS",9,600.9]
["RUSCTY_2_UNITS",10,606.1]
["RUSCTY_2_UNITS",11,615.17999999999995]
["RUSCTY_2_UNITS",12,615.17999999999995]
["RVRVEW_1_UNITA1",1,47.6]
["RVRVEW_1_UNITA1",2,47.6]
["RVRVEW_1_UNITA1",3,47.6]
["RVRVEW_1_UNITA1",4,47.6]
["RVRVEW_1_UNITA1",5,47.6]
["RVRVEW_1_UNITA1",6,47.6]
["RVRVEW_1_UNITA1",7,47.6]
["RVRVEW_1_UNITA1",8,47.6]
["RVRVEW_1_UNITA1",9,47.6]
["RVRVEW_1_UNITA1",10,47.6]
["RVRVEW_1_UNITA1",11,47.6]
["RVRVEW_1_UNITA1",12,47.6]
["RVSIDE_2_RERCU3",1,49]
["RVSIDE_2_RERCU3",2,49]
["RVSIDE_2_RERCU3",3,49]
["RVSIDE_2_RERCU3",4,49]
["RVSIDE_2_RERCU3",5,49]
["RVSIDE_2_RERCU3",6,49]
["RVSIDE_2_RERCU3",7,49]
["RVSIDE_2_RERCU3",8,49]
["RVSIDE_2_RERCU3",9,49]
["RVSIDE_2_RERCU3",10,49]
["RVSIDE_2_RERCU3",11,49]
["RVSIDE_2_RERCU3",12,49]
["RVSIDE_2_RERCU4",1,49]
["RVSIDE_2_RERCU4",2,49]
["RVSIDE_2_RERCU4",3,49]
["RVSIDE_2_RERCU4",4,49]
["RVSIDE_2_RERCU4",5,49]
["RVSIDE_2_RERCU4",6,49]
["RVSIDE_2_RERCU4",7,49]
["RVSIDE_2_RERCU4",8,49]
["RVSIDE_2_RERCU4",9,49]
["RVSIDE_2_RERCU4",10,49]
["RVSIDE_2_RERCU4",11,49]
["RVSIDE_2_RERCU4",12,49]
["RVSIDE_6_RERCU1",1,48.35]
["RVSIDE_6_RERCU1",2,48.35]
["RVSIDE_6_RERCU1",3,48.35]
["RVSIDE_6_RERCU1",4,48.35]
["RVSIDE_6_RERCU1",5,48.35]
["RVSIDE_6_RERCU1",6,48.35]
["RVSIDE_6_RERCU1",7,48.35]
["RVSIDE_6_RERCU1",8,48.35]
["RVSIDE_6_RERCU1",9,48.35]
["RVSIDE_6_RERCU1",10,48.35]
["RVSIDE_6_RERCU1",11,48.35]
["RVSIDE_6_RERCU1",12,48.35]
["RVSIDE_6_RERCU2",1,48.5]
["RVSIDE_6_RERCU2",2,48.5]
["RVSIDE_6_RERCU2",3,48.5]
["RVSIDE_6_RERCU2",4,48.5]
["RVSIDE_6_RERCU2",5,48.5]
["RVSIDE_6_RERCU2",6,48.5]
["RVSIDE_6_RERCU2",7,48.5]
["RVSIDE_6_RERCU2",8,48.5]
["RVSIDE_6_RERCU2",9,48.5]
["RVSIDE_6_RERCU2",10,48.5]
["RVSIDE_6_RERCU2",11,48.5]
["RVSIDE_6_RERCU2",12,48.5]
["RVSIDE_6_SOLAR1",1,0.03]
["RVSIDE_6_SOLAR1",2,0.23]
["RVSIDE_6_SOLAR1",3,0.26]
["RVSIDE_6_SOLAR1",4,0.33]
["RVSIDE_6_SOLAR1",5,0.48]
["RVSIDE_6_SOLAR1",6,0.98]
["RVSIDE_6_SOLAR1",7,1.08]
["RVSIDE_6_SOLAR1",8,0.93]
["RVSIDE_6_SOLAR1",9,0.83]
["RVSIDE_6_SOLAR1",10,0.56000000000000005]
["RVSIDE_6_SOLAR1",11,0.43]
["RVSIDE_6_SOLAR1",12,0.26]
["RVSIDE_6_SPRING",1,36]
["RVSIDE_6_SPRING",2,36]
["RVSIDE_6_SPRING",3,36]
["RVSIDE_6_SPRING",4,36]
["RVSIDE_6_SPRING",5,36]
["RVSIDE_6_SPRING",6,36]
["RVSIDE_6_SPRING",7,36]
["RVSIDE_6_SPRING",8,36]
["RVSIDE_6_SPRING",9,36]
["RVSIDE_6_SPRING",10,36]
["RVSIDE_6_SPRING",11,36]
["RVSIDE_6_SPRING",12,36]
["S_RITA_6_SOLAR1",1,0]
["S_RITA_6_SOLAR1",2,0]
["S_RITA_6_SOLAR1",3,0]
["S_RITA_6_SOLAR1",4,0]
["S_RITA_6_SOLAR1",5,0]
["S_RITA_6_SOLAR1",6,0]
["S_RITA_6_SOLAR1",7,0]
["S_RITA_6_SOLAR1",8,0]
["S_RITA_6_SOLAR1",9,0]
["S_RITA_6_SOLAR1",10,0]
["S_RITA_6_SOLAR1",11,0]
["S_RITA_6_SOLAR1",12,0]
["SALIRV_2_UNIT",1,23.37]
["SALIRV_2_UNIT",2,23.13]
["SALIRV_2_UNIT",3,23.69]
["SALIRV_2_UNIT",4,22.06]
["SALIRV_2_UNIT",5,17.87]
["SALIRV_2_UNIT",6,19.170000000000002]
["SALIRV_2_UNIT",7,17.97]
["SALIRV_2_UNIT",8,19.899999999999999]
["SALIRV_2_UNIT",9,20.170000000000002]
["SALIRV_2_UNIT",10,19.8]
["SALIRV_2_UNIT",11,21.77]
["SALIRV_2_UNIT",12,23.52]
["SALTSP_7_UNITS",1,1.32]
["SALTSP_7_UNITS",2,4]
["SALTSP_7_UNITS",3,3.2]
["SALTSP_7_UNITS",4,0.4]
["SALTSP_7_UNITS",5,20.64]
["SALTSP_7_UNITS",6,16.91]
["SALTSP_7_UNITS",7,16.93]
["SALTSP_7_UNITS",8,23.46]
["SALTSP_7_UNITS",9,6.08]
["SALTSP_7_UNITS",10,4.76]
["SALTSP_7_UNITS",11,5.0999999999999996]
["SALTSP_7_UNITS",12,25.82]
["SAMPSN_6_KELCO1",1,1.03]
["SAMPSN_6_KELCO1",2,1.03]
["SAMPSN_6_KELCO1",3,2.04]
["SAMPSN_6_KELCO1",4,3.94]
["SAMPSN_6_KELCO1",5,3.56]
["SAMPSN_6_KELCO1",6,2.89]
["SAMPSN_6_KELCO1",7,2.54]
["SAMPSN_6_KELCO1",8,1.51]
["SAMPSN_6_KELCO1",9,2.27]
["SAMPSN_6_KELCO1",10,3.44]
["SAMPSN_6_KELCO1",11,2.5499999999999998]
["SAMPSN_6_KELCO1",12,1.19]
["SANBRN_2_EESSB2",1,0.52]
["SANBRN_2_EESSB2",2,3.9]
["SANBRN_2_EESSB2",3,4.55]
["SANBRN_2_EESSB2",4,5.72]
["SANBRN_2_EESSB2",5,8.32]
["SANBRN_2_EESSB2",6,17.03]
["SANBRN_2_EESSB2",7,18.72]
["SANBRN_2_EESSB2",8,16.12]
["SANBRN_2_EESSB2",9,14.43]
["SANBRN_2_EESSB2",10,9.6199999999999992]
["SANBRN_2_EESSB2",11,7.41]
["SANBRN_2_EESSB2",12,4.55]
["SANBRN_2_ES1BT3",1,22.08]
["SANBRN_2_ES1BT3",2,22.72]
["SANBRN_2_ES1BT3",3,22.9]
["SANBRN_2_ES1BT3",4,23.26]
["SANBRN_2_ES1BT3",5,23.88]
["SANBRN_2_ES1BT3",6,25.94]
["SANBRN_2_ES1BT3",7,26.33]
["SANBRN_2_ES1BT3",8,25.64]
["SANBRN_2_ES1BT3",9,25.07]
["SANBRN_2_ES1BT3",10,23.91]
["SANBRN_2_ES1BT3",11,23.23]
["SANBRN_2_ES1BT3",12,22.5]
["SANBRN_2_ES2SB3",1,18.059999999999999]
["SANBRN_2_ES2SB3",2,18.600000000000001]
["SANBRN_2_ES2SB3",3,18.75]
["SANBRN_2_ES2SB3",4,19.04]
["SANBRN_2_ES2SB3",5,19.559999999999999]
["SANBRN_2_ES2SB3",6,21.26]
["SANBRN_2_ES2SB3",7,21.58]
["SANBRN_2_ES2SB3",8,21.01]
["SANBRN_2_ES2SB3",9,20.55]
["SANBRN_2_ES2SB3",10,19.579999999999998]
["SANBRN_2_ES2SB3",11,19.02]
["SANBRN_2_ES2SB3",12,18.420000000000002]
["SANBRN_2_ESABT1",1,50]
["SANBRN_2_ESABT1",2,50]
["SANBRN_2_ESABT1",3,50]
["SANBRN_2_ESABT1",4,50]
["SANBRN_2_ESABT1",5,50]
["SANBRN_2_ESABT1",6,50]
["SANBRN_2_ESABT1",7,50]
["SANBRN_2_ESABT1",8,50]
["SANBRN_2_ESABT1",9,50]
["SANBRN_2_ESABT1",10,50]
["SANBRN_2_ESABT1",11,50]
["SANBRN_2_ESABT1",12,50]
["SANBRN_2_ESBBT1",1,100]
["SANBRN_2_ESBBT1",2,100]
["SANBRN_2_ESBBT1",3,100]
["SANBRN_2_ESBBT1",4,100]
["SANBRN_2_ESBBT1",5,100]
["SANBRN_2_ESBBT1",6,100]
["SANBRN_2_ESBBT1",7,100]
["SANBRN_2_ESBBT1",8,100]
["SANBRN_2_ESBBT1",9,100]
["SANBRN_2_ESBBT1",10,100]
["SANBRN_2_ESBBT1",11,100]
["SANBRN_2_ESBBT1",12,100]
["SANBRN_2_SS2SB4",1,0]
["SANBRN_2_SS2SB4",2,0]
["SANBRN_2_SS2SB4",3,0]
["SANBRN_2_SS2SB4",4,0]
["SANBRN_2_SS2SB4",5,0]
["SANBRN_2_SS2SB4",6,0]
["SANBRN_2_SS2SB4",7,0]
["SANBRN_2_SS2SB4",8,0]
["SANBRN_2_SS2SB4",9,0]
["SANBRN_2_SS2SB4",10,0]
["SANBRN_2_SS2SB4",11,0]
["SANBRN_2_SS2SB4",12,0]
["SANDLT_2_SUNITS",1,1.1000000000000001]
["SANDLT_2_SUNITS",2,8.25]
["SANDLT_2_SUNITS",3,9.6300000000000008]
["SANDLT_2_SUNITS",4,12.1]
["SANDLT_2_SUNITS",5,17.600000000000001]
["SANDLT_2_SUNITS",6,36.03]
["SANDLT_2_SUNITS",7,39.6]
["SANDLT_2_SUNITS",8,34.1]
["SANDLT_2_SUNITS",9,30.53]
["SANDLT_2_SUNITS",10,20.350000000000001]
["SANDLT_2_SUNITS",11,15.68]
["SANDLT_2_SUNITS",12,9.6300000000000008]
["SANITR_6_UNITS",1,1.27]
["SANITR_6_UNITS",2,1.2]
["SANITR_6_UNITS",3,1.4]
["SANITR_6_UNITS",4,1.34]
["SANITR_6_UNITS",5,1.1299999999999999]
["SANITR_6_UNITS",6,1.47]
["SANITR_6_UNITS",7,1.4]
["SANITR_6_UNITS",8,1.52]
["SANITR_6_UNITS",9,1.52]
["SANITR_6_UNITS",10,1.32]
["SANITR_6_UNITS",11,0.97]
["SANITR_6_UNITS",12,1.1000000000000001]
["SANLOB_1_LNDFIL",1,0]
["SANLOB_1_LNDFIL",2,0]
["SANLOB_1_LNDFIL",3,0]
["SANLOB_1_LNDFIL",4,0]
["SANLOB_1_LNDFIL",5,0]
["SANLOB_1_LNDFIL",6,0]
["SANLOB_1_LNDFIL",7,0]
["SANLOB_1_LNDFIL",8,0]
["SANLOB_1_LNDFIL",9,0]
["SANLOB_1_LNDFIL",10,0]
["SANLOB_1_LNDFIL",11,0]
["SANLOB_1_LNDFIL",12,0]
["SANLOB_1_OSFBM1",1,0]
["SANLOB_1_OSFBM1",2,0]
["SANLOB_1_OSFBM1",3,0]
["SANLOB_1_OSFBM1",4,0]
["SANLOB_1_OSFBM1",5,0]
["SANLOB_1_OSFBM1",6,0]
["SANLOB_1_OSFBM1",7,0]
["SANLOB_1_OSFBM1",8,0]
["SANLOB_1_OSFBM1",9,0]
["SANLOB_1_OSFBM1",10,0]
["SANLOB_1_OSFBM1",11,0]
["SANLOB_1_OSFBM1",12,0]
["SANTFG_7_UNITS",1,72]
["SANTFG_7_UNITS",2,72]
["SANTFG_7_UNITS",3,72]
["SANTFG_7_UNITS",4,72]
["SANTFG_7_UNITS",5,72]
["SANTFG_7_UNITS",6,72]
["SANTFG_7_UNITS",7,72]
["SANTFG_7_UNITS",8,72]
["SANTFG_7_UNITS",9,72]
["SANTFG_7_UNITS",10,72]
["SANTFG_7_UNITS",11,72]
["SANTFG_7_UNITS",12,72]
["SANTGO_2_LNDFL1",1,19.32]
["SANTGO_2_LNDFL1",2,19.59]
["SANTGO_2_LNDFL1",3,18.690000000000001]
["SANTGO_2_LNDFL1",4,19.03]
["SANTGO_2_LNDFL1",5,18.57]
["SANTGO_2_LNDFL1",6,19.53]
["SANTGO_2_LNDFL1",7,18.739999999999998]
["SANTGO_2_LNDFL1",8,18.55]
["SANTGO_2_LNDFL1",9,18.399999999999999]
["SANTGO_2_LNDFL1",10,17.75]
["SANTGO_2_LNDFL1",11,18.75]
["SANTGO_2_LNDFL1",12,19.600000000000001]
["SANTGO_2_MABBT1",1,2]
["SANTGO_2_MABBT1",2,2]
["SANTGO_2_MABBT1",3,2]
["SANTGO_2_MABBT1",4,2]
["SANTGO_2_MABBT1",5,2]
["SANTGO_2_MABBT1",6,2]
["SANTGO_2_MABBT1",7,2]
["SANTGO_2_MABBT1",8,2]
["SANTGO_2_MABBT1",9,2]
["SANTGO_2_MABBT1",10,2]
["SANTGO_2_MABBT1",11,2]
["SANTGO_2_MABBT1",12,2]
["SANWD_1_QF",1,5.48]
["SANWD_1_QF",2,5.83]
["SANWD_1_QF",3,5.12]
["SANWD_1_QF",4,4.9000000000000004]
["SANWD_1_QF",5,5.22]
["SANWD_1_QF",6,4.78]
["SANWD_1_QF",7,4.4400000000000004]
["SANWD_1_QF",8,3.37]
["SANWD_1_QF",9,3.49]
["SANWD_1_QF",10,3.23]
["SANWD_1_QF",11,4.3600000000000003]
["SANWD_1_QF",12,5.28]
["SAUGUS_6_CREST",1,0]
["SAUGUS_6_CREST",2,0]
["SAUGUS_6_CREST",3,0]
["SAUGUS_6_CREST",4,0]
["SAUGUS_6_CREST",5,0]
["SAUGUS_6_CREST",6,0]
["SAUGUS_6_CREST",7,0]
["SAUGUS_6_CREST",8,0]
["SAUGUS_6_CREST",9,0]
["SAUGUS_6_CREST",10,0]
["SAUGUS_6_CREST",11,0]
["SAUGUS_6_CREST",12,0]
["SAUGUS_6_MWDFTH",1,4]
["SAUGUS_6_MWDFTH",2,3]
["SAUGUS_6_MWDFTH",3,4.4000000000000004]
["SAUGUS_6_MWDFTH",4,5.2]
["SAUGUS_6_MWDFTH",5,6]
["SAUGUS_6_MWDFTH",6,6.6]
["SAUGUS_6_MWDFTH",7,7]
["SAUGUS_6_MWDFTH",8,7]
["SAUGUS_6_MWDFTH",9,7]
["SAUGUS_6_MWDFTH",10,6.8]
["SAUGUS_6_MWDFTH",11,6.8]
["SAUGUS_6_MWDFTH",12,7]
["SAUGUS_6_QF",1,0.06]
["SAUGUS_6_QF",2,0.06]
["SAUGUS_6_QF",3,0.11]
["SAUGUS_6_QF",4,0.37]
["SAUGUS_6_QF",5,0.18]
["SAUGUS_6_QF",6,0.23]
["SAUGUS_6_QF",7,0.38]
["SAUGUS_6_QF",8,0.55000000000000004]
["SAUGUS_6_QF",9,1]
["SAUGUS_6_QF",10,1]
["SAUGUS_6_QF",11,1]
["SAUGUS_6_QF",12,0.97]
["SAUGUS_7_CHIQCN",1,6.23]
["SAUGUS_7_CHIQCN",2,6]
["SAUGUS_7_CHIQCN",3,6.05]
["SAUGUS_7_CHIQCN",4,5.95]
["SAUGUS_7_CHIQCN",5,5.85]
["SAUGUS_7_CHIQCN",6,5.57]
["SAUGUS_7_CHIQCN",7,5.34]
["SAUGUS_7_CHIQCN",8,5.35]
["SAUGUS_7_CHIQCN",9,5.14]
["SAUGUS_7_CHIQCN",10,5.38]
["SAUGUS_7_CHIQCN",11,5.5]
["SAUGUS_7_CHIQCN",12,5.5]
["SBERDO_2_PSP3",1,555]
["SBERDO_2_PSP3",2,555]
["SBERDO_2_PSP3",3,555]
["SBERDO_2_PSP3",4,555]
["SBERDO_2_PSP3",5,555]
["SBERDO_2_PSP3",6,555]
["SBERDO_2_PSP3",7,555]
["SBERDO_2_PSP3",8,555]
["SBERDO_2_PSP3",9,555]
["SBERDO_2_PSP3",10,555]
["SBERDO_2_PSP3",11,555]
["SBERDO_2_PSP3",12,555]
["SBERDO_2_PSP4",1,555]
["SBERDO_2_PSP4",2,555]
["SBERDO_2_PSP4",3,555]
["SBERDO_2_PSP4",4,555]
["SBERDO_2_PSP4",5,555]
["SBERDO_2_PSP4",6,555]
["SBERDO_2_PSP4",7,555]
["SBERDO_2_PSP4",8,555]
["SBERDO_2_PSP4",9,555]
["SBERDO_2_PSP4",10,555]
["SBERDO_2_PSP4",11,555]
["SBERDO_2_PSP4",12,555]
["SBERDO_2_REDLND",1,0.01]
["SBERDO_2_REDLND",2,0.06]
["SBERDO_2_REDLND",3,7.0000000000000007E-2]
["SBERDO_2_REDLND",4,0.09]
["SBERDO_2_REDLND",5,0.13]
["SBERDO_2_REDLND",6,0.26]
["SBERDO_2_REDLND",7,0.28999999999999998]
["SBERDO_2_REDLND",8,0.25]
["SBERDO_2_REDLND",9,0.22]
["SBERDO_2_REDLND",10,0.15]
["SBERDO_2_REDLND",11,0.11]
["SBERDO_2_REDLND",12,7.0000000000000007E-2]
["SBERDO_2_RTS005",1,0.01]
["SBERDO_2_RTS005",2,0.08]
["SBERDO_2_RTS005",3,0.09]
["SBERDO_2_RTS005",4,0.11]
["SBERDO_2_RTS005",5,0.16]
["SBERDO_2_RTS005",6,0.33]
["SBERDO_2_RTS005",7,0.36]
["SBERDO_2_RTS005",8,0.31]
["SBERDO_2_RTS005",9,0.28000000000000003]
["SBERDO_2_RTS005",10,0.19]
["SBERDO_2_RTS005",11,0.14000000000000001]
["SBERDO_2_RTS005",12,0.09]
["SBERDO_2_RTS007",1,0.01]
["SBERDO_2_RTS007",2,0.08]
["SBERDO_2_RTS007",3,0.09]
["SBERDO_2_RTS007",4,0.11]
["SBERDO_2_RTS007",5,0.16]
["SBERDO_2_RTS007",6,0.33]
["SBERDO_2_RTS007",7,0.36]
["SBERDO_2_RTS007",8,0.31]
["SBERDO_2_RTS007",9,0.28000000000000003]
["SBERDO_2_RTS007",10,0.19]
["SBERDO_2_RTS007",11,0.14000000000000001]
["SBERDO_2_RTS007",12,0.09]
["SBERDO_2_RTS011",1,0.01]
["SBERDO_2_RTS011",2,0.11]
["SBERDO_2_RTS011",3,0.12]
["SBERDO_2_RTS011",4,0.15]
["SBERDO_2_RTS011",5,0.22]
["SBERDO_2_RTS011",6,0.46]
["SBERDO_2_RTS011",7,0.5]
["SBERDO_2_RTS011",8,0.43]
["SBERDO_2_RTS011",9,0.39]
["SBERDO_2_RTS011",10,0.26]
["SBERDO_2_RTS011",11,0.2]
["SBERDO_2_RTS011",12,0.12]
["SBERDO_2_RTS013",1,0.01]
["SBERDO_2_RTS013",2,0.11]
["SBERDO_2_RTS013",3,0.12]
["SBERDO_2_RTS013",4,0.15]
["SBERDO_2_RTS013",5,0.22]
["SBERDO_2_RTS013",6,0.46]
["SBERDO_2_RTS013",7,0.5]
["SBERDO_2_RTS013",8,0.43]
["SBERDO_2_RTS013",9,0.39]
["SBERDO_2_RTS013",10,0.26]
["SBERDO_2_RTS013",11,0.2]
["SBERDO_2_RTS013",12,0.12]
["SBERDO_2_RTS016",1,0.01]
["SBERDO_2_RTS016",2,0.05]
["SBERDO_2_RTS016",3,0.05]
["SBERDO_2_RTS016",4,7.0000000000000007E-2]
["SBERDO_2_RTS016",5,0.1]
["SBERDO_2_RTS016",6,0.2]
["SBERDO_2_RTS016",7,0.22]
["SBERDO_2_RTS016",8,0.19]
["SBERDO_2_RTS016",9,0.17]
["SBERDO_2_RTS016",10,0.11]
["SBERDO_2_RTS016",11,0.09]
["SBERDO_2_RTS016",12,0.05]
["SBERDO_2_RTS048",1,0]
["SBERDO_2_RTS048",2,0]
["SBERDO_2_RTS048",3,0]
["SBERDO_2_RTS048",4,0]
["SBERDO_2_RTS048",5,0]
["SBERDO_2_RTS048",6,0]
["SBERDO_2_RTS048",7,0]
["SBERDO_2_RTS048",8,0]
["SBERDO_2_RTS048",9,0]
["SBERDO_2_RTS048",10,0]
["SBERDO_2_RTS048",11,0]
["SBERDO_2_RTS048",12,0]
["SBERDO_2_SNTANA",1,0.76]
["SBERDO_2_SNTANA",2,0.48]
["SBERDO_2_SNTANA",3,0.22]
["SBERDO_2_SNTANA",4,0]
["SBERDO_2_SNTANA",5,0.1]
["SBERDO_2_SNTANA",6,0]
["SBERDO_2_SNTANA",7,0]
["SBERDO_2_SNTANA",8,0.27]
["SBERDO_2_SNTANA",9,0.23]
["SBERDO_2_SNTANA",10,0.3]
["SBERDO_2_SNTANA",11,0.33]
["SBERDO_2_SNTANA",12,0.44]
["SBERDO_6_MILLCK",1,1.33]
["SBERDO_6_MILLCK",2,1.06]
["SBERDO_6_MILLCK",3,1.06]
["SBERDO_6_MILLCK",4,1.08]
["SBERDO_6_MILLCK",5,0.66]
["SBERDO_6_MILLCK",6,0.82]
["SBERDO_6_MILLCK",7,1.35]
["SBERDO_6_MILLCK",8,1.37]
["SBERDO_6_MILLCK",9,1.22]
["SBERDO_6_MILLCK",10,1.1100000000000001]
["SBERDO_6_MILLCK",11,1.34]
["SBERDO_6_MILLCK",12,1.34]
["SCHLTE_1_PL1X3",1,336.04]
["SCHLTE_1_PL1X3",2,336.04]
["SCHLTE_1_PL1X3",3,336.04]
["SCHLTE_1_PL1X3",4,336.04]
["SCHLTE_1_PL1X3",5,336.04]
["SCHLTE_1_PL1X3",6,336.04]
["SCHLTE_1_PL1X3",7,336.04]
["SCHLTE_1_PL1X3",8,336.04]
["SCHLTE_1_PL1X3",9,336.04]
["SCHLTE_1_PL1X3",10,336.04]
["SCHLTE_1_PL1X3",11,336.04]
["SCHLTE_1_PL1X3",12,336.04]
["SCHNDR_1_FIVPTS",1,0.06]
["SCHNDR_1_FIVPTS",2,0.45]
["SCHNDR_1_FIVPTS",3,0.53]
["SCHNDR_1_FIVPTS",4,0.66]
["SCHNDR_1_FIVPTS",5,0.96]
["SCHNDR_1_FIVPTS",6,1.97]
["SCHNDR_1_FIVPTS",7,2.16]
["SCHNDR_1_FIVPTS",8,1.86]
["SCHNDR_1_FIVPTS",9,1.67]
["SCHNDR_1_FIVPTS",10,1.1100000000000001]
["SCHNDR_1_FIVPTS",11,0.86]
["SCHNDR_1_FIVPTS",12,0.53]
["SCHNDR_1_OS2BM2",1,0]
["SCHNDR_1_OS2BM2",2,0]
["SCHNDR_1_OS2BM2",3,0]
["SCHNDR_1_OS2BM2",4,0]
["SCHNDR_1_OS2BM2",5,0]
["SCHNDR_1_OS2BM2",6,0]
["SCHNDR_1_OS2BM2",7,0]
["SCHNDR_1_OS2BM2",8,0]
["SCHNDR_1_OS2BM2",9,0]
["SCHNDR_1_OS2BM2",10,0]
["SCHNDR_1_OS2BM2",11,0]
["SCHNDR_1_OS2BM2",12,0]
["SCHNDR_1_WSTSDE",1,0.06]
["SCHNDR_1_WSTSDE",2,0.45]
["SCHNDR_1_WSTSDE",3,0.53]
["SCHNDR_1_WSTSDE",4,0.66]
["SCHNDR_1_WSTSDE",5,0.96]
["SCHNDR_1_WSTSDE",6,1.97]
["SCHNDR_1_WSTSDE",7,2.16]
["SCHNDR_1_WSTSDE",8,1.86]
["SCHNDR_1_WSTSDE",9,1.67]
["SCHNDR_1_WSTSDE",10,1.1100000000000001]
["SCHNDR_1_WSTSDE",11,0.86]
["SCHNDR_1_WSTSDE",12,0.53]
["SEARLS_7_ARGUS",1,4.75]
["SEARLS_7_ARGUS",2,5.75]
["SEARLS_7_ARGUS",3,4.49]
["SEARLS_7_ARGUS",4,4.47]
["SEARLS_7_ARGUS",5,3.15]
["SEARLS_7_ARGUS",6,2.06]
["SEARLS_7_ARGUS",7,1.1399999999999999]
["SEARLS_7_ARGUS",8,1.48]
["SEARLS_7_ARGUS",9,3.39]
["SEARLS_7_ARGUS",10,4.18]
["SEARLS_7_ARGUS",11,3.73]
["SEARLS_7_ARGUS",12,4.6100000000000003]
["SEGS_1_SR2SL2",1,0.08]
["SEGS_1_SR2SL2",2,0.6]
["SEGS_1_SR2SL2",3,0.7]
["SEGS_1_SR2SL2",4,0.88]
["SEGS_1_SR2SL2",5,1.28]
["SEGS_1_SR2SL2",6,2.62]
["SEGS_1_SR2SL2",7,2.88]
["SEGS_1_SR2SL2",8,2.48]
["SEGS_1_SR2SL2",9,2.2200000000000002]
["SEGS_1_SR2SL2",10,1.48]
["SEGS_1_SR2SL2",11,1.1399999999999999]
["SEGS_1_SR2SL2",12,0.7]
["SENTNL_2_CTG1",1,107.68]
["SENTNL_2_CTG1",2,107.68]
["SENTNL_2_CTG1",3,107.68]
["SENTNL_2_CTG1",4,107.68]
["SENTNL_2_CTG1",5,107.68]
["SENTNL_2_CTG1",6,107.68]
["SENTNL_2_CTG1",7,107.68]
["SENTNL_2_CTG1",8,107.68]
["SENTNL_2_CTG1",9,107.68]
["SENTNL_2_CTG1",10,107.68]
["SENTNL_2_CTG1",11,107.68]
["SENTNL_2_CTG1",12,107.68]
["SENTNL_2_CTG2",1,103.98]
["SENTNL_2_CTG2",2,103.98]
["SENTNL_2_CTG2",3,103.98]
["SENTNL_2_CTG2",4,103.98]
["SENTNL_2_CTG2",5,103.98]
["SENTNL_2_CTG2",6,103.98]
["SENTNL_2_CTG2",7,103.98]
["SENTNL_2_CTG2",8,103.98]
["SENTNL_2_CTG2",9,103.98]
["SENTNL_2_CTG2",10,103.98]
["SENTNL_2_CTG2",11,103.98]
["SENTNL_2_CTG2",12,103.98]
["SENTNL_2_CTG3",1,105.69]
["SENTNL_2_CTG3",2,105.69]
["SENTNL_2_CTG3",3,105.69]
["SENTNL_2_CTG3",4,105.69]
["SENTNL_2_CTG3",5,105.69]
["SENTNL_2_CTG3",6,105.69]
["SENTNL_2_CTG3",7,105.69]
["SENTNL_2_CTG3",8,105.69]
["SENTNL_2_CTG3",9,105.69]
["SENTNL_2_CTG3",10,105.69]
["SENTNL_2_CTG3",11,105.69]
["SENTNL_2_CTG3",12,105.69]
["SENTNL_2_CTG4",1,106.55]
["SENTNL_2_CTG4",2,106.55]
["SENTNL_2_CTG4",3,106.55]
["SENTNL_2_CTG4",4,106.55]
["SENTNL_2_CTG4",5,106.55]
["SENTNL_2_CTG4",6,106.55]
["SENTNL_2_CTG4",7,106.55]
["SENTNL_2_CTG4",8,106.55]
["SENTNL_2_CTG4",9,106.55]
["SENTNL_2_CTG4",10,106.55]
["SENTNL_2_CTG4",11,106.55]
["SENTNL_2_CTG4",12,106.55]
["SENTNL_2_CTG5",1,107.52]
["SENTNL_2_CTG5",2,107.52]
["SENTNL_2_CTG5",3,107.52]
["SENTNL_2_CTG5",4,107.52]
["SENTNL_2_CTG5",5,107.52]
["SENTNL_2_CTG5",6,107.52]
["SENTNL_2_CTG5",7,107.52]
["SENTNL_2_CTG5",8,107.52]
["SENTNL_2_CTG5",9,107.52]
["SENTNL_2_CTG5",10,107.52]
["SENTNL_2_CTG5",11,107.52]
["SENTNL_2_CTG5",12,107.52]
["SENTNL_2_CTG6",1,105]
["SENTNL_2_CTG6",2,105]
["SENTNL_2_CTG6",3,105]
["SENTNL_2_CTG6",4,105]
["SENTNL_2_CTG6",5,105]
["SENTNL_2_CTG6",6,105]
["SENTNL_2_CTG6",7,105]
["SENTNL_2_CTG6",8,105]
["SENTNL_2_CTG6",9,105]
["SENTNL_2_CTG6",10,105]
["SENTNL_2_CTG6",11,105]
["SENTNL_2_CTG6",12,105]
["SENTNL_2_CTG7",1,106.73]
["SENTNL_2_CTG7",2,106.73]
["SENTNL_2_CTG7",3,106.73]
["SENTNL_2_CTG7",4,106.73]
["SENTNL_2_CTG7",5,106.73]
["SENTNL_2_CTG7",6,106.73]
["SENTNL_2_CTG7",7,106.73]
["SENTNL_2_CTG7",8,106.73]
["SENTNL_2_CTG7",9,106.73]
["SENTNL_2_CTG7",10,106.73]
["SENTNL_2_CTG7",11,106.73]
["SENTNL_2_CTG7",12,106.73]
["SENTNL_2_CTG8",1,106.85]
["SENTNL_2_CTG8",2,106.85]
["SENTNL_2_CTG8",3,106.85]
["SENTNL_2_CTG8",4,106.85]
["SENTNL_2_CTG8",5,106.85]
["SENTNL_2_CTG8",6,106.85]
["SENTNL_2_CTG8",7,106.85]
["SENTNL_2_CTG8",8,106.85]
["SENTNL_2_CTG8",9,106.85]
["SENTNL_2_CTG8",10,106.85]
["SENTNL_2_CTG8",11,106.85]
["SENTNL_2_CTG8",12,106.85]
["SGREGY_6_SANGER",1,48.08]
["SGREGY_6_SANGER",2,48.08]
["SGREGY_6_SANGER",3,48.08]
["SGREGY_6_SANGER",4,48.08]
["SGREGY_6_SANGER",5,48.08]
["SGREGY_6_SANGER",6,48.08]
["SGREGY_6_SANGER",7,48.08]
["SGREGY_6_SANGER",8,48.08]
["SGREGY_6_SANGER",9,48.08]
["SGREGY_6_SANGER",10,48.08]
["SGREGY_6_SANGER",11,48.08]
["SGREGY_6_SANGER",12,48.08]
["SHELRF_1_UNITS",1,2.99]
["SHELRF_1_UNITS",2,1.98]
["SHELRF_1_UNITS",3,0.74]
["SHELRF_1_UNITS",4,3.08]
["SHELRF_1_UNITS",5,3.35]
["SHELRF_1_UNITS",6,3.47]
["SHELRF_1_UNITS",7,4.71]
["SHELRF_1_UNITS",8,5.67]
["SHELRF_1_UNITS",9,5.4]
["SHELRF_1_UNITS",10,3.35]
["SHELRF_1_UNITS",11,6.65]
["SHELRF_1_UNITS",12,3.18]
["SHUTLE_6_CREST",1,0]
["SHUTLE_6_CREST",2,0]
["SHUTLE_6_CREST",3,0]
["SHUTLE_6_CREST",4,0]
["SHUTLE_6_CREST",5,0]
["SHUTLE_6_CREST",6,0]
["SHUTLE_6_CREST",7,0]
["SHUTLE_6_CREST",8,0]
["SHUTLE_6_CREST",9,0]
["SHUTLE_6_CREST",10,0]
["SHUTLE_6_CREST",11,0]
["SHUTLE_6_CREST",12,0]
["SIERRA_1_UNITS",1,52.43]
["SIERRA_1_UNITS",2,52.43]
["SIERRA_1_UNITS",3,52.43]
["SIERRA_1_UNITS",4,52.43]
["SIERRA_1_UNITS",5,52.43]
["SIERRA_1_UNITS",6,52.43]
["SIERRA_1_UNITS",7,52.43]
["SIERRA_1_UNITS",8,52.43]
["SIERRA_1_UNITS",9,52.43]
["SIERRA_1_UNITS",10,52.43]
["SIERRA_1_UNITS",11,52.43]
["SIERRA_1_UNITS",12,52.43]
["SISQUC_1_SMARIA",1,1.01]
["SISQUC_1_SMARIA",2,1.04]
["SISQUC_1_SMARIA",3,1.02]
["SISQUC_1_SMARIA",4,1.03]
["SISQUC_1_SMARIA",5,1.03]
["SISQUC_1_SMARIA",6,1.07]
["SISQUC_1_SMARIA",7,1.06]
["SISQUC_1_SMARIA",8,1.07]
["SISQUC_1_SMARIA",9,1.04]
["SISQUC_1_SMARIA",10,1.02]
["SISQUC_1_SMARIA",11,1]
["SISQUC_1_SMARIA",12,0.95]
["SKERN_6_SOLAR1",1,0.08]
["SKERN_6_SOLAR1",2,0.6]
["SKERN_6_SOLAR1",3,0.7]
["SKERN_6_SOLAR1",4,0.88]
["SKERN_6_SOLAR1",5,1.28]
["SKERN_6_SOLAR1",6,2.62]
["SKERN_6_SOLAR1",7,2.88]
["SKERN_6_SOLAR1",8,2.48]
["SKERN_6_SOLAR1",9,2.2200000000000002]
["SKERN_6_SOLAR1",10,1.48]
["SKERN_6_SOLAR1",11,1.1399999999999999]
["SKERN_6_SOLAR1",12,0.7]
["SKERN_6_SOLAR2",1,0.04]
["SKERN_6_SOLAR2",2,0.3]
["SKERN_6_SOLAR2",3,0.35]
["SKERN_6_SOLAR2",4,0.44]
["SKERN_6_SOLAR2",5,0.64]
["SKERN_6_SOLAR2",6,1.31]
["SKERN_6_SOLAR2",7,1.44]
["SKERN_6_SOLAR2",8,1.24]
["SKERN_6_SOLAR2",9,1.1100000000000001]
["SKERN_6_SOLAR2",10,0.74]
["SKERN_6_SOLAR2",11,0.56999999999999995]
["SKERN_6_SOLAR2",12,0.35]
["SLATE_2_SLASR1",1,0.2]
["SLATE_2_SLASR1",2,1.52]
["SLATE_2_SLASR1",3,1.77]
["SLATE_2_SLASR1",4,2.2200000000000002]
["SLATE_2_SLASR1",5,3.23]
["SLATE_2_SLASR1",6,6.62]
["SLATE_2_SLASR1",7,7.27]
["SLATE_2_SLASR1",8,6.26]
["SLATE_2_SLASR1",9,5.61]
["SLATE_2_SLASR1",10,3.74]
["SLATE_2_SLASR1",11,2.88]
["SLATE_2_SLASR1",12,1.77]
["SLATE_2_SLASR2",1,46.69]
["SLATE_2_SLASR2",2,48.27]
["SLATE_2_SLASR2",3,48.7]
["SLATE_2_SLASR2",4,49.53]
["SLATE_2_SLASR2",5,51.01]
["SLATE_2_SLASR2",6,55.94]
["SLATE_2_SLASR2",7,56.86]
["SLATE_2_SLASR2",8,55.24]
["SLATE_2_SLASR2",9,53.94]
["SLATE_2_SLASR2",10,51.16]
["SLATE_2_SLASR2",11,49.58]
["SLATE_2_SLASR2",12,47.86]
["SLATE_2_SLASR3",1,33.89]
["SLATE_2_SLASR3",2,35.04]
["SLATE_2_SLASR3",3,35.340000000000003]
["SLATE_2_SLASR3",4,35.950000000000003]
["SLATE_2_SLASR3",5,37.03]
["SLATE_2_SLASR3",6,40.6]
["SLATE_2_SLASR3",7,41.27]
["SLATE_2_SLASR3",8,40.1]
["SLATE_2_SLASR3",9,39.15]
["SLATE_2_SLASR3",10,37.130000000000003]
["SLATE_2_SLASR3",11,35.99]
["SLATE_2_SLASR3",12,34.729999999999997]
["SLATE_2_SLASR4",1,50.06]
["SLATE_2_SLASR4",2,50.8]
["SLATE_2_SLASR4",3,51.07]
["SLATE_2_SLASR4",4,51.63]
["SLATE_2_SLASR4",5,52.49]
["SLATE_2_SLASR4",6,55.31]
["SLATE_2_SLASR4",7,55.82]
["SLATE_2_SLASR4",8,54.81]
["SLATE_2_SLASR4",9,53.89]
["SLATE_2_SLASR4",10,52.27]
["SLATE_2_SLASR4",11,51.21]
["SLATE_2_SLASR4",12,50.16]
["SLATE_2_SLASR5",1,10.07]
["SLATE_2_SLASR5",2,10.56]
["SLATE_2_SLASR5",3,10.68]
["SLATE_2_SLASR5",4,10.91]
["SLATE_2_SLASR5",5,11.35]
["SLATE_2_SLASR5",6,12.82]
["SLATE_2_SLASR5",7,13.09]
["SLATE_2_SLASR5",8,12.62]
["SLATE_2_SLASR5",9,12.26]
["SLATE_2_SLASR5",10,11.45]
["SLATE_2_SLASR5",11,11]
["SLATE_2_SLASR5",12,10.5]
["SLRMS3_2_SRMSR1",1,1]
["SLRMS3_2_SRMSR1",2,7.5]
["SLRMS3_2_SRMSR1",3,8.75]
["SLRMS3_2_SRMSR1",4,11]
["SLRMS3_2_SRMSR1",5,16]
["SLRMS3_2_SRMSR1",6,32.75]
["SLRMS3_2_SRMSR1",7,36]
["SLRMS3_2_SRMSR1",8,31]
["SLRMS3_2_SRMSR1",9,27.75]
["SLRMS3_2_SRMSR1",10,18.5]
["SLRMS3_2_SRMSR1",11,14.25]
["SLRMS3_2_SRMSR1",12,8.75]
["SLST13_2_SOLAR1",1,0.43]
["SLST13_2_SOLAR1",2,3.23]
["SLST13_2_SOLAR1",3,3.77]
["SLST13_2_SOLAR1",4,4.7300000000000004]
["SLST13_2_SOLAR1",5,6.89]
["SLST13_2_SOLAR1",6,14.1]
["SLST13_2_SOLAR1",7,15.49]
["SLST13_2_SOLAR1",8,13.34]
["SLST13_2_SOLAR1",9,11.94]
["SLST13_2_SOLAR1",10,7.96]
["SLST13_2_SOLAR1",11,6.13]
["SLST13_2_SOLAR1",12,3.77]
["SLSTR1_2_SOLAR1",1,1.24]
["SLSTR1_2_SOLAR1",2,9.3000000000000007]
["SLSTR1_2_SOLAR1",3,10.85]
["SLSTR1_2_SOLAR1",4,13.64]
["SLSTR1_2_SOLAR1",5,19.84]
["SLSTR1_2_SOLAR1",6,40.61]
["SLSTR1_2_SOLAR1",7,44.64]
["SLSTR1_2_SOLAR1",8,38.44]
["SLSTR1_2_SOLAR1",9,34.409999999999997]
["SLSTR1_2_SOLAR1",10,22.94]
["SLSTR1_2_SOLAR1",11,17.670000000000002]
["SLSTR1_2_SOLAR1",12,10.85]
["SLSTR2_2_SOLAR2",1,1.1000000000000001]
["SLSTR2_2_SOLAR2",2,8.2799999999999994]
["SLSTR2_2_SOLAR2",3,9.66]
["SLSTR2_2_SOLAR2",4,12.14]
["SLSTR2_2_SOLAR2",5,17.66]
["SLSTR2_2_SOLAR2",6,36.159999999999997]
["SLSTR2_2_SOLAR2",7,39.74]
["SLSTR2_2_SOLAR2",8,34.22]
["SLSTR2_2_SOLAR2",9,30.64]
["SLSTR2_2_SOLAR2",10,20.420000000000002]
["SLSTR2_2_SOLAR2",11,15.73]
["SLSTR2_2_SOLAR2",12,9.66]
["SLUISP_2_UNITS",1,0]
["SLUISP_2_UNITS",2,0]
["SLUISP_2_UNITS",3,0]
["SLUISP_2_UNITS",4,61.99]
["SLUISP_2_UNITS",5,68.099999999999994]
["SLUISP_2_UNITS",6,51.62]
["SLUISP_2_UNITS",7,0]
["SLUISP_2_UNITS",8,0]
["SLUISP_2_UNITS",9,0]
["SLUISP_2_UNITS",10,44.07]
["SLUISP_2_UNITS",11,0]
["SLUISP_2_UNITS",12,0]
["SLYCRK_1_UNIT 1",1,13]
["SLYCRK_1_UNIT 1",2,13]
["SLYCRK_1_UNIT 1",3,13]
["SLYCRK_1_UNIT 1",4,13]
["SLYCRK_1_UNIT 1",5,13]
["SLYCRK_1_UNIT 1",6,13]
["SLYCRK_1_UNIT 1",7,13]
["SLYCRK_1_UNIT 1",8,13]
["SLYCRK_1_UNIT 1",9,13]
["SLYCRK_1_UNIT 1",10,13]
["SLYCRK_1_UNIT 1",11,13]
["SLYCRK_1_UNIT 1",12,13]
["SMPRIP_1_SMPSON",1,46.05]
["SMPRIP_1_SMPSON",2,46.05]
["SMPRIP_1_SMPSON",3,46.05]
["SMPRIP_1_SMPSON",4,46.05]
["SMPRIP_1_SMPSON",5,46.05]
["SMPRIP_1_SMPSON",6,46.05]
["SMPRIP_1_SMPSON",7,46.05]
["SMPRIP_1_SMPSON",8,46.05]
["SMPRIP_1_SMPSON",9,46.05]
["SMPRIP_1_SMPSON",10,46.05]
["SMPRIP_1_SMPSON",11,46.05]
["SMPRIP_1_SMPSON",12,46.05]
["SMRCOS_6_LNDFIL",1,1.5]
["SMRCOS_6_LNDFIL",2,1.5]
["SMRCOS_6_LNDFIL",3,1.5]
["SMRCOS_6_LNDFIL",4,1.5]
["SMRCOS_6_LNDFIL",5,1.49]
["SMRCOS_6_LNDFIL",6,1.48]
["SMRCOS_6_LNDFIL",7,1.5]
["SMRCOS_6_LNDFIL",8,1.5]
["SMRCOS_6_LNDFIL",9,1.5]
["SMRCOS_6_LNDFIL",10,1.5]
["SMRCOS_6_LNDFIL",11,1.5]
["SMRCOS_6_LNDFIL",12,1.5]
["SMUDGO_7_UNIT 1",1,47]
["SMUDGO_7_UNIT 1",2,47]
["SMUDGO_7_UNIT 1",3,47]
["SMUDGO_7_UNIT 1",4,47]
["SMUDGO_7_UNIT 1",5,47]
["SMUDGO_7_UNIT 1",6,47]
["SMUDGO_7_UNIT 1",7,47]
["SMUDGO_7_UNIT 1",8,47]
["SMUDGO_7_UNIT 1",9,47]
["SMUDGO_7_UNIT 1",10,47]
["SMUDGO_7_UNIT 1",11,47]
["SMUDGO_7_UNIT 1",12,47]
["SMYRNA_1_DL1SR1",1,0]
["SMYRNA_1_DL1SR1",2,0.03]
["SMYRNA_1_DL1SR1",3,0.04]
["SMYRNA_1_DL1SR1",4,0.04]
["SMYRNA_1_DL1SR1",5,0.06]
["SMYRNA_1_DL1SR1",6,0.13]
["SMYRNA_1_DL1SR1",7,0.14000000000000001]
["SMYRNA_1_DL1SR1",8,0.12]
["SMYRNA_1_DL1SR1",9,0.11]
["SMYRNA_1_DL1SR1",10,7.0000000000000007E-2]
["SMYRNA_1_DL1SR1",11,0.06]
["SMYRNA_1_DL1SR1",12,0.04]
["SNCLRA_2_HOWLNG",1,7.04]
["SNCLRA_2_HOWLNG",2,7.24]
["SNCLRA_2_HOWLNG",3,6.32]
["SNCLRA_2_HOWLNG",4,5.33]
["SNCLRA_2_HOWLNG",5,7.09]
["SNCLRA_2_HOWLNG",6,7.17]
["SNCLRA_2_HOWLNG",7,5.49]
["SNCLRA_2_HOWLNG",8,4.08]
["SNCLRA_2_HOWLNG",9,5.15]
["SNCLRA_2_HOWLNG",10,6.71]
["SNCLRA_2_HOWLNG",11,6.37]
["SNCLRA_2_HOWLNG",12,4]
["SNCLRA_2_SILBT1",1,11]
["SNCLRA_2_SILBT1",2,11]
["SNCLRA_2_SILBT1",3,11]
["SNCLRA_2_SILBT1",4,11]
["SNCLRA_2_SILBT1",5,11]
["SNCLRA_2_SILBT1",6,11]
["SNCLRA_2_SILBT1",7,11]
["SNCLRA_2_SILBT1",8,11]
["SNCLRA_2_SILBT1",9,11]
["SNCLRA_2_SILBT1",10,11]
["SNCLRA_2_SILBT1",11,11]
["SNCLRA_2_SILBT1",12,11]
["SNCLRA_2_SPRHYD",1,7.0000000000000007E-2]
["SNCLRA_2_SPRHYD",2,0.01]
["SNCLRA_2_SPRHYD",3,7.0000000000000007E-2]
["SNCLRA_2_SPRHYD",4,0.06]
["SNCLRA_2_SPRHYD",5,0.06]
["SNCLRA_2_SPRHYD",6,0.15]
["SNCLRA_2_SPRHYD",7,0.17]
["SNCLRA_2_SPRHYD",8,0.19]
["SNCLRA_2_SPRHYD",9,0.17]
["SNCLRA_2_SPRHYD",10,0.17]
["SNCLRA_2_SPRHYD",11,0.05]
["SNCLRA_2_SPRHYD",12,0.03]
["SNCLRA_2_UNIT",1,27.5]
["SNCLRA_2_UNIT",2,27.5]
["SNCLRA_2_UNIT",3,27.5]
["SNCLRA_2_UNIT",4,27.5]
["SNCLRA_2_UNIT",5,27.5]
["SNCLRA_2_UNIT",6,27.5]
["SNCLRA_2_UNIT",7,27.5]
["SNCLRA_2_UNIT",8,27.5]
["SNCLRA_2_UNIT",9,27.5]
["SNCLRA_2_UNIT",10,27.5]
["SNCLRA_2_UNIT",11,27.5]
["SNCLRA_2_UNIT",12,27.5]
["SNCLRA_2_UNIT1",1,14.25]
["SNCLRA_2_UNIT1",2,14.31]
["SNCLRA_2_UNIT1",3,13.67]
["SNCLRA_2_UNIT1",4,10]
["SNCLRA_2_UNIT1",5,11.21]
["SNCLRA_2_UNIT1",6,11.34]
["SNCLRA_2_UNIT1",7,10.86]
["SNCLRA_2_UNIT1",8,11.3]
["SNCLRA_2_UNIT1",9,11.05]
["SNCLRA_2_UNIT1",10,8.8000000000000007]
["SNCLRA_2_UNIT1",11,10.08]
["SNCLRA_2_UNIT1",12,11.23]
["SNCLRA_2_VESBT1",1,100]
["SNCLRA_2_VESBT1",2,100]
["SNCLRA_2_VESBT1",3,100]
["SNCLRA_2_VESBT1",4,100]
["SNCLRA_2_VESBT1",5,100]
["SNCLRA_2_VESBT1",6,100]
["SNCLRA_2_VESBT1",7,100]
["SNCLRA_2_VESBT1",8,100]
["SNCLRA_2_VESBT1",9,100]
["SNCLRA_2_VESBT1",10,100]
["SNCLRA_2_VESBT1",11,100]
["SNCLRA_2_VESBT1",12,100]
["SNCLRA_6_OXGEN",1,47.7]
["SNCLRA_6_OXGEN",2,47.7]
["SNCLRA_6_OXGEN",3,47.7]
["SNCLRA_6_OXGEN",4,47.7]
["SNCLRA_6_OXGEN",5,47.7]
["SNCLRA_6_OXGEN",6,47.7]
["SNCLRA_6_OXGEN",7,47.7]
["SNCLRA_6_OXGEN",8,47.7]
["SNCLRA_6_OXGEN",9,47.7]
["SNCLRA_6_OXGEN",10,47.7]
["SNCLRA_6_OXGEN",11,47.7]
["SNCLRA_6_OXGEN",12,47.7]
["SNCLRA_6_PROCGN",1,21.67]
["SNCLRA_6_PROCGN",2,17.27]
["SNCLRA_6_PROCGN",3,21.67]
["SNCLRA_6_PROCGN",4,21.67]
["SNCLRA_6_PROCGN",5,21.35]
["SNCLRA_6_PROCGN",6,21.7]
["SNCLRA_6_PROCGN",7,20.79]
["SNCLRA_6_PROCGN",8,12.74]
["SNCLRA_6_PROCGN",9,12.55]
["SNCLRA_6_PROCGN",10,12.74]
["SNCLRA_6_PROCGN",11,12.27]
["SNCLRA_6_PROCGN",12,13.32]
["SNCLRA_6_QF",1,0]
["SNCLRA_6_QF",2,0]
["SNCLRA_6_QF",3,0]
["SNCLRA_6_QF",4,0]
["SNCLRA_6_QF",5,0]
["SNCLRA_6_QF",6,0]
["SNCLRA_6_QF",7,0]
["SNCLRA_6_QF",8,0]
["SNCLRA_6_QF",9,0]
["SNCLRA_6_QF",10,0]
["SNCLRA_6_QF",11,0.11]
["SNCLRA_6_QF",12,0.22]
["SNDBAR_7_UNIT 1",1,6.45]
["SNDBAR_7_UNIT 1",2,3.95]
["SNDBAR_7_UNIT 1",3,5.65]
["SNDBAR_7_UNIT 1",4,8.3000000000000007]
["SNDBAR_7_UNIT 1",5,8.3000000000000007]
["SNDBAR_7_UNIT 1",6,7.45]
["SNDBAR_7_UNIT 1",7,7.4]
["SNDBAR_7_UNIT 1",8,7.75]
["SNDBAR_7_UNIT 1",9,5.0999999999999996]
["SNDBAR_7_UNIT 1",10,1.22]
["SNDBAR_7_UNIT 1",11,7.19]
["SNDBAR_7_UNIT 1",12,12.58]
["SNMALF_6_UNITS",1,3.44]
["SNMALF_6_UNITS",2,2.82]
["SNMALF_6_UNITS",3,3.42]
["SNMALF_6_UNITS",4,3.4]
["SNMALF_6_UNITS",5,2.77]
["SNMALF_6_UNITS",6,2.5]
["SNMALF_6_UNITS",7,3.39]
["SNMALF_6_UNITS",8,3.43]
["SNMALF_6_UNITS",9,3.03]
["SNMALF_6_UNITS",10,3.02]
["SNMALF_6_UNITS",11,3.21]
["SNMALF_6_UNITS",12,3.08]
["SOUTH_2_UNIT",1,2.86]
["SOUTH_2_UNIT",2,2.93]
["SOUTH_2_UNIT",3,2.9]
["SOUTH_2_UNIT",4,2.34]
["SOUTH_2_UNIT",5,2.96]
["SOUTH_2_UNIT",6,0.8]
["SOUTH_2_UNIT",7,1.64]
["SOUTH_2_UNIT",8,1.56]
["SOUTH_2_UNIT",9,1.62]
["SOUTH_2_UNIT",10,1.2]
["SOUTH_2_UNIT",11,1.43]
["SOUTH_2_UNIT",12,1.73]
["SPAULD_6_UNIT 3",1,1.01]
["SPAULD_6_UNIT 3",2,0.87]
["SPAULD_6_UNIT 3",3,1.5]
["SPAULD_6_UNIT 3",4,2.4]
["SPAULD_6_UNIT 3",5,3.76]
["SPAULD_6_UNIT 3",6,1.1499999999999999]
["SPAULD_6_UNIT 3",7,3.66]
["SPAULD_6_UNIT 3",8,3.76]
["SPAULD_6_UNIT 3",9,2.7]
["SPAULD_6_UNIT 3",10,2.0499999999999998]
["SPAULD_6_UNIT 3",11,1.2]
["SPAULD_6_UNIT 3",12,0.9]
["SPAULD_6_UNIT12",1,2.5]
["SPAULD_6_UNIT12",2,2.1]
["SPAULD_6_UNIT12",3,1.96]
["SPAULD_6_UNIT12",4,2.16]
["SPAULD_6_UNIT12",5,5.22]
["SPAULD_6_UNIT12",6,4.4000000000000004]
["SPAULD_6_UNIT12",7,3.41]
["SPAULD_6_UNIT12",8,3.63]
["SPAULD_6_UNIT12",9,1.2]
["SPAULD_6_UNIT12",10,1.2]
["SPAULD_6_UNIT12",11,1.6]
["SPAULD_6_UNIT12",12,2.56]
["SPBURN_2_UNIT 1",1,6.99]
["SPBURN_2_UNIT 1",2,9.4]
["SPBURN_2_UNIT 1",3,9.61]
["SPBURN_2_UNIT 1",4,9.44]
["SPBURN_2_UNIT 1",5,9.67]
["SPBURN_2_UNIT 1",6,12.33]
["SPBURN_2_UNIT 1",7,12.59]
["SPBURN_2_UNIT 1",8,12.22]
["SPBURN_2_UNIT 1",9,12.51]
["SPBURN_2_UNIT 1",10,11.99]
["SPBURN_2_UNIT 1",11,11.99]
["SPBURN_2_UNIT 1",12,9.0299999999999994]
["SPBURN_7_SNOWMT",1,0.5]
["SPBURN_7_SNOWMT",2,0.65]
["SPBURN_7_SNOWMT",3,1.01]
["SPBURN_7_SNOWMT",4,1.38]
["SPBURN_7_SNOWMT",5,1.1100000000000001]
["SPBURN_7_SNOWMT",6,0.19]
["SPBURN_7_SNOWMT",7,0]
["SPBURN_7_SNOWMT",8,0]
["SPBURN_7_SNOWMT",9,0]
["SPBURN_7_SNOWMT",10,0.01]
["SPBURN_7_SNOWMT",11,0.01]
["SPBURN_7_SNOWMT",12,7.0000000000000007E-2]
["SPI LI_2_UNIT 1",1,7.39]
["SPI LI_2_UNIT 1",2,6.58]
["SPI LI_2_UNIT 1",3,6.4]
["SPI LI_2_UNIT 1",4,6.26]
["SPI LI_2_UNIT 1",5,8.02]
["SPI LI_2_UNIT 1",6,9.44]
["SPI LI_2_UNIT 1",7,9.48]
["SPI LI_2_UNIT 1",8,9.66]
["SPI LI_2_UNIT 1",9,9.3000000000000007]
["SPI LI_2_UNIT 1",10,8.35]
["SPI LI_2_UNIT 1",11,6.4]
["SPI LI_2_UNIT 1",12,7.07]
["SPIAND_1_ANDSN2",1,16.53]
["SPIAND_1_ANDSN2",2,16.739999999999998]
["SPIAND_1_ANDSN2",3,17.079999999999998]
["SPIAND_1_ANDSN2",4,16.89]
["SPIAND_1_ANDSN2",5,18.38]
["SPIAND_1_ANDSN2",6,17.87]
["SPIAND_1_ANDSN2",7,18.079999999999998]
["SPIAND_1_ANDSN2",8,18.66]
["SPIAND_1_ANDSN2",9,18.52]
["SPIAND_1_ANDSN2",10,15.31]
["SPIAND_1_ANDSN2",11,14.63]
["SPIAND_1_ANDSN2",12,15.02]
["SPICER_1_UNITS",1,6]
["SPICER_1_UNITS",2,6]
["SPICER_1_UNITS",3,6]
["SPICER_1_UNITS",4,6]
["SPICER_1_UNITS",5,6]
["SPICER_1_UNITS",6,6]
["SPICER_1_UNITS",7,6]
["SPICER_1_UNITS",8,6]
["SPICER_1_UNITS",9,6]
["SPICER_1_UNITS",10,6]
["SPICER_1_UNITS",11,6]
["SPICER_1_UNITS",12,6]
["SPIFBD_1_PL1X2",1,2.48]
["SPIFBD_1_PL1X2",2,2.2599999999999998]
["SPIFBD_1_PL1X2",3,2.5299999999999998]
["SPIFBD_1_PL1X2",4,2.77]
["SPIFBD_1_PL1X2",5,3.32]
["SPIFBD_1_PL1X2",6,3.28]
["SPIFBD_1_PL1X2",7,3.53]
["SPIFBD_1_PL1X2",8,3.67]
["SPIFBD_1_PL1X2",9,3.39]
["SPIFBD_1_PL1X2",10,3]
["SPIFBD_1_PL1X2",11,2.74]
["SPIFBD_1_PL1X2",12,2.6]
["SPQUIN_6_SRPCQU",1,18.25]
["SPQUIN_6_SRPCQU",2,15.95]
["SPQUIN_6_SRPCQU",3,16.059999999999999]
["SPQUIN_6_SRPCQU",4,9.27]
["SPQUIN_6_SRPCQU",5,19.18]
["SPQUIN_6_SRPCQU",6,21.47]
["SPQUIN_6_SRPCQU",7,19.27]
["SPQUIN_6_SRPCQU",8,14.51]
["SPQUIN_6_SRPCQU",9,12.65]
["SPQUIN_6_SRPCQU",10,8.73]
["SPQUIN_6_SRPCQU",11,7.99]
["SPQUIN_6_SRPCQU",12,15.7]
["SPRGAP_1_UNIT 1",1,1.81]
["SPRGAP_1_UNIT 1",2,1.23]
["SPRGAP_1_UNIT 1",3,2.86]
["SPRGAP_1_UNIT 1",4,5.08]
["SPRGAP_1_UNIT 1",5,4.71]
["SPRGAP_1_UNIT 1",6,2.75]
["SPRGAP_1_UNIT 1",7,1.74]
["SPRGAP_1_UNIT 1",8,0.09]
["SPRGAP_1_UNIT 1",9,3.21]
["SPRGAP_1_UNIT 1",10,3.35]
["SPRGAP_1_UNIT 1",11,2]
["SPRGAP_1_UNIT 1",12,2.99]
["SPRGVL_2_CREST",1,0]
["SPRGVL_2_CREST",2,0]
["SPRGVL_2_CREST",3,0]
["SPRGVL_2_CREST",4,0]
["SPRGVL_2_CREST",5,0]
["SPRGVL_2_CREST",6,0]
["SPRGVL_2_CREST",7,0]
["SPRGVL_2_CREST",8,0]
["SPRGVL_2_CREST",9,0]
["SPRGVL_2_CREST",10,0]
["SPRGVL_2_CREST",11,0]
["SPRGVL_2_CREST",12,0]
["SPRGVL_2_EXETPV",1,0]
["SPRGVL_2_EXETPV",2,0]
["SPRGVL_2_EXETPV",3,0]
["SPRGVL_2_EXETPV",4,0]
["SPRGVL_2_EXETPV",5,0]
["SPRGVL_2_EXETPV",6,0]
["SPRGVL_2_EXETPV",7,0]
["SPRGVL_2_EXETPV",8,0]
["SPRGVL_2_EXETPV",9,0]
["SPRGVL_2_EXETPV",10,0]
["SPRGVL_2_EXETPV",11,0]
["SPRGVL_2_EXETPV",12,0]
["SPRGVL_2_LINDPV",1,0]
["SPRGVL_2_LINDPV",2,0]
["SPRGVL_2_LINDPV",3,0]
["SPRGVL_2_LINDPV",4,0]
["SPRGVL_2_LINDPV",5,0]
["SPRGVL_2_LINDPV",6,0]
["SPRGVL_2_LINDPV",7,0]
["SPRGVL_2_LINDPV",8,0]
["SPRGVL_2_LINDPV",9,0]
["SPRGVL_2_LINDPV",10,0]
["SPRGVL_2_LINDPV",11,0]
["SPRGVL_2_LINDPV",12,0]
["SPRGVL_2_PORTPV",1,0]
["SPRGVL_2_PORTPV",2,0]
["SPRGVL_2_PORTPV",3,0]
["SPRGVL_2_PORTPV",4,0]
["SPRGVL_2_PORTPV",5,0]
["SPRGVL_2_PORTPV",6,0]
["SPRGVL_2_PORTPV",7,0]
["SPRGVL_2_PORTPV",8,0]
["SPRGVL_2_PORTPV",9,0]
["SPRGVL_2_PORTPV",10,0]
["SPRGVL_2_PORTPV",11,0]
["SPRGVL_2_PORTPV",12,0]
["SPRGVL_2_TULESC",1,0]
["SPRGVL_2_TULESC",2,0]
["SPRGVL_2_TULESC",3,0]
["SPRGVL_2_TULESC",4,0]
["SPRGVL_2_TULESC",5,0]
["SPRGVL_2_TULESC",6,0]
["SPRGVL_2_TULESC",7,0]
["SPRGVL_2_TULESC",8,0]
["SPRGVL_2_TULESC",9,0]
["SPRGVL_2_TULESC",10,0]
["SPRGVL_2_TULESC",11,0]
["SPRGVL_2_TULESC",12,0]
["SRINTL_6_UNIT",1,1.26]
["SRINTL_6_UNIT",2,1.18]
["SRINTL_6_UNIT",3,1.27]
["SRINTL_6_UNIT",4,1.3]
["SRINTL_6_UNIT",5,1.1299999999999999]
["SRINTL_6_UNIT",6,0.98]
["SRINTL_6_UNIT",7,0.94]
["SRINTL_6_UNIT",8,0.88]
["SRINTL_6_UNIT",9,0.9]
["SRINTL_6_UNIT",10,1.01]
["SRINTL_6_UNIT",11,1.17]
["SRINTL_6_UNIT",12,1.26]
["STANIS_7_UNIT 1",1,59]
["STANIS_7_UNIT 1",2,53.6]
["STANIS_7_UNIT 1",3,52.31]
["STANIS_7_UNIT 1",4,29.44]
["STANIS_7_UNIT 1",5,29.68]
["STANIS_7_UNIT 1",6,59]
["STANIS_7_UNIT 1",7,70.84]
["STANIS_7_UNIT 1",8,73.92]
["STANIS_7_UNIT 1",9,56.65]
["STANIS_7_UNIT 1",10,5.04]
["STANIS_7_UNIT 1",11,0]
["STANIS_7_UNIT 1",12,62.99]
["STANTN_2_STAGT1",1,49.65]
["STANTN_2_STAGT1",2,49.65]
["STANTN_2_STAGT1",3,49.65]
["STANTN_2_STAGT1",4,49.65]
["STANTN_2_STAGT1",5,49.65]
["STANTN_2_STAGT1",6,49.65]
["STANTN_2_STAGT1",7,49.65]
["STANTN_2_STAGT1",8,49.65]
["STANTN_2_STAGT1",9,49.65]
["STANTN_2_STAGT1",10,49.65]
["STANTN_2_STAGT1",11,49.65]
["STANTN_2_STAGT1",12,49.65]
["STANTN_2_STAGT2",1,49.65]
["STANTN_2_STAGT2",2,49.65]
["STANTN_2_STAGT2",3,49.65]
["STANTN_2_STAGT2",4,49.65]
["STANTN_2_STAGT2",5,49.65]
["STANTN_2_STAGT2",6,49.65]
["STANTN_2_STAGT2",7,49.65]
["STANTN_2_STAGT2",8,49.65]
["STANTN_2_STAGT2",9,49.65]
["STANTN_2_STAGT2",10,49.65]
["STANTN_2_STAGT2",11,49.65]
["STANTN_2_STAGT2",12,49.65]
["STIGCT_2_LODI",1,49.5]
["STIGCT_2_LODI",2,49.5]
["STIGCT_2_LODI",3,49.5]
["STIGCT_2_LODI",4,49.5]
["STIGCT_2_LODI",5,49.5]
["STIGCT_2_LODI",6,49.5]
["STIGCT_2_LODI",7,49.5]
["STIGCT_2_LODI",8,49.5]
["STIGCT_2_LODI",9,49.5]
["STIGCT_2_LODI",10,49.5]
["STIGCT_2_LODI",11,49.5]
["STIGCT_2_LODI",12,49.5]
["STNRES_1_UNIT",1,14.53]
["STNRES_1_UNIT",2,19.27]
["STNRES_1_UNIT",3,19.71]
["STNRES_1_UNIT",4,17.93]
["STNRES_1_UNIT",5,13.83]
["STNRES_1_UNIT",6,17.87]
["STNRES_1_UNIT",7,19.8]
["STNRES_1_UNIT",8,19.600000000000001]
["STNRES_1_UNIT",9,19.55]
["STNRES_1_UNIT",10,18.87]
["STNRES_1_UNIT",11,19.079999999999998]
["STNRES_1_UNIT",12,18.45]
["STOILS_1_UNITS",1,0]
["STOILS_1_UNITS",2,7.46]
["STOILS_1_UNITS",3,0.19]
["STOILS_1_UNITS",4,0]
["STOILS_1_UNITS",5,0]
["STOILS_1_UNITS",6,0]
["STOILS_1_UNITS",7,6.49]
["STOILS_1_UNITS",8,3.33]
["STOILS_1_UNITS",9,0]
["STOILS_1_UNITS",10,11.34]
["STOILS_1_UNITS",11,16.559999999999999]
["STOILS_1_UNITS",12,0]
["STOREY_2_MDRCH2",1,0]
["STOREY_2_MDRCH2",2,0]
["STOREY_2_MDRCH2",3,0.05]
["STOREY_2_MDRCH2",4,0.14000000000000001]
["STOREY_2_MDRCH2",5,0.18]
["STOREY_2_MDRCH2",6,0.31]
["STOREY_2_MDRCH2",7,0.33]
["STOREY_2_MDRCH2",8,0.17]
["STOREY_2_MDRCH2",9,0.13]
["STOREY_2_MDRCH2",10,0.14000000000000001]
["STOREY_2_MDRCH2",11,0]
["STOREY_2_MDRCH2",12,0]
["STOREY_2_MDRCH3",1,0]
["STOREY_2_MDRCH3",2,0]
["STOREY_2_MDRCH3",3,0]
["STOREY_2_MDRCH3",4,0.05]
["STOREY_2_MDRCH3",5,7.0000000000000007E-2]
["STOREY_2_MDRCH3",6,0.2]
["STOREY_2_MDRCH3",7,0.23]
["STOREY_2_MDRCH3",8,0.1]
["STOREY_2_MDRCH3",9,0.06]
["STOREY_2_MDRCH3",10,7.0000000000000007E-2]
["STOREY_2_MDRCH3",11,0]
["STOREY_2_MDRCH3",12,0]
["STOREY_2_MDRCH4",1,0]
["STOREY_2_MDRCH4",2,0]
["STOREY_2_MDRCH4",3,0.03]
["STOREY_2_MDRCH4",4,0.23]
["STOREY_2_MDRCH4",5,0.22]
["STOREY_2_MDRCH4",6,0.35]
["STOREY_2_MDRCH4",7,0.39]
["STOREY_2_MDRCH4",8,0.17]
["STOREY_2_MDRCH4",9,0.08]
["STOREY_2_MDRCH4",10,0.08]
["STOREY_2_MDRCH4",11,0]
["STOREY_2_MDRCH4",12,0]
["STOREY_7_MDRCHW",1,0]
["STOREY_7_MDRCHW",2,0]
["STOREY_7_MDRCHW",3,0.12]
["STOREY_7_MDRCHW",4,0.44]
["STOREY_7_MDRCHW",5,0.4]
["STOREY_7_MDRCHW",6,0.71]
["STOREY_7_MDRCHW",7,0.91]
["STOREY_7_MDRCHW",8,0.06]
["STOREY_7_MDRCHW",9,0]
["STOREY_7_MDRCHW",10,0.13]
["STOREY_7_MDRCHW",11,0]
["STOREY_7_MDRCHW",12,0]
["STROUD_6_SOLAR",1,0.08]
["STROUD_6_SOLAR",2,0.6]
["STROUD_6_SOLAR",3,0.7]
["STROUD_6_SOLAR",4,0.88]
["STROUD_6_SOLAR",5,1.28]
["STROUD_6_SOLAR",6,2.62]
["STROUD_6_SOLAR",7,2.88]
["STROUD_6_SOLAR",8,2.48]
["STROUD_6_SOLAR",9,2.2200000000000002]
["STROUD_6_SOLAR",10,1.48]
["STROUD_6_SOLAR",11,1.1399999999999999]
["STROUD_6_SOLAR",12,0.7]
["STROUD_6_WWHSR1",1,0]
["STROUD_6_WWHSR1",2,0]
["STROUD_6_WWHSR1",3,0]
["STROUD_6_WWHSR1",4,0]
["STROUD_6_WWHSR1",5,0]
["STROUD_6_WWHSR1",6,0]
["STROUD_6_WWHSR1",7,0]
["STROUD_6_WWHSR1",8,0]
["STROUD_6_WWHSR1",9,0]
["STROUD_6_WWHSR1",10,0]
["STROUD_6_WWHSR1",11,0]
["STROUD_6_WWHSR1",12,0]
["SUMWHT_6_SWSSR1",1,7.0000000000000007E-2]
["SUMWHT_6_SWSSR1",2,0.56000000000000005]
["SUMWHT_6_SWSSR1",3,0.65]
["SUMWHT_6_SWSSR1",4,0.81]
["SUMWHT_6_SWSSR1",5,1.18]
["SUMWHT_6_SWSSR1",6,2.42]
["SUMWHT_6_SWSSR1",7,2.66]
["SUMWHT_6_SWSSR1",8,2.29]
["SUMWHT_6_SWSSR1",9,2.0499999999999998]
["SUMWHT_6_SWSSR1",10,1.37]
["SUMWHT_6_SWSSR1",11,1.05]
["SUMWHT_6_SWSSR1",12,0.65]
["SUNCAT_2_A1ABT1",1,47]
["SUNCAT_2_A1ABT1",2,47]
["SUNCAT_2_A1ABT1",3,47]
["SUNCAT_2_A1ABT1",4,47]
["SUNCAT_2_A1ABT1",5,47]
["SUNCAT_2_A1ABT1",6,47]
["SUNCAT_2_A1ABT1",7,47]
["SUNCAT_2_A1ABT1",8,47]
["SUNCAT_2_A1ABT1",9,47]
["SUNCAT_2_A1ABT1",10,47]
["SUNCAT_2_A1ABT1",11,47]
["SUNCAT_2_A1ABT1",12,47]
["SUNCAT_2_A1BBT1",1,63]
["SUNCAT_2_A1BBT1",2,63]
["SUNCAT_2_A1BBT1",3,63]
["SUNCAT_2_A1BBT1",4,63]
["SUNCAT_2_A1BBT1",5,63]
["SUNCAT_2_A1BBT1",6,63]
["SUNCAT_2_A1BBT1",7,63]
["SUNCAT_2_A1BBT1",8,63]
["SUNCAT_2_A1BBT1",9,63]
["SUNCAT_2_A1BBT1",10,63]
["SUNCAT_2_A1BBT1",11,63]
["SUNCAT_2_A1BBT1",12,63]
["SUNCAT_2_A2ABT2",1,104.28]
["SUNCAT_2_A2ABT2",2,132]
["SUNCAT_2_A2ABT2",3,132]
["SUNCAT_2_A2ABT2",4,132]
["SUNCAT_2_A2ABT2",5,132]
["SUNCAT_2_A2ABT2",6,132]
["SUNCAT_2_A2ABT2",7,132]
["SUNCAT_2_A2ABT2",8,132]
["SUNCAT_2_A2ABT2",9,132]
["SUNCAT_2_A2ABT2",10,132]
["SUNCAT_2_A2ABT2",11,119.45]
["SUNCAT_2_A2ABT2",12,85.72]
["SUNRIS_2_PL1X3",1,586.02]
["SUNRIS_2_PL1X3",2,586.02]
["SUNRIS_2_PL1X3",3,586.02]
["SUNRIS_2_PL1X3",4,586.02]
["SUNRIS_2_PL1X3",5,586.02]
["SUNRIS_2_PL1X3",6,586.02]
["SUNRIS_2_PL1X3",7,586.02]
["SUNRIS_2_PL1X3",8,586.02]
["SUNRIS_2_PL1X3",9,586.02]
["SUNRIS_2_PL1X3",10,586.02]
["SUNRIS_2_PL1X3",11,586.02]
["SUNRIS_2_PL1X3",12,586.02]
["SUNSET_2_UNITS",1,248]
["SUNSET_2_UNITS",2,248]
["SUNSET_2_UNITS",3,248]
["SUNSET_2_UNITS",4,245]
["SUNSET_2_UNITS",5,240]
["SUNSET_2_UNITS",6,234]
["SUNSET_2_UNITS",7,229]
["SUNSET_2_UNITS",8,229]
["SUNSET_2_UNITS",9,231]
["SUNSET_2_UNITS",10,243]
["SUNSET_2_UNITS",11,246]
["SUNSET_2_UNITS",12,248]
["SUNSHN_2_LNDFL",1,18.100000000000001]
["SUNSHN_2_LNDFL",2,17.52]
["SUNSHN_2_LNDFL",3,17.850000000000001]
["SUNSHN_2_LNDFL",4,16.8]
["SUNSHN_2_LNDFL",5,17.649999999999999]
["SUNSHN_2_LNDFL",6,17.53]
["SUNSHN_2_LNDFL",7,16.940000000000001]
["SUNSHN_2_LNDFL",8,16.440000000000001]
["SUNSHN_2_LNDFL",9,16.72]
["SUNSHN_2_LNDFL",10,16.329999999999998]
["SUNSHN_2_LNDFL",11,17.260000000000002]
["SUNSHN_2_LNDFL",12,16.010000000000002]
["SUNSLR_1_SSVSR1",1,0.4]
["SUNSLR_1_SSVSR1",2,3]
["SUNSLR_1_SSVSR1",3,3.5]
["SUNSLR_1_SSVSR1",4,4.4000000000000004]
["SUNSLR_1_SSVSR1",5,6.4]
["SUNSLR_1_SSVSR1",6,13.1]
["SUNSLR_1_SSVSR1",7,14.4]
["SUNSLR_1_SSVSR1",8,12.4]
["SUNSLR_1_SSVSR1",9,11.1]
["SUNSLR_1_SSVSR1",10,7.4]
["SUNSLR_1_SSVSR1",11,5.7]
["SUNSLR_1_SSVSR1",12,3.5]
["SUNSPT_2_WNASR1",1,0.08]
["SUNSPT_2_WNASR1",2,0.6]
["SUNSPT_2_WNASR1",3,0.7]
["SUNSPT_2_WNASR1",4,0.88]
["SUNSPT_2_WNASR1",5,1.28]
["SUNSPT_2_WNASR1",6,2.62]
["SUNSPT_2_WNASR1",7,2.88]
["SUNSPT_2_WNASR1",8,2.48]
["SUNSPT_2_WNASR1",9,2.2200000000000002]
["SUNSPT_2_WNASR1",10,1.48]
["SUNSPT_2_WNASR1",11,1.1399999999999999]
["SUNSPT_2_WNASR1",12,0.7]
["SUNST2_5_SS2SR1",1,0.6]
["SUNST2_5_SS2SR1",2,4.5]
["SUNST2_5_SS2SR1",3,5.25]
["SUNST2_5_SS2SR1",4,6.6]
["SUNST2_5_SS2SR1",5,9.6]
["SUNST2_5_SS2SR1",6,19.649999999999999]
["SUNST2_5_SS2SR1",7,21.6]
["SUNST2_5_SS2SR1",8,18.600000000000001]
["SUNST2_5_SS2SR1",9,16.649999999999999]
["SUNST2_5_SS2SR1",10,11.1]
["SUNST2_5_SS2SR1",11,8.5500000000000007]
["SUNST2_5_SS2SR1",12,5.25]
["SYCAMR_2_UNIT 1",1,74]
["SYCAMR_2_UNIT 1",2,74]
["SYCAMR_2_UNIT 1",3,74]
["SYCAMR_2_UNIT 1",4,74]
["SYCAMR_2_UNIT 1",5,74]
["SYCAMR_2_UNIT 1",6,74]
["SYCAMR_2_UNIT 1",7,74]
["SYCAMR_2_UNIT 1",8,74]
["SYCAMR_2_UNIT 1",9,74]
["SYCAMR_2_UNIT 1",10,74]
["SYCAMR_2_UNIT 1",11,74]
["SYCAMR_2_UNIT 1",12,74]
["SYCAMR_2_UNIT 2",1,76]
["SYCAMR_2_UNIT 2",2,76]
["SYCAMR_2_UNIT 2",3,76]
["SYCAMR_2_UNIT 2",4,76]
["SYCAMR_2_UNIT 2",5,76]
["SYCAMR_2_UNIT 2",6,76]
["SYCAMR_2_UNIT 2",7,76]
["SYCAMR_2_UNIT 2",8,76]
["SYCAMR_2_UNIT 2",9,76]
["SYCAMR_2_UNIT 2",10,76]
["SYCAMR_2_UNIT 2",11,76]
["SYCAMR_2_UNIT 2",12,76]
["SYCAMR_2_UNIT 3",1,74]
["SYCAMR_2_UNIT 3",2,74]
["SYCAMR_2_UNIT 3",3,74]
["SYCAMR_2_UNIT 3",4,74]
["SYCAMR_2_UNIT 3",5,74]
["SYCAMR_2_UNIT 3",6,74]
["SYCAMR_2_UNIT 3",7,74]
["SYCAMR_2_UNIT 3",8,74]
["SYCAMR_2_UNIT 3",9,74]
["SYCAMR_2_UNIT 3",10,74]
["SYCAMR_2_UNIT 3",11,74]
["SYCAMR_2_UNIT 3",12,74]
["SYCAMR_2_UNIT 4",1,76]
["SYCAMR_2_UNIT 4",2,76]
["SYCAMR_2_UNIT 4",3,76]
["SYCAMR_2_UNIT 4",4,76]
["SYCAMR_2_UNIT 4",5,76]
["SYCAMR_2_UNIT 4",6,76]
["SYCAMR_2_UNIT 4",7,76]
["SYCAMR_2_UNIT 4",8,76]
["SYCAMR_2_UNIT 4",9,76]
["SYCAMR_2_UNIT 4",10,76]
["SYCAMR_2_UNIT 4",11,76]
["SYCAMR_2_UNIT 4",12,76]
["TANHIL_6_SOLART",1,11.52]
["TANHIL_6_SOLART",2,11.84]
["TANHIL_6_SOLART",3,11.48]
["TANHIL_6_SOLART",4,10.039999999999999]
["TANHIL_6_SOLART",5,11.68]
["TANHIL_6_SOLART",6,11.01]
["TANHIL_6_SOLART",7,11.07]
["TANHIL_6_SOLART",8,10.82]
["TANHIL_6_SOLART",9,11.09]
["TANHIL_6_SOLART",10,9.36]
["TANHIL_6_SOLART",11,8.91]
["TANHIL_6_SOLART",12,11.87]
["TBLMTN_6_QF",1,0.21]
["TBLMTN_6_QF",2,0.32]
["TBLMTN_6_QF",3,0.3]
["TBLMTN_6_QF",4,0.38]
["TBLMTN_6_QF",5,0.26]
["TBLMTN_6_QF",6,0.21]
["TBLMTN_6_QF",7,0.22]
["TBLMTN_6_QF",8,0.21]
["TBLMTN_6_QF",9,0.2]
["TBLMTN_6_QF",10,0.15]
["TBLMTN_6_QF",11,0.18]
["TBLMTN_6_QF",12,0.19]
["TEHAPI_2_PW1WD1",1,8.39]
["TEHAPI_2_PW1WD1",2,8.92]
["TEHAPI_2_PW1WD1",3,7.84]
["TEHAPI_2_PW1WD1",4,7.51]
["TEHAPI_2_PW1WD1",5,7.99]
["TEHAPI_2_PW1WD1",6,7.32]
["TEHAPI_2_PW1WD1",7,6.8]
["TEHAPI_2_PW1WD1",8,5.17]
["TEHAPI_2_PW1WD1",9,5.34]
["TEHAPI_2_PW1WD1",10,4.95]
["TEHAPI_2_PW1WD1",11,6.68]
["TEHAPI_2_PW1WD1",12,8.09]
["TEHAPI_2_PW2WD2",1,2.54]
["TEHAPI_2_PW2WD2",2,2.71]
["TEHAPI_2_PW2WD2",3,2.38]
["TEHAPI_2_PW2WD2",4,2.2799999999999998]
["TEHAPI_2_PW2WD2",5,2.42]
["TEHAPI_2_PW2WD2",6,2.2200000000000002]
["TEHAPI_2_PW2WD2",7,2.06]
["TEHAPI_2_PW2WD2",8,1.57]
["TEHAPI_2_PW2WD2",9,1.62]
["TEHAPI_2_PW2WD2",10,1.5]
["TEHAPI_2_PW2WD2",11,2.02]
["TEHAPI_2_PW2WD2",12,2.4500000000000002]
["TEHAPI_2_WIND1",1,2.63]
["TEHAPI_2_WIND1",2,2.8]
["TEHAPI_2_WIND1",3,2.46]
["TEHAPI_2_WIND1",4,2.36]
["TEHAPI_2_WIND1",5,2.5099999999999998]
["TEHAPI_2_WIND1",6,2.2999999999999998]
["TEHAPI_2_WIND1",7,2.13]
["TEHAPI_2_WIND1",8,1.62]
["TEHAPI_2_WIND1",9,1.67]
["TEHAPI_2_WIND1",10,1.55]
["TEHAPI_2_WIND1",11,2.09]
["TEHAPI_2_WIND1",12,2.54]
["TEHAPI_2_WIND2",1,3.55]
["TEHAPI_2_WIND2",2,3.78]
["TEHAPI_2_WIND2",3,3.32]
["TEHAPI_2_WIND2",4,3.18]
["TEHAPI_2_WIND2",5,3.38]
["TEHAPI_2_WIND2",6,3.1]
["TEHAPI_2_WIND2",7,2.88]
["TEHAPI_2_WIND2",8,2.19]
["TEHAPI_2_WIND2",9,2.2599999999999998]
["TEHAPI_2_WIND2",10,2.1]
["TEHAPI_2_WIND2",11,2.83]
["TEHAPI_2_WIND2",12,3.43]
["TENGEN_2_PL1X2",1,40.200000000000003]
["TENGEN_2_PL1X2",2,40.200000000000003]
["TENGEN_2_PL1X2",3,40.200000000000003]
["TENGEN_2_PL1X2",4,40.200000000000003]
["TENGEN_2_PL1X2",5,40.200000000000003]
["TENGEN_2_PL1X2",6,40.200000000000003]
["TENGEN_2_PL1X2",7,40.200000000000003]
["TENGEN_2_PL1X2",8,40.200000000000003]
["TENGEN_2_PL1X2",9,40.200000000000003]
["TENGEN_2_PL1X2",10,40.200000000000003]
["TENGEN_2_PL1X2",11,40.200000000000003]
["TENGEN_2_PL1X2",12,40.200000000000003]
["TERMEX_2_PL1X3",1,605]
["TERMEX_2_PL1X3",2,605]
["TERMEX_2_PL1X3",3,605]
["TERMEX_2_PL1X3",4,605]
["TERMEX_2_PL1X3",5,601]
["TERMEX_2_PL1X3",6,593]
["TERMEX_2_PL1X3",7,591]
["TERMEX_2_PL1X3",8,593]
["TERMEX_2_PL1X3",9,596]
["TERMEX_2_PL1X3",10,605]
["TERMEX_2_PL1X3",11,605]
["TERMEX_2_PL1X3",12,605]
["TESLA_1_QF",1,0.06]
["TESLA_1_QF",2,0.15]
["TESLA_1_QF",3,0.19]
["TESLA_1_QF",4,0.16]
["TESLA_1_QF",5,0.22]
["TESLA_1_QF",6,0.35]
["TESLA_1_QF",7,0.34]
["TESLA_1_QF",8,0.35]
["TESLA_1_QF",9,0.3]
["TESLA_1_QF",10,0.11]
["TESLA_1_QF",11,0.05]
["TESLA_1_QF",12,0.04]
["TIDWTR_2_UNITS",1,23.95]
["TIDWTR_2_UNITS",2,26.89]
["TIDWTR_2_UNITS",3,22.49]
["TIDWTR_2_UNITS",4,25.94]
["TIDWTR_2_UNITS",5,38.840000000000003]
["TIDWTR_2_UNITS",6,42.92]
["TIDWTR_2_UNITS",7,43.59]
["TIDWTR_2_UNITS",8,54.77]
["TIDWTR_2_UNITS",9,62.6]
["TIDWTR_2_UNITS",10,59.22]
["TIDWTR_2_UNITS",11,33.119999999999997]
["TIDWTR_2_UNITS",12,31.26]
["TIFFNY_1_DILLON",1,7.95]
["TIFFNY_1_DILLON",2,8.4600000000000009]
["TIFFNY_1_DILLON",3,7.43]
["TIFFNY_1_DILLON",4,7.12]
["TIFFNY_1_DILLON",5,7.57]
["TIFFNY_1_DILLON",6,6.94]
["TIFFNY_1_DILLON",7,6.45]
["TIFFNY_1_DILLON",8,4.9000000000000004]
["TIFFNY_1_DILLON",9,5.0599999999999996]
["TIFFNY_1_DILLON",10,4.6900000000000004]
["TIFFNY_1_DILLON",11,6.33]
["TIFFNY_1_DILLON",12,7.66]
["TIGRCK_7_UNITS",1,25.6]
["TIGRCK_7_UNITS",2,14.46]
["TIGRCK_7_UNITS",3,8]
["TIGRCK_7_UNITS",4,0]
["TIGRCK_7_UNITS",5,16]
["TIGRCK_7_UNITS",6,36]
["TIGRCK_7_UNITS",7,32.44]
["TIGRCK_7_UNITS",8,40.4]
["TIGRCK_7_UNITS",9,36.299999999999997]
["TIGRCK_7_UNITS",10,30.77]
["TIGRCK_7_UNITS",11,29.62]
["TIGRCK_7_UNITS",12,30.16]
["TKOPWR_6_HYDRO",1,0.48]
["TKOPWR_6_HYDRO",2,0.82]
["TKOPWR_6_HYDRO",3,0.88]
["TKOPWR_6_HYDRO",4,0.52]
["TKOPWR_6_HYDRO",5,0.25]
["TKOPWR_6_HYDRO",6,0.06]
["TKOPWR_6_HYDRO",7,0]
["TKOPWR_6_HYDRO",8,0]
["TKOPWR_6_HYDRO",9,0]
["TKOPWR_6_HYDRO",10,0.04]
["TKOPWR_6_HYDRO",11,0.04]
["TKOPWR_6_HYDRO",12,0.01]
["TMPLTN_2_SOLAR",1,0.01]
["TMPLTN_2_SOLAR",2,0.05]
["TMPLTN_2_SOLAR",3,0.05]
["TMPLTN_2_SOLAR",4,7.0000000000000007E-2]
["TMPLTN_2_SOLAR",5,0.1]
["TMPLTN_2_SOLAR",6,0.2]
["TMPLTN_2_SOLAR",7,0.22]
["TMPLTN_2_SOLAR",8,0.19]
["TMPLTN_2_SOLAR",9,0.17]
["TMPLTN_2_SOLAR",10,0.11]
["TMPLTN_2_SOLAR",11,0.09]
["TMPLTN_2_SOLAR",12,0.05]
["TOADTW_6_UNIT",1,0.4]
["TOADTW_6_UNIT",2,0.47]
["TOADTW_6_UNIT",3,0.31]
["TOADTW_6_UNIT",4,0.16]
["TOADTW_6_UNIT",5,0.55000000000000004]
["TOADTW_6_UNIT",6,0.36]
["TOADTW_6_UNIT",7,0.44]
["TOADTW_6_UNIT",8,0.24]
["TOADTW_6_UNIT",9,0.1]
["TOADTW_6_UNIT",10,7.0000000000000007E-2]
["TOADTW_6_UNIT",11,0.12]
["TOADTW_6_UNIT",12,0.14000000000000001]
["TOPAZ_2_SOLAR",1,2.2000000000000002]
["TOPAZ_2_SOLAR",2,16.5]
["TOPAZ_2_SOLAR",3,19.25]
["TOPAZ_2_SOLAR",4,24.2]
["TOPAZ_2_SOLAR",5,35.200000000000003]
["TOPAZ_2_SOLAR",6,72.05]
["TOPAZ_2_SOLAR",7,79.2]
["TOPAZ_2_SOLAR",8,68.2]
["TOPAZ_2_SOLAR",9,61.05]
["TOPAZ_2_SOLAR",10,40.700000000000003]
["TOPAZ_2_SOLAR",11,31.35]
["TOPAZ_2_SOLAR",12,19.25]
["TORTLA_1_SOLAR",1,0.08]
["TORTLA_1_SOLAR",2,0.6]
["TORTLA_1_SOLAR",3,0.7]
["TORTLA_1_SOLAR",4,0.88]
["TORTLA_1_SOLAR",5,1.28]
["TORTLA_1_SOLAR",6,2.62]
["TORTLA_1_SOLAR",7,2.88]
["TORTLA_1_SOLAR",8,2.48]
["TORTLA_1_SOLAR",9,2.2200000000000002]
["TORTLA_1_SOLAR",10,1.48]
["TORTLA_1_SOLAR",11,1.1399999999999999]
["TORTLA_1_SOLAR",12,0.7]
["TRNQL8_2_AMASR1",1,0.08]
["TRNQL8_2_AMASR1",2,0.6]
["TRNQL8_2_AMASR1",3,0.7]
["TRNQL8_2_AMASR1",4,0.88]
["TRNQL8_2_AMASR1",5,1.28]
["TRNQL8_2_AMASR1",6,2.62]
["TRNQL8_2_AMASR1",7,2.88]
["TRNQL8_2_AMASR1",8,2.48]
["TRNQL8_2_AMASR1",9,2.2200000000000002]
["TRNQL8_2_AMASR1",10,1.48]
["TRNQL8_2_AMASR1",11,1.1399999999999999]
["TRNQL8_2_AMASR1",12,0.7]
["TRNQL8_2_AZUSR1",1,0.08]
["TRNQL8_2_AZUSR1",2,0.6]
["TRNQL8_2_AZUSR1",3,0.7]
["TRNQL8_2_AZUSR1",4,0.88]
["TRNQL8_2_AZUSR1",5,1.28]
["TRNQL8_2_AZUSR1",6,2.62]
["TRNQL8_2_AZUSR1",7,2.88]
["TRNQL8_2_AZUSR1",8,2.48]
["TRNQL8_2_AZUSR1",9,2.2200000000000002]
["TRNQL8_2_AZUSR1",10,1.48]
["TRNQL8_2_AZUSR1",11,1.1399999999999999]
["TRNQL8_2_AZUSR1",12,0.7]
["TRNQL8_2_ROJSR1",1,0.4]
["TRNQL8_2_ROJSR1",2,3]
["TRNQL8_2_ROJSR1",3,3.5]
["TRNQL8_2_ROJSR1",4,4.4000000000000004]
["TRNQL8_2_ROJSR1",5,6.4]
["TRNQL8_2_ROJSR1",6,13.1]
["TRNQL8_2_ROJSR1",7,14.4]
["TRNQL8_2_ROJSR1",8,12.4]
["TRNQL8_2_ROJSR1",9,11.1]
["TRNQL8_2_ROJSR1",10,7.4]
["TRNQL8_2_ROJSR1",11,5.7]
["TRNQL8_2_ROJSR1",12,3.5]
["TRNQL8_2_VERSR1",1,0.24]
["TRNQL8_2_VERSR1",2,1.8]
["TRNQL8_2_VERSR1",3,2.1]
["TRNQL8_2_VERSR1",4,2.64]
["TRNQL8_2_VERSR1",5,3.84]
["TRNQL8_2_VERSR1",6,7.86]
["TRNQL8_2_VERSR1",7,8.64]
["TRNQL8_2_VERSR1",8,7.44]
["TRNQL8_2_VERSR1",9,6.66]
["TRNQL8_2_VERSR1",10,4.4400000000000004]
["TRNQL8_2_VERSR1",11,3.42]
["TRNQL8_2_VERSR1",12,2.1]
["TRNQLT_2_RETBT1",1,72]
["TRNQLT_2_RETBT1",2,72]
["TRNQLT_2_RETBT1",3,72]
["TRNQLT_2_RETBT1",4,72]
["TRNQLT_2_RETBT1",5,72]
["TRNQLT_2_RETBT1",6,72]
["TRNQLT_2_RETBT1",7,72]
["TRNQLT_2_RETBT1",8,72]
["TRNQLT_2_RETBT1",9,72]
["TRNQLT_2_RETBT1",10,72]
["TRNQLT_2_RETBT1",11,72]
["TRNQLT_2_RETBT1",12,72]
["TRNQLT_2_SOLAR",1,0.45]
["TRNQLT_2_SOLAR",2,4.21]
["TRNQLT_2_SOLAR",3,5.12]
["TRNQLT_2_SOLAR",4,7]
["TRNQLT_2_SOLAR",5,10.26]
["TRNQLT_2_SOLAR",6,22.36]
["TRNQLT_2_SOLAR",7,24.76]
["TRNQLT_2_SOLAR",8,20.73]
["TRNQLT_2_SOLAR",9,17.82]
["TRNQLT_2_SOLAR",10,10.7]
["TRNQLT_2_SOLAR",11,7.33]
["TRNQLT_2_SOLAR",12,3.38]
["TRNSWD_1_QF",1,6.89]
["TRNSWD_1_QF",2,7.32]
["TRNSWD_1_QF",3,6.44]
["TRNSWD_1_QF",4,6.17]
["TRNSWD_1_QF",5,6.56]
["TRNSWD_1_QF",6,6.01]
["TRNSWD_1_QF",7,5.58]
["TRNSWD_1_QF",8,4.24]
["TRNSWD_1_QF",9,4.38]
["TRNSWD_1_QF",10,4.07]
["TRNSWD_1_QF",11,5.48]
["TRNSWD_1_QF",12,6.64]
["TULARE_2_TULBM1",1,0]
["TULARE_2_TULBM1",2,0]
["TULARE_2_TULBM1",3,0]
["TULARE_2_TULBM1",4,0]
["TULARE_2_TULBM1",5,0]
["TULARE_2_TULBM1",6,0]
["TULARE_2_TULBM1",7,0]
["TULARE_2_TULBM1",8,0]
["TULARE_2_TULBM1",9,0]
["TULARE_2_TULBM1",10,0]
["TULARE_2_TULBM1",11,0]
["TULARE_2_TULBM1",12,0]
["TULEWD_1_TULWD1",1,23.06]
["TULEWD_1_TULWD1",2,24.53]
["TULEWD_1_TULWD1",3,21.55]
["TULEWD_1_TULWD1",4,20.65]
["TULEWD_1_TULWD1",5,21.95]
["TULEWD_1_TULWD1",6,20.12]
["TULEWD_1_TULWD1",7,18.7]
["TULEWD_1_TULWD1",8,14.21]
["TULEWD_1_TULWD1",9,14.68]
["TULEWD_1_TULWD1",10,13.61]
["TULEWD_1_TULWD1",11,18.350000000000001]
["TULEWD_1_TULWD1",12,22.22]
["TULLCK_7_UNITS",1,4.09]
["TULLCK_7_UNITS",2,9.0299999999999994]
["TULLCK_7_UNITS",3,15.19]
["TULLCK_7_UNITS",4,19.61]
["TULLCK_7_UNITS",5,21.79]
["TULLCK_7_UNITS",6,24.04]
["TULLCK_7_UNITS",7,22.18]
["TULLCK_7_UNITS",8,19.14]
["TULLCK_7_UNITS",9,14.14]
["TULLCK_7_UNITS",10,9.7899999999999991]
["TULLCK_7_UNITS",11,2.93]
["TULLCK_7_UNITS",12,5.99]
["TUPMAN_1_BIOGAS",1,0.32]
["TUPMAN_1_BIOGAS",2,0.33]
["TUPMAN_1_BIOGAS",3,0.33]
["TUPMAN_1_BIOGAS",4,0.34]
["TUPMAN_1_BIOGAS",5,0.36]
["TUPMAN_1_BIOGAS",6,0.36]
["TUPMAN_1_BIOGAS",7,0.34]
["TUPMAN_1_BIOGAS",8,0.34]
["TUPMAN_1_BIOGAS",9,0.35]
["TUPMAN_1_BIOGAS",10,0.32]
["TUPMAN_1_BIOGAS",11,0.3]
["TUPMAN_1_BIOGAS",12,0.3]
["TVYVLY_6_KRSHY1",1,0.81]
["TVYVLY_6_KRSHY1",2,0.81]
["TVYVLY_6_KRSHY1",3,0.28000000000000003]
["TVYVLY_6_KRSHY1",4,0.28000000000000003]
["TVYVLY_6_KRSHY1",5,0.28000000000000003]
["TVYVLY_6_KRSHY1",6,0.81]
["TVYVLY_6_KRSHY1",7,0.98]
["TVYVLY_6_KRSHY1",8,1]
["TVYVLY_6_KRSHY1",9,1.04]
["TVYVLY_6_KRSHY1",10,1.04]
["TVYVLY_6_KRSHY1",11,1.04]
["TVYVLY_6_KRSHY1",12,1.04]
["TWISSL_6_SOLAR",1,0.01]
["TWISSL_6_SOLAR",2,0.05]
["TWISSL_6_SOLAR",3,0.05]
["TWISSL_6_SOLAR",4,7.0000000000000007E-2]
["TWISSL_6_SOLAR",5,0.1]
["TWISSL_6_SOLAR",6,0.2]
["TWISSL_6_SOLAR",7,0.22]
["TWISSL_6_SOLAR",8,0.19]
["TWISSL_6_SOLAR",9,0.17]
["TWISSL_6_SOLAR",10,0.11]
["TWISSL_6_SOLAR",11,0.09]
["TWISSL_6_SOLAR",12,0.05]
["TWISSL_6_SOLAR1",1,0.08]
["TWISSL_6_SOLAR1",2,0.6]
["TWISSL_6_SOLAR1",3,0.7]
["TWISSL_6_SOLAR1",4,0.88]
["TWISSL_6_SOLAR1",5,1.28]
["TWISSL_6_SOLAR1",6,2.62]
["TWISSL_6_SOLAR1",7,2.88]
["TWISSL_6_SOLAR1",8,2.48]
["TWISSL_6_SOLAR1",9,2.2200000000000002]
["TWISSL_6_SOLAR1",10,1.48]
["TWISSL_6_SOLAR1",11,1.1399999999999999]
["TWISSL_6_SOLAR1",12,0.7]
["TX-ELK_6_ECKSR2",1,0]
["TX-ELK_6_ECKSR2",2,0]
["TX-ELK_6_ECKSR2",3,0]
["TX-ELK_6_ECKSR2",4,0]
["TX-ELK_6_ECKSR2",5,0]
["TX-ELK_6_ECKSR2",6,0]
["TX-ELK_6_ECKSR2",7,0]
["TX-ELK_6_ECKSR2",8,0]
["TX-ELK_6_ECKSR2",9,0]
["TX-ELK_6_ECKSR2",10,0]
["TX-ELK_6_ECKSR2",11,0]
["TX-ELK_6_ECKSR2",12,0]
["TX-ELK_6_SOLAR1",1,0]
["TX-ELK_6_SOLAR1",2,0]
["TX-ELK_6_SOLAR1",3,0]
["TX-ELK_6_SOLAR1",4,0]
["TX-ELK_6_SOLAR1",5,0]
["TX-ELK_6_SOLAR1",6,0]
["TX-ELK_6_SOLAR1",7,0]
["TX-ELK_6_SOLAR1",8,0]
["TX-ELK_6_SOLAR1",9,0]
["TX-ELK_6_SOLAR1",10,0]
["TX-ELK_6_SOLAR1",11,0]
["TX-ELK_6_SOLAR1",12,0]
["TXMCKT_6_UNIT",1,3.47]
["TXMCKT_6_UNIT",2,3.33]
["TXMCKT_6_UNIT",3,4.12]
["TXMCKT_6_UNIT",4,5.08]
["TXMCKT_6_UNIT",5,3.75]
["TXMCKT_6_UNIT",6,3.83]
["TXMCKT_6_UNIT",7,3.5]
["TXMCKT_6_UNIT",8,3.33]
["TXMCKT_6_UNIT",9,3.46]
["TXMCKT_6_UNIT",10,3.67]
["TXMCKT_6_UNIT",11,3.69]
["TXMCKT_6_UNIT",12,4.0999999999999996]
["UKIAH_7_LAKEMN",1,1.7]
["UKIAH_7_LAKEMN",2,1.7]
["UKIAH_7_LAKEMN",3,1.7]
["UKIAH_7_LAKEMN",4,1.7]
["UKIAH_7_LAKEMN",5,1.7]
["UKIAH_7_LAKEMN",6,1.7]
["UKIAH_7_LAKEMN",7,1.7]
["UKIAH_7_LAKEMN",8,1.7]
["UKIAH_7_LAKEMN",9,1.7]
["UKIAH_7_LAKEMN",10,1.7]
["UKIAH_7_LAKEMN",11,1.7]
["UKIAH_7_LAKEMN",12,1.7]
["ULTPCH_1_UNIT 1",1,17.989999999999998]
["ULTPCH_1_UNIT 1",2,18]
["ULTPCH_1_UNIT 1",3,14.98]
["ULTPCH_1_UNIT 1",4,16.8]
["ULTPCH_1_UNIT 1",5,17.739999999999998]
["ULTPCH_1_UNIT 1",6,14.2]
["ULTPCH_1_UNIT 1",7,17.149999999999999]
["ULTPCH_1_UNIT 1",8,17.98]
["ULTPCH_1_UNIT 1",9,17.61]
["ULTPCH_1_UNIT 1",10,16.55]
["ULTPCH_1_UNIT 1",11,14.91]
["ULTPCH_1_UNIT 1",12,17.809999999999999]
["ULTPFR_1_UNIT 1",1,23.98]
["ULTPFR_1_UNIT 1",2,23.03]
["ULTPFR_1_UNIT 1",3,24.3]
["ULTPFR_1_UNIT 1",4,21.66]
["ULTPFR_1_UNIT 1",5,23.54]
["ULTPFR_1_UNIT 1",6,24.04]
["ULTPFR_1_UNIT 1",7,24.01]
["ULTPFR_1_UNIT 1",8,19.46]
["ULTPFR_1_UNIT 1",9,15.53]
["ULTPFR_1_UNIT 1",10,15.75]
["ULTPFR_1_UNIT 1",11,23.88]
["ULTPFR_1_UNIT 1",12,22.8]
["ULTRCK_2_UNIT",1,15.36]
["ULTRCK_2_UNIT",2,20.65]
["ULTRCK_2_UNIT",3,15.39]
["ULTRCK_2_UNIT",4,23.85]
["ULTRCK_2_UNIT",5,21.52]
["ULTRCK_2_UNIT",6,23.36]
["ULTRCK_2_UNIT",7,21.69]
["ULTRCK_2_UNIT",8,23.11]
["ULTRCK_2_UNIT",9,19.79]
["ULTRCK_2_UNIT",10,23.06]
["ULTRCK_2_UNIT",11,23.55]
["ULTRCK_2_UNIT",12,22.98]
["UNCHEM_1_UNIT",1,12.22]
["UNCHEM_1_UNIT",2,12.39]
["UNCHEM_1_UNIT",3,13.5]
["UNCHEM_1_UNIT",4,12.81]
["UNCHEM_1_UNIT",5,12.87]
["UNCHEM_1_UNIT",6,13.38]
["UNCHEM_1_UNIT",7,12.36]
["UNCHEM_1_UNIT",8,13.41]
["UNCHEM_1_UNIT",9,13.6]
["UNCHEM_1_UNIT",10,12.54]
["UNCHEM_1_UNIT",11,13.36]
["UNCHEM_1_UNIT",12,13.35]
["UNOCAL_1_UNITS",1,4.41]
["UNOCAL_1_UNITS",2,5.37]
["UNOCAL_1_UNITS",3,5.61]
["UNOCAL_1_UNITS",4,4.0999999999999996]
["UNOCAL_1_UNITS",5,2.68]
["UNOCAL_1_UNITS",6,2.5099999999999998]
["UNOCAL_1_UNITS",7,2.3199999999999998]
["UNOCAL_1_UNITS",8,2.12]
["UNOCAL_1_UNITS",9,2.33]
["UNOCAL_1_UNITS",10,6.33]
["UNOCAL_1_UNITS",11,6.89]
["UNOCAL_1_UNITS",12,5.75]
["UNVRSY_1_UNIT 1",1,35.979999999999997]
["UNVRSY_1_UNIT 1",2,31.41]
["UNVRSY_1_UNIT 1",3,35.869999999999997]
["UNVRSY_1_UNIT 1",4,31.66]
["UNVRSY_1_UNIT 1",5,34.96]
["UNVRSY_1_UNIT 1",6,34.200000000000003]
["UNVRSY_1_UNIT 1",7,33.49]
["UNVRSY_1_UNIT 1",8,32.99]
["UNVRSY_1_UNIT 1",9,32.630000000000003]
["UNVRSY_1_UNIT 1",10,29.54]
["UNVRSY_1_UNIT 1",11,35.19]
["UNVRSY_1_UNIT 1",12,35.450000000000003]
["USWND2_1_WIND1",1,14.11]
["USWND2_1_WIND1",2,15.14]
["USWND2_1_WIND1",3,13.5]
["USWND2_1_WIND1",4,14.26]
["USWND2_1_WIND1",5,14.75]
["USWND2_1_WIND1",6,10.88]
["USWND2_1_WIND1",7,9.68]
["USWND2_1_WIND1",8,9.09]
["USWND2_1_WIND1",9,9.33]
["USWND2_1_WIND1",10,7.82]
["USWND2_1_WIND1",11,9.8800000000000008]
["USWND2_1_WIND1",12,12.63]
["USWND2_1_WIND2",1,14.11]
["USWND2_1_WIND2",2,15.14]
["USWND2_1_WIND2",3,13.5]
["USWND2_1_WIND2",4,14.26]
["USWND2_1_WIND2",5,14.75]
["USWND2_1_WIND2",6,10.88]
["USWND2_1_WIND2",7,9.68]
["USWND2_1_WIND2",8,9.09]
["USWND2_1_WIND2",9,9.33]
["USWND2_1_WIND2",10,7.82]
["USWND2_1_WIND2",11,9.8800000000000008]
["USWND2_1_WIND2",12,12.63]
["USWND2_1_WIND3",1,15.1]
["USWND2_1_WIND3",2,16.21]
["USWND2_1_WIND3",3,14.45]
["USWND2_1_WIND3",4,15.27]
["USWND2_1_WIND3",5,15.8]
["USWND2_1_WIND3",6,11.65]
["USWND2_1_WIND3",7,10.36]
["USWND2_1_WIND3",8,9.73]
["USWND2_1_WIND3",9,9.99]
["USWND2_1_WIND3",10,8.3800000000000008]
["USWND2_1_WIND3",11,10.58]
["USWND2_1_WIND3",12,13.52]
["USWND4_2_UNIT2",1,7.4]
["USWND4_2_UNIT2",2,7.4]
["USWND4_2_UNIT2",3,7.35]
["USWND4_2_UNIT2",4,6.41]
["USWND4_2_UNIT2",5,7.4]
["USWND4_2_UNIT2",6,7.4]
["USWND4_2_UNIT2",7,7.4]
["USWND4_2_UNIT2",8,7.4]
["USWND4_2_UNIT2",9,7.4]
["USWND4_2_UNIT2",10,7.23]
["USWND4_2_UNIT2",11,7.4]
["USWND4_2_UNIT2",12,7.4]
["USWNDR_2_LABWD1",1,2.96]
["USWNDR_2_LABWD1",2,3.17]
["USWNDR_2_LABWD1",3,2.83]
["USWNDR_2_LABWD1",4,2.99]
["USWNDR_2_LABWD1",5,3.09]
["USWNDR_2_LABWD1",6,2.2799999999999998]
["USWNDR_2_LABWD1",7,2.0299999999999998]
["USWNDR_2_LABWD1",8,1.9]
["USWNDR_2_LABWD1",9,1.96]
["USWNDR_2_LABWD1",10,1.64]
["USWNDR_2_LABWD1",11,2.0699999999999998]
["USWNDR_2_LABWD1",12,2.65]
["USWNDR_2_SMUD",1,33.549999999999997]
["USWNDR_2_SMUD",2,36]
["USWNDR_2_SMUD",3,32.11]
["USWNDR_2_SMUD",4,33.92]
["USWNDR_2_SMUD",5,35.090000000000003]
["USWNDR_2_SMUD",6,25.89]
["USWNDR_2_SMUD",7,23.02]
["USWNDR_2_SMUD",8,21.62]
["USWNDR_2_SMUD",9,22.2]
["USWNDR_2_SMUD",10,18.600000000000001]
["USWNDR_2_SMUD",11,23.5]
["USWNDR_2_SMUD",12,30.04]
["USWNDR_2_SMUD2",1,41.97]
["USWNDR_2_SMUD2",2,45.03]
["USWNDR_2_SMUD2",3,40.159999999999997]
["USWNDR_2_SMUD2",4,42.42]
["USWNDR_2_SMUD2",5,43.89]
["USWNDR_2_SMUD2",6,32.380000000000003]
["USWNDR_2_SMUD2",7,28.79]
["USWNDR_2_SMUD2",8,27.04]
["USWNDR_2_SMUD2",9,27.77]
["USWNDR_2_SMUD2",10,23.27]
["USWNDR_2_SMUD2",11,29.4]
["USWNDR_2_SMUD2",12,37.57]
["USWPFK_6_FRICK",1,3.28]
["USWPFK_6_FRICK",2,3.52]
["USWPFK_6_FRICK",3,3.14]
["USWPFK_6_FRICK",4,3.32]
["USWPFK_6_FRICK",5,3.43]
["USWPFK_6_FRICK",6,2.5299999999999998]
["USWPFK_6_FRICK",7,2.25]
["USWPFK_6_FRICK",8,2.12]
["USWPFK_6_FRICK",9,2.17]
["USWPFK_6_FRICK",10,1.82]
["USWPFK_6_FRICK",11,2.2999999999999998]
["USWPFK_6_FRICK",12,2.94]
["USWPJR_2_UNITS",1,25.68]
["USWPJR_2_UNITS",2,27.55]
["USWPJR_2_UNITS",3,24.57]
["USWPJR_2_UNITS",4,25.96]
["USWPJR_2_UNITS",5,26.86]
["USWPJR_2_UNITS",6,19.809999999999999]
["USWPJR_2_UNITS",7,17.62]
["USWPJR_2_UNITS",8,16.55]
["USWPJR_2_UNITS",9,16.989999999999998]
["USWPJR_2_UNITS",10,14.24]
["USWPJR_2_UNITS",11,17.989999999999998]
["USWPJR_2_UNITS",12,22.99]
["VACADX_1_SOLAR",1,0.01]
["VACADX_1_SOLAR",2,0.08]
["VACADX_1_SOLAR",3,0.09]
["VACADX_1_SOLAR",4,0.11]
["VACADX_1_SOLAR",5,0.16]
["VACADX_1_SOLAR",6,0.33]
["VACADX_1_SOLAR",7,0.36]
["VACADX_1_SOLAR",8,0.31]
["VACADX_1_SOLAR",9,0.28000000000000003]
["VACADX_1_SOLAR",10,0.19]
["VACADX_1_SOLAR",11,0.14000000000000001]
["VACADX_1_SOLAR",12,0.09]
["VACADX_1_UNITA1",1,50.61]
["VACADX_1_UNITA1",2,50.61]
["VACADX_1_UNITA1",3,50.61]
["VACADX_1_UNITA1",4,50.61]
["VACADX_1_UNITA1",5,50.61]
["VACADX_1_UNITA1",6,50.61]
["VACADX_1_UNITA1",7,50.61]
["VACADX_1_UNITA1",8,50.61]
["VACADX_1_UNITA1",9,50.61]
["VACADX_1_UNITA1",10,50.61]
["VACADX_1_UNITA1",11,50.61]
["VACADX_1_UNITA1",12,50.61]
["VALLEY_5_PERRIS",1,7.94]
["VALLEY_5_PERRIS",2,7.94]
["VALLEY_5_PERRIS",3,7.94]
["VALLEY_5_PERRIS",4,7.94]
["VALLEY_5_PERRIS",5,7.94]
["VALLEY_5_PERRIS",6,7.94]
["VALLEY_5_PERRIS",7,7.94]
["VALLEY_5_PERRIS",8,7.94]
["VALLEY_5_PERRIS",9,7.94]
["VALLEY_5_PERRIS",10,7.94]
["VALLEY_5_PERRIS",11,7.94]
["VALLEY_5_PERRIS",12,7.94]
["VALLEY_5_REDMTN",1,0]
["VALLEY_5_REDMTN",2,0]
["VALLEY_5_REDMTN",3,0]
["VALLEY_5_REDMTN",4,0]
["VALLEY_5_REDMTN",5,0]
["VALLEY_5_REDMTN",6,0]
["VALLEY_5_REDMTN",7,0]
["VALLEY_5_REDMTN",8,1.21]
["VALLEY_5_REDMTN",9,1.33]
["VALLEY_5_REDMTN",10,1.44]
["VALLEY_5_REDMTN",11,1.31]
["VALLEY_5_REDMTN",12,1.01]
["VALLEY_5_SOLAR1",1,0]
["VALLEY_5_SOLAR1",2,0]
["VALLEY_5_SOLAR1",3,0]
["VALLEY_5_SOLAR1",4,0]
["VALLEY_5_SOLAR1",5,0]
["VALLEY_5_SOLAR1",6,0]
["VALLEY_5_SOLAR1",7,0]
["VALLEY_5_SOLAR1",8,0]
["VALLEY_5_SOLAR1",9,0]
["VALLEY_5_SOLAR1",10,0]
["VALLEY_5_SOLAR1",11,0]
["VALLEY_5_SOLAR1",12,0]
["VALLEY_5_SOLAR2",1,0.08]
["VALLEY_5_SOLAR2",2,0.6]
["VALLEY_5_SOLAR2",3,0.7]
["VALLEY_5_SOLAR2",4,0.88]
["VALLEY_5_SOLAR2",5,1.28]
["VALLEY_5_SOLAR2",6,2.62]
["VALLEY_5_SOLAR2",7,2.88]
["VALLEY_5_SOLAR2",8,2.48]
["VALLEY_5_SOLAR2",9,2.2200000000000002]
["VALLEY_5_SOLAR2",10,1.48]
["VALLEY_5_SOLAR2",11,1.1399999999999999]
["VALLEY_5_SOLAR2",12,0.7]
["VALTNE_2_AVASR1",1,0.4]
["VALTNE_2_AVASR1",2,3]
["VALTNE_2_AVASR1",3,3.5]
["VALTNE_2_AVASR1",4,4.4000000000000004]
["VALTNE_2_AVASR1",5,6.4]
["VALTNE_2_AVASR1",6,13.1]
["VALTNE_2_AVASR1",7,14.4]
["VALTNE_2_AVASR1",8,12.4]
["VALTNE_2_AVASR1",9,11.1]
["VALTNE_2_AVASR1",10,7.4]
["VALTNE_2_AVASR1",11,5.7]
["VALTNE_2_AVASR1",12,3.5]
["VALTNE_2_TBBBT1",2,19.350000000000001]
["VALTNE_2_TBBBT1",3,19.62]
["VALTNE_2_TBBBT1",4,20.14]
["VALTNE_2_TBBBT1",5,21.16]
["VALTNE_2_TBBBT1",6,24.54]
["VALTNE_2_TBBBT1",7,25.18]
["VALTNE_2_TBBBT1",8,24.11]
["VALTNE_2_TBBBT1",9,23.32]
["VALTNE_2_TBBBT1",10,21.43]
["VALTNE_2_TBBBT1",11,20.45]
["VALTNE_2_TBBBT1",12,19.3]
["VALTNE_2_TRSBT1",2,23.62]
["VALTNE_2_TRSBT1",3,23.95]
["VALTNE_2_TRSBT1",4,24.58]
["VALTNE_2_TRSBT1",5,25.8]
["VALTNE_2_TRSBT1",6,29.87]
["VALTNE_2_TRSBT1",7,30.65]
["VALTNE_2_TRSBT1",8,29.36]
["VALTNE_2_TRSBT1",9,28.4]
["VALTNE_2_TRSBT1",10,26.13]
["VALTNE_2_TRSBT1",11,24.94]
["VALTNE_2_TRSBT1",12,23.55]
["VEAVST_1_SOLAR",1,0]
["VEAVST_1_SOLAR",2,0]
["VEAVST_1_SOLAR",3,0]
["VEAVST_1_SOLAR",4,0]
["VEAVST_1_SOLAR",5,0]
["VEAVST_1_SOLAR",6,0]
["VEAVST_1_SOLAR",7,0]
["VEAVST_1_SOLAR",8,0]
["VEAVST_1_SOLAR",9,0]
["VEAVST_1_SOLAR",10,0]
["VEAVST_1_SOLAR",11,0]
["VEAVST_1_SOLAR",12,0]
["VEDDER_1_SEKERN",1,0.33]
["VEDDER_1_SEKERN",2,2.67]
["VEDDER_1_SEKERN",3,2.78]
["VEDDER_1_SEKERN",4,2.1]
["VEDDER_1_SEKERN",5,2.12]
["VEDDER_1_SEKERN",6,1.27]
["VEDDER_1_SEKERN",7,2.02]
["VEDDER_1_SEKERN",8,2.37]
["VEDDER_1_SEKERN",9,3.45]
["VEDDER_1_SEKERN",10,3.51]
["VEDDER_1_SEKERN",11,2.38]
["VEDDER_1_SEKERN",12,1.8]
["VEGA_6_SOLAR1",1,0]
["VEGA_6_SOLAR1",2,0]
["VEGA_6_SOLAR1",3,0]
["VEGA_6_SOLAR1",4,0]
["VEGA_6_SOLAR1",5,0]
["VEGA_6_SOLAR1",6,0]
["VEGA_6_SOLAR1",7,0]
["VEGA_6_SOLAR1",8,0]
["VEGA_6_SOLAR1",9,0]
["VEGA_6_SOLAR1",10,0]
["VEGA_6_SOLAR1",11,0]
["VEGA_6_SOLAR1",12,0]
["VENWD_1_WIND3",1,7.87]
["VENWD_1_WIND3",2,8.3699999999999992]
["VENWD_1_WIND3",3,7.35]
["VENWD_1_WIND3",4,7.04]
["VENWD_1_WIND3",5,7.49]
["VENWD_1_WIND3",6,6.87]
["VENWD_1_WIND3",7,6.38]
["VENWD_1_WIND3",8,4.8499999999999996]
["VENWD_1_WIND3",9,5.01]
["VENWD_1_WIND3",10,4.6500000000000004]
["VENWD_1_WIND3",11,6.26]
["VENWD_1_WIND3",12,7.58]
["VERNON_6_GONZL1",1,5.75]
["VERNON_6_GONZL1",2,5.75]
["VERNON_6_GONZL1",3,5.75]
["VERNON_6_GONZL1",4,5.75]
["VERNON_6_GONZL1",5,5.75]
["VERNON_6_GONZL1",6,5.75]
["VERNON_6_GONZL1",7,5.75]
["VERNON_6_GONZL1",8,5.75]
["VERNON_6_GONZL1",9,5.75]
["VERNON_6_GONZL1",10,5.75]
["VERNON_6_GONZL1",11,5.75]
["VERNON_6_GONZL1",12,5.75]
["VERNON_6_GONZL2",1,5.75]
["VERNON_6_GONZL2",2,5.75]
["VERNON_6_GONZL2",3,5.75]
["VERNON_6_GONZL2",4,5.75]
["VERNON_6_GONZL2",5,5.75]
["VERNON_6_GONZL2",6,5.75]
["VERNON_6_GONZL2",7,5.75]
["VERNON_6_GONZL2",8,5.75]
["VERNON_6_GONZL2",9,5.75]
["VERNON_6_GONZL2",10,5.75]
["VERNON_6_GONZL2",11,5.75]
["VERNON_6_GONZL2",12,5.75]
["VERNON_6_MALBRG",1,134]
["VERNON_6_MALBRG",2,134]
["VERNON_6_MALBRG",3,134]
["VERNON_6_MALBRG",4,134]
["VERNON_6_MALBRG",5,134]
["VERNON_6_MALBRG",6,134]
["VERNON_6_MALBRG",7,134]
["VERNON_6_MALBRG",8,134]
["VERNON_6_MALBRG",9,134]
["VERNON_6_MALBRG",10,134]
["VERNON_6_MALBRG",11,134]
["VERNON_6_MALBRG",12,134]
["VESTAL_2_KERN",1,10.18]
["VESTAL_2_KERN",2,16.11]
["VESTAL_2_KERN",3,15.62]
["VESTAL_2_KERN",4,24.4]
["VESTAL_2_KERN",5,28.48]
["VESTAL_2_KERN",6,20.58]
["VESTAL_2_KERN",7,12.19]
["VESTAL_2_KERN",8,10.18]
["VESTAL_2_KERN",9,5.64]
["VESTAL_2_KERN",10,4.37]
["VESTAL_2_KERN",11,7.7]
["VESTAL_2_KERN",12,9.64]
["VESTAL_2_RTS042",1,0]
["VESTAL_2_RTS042",2,0]
["VESTAL_2_RTS042",3,0]
["VESTAL_2_RTS042",4,0]
["VESTAL_2_RTS042",5,0]
["VESTAL_2_RTS042",6,0]
["VESTAL_2_RTS042",7,0]
["VESTAL_2_RTS042",8,0]
["VESTAL_2_RTS042",9,0]
["VESTAL_2_RTS042",10,0]
["VESTAL_2_RTS042",11,0]
["VESTAL_2_RTS042",12,0]
["VESTAL_2_SOLAR1",1,0.08]
["VESTAL_2_SOLAR1",2,0.6]
["VESTAL_2_SOLAR1",3,0.7]
["VESTAL_2_SOLAR1",4,0.88]
["VESTAL_2_SOLAR1",5,1.28]
["VESTAL_2_SOLAR1",6,2.62]
["VESTAL_2_SOLAR1",7,2.88]
["VESTAL_2_SOLAR1",8,2.48]
["VESTAL_2_SOLAR1",9,2.2200000000000002]
["VESTAL_2_SOLAR1",10,1.48]
["VESTAL_2_SOLAR1",11,1.1399999999999999]
["VESTAL_2_SOLAR1",12,0.7]
["VESTAL_2_SOLAR2",1,0.06]
["VESTAL_2_SOLAR2",2,0.42]
["VESTAL_2_SOLAR2",3,0.49]
["VESTAL_2_SOLAR2",4,0.62]
["VESTAL_2_SOLAR2",5,0.9]
["VESTAL_2_SOLAR2",6,1.83]
["VESTAL_2_SOLAR2",7,2.02]
["VESTAL_2_SOLAR2",8,1.74]
["VESTAL_2_SOLAR2",9,1.55]
["VESTAL_2_SOLAR2",10,1.04]
["VESTAL_2_SOLAR2",11,0.8]
["VESTAL_2_SOLAR2",12,0.49]
["VESTAL_2_TS5SR1",1,0.22]
["VESTAL_2_TS5SR1",2,1.67]
["VESTAL_2_TS5SR1",3,1.95]
["VESTAL_2_TS5SR1",4,2.46]
["VESTAL_2_TS5SR1",5,3.57]
["VESTAL_2_TS5SR1",6,7.31]
["VESTAL_2_TS5SR1",7,8.0399999999999991]
["VESTAL_2_TS5SR1",8,6.92]
["VESTAL_2_TS5SR1",9,6.2]
["VESTAL_2_TS5SR1",10,4.13]
["VESTAL_2_TS5SR1",11,3.18]
["VESTAL_2_TS5SR1",12,1.95]
["VESTAL_2_UNIT1",1,3.33]
["VESTAL_2_UNIT1",2,2.5499999999999998]
["VESTAL_2_UNIT1",3,3.46]
["VESTAL_2_UNIT1",4,2.8]
["VESTAL_2_UNIT1",5,3.07]
["VESTAL_2_UNIT1",6,2.88]
["VESTAL_2_UNIT1",7,2.93]
["VESTAL_2_UNIT1",8,2.83]
["VESTAL_2_UNIT1",9,3.08]
["VESTAL_2_UNIT1",10,3.44]
["VESTAL_2_UNIT1",11,3.56]
["VESTAL_2_UNIT1",12,2.93]
["VESTAL_2_WELLHD",1,49]
["VESTAL_2_WELLHD",2,49]
["VESTAL_2_WELLHD",3,49]
["VESTAL_2_WELLHD",4,49]
["VESTAL_2_WELLHD",5,49]
["VESTAL_2_WELLHD",6,49]
["VESTAL_2_WELLHD",7,49]
["VESTAL_2_WELLHD",8,49]
["VESTAL_2_WELLHD",9,49]
["VESTAL_2_WELLHD",10,49]
["VESTAL_2_WELLHD",11,49]
["VESTAL_2_WELLHD",12,49]
["VESTAL_6_QF",1,6.78]
["VESTAL_6_QF",2,4.25]
["VESTAL_6_QF",3,4.8899999999999997]
["VESTAL_6_QF",4,5.91]
["VESTAL_6_QF",5,5.96]
["VESTAL_6_QF",6,6.24]
["VESTAL_6_QF",7,5.84]
["VESTAL_6_QF",8,5.15]
["VESTAL_6_QF",9,5.07]
["VESTAL_6_QF",10,3.99]
["VESTAL_6_QF",11,4.0599999999999996]
["VESTAL_6_QF",12,4.57]
["VICTOR_1_CREST",1,0]
["VICTOR_1_CREST",2,0]
["VICTOR_1_CREST",3,0]
["VICTOR_1_CREST",4,0]
["VICTOR_1_CREST",5,0]
["VICTOR_1_CREST",6,0]
["VICTOR_1_CREST",7,0]
["VICTOR_1_CREST",8,0]
["VICTOR_1_CREST",9,0]
["VICTOR_1_CREST",10,0]
["VICTOR_1_CREST",11,0]
["VICTOR_1_CREST",12,0]
["VICTOR_1_EXSLRA",1,0.01]
["VICTOR_1_EXSLRA",2,0.06]
["VICTOR_1_EXSLRA",3,7.0000000000000007E-2]
["VICTOR_1_EXSLRA",4,0.09]
["VICTOR_1_EXSLRA",5,0.13]
["VICTOR_1_EXSLRA",6,0.26]
["VICTOR_1_EXSLRA",7,0.28999999999999998]
["VICTOR_1_EXSLRA",8,0.25]
["VICTOR_1_EXSLRA",9,0.22]
["VICTOR_1_EXSLRA",10,0.15]
["VICTOR_1_EXSLRA",11,0.11]
["VICTOR_1_EXSLRA",12,7.0000000000000007E-2]
["VICTOR_1_EXSLRB",1,0.01]
["VICTOR_1_EXSLRB",2,0.06]
["VICTOR_1_EXSLRB",3,7.0000000000000007E-2]
["VICTOR_1_EXSLRB",4,0.09]
["VICTOR_1_EXSLRB",5,0.13]
["VICTOR_1_EXSLRB",6,0.26]
["VICTOR_1_EXSLRB",7,0.28999999999999998]
["VICTOR_1_EXSLRB",8,0.25]
["VICTOR_1_EXSLRB",9,0.22]
["VICTOR_1_EXSLRB",10,0.15]
["VICTOR_1_EXSLRB",11,0.11]
["VICTOR_1_EXSLRB",12,7.0000000000000007E-2]
["VICTOR_1_LVSLR1",1,0]
["VICTOR_1_LVSLR1",2,0]
["VICTOR_1_LVSLR1",3,0]
["VICTOR_1_LVSLR1",4,0]
["VICTOR_1_LVSLR1",5,0]
["VICTOR_1_LVSLR1",6,0]
["VICTOR_1_LVSLR1",7,0]
["VICTOR_1_LVSLR1",8,0]
["VICTOR_1_LVSLR1",9,0]
["VICTOR_1_LVSLR1",10,0]
["VICTOR_1_LVSLR1",11,0]
["VICTOR_1_LVSLR1",12,0]
["VICTOR_1_LVSLR2",1,0]
["VICTOR_1_LVSLR2",2,0]
["VICTOR_1_LVSLR2",3,0]
["VICTOR_1_LVSLR2",4,0]
["VICTOR_1_LVSLR2",5,0]
["VICTOR_1_LVSLR2",6,0]
["VICTOR_1_LVSLR2",7,0]
["VICTOR_1_LVSLR2",8,0]
["VICTOR_1_LVSLR2",9,0]
["VICTOR_1_LVSLR2",10,0]
["VICTOR_1_LVSLR2",11,0]
["VICTOR_1_LVSLR2",12,0]
["VICTOR_1_SLRHES",1,0]
["VICTOR_1_SLRHES",2,0]
["VICTOR_1_SLRHES",3,0]
["VICTOR_1_SLRHES",4,0]
["VICTOR_1_SLRHES",5,0]
["VICTOR_1_SLRHES",6,0]
["VICTOR_1_SLRHES",7,0]
["VICTOR_1_SLRHES",8,0]
["VICTOR_1_SLRHES",9,0]
["VICTOR_1_SLRHES",10,0]
["VICTOR_1_SLRHES",11,0]
["VICTOR_1_SLRHES",12,0]
["VICTOR_1_SOLAR1",1,0]
["VICTOR_1_SOLAR1",2,0]
["VICTOR_1_SOLAR1",3,0]
["VICTOR_1_SOLAR1",4,0]
["VICTOR_1_SOLAR1",5,0]
["VICTOR_1_SOLAR1",6,0]
["VICTOR_1_SOLAR1",7,0]
["VICTOR_1_SOLAR1",8,0]
["VICTOR_1_SOLAR1",9,0]
["VICTOR_1_SOLAR1",10,0]
["VICTOR_1_SOLAR1",11,0]
["VICTOR_1_SOLAR1",12,0]
["VICTOR_1_SOLAR2",1,0]
["VICTOR_1_SOLAR2",2,0]
["VICTOR_1_SOLAR2",3,0]
["VICTOR_1_SOLAR2",4,0]
["VICTOR_1_SOLAR2",5,0]
["VICTOR_1_SOLAR2",6,0]
["VICTOR_1_SOLAR2",7,0]
["VICTOR_1_SOLAR2",8,0]
["VICTOR_1_SOLAR2",9,0]
["VICTOR_1_SOLAR2",10,0]
["VICTOR_1_SOLAR2",11,0]
["VICTOR_1_SOLAR2",12,0]
["VICTOR_1_SOLAR3",1,0.03]
["VICTOR_1_SOLAR3",2,0.21]
["VICTOR_1_SOLAR3",3,0.25]
["VICTOR_1_SOLAR3",4,0.31]
["VICTOR_1_SOLAR3",5,0.45]
["VICTOR_1_SOLAR3",6,0.92]
["VICTOR_1_SOLAR3",7,1.01]
["VICTOR_1_SOLAR3",8,0.87]
["VICTOR_1_SOLAR3",9,0.78]
["VICTOR_1_SOLAR3",10,0.52]
["VICTOR_1_SOLAR3",11,0.4]
["VICTOR_1_SOLAR3",12,0.25]
["VICTOR_1_SOLAR4",1,0]
["VICTOR_1_SOLAR4",2,0]
["VICTOR_1_SOLAR4",3,0]
["VICTOR_1_SOLAR4",4,0]
["VICTOR_1_SOLAR4",5,0]
["VICTOR_1_SOLAR4",6,0]
["VICTOR_1_SOLAR4",7,0]
["VICTOR_1_SOLAR4",8,0]
["VICTOR_1_SOLAR4",9,0]
["VICTOR_1_SOLAR4",10,0]
["VICTOR_1_SOLAR4",11,0]
["VICTOR_1_SOLAR4",12,0]
["VICTOR_1_VDRYFA",1,0.02]
["VICTOR_1_VDRYFA",2,0.15]
["VICTOR_1_VDRYFA",3,0.18]
["VICTOR_1_VDRYFA",4,0.22]
["VICTOR_1_VDRYFA",5,0.32]
["VICTOR_1_VDRYFA",6,0.66]
["VICTOR_1_VDRYFA",7,0.72]
["VICTOR_1_VDRYFA",8,0.62]
["VICTOR_1_VDRYFA",9,0.56000000000000005]
["VICTOR_1_VDRYFA",10,0.37]
["VICTOR_1_VDRYFA",11,0.28999999999999998]
["VICTOR_1_VDRYFA",12,0.18]
["VICTOR_1_VDRYFB",1,0]
["VICTOR_1_VDRYFB",2,0]
["VICTOR_1_VDRYFB",3,0]
["VICTOR_1_VDRYFB",4,0]
["VICTOR_1_VDRYFB",5,0]
["VICTOR_1_VDRYFB",6,0]
["VICTOR_1_VDRYFB",7,0]
["VICTOR_1_VDRYFB",8,0]
["VICTOR_1_VDRYFB",9,0]
["VICTOR_1_VDRYFB",10,0]
["VICTOR_1_VDRYFB",11,0]
["VICTOR_1_VDRYFB",12,0]
["VILLPK_2_VALLYV",1,4.0999999999999996]
["VILLPK_2_VALLYV",2,4.0999999999999996]
["VILLPK_2_VALLYV",3,4.0999999999999996]
["VILLPK_2_VALLYV",4,4.0999999999999996]
["VILLPK_2_VALLYV",5,4.0999999999999996]
["VILLPK_2_VALLYV",6,4.0999999999999996]
["VILLPK_2_VALLYV",7,4.0999999999999996]
["VILLPK_2_VALLYV",8,4.0999999999999996]
["VILLPK_2_VALLYV",9,4.0999999999999996]
["VILLPK_2_VALLYV",10,4.0999999999999996]
["VILLPK_2_VALLYV",11,4.0999999999999996]
["VILLPK_2_VALLYV",12,4.0999999999999996]
["VILLPK_6_MWDYOR",1,1.6]
["VILLPK_6_MWDYOR",2,2.8]
["VILLPK_6_MWDYOR",3,2]
["VILLPK_6_MWDYOR",4,2.4]
["VILLPK_6_MWDYOR",5,2.8]
["VILLPK_6_MWDYOR",6,2.8]
["VILLPK_6_MWDYOR",7,4]
["VILLPK_6_MWDYOR",8,4]
["VILLPK_6_MWDYOR",9,3.92]
["VILLPK_6_MWDYOR",10,0]
["VILLPK_6_MWDYOR",11,0]
["VILLPK_6_MWDYOR",12,0]
["VISTA_2_FCELL",1,0]
["VISTA_2_FCELL",2,0]
["VISTA_2_FCELL",3,0]
["VISTA_2_FCELL",4,0]
["VISTA_2_FCELL",5,0]
["VISTA_2_FCELL",6,0]
["VISTA_2_FCELL",7,0]
["VISTA_2_FCELL",8,0]
["VISTA_2_FCELL",9,0]
["VISTA_2_FCELL",10,0]
["VISTA_2_FCELL",11,0]
["VISTA_2_FCELL",12,0]
["VISTA_2_RIALTO",1,0]
["VISTA_2_RIALTO",2,0.03]
["VISTA_2_RIALTO",3,0.04]
["VISTA_2_RIALTO",4,0.04]
["VISTA_2_RIALTO",5,0.06]
["VISTA_2_RIALTO",6,0.13]
["VISTA_2_RIALTO",7,0.14000000000000001]
["VISTA_2_RIALTO",8,0.12]
["VISTA_2_RIALTO",9,0.11]
["VISTA_2_RIALTO",10,7.0000000000000007E-2]
["VISTA_2_RIALTO",11,0.06]
["VISTA_2_RIALTO",12,0.04]
["VISTA_2_RTS028",1,0.01]
["VISTA_2_RTS028",2,0.11]
["VISTA_2_RTS028",3,0.12]
["VISTA_2_RTS028",4,0.15]
["VISTA_2_RTS028",5,0.22]
["VISTA_2_RTS028",6,0.46]
["VISTA_2_RTS028",7,0.5]
["VISTA_2_RTS028",8,0.43]
["VISTA_2_RTS028",9,0.39]
["VISTA_2_RTS028",10,0.26]
["VISTA_2_RTS028",11,0.2]
["VISTA_2_RTS028",12,0.12]
["VISTA_6_QF",1,0]
["VISTA_6_QF",2,0]
["VISTA_6_QF",3,0]
["VISTA_6_QF",4,0.04]
["VISTA_6_QF",5,0.06]
["VISTA_6_QF",6,7.0000000000000007E-2]
["VISTA_6_QF",7,0.11]
["VISTA_6_QF",8,0.11]
["VISTA_6_QF",9,0.1]
["VISTA_6_QF",10,0.05]
["VISTA_6_QF",11,0.03]
["VISTA_6_QF",12,0.02]
["VISTRA_5_DALBT1",1,100]
["VISTRA_5_DALBT1",2,100]
["VISTRA_5_DALBT1",3,100]
["VISTRA_5_DALBT1",4,100]
["VISTRA_5_DALBT1",5,100]
["VISTRA_5_DALBT1",6,100]
["VISTRA_5_DALBT1",7,100]
["VISTRA_5_DALBT1",8,100]
["VISTRA_5_DALBT1",9,100]
["VISTRA_5_DALBT1",10,100]
["VISTRA_5_DALBT1",11,100]
["VISTRA_5_DALBT1",12,100]
["VISTRA_5_DALBT2",1,100]
["VISTRA_5_DALBT2",2,100]
["VISTRA_5_DALBT2",3,100]
["VISTRA_5_DALBT2",4,100]
["VISTRA_5_DALBT2",5,100]
["VISTRA_5_DALBT2",6,100]
["VISTRA_5_DALBT2",7,100]
["VISTRA_5_DALBT2",8,100]
["VISTRA_5_DALBT2",9,100]
["VISTRA_5_DALBT2",10,100]
["VISTRA_5_DALBT2",11,100]
["VISTRA_5_DALBT2",12,100]
["VISTRA_5_DALBT3",1,100]
["VISTRA_5_DALBT3",2,100]
["VISTRA_5_DALBT3",3,100]
["VISTRA_5_DALBT3",4,100]
["VISTRA_5_DALBT3",5,100]
["VISTRA_5_DALBT3",6,100]
["VISTRA_5_DALBT3",7,100]
["VISTRA_5_DALBT3",8,100]
["VISTRA_5_DALBT3",9,100]
["VISTRA_5_DALBT3",10,100]
["VISTRA_5_DALBT3",11,100]
["VISTRA_5_DALBT3",12,100]
["VISTRA_5_DALBT4",1,100]
["VISTRA_5_DALBT4",2,100]
["VISTRA_5_DALBT4",3,100]
["VISTRA_5_DALBT4",4,100]
["VISTRA_5_DALBT4",5,100]
["VISTRA_5_DALBT4",6,100]
["VISTRA_5_DALBT4",7,100]
["VISTRA_5_DALBT4",8,100]
["VISTRA_5_DALBT4",9,100]
["VISTRA_5_DALBT4",10,100]
["VISTRA_5_DALBT4",11,100]
["VISTRA_5_DALBT4",12,100]
["VISTRA_5_PLABT1",6,100.4]
["VISTRA_5_PLABT1",7,100.4]
["VISTRA_5_PLABT1",8,100.4]
["VISTRA_5_PLABT1",9,100.4]
["VISTRA_5_PLABT1",10,100.4]
["VISTRA_5_PLABT1",11,100.4]
["VISTRA_5_PLABT1",12,100.4]
["VISTRA_5_PLABT3",6,74.599999999999994]
["VISTRA_5_PLABT3",7,74.599999999999994]
["VISTRA_5_PLABT3",8,74.599999999999994]
["VISTRA_5_PLABT3",9,74.599999999999994]
["VISTRA_5_PLABT3",10,74.599999999999994]
["VISTRA_5_PLABT3",11,74.599999999999994]
["VISTRA_5_PLABT3",12,74.599999999999994]
["VLCNTR_6_VCEBT1",1,54]
["VLCNTR_6_VCEBT1",2,54]
["VLCNTR_6_VCEBT1",3,54]
["VLCNTR_6_VCEBT1",4,54]
["VLCNTR_6_VCEBT1",5,54]
["VLCNTR_6_VCEBT1",6,54]
["VLCNTR_6_VCEBT1",7,54]
["VLCNTR_6_VCEBT1",8,54]
["VLCNTR_6_VCEBT1",9,54]
["VLCNTR_6_VCEBT1",10,54]
["VLCNTR_6_VCEBT1",11,54]
["VLCNTR_6_VCEBT1",12,54]
["VLCNTR_6_VCEBT2",1,50]
["VLCNTR_6_VCEBT2",2,50]
["VLCNTR_6_VCEBT2",3,50]
["VLCNTR_6_VCEBT2",4,50]
["VLCNTR_6_VCEBT2",5,50]
["VLCNTR_6_VCEBT2",6,50]
["VLCNTR_6_VCEBT2",7,50]
["VLCNTR_6_VCEBT2",8,50]
["VLCNTR_6_VCEBT2",9,50]
["VLCNTR_6_VCEBT2",10,50]
["VLCNTR_6_VCEBT2",11,50]
["VLCNTR_6_VCEBT2",12,50]
["VLCNTR_6_VCSLR",1,0.01]
["VLCNTR_6_VCSLR",2,7.0000000000000007E-2]
["VLCNTR_6_VCSLR",3,0.08]
["VLCNTR_6_VCSLR",4,0.1]
["VLCNTR_6_VCSLR",5,0.15]
["VLCNTR_6_VCSLR",6,0.31]
["VLCNTR_6_VCSLR",7,0.34]
["VLCNTR_6_VCSLR",8,0.28999999999999998]
["VLCNTR_6_VCSLR",9,0.26]
["VLCNTR_6_VCSLR",10,0.17]
["VLCNTR_6_VCSLR",11,0.13]
["VLCNTR_6_VCSLR",12,0.08]
["VLCNTR_6_VCSLR1",1,0.01]
["VLCNTR_6_VCSLR1",2,0.08]
["VLCNTR_6_VCSLR1",3,0.09]
["VLCNTR_6_VCSLR1",4,0.11]
["VLCNTR_6_VCSLR1",5,0.16]
["VLCNTR_6_VCSLR1",6,0.33]
["VLCNTR_6_VCSLR1",7,0.36]
["VLCNTR_6_VCSLR1",8,0.31]
["VLCNTR_6_VCSLR1",9,0.28000000000000003]
["VLCNTR_6_VCSLR1",10,0.19]
["VLCNTR_6_VCSLR1",11,0.14000000000000001]
["VLCNTR_6_VCSLR1",12,0.09]
["VLCNTR_6_VCSLR2",1,0.02]
["VLCNTR_6_VCSLR2",2,0.15]
["VLCNTR_6_VCSLR2",3,0.18]
["VLCNTR_6_VCSLR2",4,0.22]
["VLCNTR_6_VCSLR2",5,0.32]
["VLCNTR_6_VCSLR2",6,0.66]
["VLCNTR_6_VCSLR2",7,0.72]
["VLCNTR_6_VCSLR2",8,0.62]
["VLCNTR_6_VCSLR2",9,0.56000000000000005]
["VLCNTR_6_VCSLR2",10,0.37]
["VLCNTR_6_VCSLR2",11,0.28999999999999998]
["VLCNTR_6_VCSLR2",12,0.18]
["VLYHOM_7_SSJID",1,0]
["VLYHOM_7_SSJID",2,0]
["VLYHOM_7_SSJID",3,0]
["VLYHOM_7_SSJID",4,0.49]
["VLYHOM_7_SSJID",5,0.16]
["VLYHOM_7_SSJID",6,0.19]
["VLYHOM_7_SSJID",7,0.75]
["VLYHOM_7_SSJID",8,0.54]
["VLYHOM_7_SSJID",9,0.09]
["VLYHOM_7_SSJID",10,0]
["VLYHOM_7_SSJID",11,0]
["VLYHOM_7_SSJID",12,0]
["VOLTA_2_UNIT 1",1,4.6900000000000004]
["VOLTA_2_UNIT 1",2,5.15]
["VOLTA_2_UNIT 1",3,3.64]
["VOLTA_2_UNIT 1",4,2.94]
["VOLTA_2_UNIT 1",5,3.96]
["VOLTA_2_UNIT 1",6,3.38]
["VOLTA_2_UNIT 1",7,2.7]
["VOLTA_2_UNIT 1",8,2.44]
["VOLTA_2_UNIT 1",9,3.05]
["VOLTA_2_UNIT 1",10,2.2599999999999998]
["VOLTA_2_UNIT 1",11,2.75]
["VOLTA_2_UNIT 1",12,3.79]
["VOLTA_2_UNIT 2",1,0.34]
["VOLTA_2_UNIT 2",2,0.43]
["VOLTA_2_UNIT 2",3,0.48]
["VOLTA_2_UNIT 2",4,0.42]
["VOLTA_2_UNIT 2",5,0.5]
["VOLTA_2_UNIT 2",6,0.39]
["VOLTA_2_UNIT 2",7,0.32]
["VOLTA_2_UNIT 2",8,0.23]
["VOLTA_2_UNIT 2",9,0.36]
["VOLTA_2_UNIT 2",10,0.12]
["VOLTA_2_UNIT 2",11,0.16]
["VOLTA_2_UNIT 2",12,0.22]
["VOLTA_6_BAILCK",1,0]
["VOLTA_6_BAILCK",2,0]
["VOLTA_6_BAILCK",3,0]
["VOLTA_6_BAILCK",4,0]
["VOLTA_6_BAILCK",5,0]
["VOLTA_6_BAILCK",6,0]
["VOLTA_6_BAILCK",7,0]
["VOLTA_6_BAILCK",8,0]
["VOLTA_6_BAILCK",9,0]
["VOLTA_6_BAILCK",10,0]
["VOLTA_6_BAILCK",11,0]
["VOLTA_6_BAILCK",12,0]
["VOLTA_6_DIGHYD",1,0.3]
["VOLTA_6_DIGHYD",2,0.31]
["VOLTA_6_DIGHYD",3,0.38]
["VOLTA_6_DIGHYD",4,0.46]
["VOLTA_6_DIGHYD",5,0.36]
["VOLTA_6_DIGHYD",6,0.38]
["VOLTA_6_DIGHYD",7,0.32]
["VOLTA_6_DIGHYD",8,0.28999999999999998]
["VOLTA_6_DIGHYD",9,0.28000000000000003]
["VOLTA_6_DIGHYD",10,0.23]
["VOLTA_6_DIGHYD",11,0.24]
["VOLTA_6_DIGHYD",12,0.28999999999999998]
["VOLTA_7_PONHY1",1,0.47]
["VOLTA_7_PONHY1",2,0.45]
["VOLTA_7_PONHY1",3,0.51]
["VOLTA_7_PONHY1",4,0.4]
["VOLTA_7_PONHY1",5,0.46]
["VOLTA_7_PONHY1",6,0.35]
["VOLTA_7_PONHY1",7,0.3]
["VOLTA_7_PONHY1",8,0.27]
["VOLTA_7_PONHY1",9,0.27]
["VOLTA_7_PONHY1",10,0.24]
["VOLTA_7_PONHY1",11,0.22]
["VOLTA_7_PONHY1",12,0.26]
["VOLTA_7_QFUNTS",1,0.15]
["VOLTA_7_QFUNTS",2,0.15]
["VOLTA_7_QFUNTS",3,0.15]
["VOLTA_7_QFUNTS",4,0.15]
["VOLTA_7_QFUNTS",5,0.15]
["VOLTA_7_QFUNTS",6,0.15]
["VOLTA_7_QFUNTS",7,0.15]
["VOLTA_7_QFUNTS",8,0.05]
["VOLTA_7_QFUNTS",9,0.03]
["VOLTA_7_QFUNTS",10,0.02]
["VOLTA_7_QFUNTS",11,0.04]
["VOLTA_7_QFUNTS",12,0.06]
["VOYAGR_2_VOAWD5",1,2.4700000000000002]
["VOYAGR_2_VOAWD5",2,2.63]
["VOYAGR_2_VOAWD5",3,2.31]
["VOYAGR_2_VOAWD5",4,2.21]
["VOYAGR_2_VOAWD5",5,2.35]
["VOYAGR_2_VOAWD5",6,2.16]
["VOYAGR_2_VOAWD5",7,2]
["VOYAGR_2_VOAWD5",8,1.52]
["VOYAGR_2_VOAWD5",9,1.57]
["VOYAGR_2_VOAWD5",10,1.46]
["VOYAGR_2_VOAWD5",11,1.97]
["VOYAGR_2_VOAWD5",12,2.38]
["VOYAGR_2_VOYWD1",1,22.78]
["VOYAGR_2_VOYWD1",2,24.23]
["VOYAGR_2_VOYWD1",3,21.29]
["VOYAGR_2_VOYWD1",4,20.39]
["VOYAGR_2_VOYWD1",5,21.69]
["VOYAGR_2_VOYWD1",6,19.88]
["VOYAGR_2_VOYWD1",7,18.47]
["VOYAGR_2_VOYWD1",8,14.03]
["VOYAGR_2_VOYWD1",9,14.5]
["VOYAGR_2_VOYWD1",10,13.45]
["VOYAGR_2_VOYWD1",11,18.12]
["VOYAGR_2_VOYWD1",12,21.95]
["VOYAGR_2_VOYWD2",1,22.33]
["VOYAGR_2_VOYWD2",2,23.75]
["VOYAGR_2_VOYWD2",3,20.86]
["VOYAGR_2_VOYWD2",4,19.989999999999998]
["VOYAGR_2_VOYWD2",5,21.26]
["VOYAGR_2_VOYWD2",6,19.48]
["VOYAGR_2_VOYWD2",7,18.100000000000001]
["VOYAGR_2_VOYWD2",8,13.75]
["VOYAGR_2_VOYWD2",9,14.21]
["VOYAGR_2_VOYWD2",10,13.18]
["VOYAGR_2_VOYWD2",11,17.760000000000002]
["VOYAGR_2_VOYWD2",12,21.52]
["VOYAGR_2_VOYWD3",1,7.5]
["VOYAGR_2_VOYWD3",2,7.98]
["VOYAGR_2_VOYWD3",3,7.01]
["VOYAGR_2_VOYWD3",4,6.72]
["VOYAGR_2_VOYWD3",5,7.14]
["VOYAGR_2_VOYWD3",6,6.55]
["VOYAGR_2_VOYWD3",7,6.08]
["VOYAGR_2_VOYWD3",8,4.62]
["VOYAGR_2_VOYWD3",9,4.7699999999999996]
["VOYAGR_2_VOYWD3",10,4.43]
["VOYAGR_2_VOYWD3",11,5.97]
["VOYAGR_2_VOYWD3",12,7.23]
["VOYAGR_2_VOYWD4",1,3.71]
["VOYAGR_2_VOYWD4",2,3.95]
["VOYAGR_2_VOYWD4",3,3.47]
["VOYAGR_2_VOYWD4",4,3.32]
["VOYAGR_2_VOYWD4",5,3.53]
["VOYAGR_2_VOYWD4",6,3.24]
["VOYAGR_2_VOYWD4",7,3.01]
["VOYAGR_2_VOYWD4",8,2.29]
["VOYAGR_2_VOYWD4",9,2.36]
["VOYAGR_2_VOYWD4",10,2.19]
["VOYAGR_2_VOYWD4",11,2.95]
["VOYAGR_2_VOYWD4",12,3.58]
["VSTAES_6_VESBT1",1,10]
["VSTAES_6_VESBT1",2,10]
["VSTAES_6_VESBT1",3,10]
["VSTAES_6_VESBT1",4,10]
["VSTAES_6_VESBT1",5,10]
["VSTAES_6_VESBT1",6,10]
["VSTAES_6_VESBT1",7,10]
["VSTAES_6_VESBT1",8,10]
["VSTAES_6_VESBT1",9,10]
["VSTAES_6_VESBT1",10,10]
["VSTAES_6_VESBT1",11,10]
["VSTAES_6_VESBT1",12,10]
["WADHAM_6_UNIT",1,25.08]
["WADHAM_6_UNIT",2,25.07]
["WADHAM_6_UNIT",3,24.79]
["WADHAM_6_UNIT",4,22.47]
["WADHAM_6_UNIT",5,24.7]
["WADHAM_6_UNIT",6,24.71]
["WADHAM_6_UNIT",7,24.08]
["WADHAM_6_UNIT",8,24.52]
["WADHAM_6_UNIT",9,24.31]
["WADHAM_6_UNIT",10,23.59]
["WADHAM_6_UNIT",11,14.1]
["WADHAM_6_UNIT",12,24.59]
["WALCRK_2_CTG1",1,96.43]
["WALCRK_2_CTG1",2,96.43]
["WALCRK_2_CTG1",3,96.43]
["WALCRK_2_CTG1",4,96.43]
["WALCRK_2_CTG1",5,96.43]
["WALCRK_2_CTG1",6,96.43]
["WALCRK_2_CTG1",7,96.43]
["WALCRK_2_CTG1",8,96.43]
["WALCRK_2_CTG1",9,96.43]
["WALCRK_2_CTG1",10,96.43]
["WALCRK_2_CTG1",11,96.43]
["WALCRK_2_CTG1",12,96.43]
["WALCRK_2_CTG2",1,96.91]
["WALCRK_2_CTG2",2,96.91]
["WALCRK_2_CTG2",3,96.91]
["WALCRK_2_CTG2",4,96.91]
["WALCRK_2_CTG2",5,96.91]
["WALCRK_2_CTG2",6,96.91]
["WALCRK_2_CTG2",7,96.91]
["WALCRK_2_CTG2",8,96.91]
["WALCRK_2_CTG2",9,96.91]
["WALCRK_2_CTG2",10,96.91]
["WALCRK_2_CTG2",11,96.91]
["WALCRK_2_CTG2",12,96.91]
["WALCRK_2_CTG3",1,96.65]
["WALCRK_2_CTG3",2,96.65]
["WALCRK_2_CTG3",3,96.65]
["WALCRK_2_CTG3",4,96.65]
["WALCRK_2_CTG3",5,96.65]
["WALCRK_2_CTG3",6,96.65]
["WALCRK_2_CTG3",7,96.65]
["WALCRK_2_CTG3",8,96.65]
["WALCRK_2_CTG3",9,96.65]
["WALCRK_2_CTG3",10,96.65]
["WALCRK_2_CTG3",11,96.65]
["WALCRK_2_CTG3",12,96.65]
["WALCRK_2_CTG4",1,96.49]
["WALCRK_2_CTG4",2,96.49]
["WALCRK_2_CTG4",3,96.49]
["WALCRK_2_CTG4",4,96.49]
["WALCRK_2_CTG4",5,96.49]
["WALCRK_2_CTG4",6,96.49]
["WALCRK_2_CTG4",7,96.49]
["WALCRK_2_CTG4",8,96.49]
["WALCRK_2_CTG4",9,96.49]
["WALCRK_2_CTG4",10,96.49]
["WALCRK_2_CTG4",11,96.49]
["WALCRK_2_CTG4",12,96.49]
["WALCRK_2_CTG5",1,96.65]
["WALCRK_2_CTG5",2,96.65]
["WALCRK_2_CTG5",3,96.65]
["WALCRK_2_CTG5",4,96.65]
["WALCRK_2_CTG5",5,96.65]
["WALCRK_2_CTG5",6,96.65]
["WALCRK_2_CTG5",7,96.65]
["WALCRK_2_CTG5",8,96.65]
["WALCRK_2_CTG5",9,96.65]
["WALCRK_2_CTG5",10,96.65]
["WALCRK_2_CTG5",11,96.65]
["WALCRK_2_CTG5",12,96.65]
["WALNUT_2_SOLAR",1,0]
["WALNUT_2_SOLAR",2,0]
["WALNUT_2_SOLAR",3,0]
["WALNUT_2_SOLAR",4,0]
["WALNUT_2_SOLAR",5,0]
["WALNUT_2_SOLAR",6,0]
["WALNUT_2_SOLAR",7,0]
["WALNUT_2_SOLAR",8,0]
["WALNUT_2_SOLAR",9,0]
["WALNUT_2_SOLAR",10,0]
["WALNUT_2_SOLAR",11,0]
["WALNUT_2_SOLAR",12,0]
["WALNUT_6_HILLGEN",1,24.29]
["WALNUT_6_HILLGEN",2,24.59]
["WALNUT_6_HILLGEN",3,24.45]
["WALNUT_6_HILLGEN",4,23.57]
["WALNUT_6_HILLGEN",5,14.5]
["WALNUT_6_HILLGEN",6,23.88]
["WALNUT_6_HILLGEN",7,23.82]
["WALNUT_6_HILLGEN",8,23.67]
["WALNUT_6_HILLGEN",9,23.62]
["WALNUT_6_HILLGEN",10,23.04]
["WALNUT_6_HILLGEN",11,22.82]
["WALNUT_6_HILLGEN",12,22.74]
["WALNUT_7_WCOVST",1,4.87]
["WALNUT_7_WCOVST",2,5.0199999999999996]
["WALNUT_7_WCOVST",3,5.52]
["WALNUT_7_WCOVST",4,5.44]
["WALNUT_7_WCOVST",5,5.34]
["WALNUT_7_WCOVST",6,5.31]
["WALNUT_7_WCOVST",7,5.25]
["WALNUT_7_WCOVST",8,5.22]
["WALNUT_7_WCOVST",9,5.21]
["WALNUT_7_WCOVST",10,4.99]
["WALNUT_7_WCOVST",11,5.18]
["WALNUT_7_WCOVST",12,5.15]
["WARNE_2_UNIT",1,41.43]
["WARNE_2_UNIT",2,45.99]
["WARNE_2_UNIT",3,41.29]
["WARNE_2_UNIT",4,42.7]
["WARNE_2_UNIT",5,41.36]
["WARNE_2_UNIT",6,42.74]
["WARNE_2_UNIT",7,41.3]
["WARNE_2_UNIT",8,40.92]
["WARNE_2_UNIT",9,59.67]
["WARNE_2_UNIT",10,58.33]
["WARNE_2_UNIT",11,56.11]
["WARNE_2_UNIT",12,42.86]
["WAUKNA_1_SOLAR",1,0.08]
["WAUKNA_1_SOLAR",2,0.6]
["WAUKNA_1_SOLAR",3,0.7]
["WAUKNA_1_SOLAR",4,0.88]
["WAUKNA_1_SOLAR",5,1.28]
["WAUKNA_1_SOLAR",6,2.62]
["WAUKNA_1_SOLAR",7,2.88]
["WAUKNA_1_SOLAR",8,2.48]
["WAUKNA_1_SOLAR",9,2.2200000000000002]
["WAUKNA_1_SOLAR",10,1.48]
["WAUKNA_1_SOLAR",11,1.1399999999999999]
["WAUKNA_1_SOLAR",12,0.7]
["WAUKNA_1_SOLAR2",1,0.08]
["WAUKNA_1_SOLAR2",2,0.59]
["WAUKNA_1_SOLAR2",3,0.69]
["WAUKNA_1_SOLAR2",4,0.87]
["WAUKNA_1_SOLAR2",5,1.26]
["WAUKNA_1_SOLAR2",6,2.59]
["WAUKNA_1_SOLAR2",7,2.84]
["WAUKNA_1_SOLAR2",8,2.4500000000000002]
["WAUKNA_1_SOLAR2",9,2.19]
["WAUKNA_1_SOLAR2",10,1.46]
["WAUKNA_1_SOLAR2",11,1.1299999999999999]
["WAUKNA_1_SOLAR2",12,0.69]
["WDLEAF_7_UNIT 1",1,60]
["WDLEAF_7_UNIT 1",2,60]
["WDLEAF_7_UNIT 1",3,60]
["WDLEAF_7_UNIT 1",4,60]
["WDLEAF_7_UNIT 1",5,60]
["WDLEAF_7_UNIT 1",6,60]
["WDLEAF_7_UNIT 1",7,60]
["WDLEAF_7_UNIT 1",8,60]
["WDLEAF_7_UNIT 1",9,60]
["WDLEAF_7_UNIT 1",10,60]
["WDLEAF_7_UNIT 1",11,60]
["WDLEAF_7_UNIT 1",12,60]
["WEBER_6_FORWRD",1,4.0199999999999996]
["WEBER_6_FORWRD",2,3.99]
["WEBER_6_FORWRD",3,3.99]
["WEBER_6_FORWRD",4,3.69]
["WEBER_6_FORWRD",5,4]
["WEBER_6_FORWRD",6,4.01]
["WEBER_6_FORWRD",7,4]
["WEBER_6_FORWRD",8,3.91]
["WEBER_6_FORWRD",9,4]
["WEBER_6_FORWRD",10,4.05]
["WEBER_6_FORWRD",11,4.05]
["WEBER_6_FORWRD",12,4.03]
["WESTPT_2_UNIT",1,9.2799999999999994]
["WESTPT_2_UNIT",2,5.44]
["WESTPT_2_UNIT",3,8.4]
["WESTPT_2_UNIT",4,2.48]
["WESTPT_2_UNIT",5,3.6]
["WESTPT_2_UNIT",6,10.8]
["WESTPT_2_UNIT",7,10.4]
["WESTPT_2_UNIT",8,11.38]
["WESTPT_2_UNIT",9,10]
["WESTPT_2_UNIT",10,10.24]
["WESTPT_2_UNIT",11,10.15]
["WESTPT_2_UNIT",12,10.08]
["WFRESN_1_SOLAR",1,0]
["WFRESN_1_SOLAR",2,0]
["WFRESN_1_SOLAR",3,0]
["WFRESN_1_SOLAR",4,0]
["WFRESN_1_SOLAR",5,0]
["WFRESN_1_SOLAR",6,0]
["WFRESN_1_SOLAR",7,0]
["WFRESN_1_SOLAR",8,0]
["WFRESN_1_SOLAR",9,0]
["WFRESN_1_SOLAR",10,0]
["WFRESN_1_SOLAR",11,0]
["WFRESN_1_SOLAR",12,0]
["WHEATL_6_LNDFIL",1,3.42]
["WHEATL_6_LNDFIL",2,3.37]
["WHEATL_6_LNDFIL",3,3.39]
["WHEATL_6_LNDFIL",4,3.26]
["WHEATL_6_LNDFIL",5,3.26]
["WHEATL_6_LNDFIL",6,3.03]
["WHEATL_6_LNDFIL",7,3.3]
["WHEATL_6_LNDFIL",8,3.13]
["WHEATL_6_LNDFIL",9,3.28]
["WHEATL_6_LNDFIL",10,3.35]
["WHEATL_6_LNDFIL",11,3.41]
["WHEATL_6_LNDFIL",12,2.72]
["WHITNY_6_SOLAR",1,0]
["WHITNY_6_SOLAR",2,0]
["WHITNY_6_SOLAR",3,0]
["WHITNY_6_SOLAR",4,0]
["WHITNY_6_SOLAR",5,0]
["WHITNY_6_SOLAR",6,0]
["WHITNY_6_SOLAR",7,0]
["WHITNY_6_SOLAR",8,0]
["WHITNY_6_SOLAR",9,0]
["WHITNY_6_SOLAR",10,0]
["WHITNY_6_SOLAR",11,0]
["WHITNY_6_SOLAR",12,0]
["WHTWTR_1_WINDA1",1,10.87]
["WHTWTR_1_WINDA1",2,11.56]
["WHTWTR_1_WINDA1",3,10.16]
["WHTWTR_1_WINDA1",4,9.73]
["WHTWTR_1_WINDA1",5,10.35]
["WHTWTR_1_WINDA1",6,9.48]
["WHTWTR_1_WINDA1",7,8.81]
["WHTWTR_1_WINDA1",8,6.69]
["WHTWTR_1_WINDA1",9,6.92]
["WHTWTR_1_WINDA1",10,6.42]
["WHTWTR_1_WINDA1",11,8.65]
["WHTWTR_1_WINDA1",12,10.47]
["WISE_1_UNIT 1",1,3.85]
["WISE_1_UNIT 1",2,5]
["WISE_1_UNIT 1",3,4.51]
["WISE_1_UNIT 1",4,6.48]
["WISE_1_UNIT 1",5,8.44]
["WISE_1_UNIT 1",6,7.84]
["WISE_1_UNIT 1",7,9.2799999999999994]
["WISE_1_UNIT 1",8,7.36]
["WISE_1_UNIT 1",9,5.84]
["WISE_1_UNIT 1",10,2.54]
["WISE_1_UNIT 1",11,0]
["WISE_1_UNIT 1",12,3.68]
["WISE_1_UNIT 2",1,0]
["WISE_1_UNIT 2",2,0]
["WISE_1_UNIT 2",3,0]
["WISE_1_UNIT 2",4,0]
["WISE_1_UNIT 2",5,0]
["WISE_1_UNIT 2",6,0]
["WISE_1_UNIT 2",7,0]
["WISE_1_UNIT 2",8,0]
["WISE_1_UNIT 2",9,0]
["WISE_1_UNIT 2",10,0]
["WISE_1_UNIT 2",11,0]
["WISE_1_UNIT 2",12,0]
["WISHON_6_UNITS",1,1.3]
["WISHON_6_UNITS",2,1.68]
["WISHON_6_UNITS",3,2.48]
["WISHON_6_UNITS",4,2.38]
["WISHON_6_UNITS",5,0.8]
["WISHON_6_UNITS",6,0.4]
["WISHON_6_UNITS",7,0]
["WISHON_6_UNITS",8,0]
["WISHON_6_UNITS",9,0]
["WISHON_6_UNITS",10,7.01]
["WISHON_6_UNITS",11,6.46]
["WISHON_6_UNITS",12,1.84]
["WISTRA_2_WRSSR1",1,0.4]
["WISTRA_2_WRSSR1",2,3]
["WISTRA_2_WRSSR1",3,3.5]
["WISTRA_2_WRSSR1",4,4.4000000000000004]
["WISTRA_2_WRSSR1",5,6.4]
["WISTRA_2_WRSSR1",6,13.1]
["WISTRA_2_WRSSR1",7,14.4]
["WISTRA_2_WRSSR1",8,12.4]
["WISTRA_2_WRSSR1",9,11.1]
["WISTRA_2_WRSSR1",10,7.4]
["WISTRA_2_WRSSR1",11,5.7]
["WISTRA_2_WRSSR1",12,3.5]
["WLDWD_1_SOLAR1",1,0.08]
["WLDWD_1_SOLAR1",2,0.6]
["WLDWD_1_SOLAR1",3,0.7]
["WLDWD_1_SOLAR1",4,0.88]
["WLDWD_1_SOLAR1",5,1.28]
["WLDWD_1_SOLAR1",6,2.62]
["WLDWD_1_SOLAR1",7,2.88]
["WLDWD_1_SOLAR1",8,2.48]
["WLDWD_1_SOLAR1",9,2.2200000000000002]
["WLDWD_1_SOLAR1",10,1.48]
["WLDWD_1_SOLAR1",11,1.1399999999999999]
["WLDWD_1_SOLAR1",12,0.7]
["WLDWD_1_SOLAR2",1,0.06]
["WLDWD_1_SOLAR2",2,0.45]
["WLDWD_1_SOLAR2",3,0.53]
["WLDWD_1_SOLAR2",4,0.66]
["WLDWD_1_SOLAR2",5,0.96]
["WLDWD_1_SOLAR2",6,1.97]
["WLDWD_1_SOLAR2",7,2.16]
["WLDWD_1_SOLAR2",8,1.86]
["WLDWD_1_SOLAR2",9,1.67]
["WLDWD_1_SOLAR2",10,1.1100000000000001]
["WLDWD_1_SOLAR2",11,0.86]
["WLDWD_1_SOLAR2",12,0.53]
["WNDMAS_2_UNIT 1",1,12.48]
["WNDMAS_2_UNIT 1",2,13.39]
["WNDMAS_2_UNIT 1",3,11.94]
["WNDMAS_2_UNIT 1",4,12.61]
["WNDMAS_2_UNIT 1",5,13.05]
["WNDMAS_2_UNIT 1",6,9.6300000000000008]
["WNDMAS_2_UNIT 1",7,8.56]
["WNDMAS_2_UNIT 1",8,8.0399999999999991]
["WNDMAS_2_UNIT 1",9,8.26]
["WNDMAS_2_UNIT 1",10,6.92]
["WNDMAS_2_UNIT 1",11,8.74]
["WNDMAS_2_UNIT 1",12,11.17]
["WNDSTR_2_WIND",1,21.2]
["WNDSTR_2_WIND",2,22.55]
["WNDSTR_2_WIND",3,19.82]
["WNDSTR_2_WIND",4,18.98]
["WNDSTR_2_WIND",5,20.190000000000001]
["WNDSTR_2_WIND",6,18.5]
["WNDSTR_2_WIND",7,17.190000000000001]
["WNDSTR_2_WIND",8,13.06]
["WNDSTR_2_WIND",9,13.49]
["WNDSTR_2_WIND",10,12.52]
["WNDSTR_2_WIND",11,16.87]
["WNDSTR_2_WIND",12,20.440000000000001]
["WOLFSK_1_UNITA1",1,46.9]
["WOLFSK_1_UNITA1",2,46.9]
["WOLFSK_1_UNITA1",3,46.9]
["WOLFSK_1_UNITA1",4,46.9]
["WOLFSK_1_UNITA1",5,46.9]
["WOLFSK_1_UNITA1",6,46.9]
["WOLFSK_1_UNITA1",7,46.9]
["WOLFSK_1_UNITA1",8,46.9]
["WOLFSK_1_UNITA1",9,46.9]
["WOLFSK_1_UNITA1",10,46.9]
["WOLFSK_1_UNITA1",11,46.9]
["WOLFSK_1_UNITA1",12,46.9]
["WOODWR_1_HYDRO",1,0]
["WOODWR_1_HYDRO",2,0]
["WOODWR_1_HYDRO",3,0]
["WOODWR_1_HYDRO",4,0]
["WOODWR_1_HYDRO",5,0]
["WOODWR_1_HYDRO",6,0]
["WOODWR_1_HYDRO",7,0]
["WOODWR_1_HYDRO",8,0]
["WOODWR_1_HYDRO",9,0]
["WOODWR_1_HYDRO",10,0]
["WOODWR_1_HYDRO",11,0]
["WOODWR_1_HYDRO",12,0]
["WRGHTP_7_AMENGY",1,0]
["WRGHTP_7_AMENGY",2,0.05]
["WRGHTP_7_AMENGY",3,0.03]
["WRGHTP_7_AMENGY",4,0.06]
["WRGHTP_7_AMENGY",5,0.17]
["WRGHTP_7_AMENGY",6,0.24]
["WRGHTP_7_AMENGY",7,0.51]
["WRGHTP_7_AMENGY",8,0.51]
["WRGHTP_7_AMENGY",9,0.51]
["WRGHTP_7_AMENGY",10,0.31]
["WRGHTP_7_AMENGY",11,0.21]
["WRGHTP_7_AMENGY",12,0.02]
["WRGTSR_2_WSFSR1",1,0.8]
["WRGTSR_2_WSFSR1",2,6]
["WRGTSR_2_WSFSR1",3,7]
["WRGTSR_2_WSFSR1",4,8.8000000000000007]
["WRGTSR_2_WSFSR1",5,12.8]
["WRGTSR_2_WSFSR1",6,26.2]
["WRGTSR_2_WSFSR1",7,28.8]
["WRGTSR_2_WSFSR1",8,24.8]
["WRGTSR_2_WSFSR1",9,22.2]
["WRGTSR_2_WSFSR1",10,14.8]
["WRGTSR_2_WSFSR1",11,11.4]
["WRGTSR_2_WSFSR1",12,7]
["WSENGY_1_UNIT 1",1,34.020000000000003]
["WSENGY_1_UNIT 1",2,34.03]
["WSENGY_1_UNIT 1",3,34.020000000000003]
["WSENGY_1_UNIT 1",4,33.450000000000003]
["WSENGY_1_UNIT 1",5,34.020000000000003]
["WSENGY_1_UNIT 1",6,34.020000000000003]
["WSENGY_1_UNIT 1",7,34.18]
["WSENGY_1_UNIT 1",8,36.25]
["WSENGY_1_UNIT 1",9,34.56]
["WSENGY_1_UNIT 1",10,34.04]
["WSENGY_1_UNIT 1",11,32.96]
["WSENGY_1_UNIT 1",12,34.04]
["WSTWND_2_M89BT2",6,0]
["WSTWND_2_M89BT2",7,0]
["WSTWND_2_M89BT2",8,0]
["WSTWND_2_M89BT2",9,0]
["WSTWND_2_M89BT2",10,0]
["WSTWND_2_M89BT2",11,0]
["WSTWND_2_M89BT2",12,0]
["WSTWND_2_M89WD1",1,14.6]
["WSTWND_2_M89WD1",2,15.53]
["WSTWND_2_M89WD1",3,13.65]
["WSTWND_2_M89WD1",4,13.08]
["WSTWND_2_M89WD1",5,13.9]
["WSTWND_2_M89WD1",6,12.74]
["WSTWND_2_M89WD1",7,11.84]
["WSTWND_2_M89WD1",8,9]
["WSTWND_2_M89WD1",9,9.2899999999999991]
["WSTWND_2_M89WD1",10,8.6199999999999992]
["WSTWND_2_M89WD1",11,11.62]
["WSTWND_2_M89WD1",12,14.08]
["WSTWND_2_M89WD2",6,12.74]
["WSTWND_2_M89WD2",7,11.84]
["WSTWND_2_M89WD2",8,9]
["WSTWND_2_M89WD2",9,9.2899999999999991]
["WSTWND_2_M89WD2",10,8.6199999999999992]
["WSTWND_2_M89WD2",11,11.62]
["WSTWND_2_M89WD2",12,14.08]
["WSTWND_2_M90WD2",1,11.45]
["WSTWND_2_M90WD2",2,12.18]
["WSTWND_2_M90WD2",3,10.7]
["WSTWND_2_M90WD2",4,10.25]
["WSTWND_2_M90WD2",5,10.9]
["WSTWND_2_M90WD2",6,10]
["WSTWND_2_M90WD2",7,9.2899999999999991]
["WSTWND_2_M90WD2",8,7.06]
["WSTWND_2_M90WD2",9,7.29]
["WSTWND_2_M90WD2",10,6.76]
["WSTWND_2_M90WD2",11,9.11]
["WSTWND_2_M90WD2",12,11.04]
["WSTWND_2_SBSBT1",6,80]
["WSTWND_2_SBSBT1",7,80]
["WSTWND_2_SBSBT1",8,80]
["WSTWND_2_SBSBT1",9,80]
["WSTWND_2_SBSBT1",10,80]
["WSTWND_2_SBSBT1",11,80]
["WSTWND_2_SBSBT1",12,80]
["YELPIN_2_YP2BT1",8,65]
["YELPIN_2_YP2BT1",9,65]
["YELPIN_2_YP2BT1",10,65]
["YELPIN_2_YP2BT1",11,65]
["YELPIN_2_YP2BT1",12,65]
["YUBACT_1_SUNSWT",1,49.97]
["YUBACT_1_SUNSWT",2,49.97]
["YUBACT_1_SUNSWT",3,49.97]
["YUBACT_1_SUNSWT",4,49.97]
["YUBACT_1_SUNSWT",5,49.97]
["YUBACT_1_SUNSWT",6,49.97]
["YUBACT_1_SUNSWT",7,49.97]
["YUBACT_1_SUNSWT",8,49.97]
["YUBACT_1_SUNSWT",9,49.97]
["YUBACT_1_SUNSWT",10,49.97]
["YUBACT_1_SUNSWT",11,49.97]
["YUBACT_1_SUNSWT",12,49.97]
["YUBACT_6_UNITA1",1,47.16]
["YUBACT_6_UNITA1",2,47.16]
["YUBACT_6_UNITA1",3,47.16]
["YUBACT_6_UNITA1",4,47.16]
["YUBACT_6_UNITA1",5,47.16]
["YUBACT_6_UNITA1",6,47.16]
["YUBACT_6_UNITA1",7,47.16]
["YUBACT_6_UNITA1",8,47.16]
["YUBACT_6_UNITA1",9,47.16]
["YUBACT_6_UNITA1",10,47.16]
["YUBACT_6_UNITA1",11,47.16]
["YUBACT_6_UNITA1",12,47.16]
["ZOND_6_UNIT",1,5.62]
["ZOND_6_UNIT",2,6.02]
["ZOND_6_UNIT",3,5.37]
["ZOND_6_UNIT",4,5.68]
["ZOND_6_UNIT",5,5.87]
["ZOND_6_UNIT",6,4.33]
["ZOND_6_UNIT",7,3.85]
["ZOND_6_UNIT",8,3.62]
["ZOND_6_UNIT",9,3.72]
["ZOND_6_UNIT",10,3.11]
["ZOND_6_UNIT",11,3.93]
["ZOND_6_UNIT",12,5.03]
["TOWNSITE_2_MEADDYN",1,90.37]
["TOWNSITE_2_MEADDYN",2,93.43]
["TOWNSITE_2_MEADDYN",3,94.25]
["TOWNSITE_2_MEADDYN",4,95.86]
["TOWNSITE_2_MEADDYN",5,98.74]
["TOWNSITE_2_MEADDYN",6,108.28]
["TOWNSITE_2_MEADDYN",7,110.06]
["TOWNSITE_2_MEADDYN",8,106.92]
["TOWNSITE_2_MEADDYN",9,104.39]
["TOWNSITE_2_MEADDYN",10,99.01]
["TOWNSITE_2_MEADDYN",11,95.97]
["TOWNSITE_2_MEADDYN",12,92.63]

{"sheet":"Resource Default Profiles","index":28,"n_rows":2305,"n_cols":5,"rows_kept":2305,"cut":false,"hidden":false,"merged":[]}
["Profile Category","Region","Month","Hour Ending","Shape Factor"]
["Solar Fixed","Norcal",1,1,0]
["Solar Fixed","Norcal",1,2,0]
["Solar Fixed","Norcal",1,3,0]
["Solar Fixed","Norcal",1,4,0]
["Solar Fixed","Norcal",1,5,0]
["Solar Fixed","Norcal",1,6,0]
["Solar Fixed","Norcal",1,7,0]
["Solar Fixed","Norcal",1,8,0.02]
["Solar Fixed","Norcal",1,9,0.17]
["Solar Fixed","Norcal",1,10,0.34]
["Solar Fixed","Norcal",1,11,0.44]
["Solar Fixed","Norcal",1,12,0.48]
["Solar Fixed","Norcal",1,13,0.48]
["Solar Fixed","Norcal",1,14,0.43]
["Solar Fixed","Norcal",1,15,0.4]
["Solar Fixed","Norcal",1,16,0.24]
["Solar Fixed","Norcal",1,17,0.05]
["Solar Fixed","Norcal",1,18,0]
["Solar Fixed","Norcal",1,19,0]
["Solar Fixed","Norcal",1,20,0]
["Solar Fixed","Norcal",1,21,0]
["Solar Fixed","Norcal",1,22,0]
["Solar Fixed","Norcal",1,23,0]
["Solar Fixed","Norcal",1,24,0]
["Solar Fixed","Norcal",2,1,0]
["Solar Fixed","Norcal",2,2,0]
["Solar Fixed","Norcal",2,3,0]
["Solar Fixed","Norcal",2,4,0]
["Solar Fixed","Norcal",2,5,0]
["Solar Fixed","Norcal",2,6,0]
["Solar Fixed","Norcal",2,7,0]
["Solar Fixed","Norcal",2,8,0.09]
["Solar Fixed","Norcal",2,9,0.37]
["Solar Fixed","Norcal",2,10,0.47]
["Solar Fixed","Norcal",2,11,0.56999999999999995]
["Solar Fixed","Norcal",2,12,0.57999999999999996]
["Solar Fixed","Norcal",2,13,0.59]
["Solar Fixed","Norcal",2,14,0.56999999999999995]
["Solar Fixed","Norcal",2,15,0.55000000000000004]
["Solar Fixed","Norcal",2,16,0.43]
["Solar Fixed","Norcal",2,17,0.21]
["Solar Fixed","Norcal",2,18,0.01]
["Solar Fixed","Norcal",2,19,0]
["Solar Fixed","Norcal",2,20,0]
["Solar Fixed","Norcal",2,21,0]
["Solar Fixed","Norcal",2,22,0]
["Solar Fixed","Norcal",2,23,0]
["Solar Fixed","Norcal",2,24,0]
["Solar Fixed","Norcal",3,1,0]
["Solar Fixed","Norcal",3,2,0]
["Solar Fixed","Norcal",3,3,0]
["Solar Fixed","Norcal",3,4,0]
["Solar Fixed","Norcal",3,5,0]
["Solar Fixed","Norcal",3,6,0]
["Solar Fixed","Norcal",3,7,0]
["Solar Fixed","Norcal",3,8,0.05]
["Solar Fixed","Norcal",3,9,0.28999999999999998]
["Solar Fixed","Norcal",3,10,0.48]
["Solar Fixed","Norcal",3,11,0.56000000000000005]
["Solar Fixed","Norcal",3,12,0.56999999999999995]
["Solar Fixed","Norcal",3,13,0.61]
["Solar Fixed","Norcal",3,14,0.59]
["Solar Fixed","Norcal",3,15,0.54]
["Solar Fixed","Norcal",3,16,0.46]
["Solar Fixed","Norcal",3,17,0.32]
["Solar Fixed","Norcal",3,18,0.09]
["Solar Fixed","Norcal",3,19,0]
["Solar Fixed","Norcal",3,20,0]
["Solar Fixed","Norcal",3,21,0]
["Solar Fixed","Norcal",3,22,0]
["Solar Fixed","Norcal",3,23,0]
["Solar Fixed","Norcal",3,24,0]
["Solar Fixed","Norcal",4,1,0]
["Solar Fixed","Norcal",4,2,0]
["Solar Fixed","Norcal",4,3,0]
["Solar Fixed","Norcal",4,4,0]
["Solar Fixed","Norcal",4,5,0]
["Solar Fixed","Norcal",4,6,0]
["Solar Fixed","Norcal",4,7,0]
["Solar Fixed","Norcal",4,8,0.16]
["Solar Fixed","Norcal",4,9,0.45]
["Solar Fixed","Norcal",4,10,0.62]
["Solar Fixed","Norcal",4,11,0.69]
["Solar Fixed","Norcal",4,12,0.74]
["Solar Fixed","Norcal",4,13,0.75]
["Solar Fixed","Norcal",4,14,0.77]
["Solar Fixed","Norcal",4,15,0.74]
["Solar Fixed","Norcal",4,16,0.7]
["Solar Fixed","Norcal",4,17,0.61]
["Solar Fixed","Norcal",4,18,0.47]
["Solar Fixed","Norcal",4,19,0.17]
["Solar Fixed","Norcal",4,20,0.01]
["Solar Fixed","Norcal",4,21,0]
["Solar Fixed","Norcal",4,22,0]
["Solar Fixed","Norcal",4,23,0]
["Solar Fixed","Norcal",4,24,0]
["Solar Fixed","Norcal",5,1,0]
["Solar Fixed","Norcal",5,2,0]
["Solar Fixed","Norcal",5,3,0]
["Solar Fixed","Norcal",5,4,0]
["Solar Fixed","Norcal",5,5,0]
["Solar Fixed","Norcal",5,6,0]
["Solar Fixed","Norcal",5,7,0.05]
["Solar Fixed","Norcal",5,8,0.31]
["Solar Fixed","Norcal",5,9,0.55000000000000004]
["Solar Fixed","Norcal",5,10,0.67]
["Solar Fixed","Norcal",5,11,0.75]
["Solar Fixed","Norcal",5,12,0.79]
["Solar Fixed","Norcal",5,13,0.78]
["Solar Fixed","Norcal",5,14,0.76]
["Solar Fixed","Norcal",5,15,0.76]
["Solar Fixed","Norcal",5,16,0.74]
["Solar Fixed","Norcal",5,17,0.65]
["Solar Fixed","Norcal",5,18,0.54]
["Solar Fixed","Norcal",5,19,0.28999999999999998]
["Solar Fixed","Norcal",5,20,0.04]
["Solar Fixed","Norcal",5,21,0]
["Solar Fixed","Norcal",5,22,0]
["Solar Fixed","Norcal",5,23,0]
["Solar Fixed","Norcal",5,24,0]
["Solar Fixed","Norcal",6,1,0]
["Solar Fixed","Norcal",6,2,0]
["Solar Fixed","Norcal",6,3,0]
["Solar Fixed","Norcal",6,4,0]
["Solar Fixed","Norcal",6,5,0]
["Solar Fixed","Norcal",6,6,0]
["Solar Fixed","Norcal",6,7,0.09]
["Solar Fixed","Norcal",6,8,0.36]
["Solar Fixed","Norcal",6,9,0.59]
["Solar Fixed","Norcal",6,10,0.73]
["Solar Fixed","Norcal",6,11,0.8]
["Solar Fixed","Norcal",6,12,0.85]
["Solar Fixed","Norcal",6,13,0.86]
["Solar Fixed","Norcal",6,14,0.87]
["Solar Fixed","Norcal",6,15,0.86]
["Solar Fixed","Norcal",6,16,0.82]
["Solar Fixed","Norcal",6,17,0.73]
["Solar Fixed","Norcal",6,18,0.6]
["Solar Fixed","Norcal",6,19,0.36]
["Solar Fixed","Norcal",6,20,0.09]
["Solar Fixed","Norcal",6,21,0]
["Solar Fixed","Norcal",6,22,0]
["Solar Fixed","Norcal",6,23,0]
["Solar Fixed","Norcal",6,24,0]
["Solar Fixed","Norcal",7,1,0]
["Solar Fixed","Norcal",7,2,0]
["Solar Fixed","Norcal",7,3,0]
["Solar Fixed","Norcal",7,4,0]
["Solar Fixed","Norcal",7,5,0]
["Solar Fixed","Norcal",7,6,0]
["Solar Fixed","Norcal",7,7,0.04]
["Solar Fixed","Norcal",7,8,0.31]
["Solar Fixed","Norcal",7,9,0.57999999999999996]
["Solar Fixed","Norcal",7,10,0.75]
["Solar Fixed","Norcal",7,11,0.83]
["Solar Fixed","Norcal",7,12,0.88]
["Solar Fixed","Norcal",7,13,0.89]
["Solar Fixed","Norcal",7,14,0.89]
["Solar Fixed","Norcal",7,15,0.87]
["Solar Fixed","Norcal",7,16,0.82]
["Solar Fixed","Norcal",7,17,0.74]
["Solar Fixed","Norcal",7,18,0.6]
["Solar Fixed","Norcal",7,19,0.36]
["Solar Fixed","Norcal",7,20,0.08]
["Solar Fixed","Norcal",7,21,0]
["Solar Fixed","Norcal",7,22,0]
["Solar Fixed","Norcal",7,23,0]
["Solar Fixed","Norcal",7,24,0]
["Solar Fixed","Norcal",8,1,0]
["Solar Fixed","Norcal",8,2,0]
["Solar Fixed","Norcal",8,3,0]
["Solar Fixed","Norcal",8,4,0]
["Solar Fixed","Norcal",8,5,0]
["Solar Fixed","Norcal",8,6,0]
["Solar Fixed","Norcal",8,7,0.01]
["Solar Fixed","Norcal",8,8,0.19]
["Solar Fixed","Norcal",8,9,0.5]
["Solar Fixed","Norcal",8,10,0.7]
["Solar Fixed","Norcal",8,11,0.81]
["Solar Fixed","Norcal",8,12,0.85]
["Solar Fixed","Norcal",8,13,0.86]
["Solar Fixed","Norcal",8,14,0.86]
["Solar Fixed","Norcal",8,15,0.84]
["Solar Fixed","Norcal",8,16,0.8]
["Solar Fixed","Norcal",8,17,0.7]
["Solar Fixed","Norcal",8,18,0.52]
["Solar Fixed","Norcal",8,19,0.21]
["Solar Fixed","Norcal",8,20,0.01]
["Solar Fixed","Norcal",8,21,0]
["Solar Fixed","Norcal",8,22,0]
["Solar Fixed","Norcal",8,23,0]
["Solar Fixed","Norcal",8,24,0]
["Solar Fixed","Norcal",9,1,0]
["Solar Fixed","Norcal",9,2,0]
["Solar Fixed","Norcal",9,3,0]
["Solar Fixed","Norcal",9,4,0]
["Solar Fixed","Norcal",9,5,0]
["Solar Fixed","Norcal",9,6,0]
["Solar Fixed","Norcal",9,7,0]
["Solar Fixed","Norcal",9,8,0.11]
["Solar Fixed","Norcal",9,9,0.42]
["Solar Fixed","Norcal",9,10,0.65]
["Solar Fixed","Norcal",9,11,0.76]
["Solar Fixed","Norcal",9,12,0.79]
["Solar Fixed","Norcal",9,13,0.81]
["Solar Fixed","Norcal",9,14,0.8]
["Solar Fixed","Norcal",9,15,0.79]
["Solar Fixed","Norcal",9,16,0.74]
["Solar Fixed","Norcal",9,17,0.62]
["Solar Fixed","Norcal",9,18,0.35]
["Solar Fixed","Norcal",9,19,0.05]
["Solar Fixed","Norcal",9,20,0]
["Solar Fixed","Norcal",9,21,0]
["Solar Fixed","Norcal",9,22,0]
["Solar Fixed","Norcal",9,23,0]
["Solar Fixed","Norcal",9,24,0]
["Solar Fixed","Norcal",10,1,0]
["Solar Fixed","Norcal",10,2,0]
["Solar Fixed","Norcal",10,3,0]
["Solar Fixed","Norcal",10,4,0]
["Solar Fixed","Norcal",10,5,0]
["Solar Fixed","Norcal",10,6,0]
["Solar Fixed","Norcal",10,7,0]
["Solar Fixed","Norcal",10,8,0.03]
["Solar Fixed","Norcal",10,9,0.3]
["Solar Fixed","Norcal",10,10,0.54]
["Solar Fixed","Norcal",10,11,0.66]
["Solar Fixed","Norcal",10,12,0.69]
["Solar Fixed","Norcal",10,13,0.7]
["Solar Fixed","Norcal",10,14,0.7]
["Solar Fixed","Norcal",10,15,0.68]
["Solar Fixed","Norcal",10,16,0.61]
["Solar Fixed","Norcal",10,17,0.45]
["Solar Fixed","Norcal",10,18,0.13]
["Solar Fixed","Norcal",10,19,0]
["Solar Fixed","Norcal",10,20,0]
["Solar Fixed","Norcal",10,21,0]
["Solar Fixed","Norcal",10,22,0]
["Solar Fixed","Norcal",10,23,0]
["Solar Fixed","Norcal",10,24,0]
["Solar Fixed","Norcal",11,1,0]
["Solar Fixed","Norcal",11,2,0]
["Solar Fixed","Norcal",11,3,0]
["Solar Fixed","Norcal",11,4,0]
["Solar Fixed","Norcal",11,5,0]
["Solar Fixed","Norcal",11,6,0]
["Solar Fixed","Norcal",11,7,0]
["Solar Fixed","Norcal",11,8,0.1]
["Solar Fixed","Norcal",11,9,0.32]
["Solar Fixed","Norcal",11,10,0.53]
["Solar Fixed","Norcal",11,11,0.6]
["Solar Fixed","Norcal",11,12,0.61]
["Solar Fixed","Norcal",11,13,0.62]
["Solar Fixed","Norcal",11,14,0.57999999999999996]
["Solar Fixed","Norcal",11,15,0.47]
["Solar Fixed","Norcal",11,16,0.28000000000000003]
["Solar Fixed","Norcal",11,17,0.03]
["Solar Fixed","Norcal",11,18,0]
["Solar Fixed","Norcal",11,19,0]
["Solar Fixed","Norcal",11,20,0]
["Solar Fixed","Norcal",11,21,0]
["Solar Fixed","Norcal",11,22,0]
["Solar Fixed","Norcal",11,23,0]
["Solar Fixed","Norcal",11,24,0]
["Solar Fixed","Norcal",12,1,0]
["Solar Fixed","Norcal",12,2,0]
["Solar Fixed","Norcal",12,3,0]
["Solar Fixed","Norcal",12,4,0]
["Solar Fixed","Norcal",12,5,0]
["Solar Fixed","Norcal",12,6,0]
["Solar Fixed","Norcal",12,7,0]
["Solar Fixed","Norcal",12,8,0.02]
["Solar Fixed","Norcal",12,9,0.15]
["Solar Fixed","Norcal",12,10,0.28000000000000003]
["Solar Fixed","Norcal",12,11,0.41]
["Solar Fixed","Norcal",12,12,0.45]
["Solar Fixed","Norcal",12,13,0.42]
["Solar Fixed","Norcal",12,14,0.38]
["Solar Fixed","Norcal",12,15,0.3]
["Solar Fixed","Norcal",12,16,0.15]
["Solar Fixed","Norcal",12,17,0.02]
["Solar Fixed","Norcal",12,18,0]
["Solar Fixed","Norcal",12,19,0]
["Solar Fixed","Norcal",12,20,0]
["Solar Fixed","Norcal",12,21,0]
["Solar Fixed","Norcal",12,22,0]
["Solar Fixed","Norcal",12,23,0]
["Solar Fixed","Norcal",12,24,0]
["Solar Fixed","Socal",1,1,0]
["Solar Fixed","Socal",1,2,0]
["Solar Fixed","Socal",1,3,0]
["Solar Fixed","Socal",1,4,0]
["Solar Fixed","Socal",1,5,0]
["Solar Fixed","Socal",1,6,0]
["Solar Fixed","Socal",1,7,0]
["Solar Fixed","Socal",1,8,0.12]
["Solar Fixed","Socal",1,9,0.42]
["Solar Fixed","Socal",1,10,0.56999999999999995]
["Solar Fixed","Socal",1,11,0.62]
["Solar Fixed","Socal",1,12,0.65]
["Solar Fixed","Socal",1,13,0.62]
["Solar Fixed","Socal",1,14,0.6]
["Solar Fixed","Socal",1,15,0.5]
["Solar Fixed","Socal",1,16,0.28000000000000003]
["Solar Fixed","Socal",1,17,0.04]
["Solar Fixed","Socal",1,18,0]
["Solar Fixed","Socal",1,19,0]
["Solar Fixed","Socal",1,20,0]
["Solar Fixed","Socal",1,21,0]
["Solar Fixed","Socal",1,22,0]
["Solar Fixed","Socal",1,23,0]
["Solar Fixed","Socal",1,24,0]
["Solar Fixed","Socal",2,1,0]
["Solar Fixed","Socal",2,2,0]
["Solar Fixed","Socal",2,3,0]
["Solar Fixed","Socal",2,4,0]
["Solar Fixed","Socal",2,5,0]
["Solar Fixed","Socal",2,6,0]
["Solar Fixed","Socal",2,7,0.01]
["Solar Fixed","Socal",2,8,0.23]
["Solar Fixed","Socal",2,9,0.54]
["Solar Fixed","Socal",2,10,0.66]
["Solar Fixed","Socal",2,11,0.7]
["Solar Fixed","Socal",2,12,0.72]
["Solar Fixed","Socal",2,13,0.71]
["Solar Fixed","Socal",2,14,0.67]
["Solar Fixed","Socal",2,15,0.61]
["Solar Fixed","Socal",2,16,0.47]
["Solar Fixed","Socal",2,17,0.17]
["Solar Fixed","Socal",2,18,0]
["Solar Fixed","Socal",2,19,0]
["Solar Fixed","Socal",2,20,0]
["Solar Fixed","Socal",2,21,0]
["Solar Fixed","Socal",2,22,0]
["Solar Fixed","Socal",2,23,0]
["Solar Fixed","Socal",2,24,0]
["Solar Fixed","Socal",3,1,0]
["Solar Fixed","Socal",3,2,0]
["Solar Fixed","Socal",3,3,0]
["Solar Fixed","Socal",3,4,0]
["Solar Fixed","Socal",3,5,0]
["Solar Fixed","Socal",3,6,0]
["Solar Fixed","Socal",3,7,0]
["Solar Fixed","Socal",3,8,0.13]
["Solar Fixed","Socal",3,9,0.46]
["Solar Fixed","Socal",3,10,0.65]
["Solar Fixed","Socal",3,11,0.72]
["Solar Fixed","Socal",3,12,0.73]
["Solar Fixed","Socal",3,13,0.73]
["Solar Fixed","Socal",3,14,0.7]
["Solar Fixed","Socal",3,15,0.65]
["Solar Fixed","Socal",3,16,0.56999999999999995]
["Solar Fixed","Socal",3,17,0.36]
["Solar Fixed","Socal",3,18,0.05]
["Solar Fixed","Socal",3,19,0]
["Solar Fixed","Socal",3,20,0]
["Solar Fixed","Socal",3,21,0]
["Solar Fixed","Socal",3,22,0]
["Solar Fixed","Socal",3,23,0]
["Solar Fixed","Socal",3,24,0]
["Solar Fixed","Socal",4,1,0]
["Solar Fixed","Socal",4,2,0]
["Solar Fixed","Socal",4,3,0]
["Solar Fixed","Socal",4,4,0]
["Solar Fixed","Socal",4,5,0]
["Solar Fixed","Socal",4,6,0]
["Solar Fixed","Socal",4,7,0.02]
["Solar Fixed","Socal",4,8,0.26]
["Solar Fixed","Socal",4,9,0.56999999999999995]
["Solar Fixed","Socal",4,10,0.72]
["Solar Fixed","Socal",4,11,0.79]
["Solar Fixed","Socal",4,12,0.82]
["Solar Fixed","Socal",4,13,0.82]
["Solar Fixed","Socal",4,14,0.8]
["Solar Fixed","Socal",4,15,0.78]
["Solar Fixed","Socal",4,16,0.71]
["Solar Fixed","Socal",4,17,0.6]
["Solar Fixed","Socal",4,18,0.42]
["Solar Fixed","Socal",4,19,0.1]
["Solar Fixed","Socal",4,20,0]
["Solar Fixed","Socal",4,21,0]
["Solar Fixed","Socal",4,22,0]
["Solar Fixed","Socal",4,23,0]
["Solar Fixed","Socal",4,24,0]
["Solar Fixed","Socal",5,1,0]
["Solar Fixed","Socal",5,2,0]
["Solar Fixed","Socal",5,3,0]
["Solar Fixed","Socal",5,4,0]
["Solar Fixed","Socal",5,5,0]
["Solar Fixed","Socal",5,6,0]
["Solar Fixed","Socal",5,7,0.1]
["Solar Fixed","Socal",5,8,0.4]
["Solar Fixed","Socal",5,9,0.61]
["Solar Fixed","Socal",5,10,0.74]
["Solar Fixed","Socal",5,11,0.82]
["Solar Fixed","Socal",5,12,0.85]
["Solar Fixed","Socal",5,13,0.86]
["Solar Fixed","Socal",5,14,0.85]
["Solar Fixed","Socal",5,15,0.84]
["Solar Fixed","Socal",5,16,0.78]
["Solar Fixed","Socal",5,17,0.67]
["Solar Fixed","Socal",5,18,0.49]
["Solar Fixed","Socal",5,19,0.19]
["Solar Fixed","Socal",5,20,0.01]
["Solar Fixed","Socal",5,21,0]
["Solar Fixed","Socal",5,22,0]
["Solar Fixed","Socal",5,23,0]
["Solar Fixed","Socal",5,24,0]
["Solar Fixed","Socal",6,1,0]
["Solar Fixed","Socal",6,2,0]
["Solar Fixed","Socal",6,3,0]
["Solar Fixed","Socal",6,4,0]
["Solar Fixed","Socal",6,5,0]
["Solar Fixed","Socal",6,6,0]
["Solar Fixed","Socal",6,7,0.14000000000000001]
["Solar Fixed","Socal",6,8,0.42]
["Solar Fixed","Socal",6,9,0.64]
["Solar Fixed","Socal",6,10,0.77]
["Solar Fixed","Socal",6,11,0.85]
["Solar Fixed","Socal",6,12,0.89]
["Solar Fixed","Socal",6,13,0.9]
["Solar Fixed","Socal",6,14,0.89]
["Solar Fixed","Socal",6,15,0.87]
["Solar Fixed","Socal",6,16,0.79]
["Solar Fixed","Socal",6,17,0.71]
["Solar Fixed","Socal",6,18,0.54]
["Solar Fixed","Socal",6,19,0.25]
["Solar Fixed","Socal",6,20,0.03]
["Solar Fixed","Socal",6,21,0]
["Solar Fixed","Socal",6,22,0]
["Solar Fixed","Socal",6,23,0]
["Solar Fixed","Socal",6,24,0]
["Solar Fixed","Socal",7,1,0]
["Solar Fixed","Socal",7,2,0]
["Solar Fixed","Socal",7,3,0]
["Solar Fixed","Socal",7,4,0]
["Solar Fixed","Socal",7,5,0]
["Solar Fixed","Socal",7,6,0]
["Solar Fixed","Socal",7,7,0.06]
["Solar Fixed","Socal",7,8,0.28999999999999998]
["Solar Fixed","Socal",7,9,0.53]
["Solar Fixed","Socal",7,10,0.69]
["Solar Fixed","Socal",7,11,0.78]
["Solar Fixed","Socal",7,12,0.85]
["Solar Fixed","Socal",7,13,0.86]
["Solar Fixed","Socal",7,14,0.85]
["Solar Fixed","Socal",7,15,0.82]
["Solar Fixed","Socal",7,16,0.76]
["Solar Fixed","Socal",7,17,0.67]
["Solar Fixed","Socal",7,18,0.5]
["Solar Fixed","Socal",7,19,0.22]
["Solar Fixed","Socal",7,20,0.03]
["Solar Fixed","Socal",7,21,0]
["Solar Fixed","Socal",7,22,0]
["Solar Fixed","Socal",7,23,0]
["Solar Fixed","Socal",7,24,0]
["Solar Fixed","Socal",8,1,0]
["Solar Fixed","Socal",8,2,0]
["Solar Fixed","Socal",8,3,0]
["Solar Fixed","Socal",8,4,0]
["Solar Fixed","Socal",8,5,0]
["Solar Fixed","Socal",8,6,0]
["Solar Fixed","Socal",8,7,0.03]
["Solar Fixed","Socal",8,8,0.26]
["Solar Fixed","Socal",8,9,0.56000000000000005]
["Solar Fixed","Socal",8,10,0.72]
["Solar Fixed","Socal",8,11,0.82]
["Solar Fixed","Socal",8,12,0.87]
["Solar Fixed","Socal",8,13,0.89]
["Solar Fixed","Socal",8,14,0.87]
["Solar Fixed","Socal",8,15,0.83]
["Solar Fixed","Socal",8,16,0.75]
["Solar Fixed","Socal",8,17,0.64]
["Solar Fixed","Socal",8,18,0.43]
["Solar Fixed","Socal",8,19,0.12]
["Solar Fixed","Socal",8,20,0]
["Solar Fixed","Socal",8,21,0]
["Solar Fixed","Socal",8,22,0]
["Solar Fixed","Socal",8,23,0]
["Solar Fixed","Socal",8,24,0]
["Solar Fixed","Socal",9,1,0]
["Solar Fixed","Socal",9,2,0]
["Solar Fixed","Socal",9,3,0]
["Solar Fixed","Socal",9,4,0]
["Solar Fixed","Socal",9,5,0]
["Solar Fixed","Socal",9,6,0]
["Solar Fixed","Socal",9,7,0.01]
["Solar Fixed","Socal",9,8,0.2]
["Solar Fixed","Socal",9,9,0.52]
["Solar Fixed","Socal",9,10,0.7]
["Solar Fixed","Socal",9,11,0.8]
["Solar Fixed","Socal",9,12,0.84]
["Solar Fixed","Socal",9,13,0.86]
["Solar Fixed","Socal",9,14,0.85]
["Solar Fixed","Socal",9,15,0.81]
["Solar Fixed","Socal",9,16,0.72]
["Solar Fixed","Socal",9,17,0.56000000000000005]
["Solar Fixed","Socal",9,18,0.25]
["Solar Fixed","Socal",9,19,0.02]
["Solar Fixed","Socal",9,20,0]
["Solar Fixed","Socal",9,21,0]
["Solar Fixed","Socal",9,22,0]
["Solar Fixed","Socal",9,23,0]
["Solar Fixed","Socal",9,24,0]
["Solar Fixed","Socal",10,1,0]
["Solar Fixed","Socal",10,2,0]
["Solar Fixed","Socal",10,3,0]
["Solar Fixed","Socal",10,4,0]
["Solar Fixed","Socal",10,5,0]
["Solar Fixed","Socal",10,6,0]
["Solar Fixed","Socal",10,7,0]
["Solar Fixed","Socal",10,8,0.11]
["Solar Fixed","Socal",10,9,0.45]
["Solar Fixed","Socal",10,10,0.65]
["Solar Fixed","Socal",10,11,0.73]
["Solar Fixed","Socal",10,12,0.78]
["Solar Fixed","Socal",10,13,0.8]
["Solar Fixed","Socal",10,14,0.78]
["Solar Fixed","Socal",10,15,0.75]
["Solar Fixed","Socal",10,16,0.66]
["Solar Fixed","Socal",10,17,0.42]
["Solar Fixed","Socal",10,18,0.08]
["Solar Fixed","Socal",10,19,0]
["Solar Fixed","Socal",10,20,0]
["Solar Fixed","Socal",10,21,0]
["Solar Fixed","Socal",10,22,0]
["Solar Fixed","Socal",10,23,0]
["Solar Fixed","Socal",10,24,0]
["Solar Fixed","Socal",11,1,0]
["Solar Fixed","Socal",11,2,0]
["Solar Fixed","Socal",11,3,0]
["Solar Fixed","Socal",11,4,0]
["Solar Fixed","Socal",11,5,0]
["Solar Fixed","Socal",11,6,0]
["Solar Fixed","Socal",11,7,0.02]
["Solar Fixed","Socal",11,8,0.25]
["Solar Fixed","Socal",11,9,0.51]
["Solar Fixed","Socal",11,10,0.64]
["Solar Fixed","Socal",11,11,0.68]
["Solar Fixed","Socal",11,12,0.7]
["Solar Fixed","Socal",11,13,0.69]
["Solar Fixed","Socal",11,14,0.62]
["Solar Fixed","Socal",11,15,0.51]
["Solar Fixed","Socal",11,16,0.24]
["Solar Fixed","Socal",11,17,0.01]
["Solar Fixed","Socal",11,18,0]
["Solar Fixed","Socal",11,19,0]
["Solar Fixed","Socal",11,20,0]
["Solar Fixed","Socal",11,21,0]
["Solar Fixed","Socal",11,22,0]
["Solar Fixed","Socal",11,23,0]
["Solar Fixed","Socal",11,24,0]
["Solar Fixed","Socal",12,1,0]
["Solar Fixed","Socal",12,2,0]
["Solar Fixed","Socal",12,3,0]
["Solar Fixed","Socal",12,4,0]
["Solar Fixed","Socal",12,5,0]
["Solar Fixed","Socal",12,6,0]
["Solar Fixed","Socal",12,7,0]
["Solar Fixed","Socal",12,8,0.12]
["Solar Fixed","Socal",12,9,0.37]
["Solar Fixed","Socal",12,10,0.48]
["Solar Fixed","Socal",12,11,0.55000000000000004]
["Solar Fixed","Socal",12,12,0.57999999999999996]
["Solar Fixed","Socal",12,13,0.56000000000000005]
["Solar Fixed","Socal",12,14,0.51]
["Solar Fixed","Socal",12,15,0.39]
["Solar Fixed","Socal",12,16,0.17]
["Solar Fixed","Socal",12,17,0.01]
["Solar Fixed","Socal",12,18,0]
["Solar Fixed","Socal",12,19,0]
["Solar Fixed","Socal",12,20,0]
["Solar Fixed","Socal",12,21,0]
["Solar Fixed","Socal",12,22,0]
["Solar Fixed","Socal",12,23,0]
["Solar Fixed","Socal",12,24,0]
["Solar Tracking","Norcal",1,1,0]
["Solar Tracking","Norcal",1,2,0]
["Solar Tracking","Norcal",1,3,0]
["Solar Tracking","Norcal",1,4,0]
["Solar Tracking","Norcal",1,5,0]
["Solar Tracking","Norcal",1,6,0]
["Solar Tracking","Norcal",1,7,0]
["Solar Tracking","Norcal",1,8,0.02]
["Solar Tracking","Norcal",1,9,0.14000000000000001]
["Solar Tracking","Norcal",1,10,0.28000000000000003]
["Solar Tracking","Norcal",1,11,0.35]
["Solar Tracking","Norcal",1,12,0.41]
["Solar Tracking","Norcal",1,13,0.4]
["Solar Tracking","Norcal",1,14,0.36]
["Solar Tracking","Norcal",1,15,0.34]
["Solar Tracking","Norcal",1,16,0.21]
["Solar Tracking","Norcal",1,17,0.05]
["Solar Tracking","Norcal",1,18,0]
["Solar Tracking","Norcal",1,19,0]
["Solar Tracking","Norcal",1,20,0]
["Solar Tracking","Norcal",1,21,0]
["Solar Tracking","Norcal",1,22,0]
["Solar Tracking","Norcal",1,23,0]
["Solar Tracking","Norcal",1,24,0]
["Solar Tracking","Norcal",2,1,0]
["Solar Tracking","Norcal",2,2,0]
["Solar Tracking","Norcal",2,3,0]
["Solar Tracking","Norcal",2,4,0]
["Solar Tracking","Norcal",2,5,0]
["Solar Tracking","Norcal",2,6,0]
["Solar Tracking","Norcal",2,7,0]
["Solar Tracking","Norcal",2,8,0.11]
["Solar Tracking","Norcal",2,9,0.47]
["Solar Tracking","Norcal",2,10,0.59]
["Solar Tracking","Norcal",2,11,0.59]
["Solar Tracking","Norcal",2,12,0.59]
["Solar Tracking","Norcal",2,13,0.59]
["Solar Tracking","Norcal",2,14,0.56999999999999995]
["Solar Tracking","Norcal",2,15,0.56000000000000005]
["Solar Tracking","Norcal",2,16,0.48]
["Solar Tracking","Norcal",2,17,0.23]
["Solar Tracking","Norcal",2,18,0.01]
["Solar Tracking","Norcal",2,19,0]
["Solar Tracking","Norcal",2,20,0]
["Solar Tracking","Norcal",2,21,0]
["Solar Tracking","Norcal",2,22,0]
["Solar Tracking","Norcal",2,23,0]
["Solar Tracking","Norcal",2,24,0]
["Solar Tracking","Norcal",3,1,0]
["Solar Tracking","Norcal",3,2,0]
["Solar Tracking","Norcal",3,3,0]
["Solar Tracking","Norcal",3,4,0]
["Solar Tracking","Norcal",3,5,0]
["Solar Tracking","Norcal",3,6,0]
["Solar Tracking","Norcal",3,7,0]
["Solar Tracking","Norcal",3,8,0.06]
["Solar Tracking","Norcal",3,9,0.36]
["Solar Tracking","Norcal",3,10,0.59]
["Solar Tracking","Norcal",3,11,0.64]
["Solar Tracking","Norcal",3,12,0.62]
["Solar Tracking","Norcal",3,13,0.62]
["Solar Tracking","Norcal",3,14,0.6]
["Solar Tracking","Norcal",3,15,0.56000000000000005]
["Solar Tracking","Norcal",3,16,0.51]
["Solar Tracking","Norcal",3,17,0.42]
["Solar Tracking","Norcal",3,18,0.11]
["Solar Tracking","Norcal",3,19,0]
["Solar Tracking","Norcal",3,20,0]
["Solar Tracking","Norcal",3,21,0]
["Solar Tracking","Norcal",3,22,0]
["Solar Tracking","Norcal",3,23,0]
["Solar Tracking","Norcal",3,24,0]
["Solar Tracking","Norcal",4,1,0]
["Solar Tracking","Norcal",4,2,0]
["Solar Tracking","Norcal",4,3,0]
["Solar Tracking","Norcal",4,4,0]
["Solar Tracking","Norcal",4,5,0]
["Solar Tracking","Norcal",4,6,0]
["Solar Tracking","Norcal",4,7,0]
["Solar Tracking","Norcal",4,8,0.23]
["Solar Tracking","Norcal",4,9,0.56999999999999995]
["Solar Tracking","Norcal",4,10,0.66]
["Solar Tracking","Norcal",4,11,0.65]
["Solar Tracking","Norcal",4,12,0.66]
["Solar Tracking","Norcal",4,13,0.69]
["Solar Tracking","Norcal",4,14,0.68]
["Solar Tracking","Norcal",4,15,0.68]
["Solar Tracking","Norcal",4,16,0.66]
["Solar Tracking","Norcal",4,17,0.64]
["Solar Tracking","Norcal",4,18,0.56000000000000005]
["Solar Tracking","Norcal",4,19,0.23]
["Solar Tracking","Norcal",4,20,0.01]
["Solar Tracking","Norcal",4,21,0]
["Solar Tracking","Norcal",4,22,0]
["Solar Tracking","Norcal",4,23,0]
["Solar Tracking","Norcal",4,24,0]
["Solar Tracking","Norcal",5,1,0]
["Solar Tracking","Norcal",5,2,0]
["Solar Tracking","Norcal",5,3,0]
["Solar Tracking","Norcal",5,4,0]
["Solar Tracking","Norcal",5,5,0]
["Solar Tracking","Norcal",5,6,0]
["Solar Tracking","Norcal",5,7,0.08]
["Solar Tracking","Norcal",5,8,0.47]
["Solar Tracking","Norcal",5,9,0.66]
["Solar Tracking","Norcal",5,10,0.69]
["Solar Tracking","Norcal",5,11,0.7]
["Solar Tracking","Norcal",5,12,0.7]
["Solar Tracking","Norcal",5,13,0.7]
["Solar Tracking","Norcal",5,14,0.7]
["Solar Tracking","Norcal",5,15,0.72]
["Solar Tracking","Norcal",5,16,0.73]
["Solar Tracking","Norcal",5,17,0.71]
["Solar Tracking","Norcal",5,18,0.67]
["Solar Tracking","Norcal",5,19,0.41]
["Solar Tracking","Norcal",5,20,0.05]
["Solar Tracking","Norcal",5,21,0]
["Solar Tracking","Norcal",5,22,0]
["Solar Tracking","Norcal",5,23,0]
["Solar Tracking","Norcal",5,24,0]
["Solar Tracking","Norcal",6,1,0]
["Solar Tracking","Norcal",6,2,0]
["Solar Tracking","Norcal",6,3,0]
["Solar Tracking","Norcal",6,4,0]
["Solar Tracking","Norcal",6,5,0]
["Solar Tracking","Norcal",6,6,0]
["Solar Tracking","Norcal",6,7,0.16]
["Solar Tracking","Norcal",6,8,0.56999999999999995]
["Solar Tracking","Norcal",6,9,0.77]
["Solar Tracking","Norcal",6,10,0.83]
["Solar Tracking","Norcal",6,11,0.84]
["Solar Tracking","Norcal",6,12,0.85]
["Solar Tracking","Norcal",6,13,0.85]
["Solar Tracking","Norcal",6,14,0.85]
["Solar Tracking","Norcal",6,15,0.84]
["Solar Tracking","Norcal",6,16,0.84]
["Solar Tracking","Norcal",6,17,0.82]
["Solar Tracking","Norcal",6,18,0.76]
["Solar Tracking","Norcal",6,19,0.55000000000000004]
["Solar Tracking","Norcal",6,20,0.15]
["Solar Tracking","Norcal",6,21,0]
["Solar Tracking","Norcal",6,22,0]
["Solar Tracking","Norcal",6,23,0]
["Solar Tracking","Norcal",6,24,0]
["Solar Tracking","Norcal",7,1,0]
["Solar Tracking","Norcal",7,2,0]
["Solar Tracking","Norcal",7,3,0]
["Solar Tracking","Norcal",7,4,0]
["Solar Tracking","Norcal",7,5,0]
["Solar Tracking","Norcal",7,6,0]
["Solar Tracking","Norcal",7,7,7.0000000000000007E-2]
["Solar Tracking","Norcal",7,8,0.46]
["Solar Tracking","Norcal",7,9,0.77]
["Solar Tracking","Norcal",7,10,0.85]
["Solar Tracking","Norcal",7,11,0.86]
["Solar Tracking","Norcal",7,12,0.86]
["Solar Tracking","Norcal",7,13,0.86]
["Solar Tracking","Norcal",7,14,0.85]
["Solar Tracking","Norcal",7,15,0.84]
["Solar Tracking","Norcal",7,16,0.84]
["Solar Tracking","Norcal",7,17,0.81]
["Solar Tracking","Norcal",7,18,0.75]
["Solar Tracking","Norcal",7,19,0.52]
["Solar Tracking","Norcal",7,20,0.12]
["Solar Tracking","Norcal",7,21,0]
["Solar Tracking","Norcal",7,22,0]
["Solar Tracking","Norcal",7,23,0]
["Solar Tracking","Norcal",7,24,0]
["Solar Tracking","Norcal",8,1,0]
["Solar Tracking","Norcal",8,2,0]
["Solar Tracking","Norcal",8,3,0]
["Solar Tracking","Norcal",8,4,0]
["Solar Tracking","Norcal",8,5,0]
["Solar Tracking","Norcal",8,6,0]
["Solar Tracking","Norcal",8,7,0.01]
["Solar Tracking","Norcal",8,8,0.28000000000000003]
["Solar Tracking","Norcal",8,9,0.65]
["Solar Tracking","Norcal",8,10,0.78]
["Solar Tracking","Norcal",8,11,0.82]
["Solar Tracking","Norcal",8,12,0.82]
["Solar Tracking","Norcal",8,13,0.82]
["Solar Tracking","Norcal",8,14,0.81]
["Solar Tracking","Norcal",8,15,0.81]
["Solar Tracking","Norcal",8,16,0.81]
["Solar Tracking","Norcal",8,17,0.78]
["Solar Tracking","Norcal",8,18,0.63]
["Solar Tracking","Norcal",8,19,0.28000000000000003]
["Solar Tracking","Norcal",8,20,0.02]
["Solar Tracking","Norcal",8,21,0]
["Solar Tracking","Norcal",8,22,0]
["Solar Tracking","Norcal",8,23,0]
["Solar Tracking","Norcal",8,24,0]
["Solar Tracking","Norcal",9,1,0]
["Solar Tracking","Norcal",9,2,0]
["Solar Tracking","Norcal",9,3,0]
["Solar Tracking","Norcal",9,4,0]
["Solar Tracking","Norcal",9,5,0]
["Solar Tracking","Norcal",9,6,0]
["Solar Tracking","Norcal",9,7,0]
["Solar Tracking","Norcal",9,8,0.14000000000000001]
["Solar Tracking","Norcal",9,9,0.52]
["Solar Tracking","Norcal",9,10,0.69]
["Solar Tracking","Norcal",9,11,0.73]
["Solar Tracking","Norcal",9,12,0.74]
["Solar Tracking","Norcal",9,13,0.73]
["Solar Tracking","Norcal",9,14,0.73]
["Solar Tracking","Norcal",9,15,0.73]
["Solar Tracking","Norcal",9,16,0.74]
["Solar Tracking","Norcal",9,17,0.67]
["Solar Tracking","Norcal",9,18,0.41]
["Solar Tracking","Norcal",9,19,0.06]
["Solar Tracking","Norcal",9,20,0]
["Solar Tracking","Norcal",9,21,0]
["Solar Tracking","Norcal",9,22,0]
["Solar Tracking","Norcal",9,23,0]
["Solar Tracking","Norcal",9,24,0]
["Solar Tracking","Norcal",10,1,0]
["Solar Tracking","Norcal",10,2,0]
["Solar Tracking","Norcal",10,3,0]
["Solar Tracking","Norcal",10,4,0]
["Solar Tracking","Norcal",10,5,0]
["Solar Tracking","Norcal",10,6,0]
["Solar Tracking","Norcal",10,7,0]
["Solar Tracking","Norcal",10,8,0.04]
["Solar Tracking","Norcal",10,9,0.33]
["Solar Tracking","Norcal",10,10,0.59]
["Solar Tracking","Norcal",10,11,0.63]
["Solar Tracking","Norcal",10,12,0.62]
["Solar Tracking","Norcal",10,13,0.6]
["Solar Tracking","Norcal",10,14,0.62]
["Solar Tracking","Norcal",10,15,0.63]
["Solar Tracking","Norcal",10,16,0.62]
["Solar Tracking","Norcal",10,17,0.5]
["Solar Tracking","Norcal",10,18,0.14000000000000001]
["Solar Tracking","Norcal",10,19,0]
["Solar Tracking","Norcal",10,20,0]
["Solar Tracking","Norcal",10,21,0]
["Solar Tracking","Norcal",10,22,0]
["Solar Tracking","Norcal",10,23,0]
["Solar Tracking","Norcal",10,24,0]
["Solar Tracking","Norcal",11,1,0]
["Solar Tracking","Norcal",11,2,0]
["Solar Tracking","Norcal",11,3,0]
["Solar Tracking","Norcal",11,4,0]
["Solar Tracking","Norcal",11,5,0]
["Solar Tracking","Norcal",11,6,0]
["Solar Tracking","Norcal",11,7,0]
["Solar Tracking","Norcal",11,8,0.09]
["Solar Tracking","Norcal",11,9,0.32]
["Solar Tracking","Norcal",11,10,0.46]
["Solar Tracking","Norcal",11,11,0.49]
["Solar Tracking","Norcal",11,12,0.48]
["Solar Tracking","Norcal",11,13,0.49]
["Solar Tracking","Norcal",11,14,0.5]
["Solar Tracking","Norcal",11,15,0.46]
["Solar Tracking","Norcal",11,16,0.27]
["Solar Tracking","Norcal",11,17,0.03]
["Solar Tracking","Norcal",11,18,0]
["Solar Tracking","Norcal",11,19,0]
["Solar Tracking","Norcal",11,20,0]
["Solar Tracking","Norcal",11,21,0]
["Solar Tracking","Norcal",11,22,0]
["Solar Tracking","Norcal",11,23,0]
["Solar Tracking","Norcal",11,24,0]
["Solar Tracking","Norcal",12,1,0]
["Solar Tracking","Norcal",12,2,0]
["Solar Tracking","Norcal",12,3,0]
["Solar Tracking","Norcal",12,4,0]
["Solar Tracking","Norcal",12,5,0]
["Solar Tracking","Norcal",12,6,0]
["Solar Tracking","Norcal",12,7,0]
["Solar Tracking","Norcal",12,8,0.02]
["Solar Tracking","Norcal",12,9,0.12]
["Solar Tracking","Norcal",12,10,0.22]
["Solar Tracking","Norcal",12,11,0.28999999999999998]
["Solar Tracking","Norcal",12,12,0.33]
["Solar Tracking","Norcal",12,13,0.34]
["Solar Tracking","Norcal",12,14,0.31]
["Solar Tracking","Norcal",12,15,0.26]
["Solar Tracking","Norcal",12,16,0.14000000000000001]
["Solar Tracking","Norcal",12,17,0.02]
["Solar Tracking","Norcal",12,18,0]
["Solar Tracking","Norcal",12,19,0]
["Solar Tracking","Norcal",12,20,0]
["Solar Tracking","Norcal",12,21,0]
["Solar Tracking","Norcal",12,22,0]
["Solar Tracking","Norcal",12,23,0]
["Solar Tracking","Norcal",12,24,0]
["Solar Tracking","Socal",1,1,0]
["Solar Tracking","Socal",1,2,0]
["Solar Tracking","Socal",1,3,0]
["Solar Tracking","Socal",1,4,0]
["Solar Tracking","Socal",1,5,0]
["Solar Tracking","Socal",1,6,0]
["Solar Tracking","Socal",1,7,0]
["Solar Tracking","Socal",1,8,0.11]
["Solar Tracking","Socal",1,9,0.4]
["Solar Tracking","Socal",1,10,0.53]
["Solar Tracking","Socal",1,11,0.55000000000000004]
["Solar Tracking","Socal",1,12,0.56999999999999995]
["Solar Tracking","Socal",1,13,0.55000000000000004]
["Solar Tracking","Socal",1,14,0.53]
["Solar Tracking","Socal",1,15,0.48]
["Solar Tracking","Socal",1,16,0.31]
["Solar Tracking","Socal",1,17,0.06]
["Solar Tracking","Socal",1,18,0]
["Solar Tracking","Socal",1,19,0]
["Solar Tracking","Socal",1,20,0]
["Solar Tracking","Socal",1,21,0]
["Solar Tracking","Socal",1,22,0]
["Solar Tracking","Socal",1,23,0]
["Solar Tracking","Socal",1,24,0]
["Solar Tracking","Socal",2,1,0]
["Solar Tracking","Socal",2,2,0]
["Solar Tracking","Socal",2,3,0]
["Solar Tracking","Socal",2,4,0]
["Solar Tracking","Socal",2,5,0]
["Solar Tracking","Socal",2,6,0]
["Solar Tracking","Socal",2,7,0.01]
["Solar Tracking","Socal",2,8,0.23]
["Solar Tracking","Socal",2,9,0.6]
["Solar Tracking","Socal",2,10,0.66]
["Solar Tracking","Socal",2,11,0.66]
["Solar Tracking","Socal",2,12,0.64]
["Solar Tracking","Socal",2,13,0.63]
["Solar Tracking","Socal",2,14,0.61]
["Solar Tracking","Socal",2,15,0.59]
["Solar Tracking","Socal",2,16,0.52]
["Solar Tracking","Socal",2,17,0.22]
["Solar Tracking","Socal",2,18,0.01]
["Solar Tracking","Socal",2,19,0]
["Solar Tracking","Socal",2,20,0]
["Solar Tracking","Socal",2,21,0]
["Solar Tracking","Socal",2,22,0]
["Solar Tracking","Socal",2,23,0]
["Solar Tracking","Socal",2,24,0]
["Solar Tracking","Socal",3,1,0]
["Solar Tracking","Socal",3,2,0]
["Solar Tracking","Socal",3,3,0]
["Solar Tracking","Socal",3,4,0]
["Solar Tracking","Socal",3,5,0]
["Solar Tracking","Socal",3,6,0]
["Solar Tracking","Socal",3,7,0]
["Solar Tracking","Socal",3,8,0.14000000000000001]
["Solar Tracking","Socal",3,9,0.51]
["Solar Tracking","Socal",3,10,0.67]
["Solar Tracking","Socal",3,11,0.7]
["Solar Tracking","Socal",3,12,0.67]
["Solar Tracking","Socal",3,13,0.66]
["Solar Tracking","Socal",3,14,0.64]
["Solar Tracking","Socal",3,15,0.6]
["Solar Tracking","Socal",3,16,0.55000000000000004]
["Solar Tracking","Socal",3,17,0.41]
["Solar Tracking","Socal",3,18,7.0000000000000007E-2]
["Solar Tracking","Socal",3,19,0]
["Solar Tracking","Socal",3,20,0]
["Solar Tracking","Socal",3,21,0]
["Solar Tracking","Socal",3,22,0]
["Solar Tracking","Socal",3,23,0]
["Solar Tracking","Socal",3,24,0]
["Solar Tracking","Socal",4,1,0]
["Solar Tracking","Socal",4,2,0]
["Solar Tracking","Socal",4,3,0]
["Solar Tracking","Socal",4,4,0]
["Solar Tracking","Socal",4,5,0]
["Solar Tracking","Socal",4,6,0]
["Solar Tracking","Socal",4,7,0.02]
["Solar Tracking","Socal",4,8,0.34]
["Solar Tracking","Socal",4,9,0.66]
["Solar Tracking","Socal",4,10,0.73]
["Solar Tracking","Socal",4,11,0.74]
["Solar Tracking","Socal",4,12,0.75]
["Solar Tracking","Socal",4,13,0.76]
["Solar Tracking","Socal",4,14,0.74]
["Solar Tracking","Socal",4,15,0.72]
["Solar Tracking","Socal",4,16,0.7]
["Solar Tracking","Socal",4,17,0.66]
["Solar Tracking","Socal",4,18,0.52]
["Solar Tracking","Socal",4,19,0.17]
["Solar Tracking","Socal",4,20,0]
["Solar Tracking","Socal",4,21,0]
["Solar Tracking","Socal",4,22,0]
["Solar Tracking","Socal",4,23,0]
["Solar Tracking","Socal",4,24,0]
["Solar Tracking","Socal",5,1,0]
["Solar Tracking","Socal",5,2,0]
["Solar Tracking","Socal",5,3,0]
["Solar Tracking","Socal",5,4,0]
["Solar Tracking","Socal",5,5,0]
["Solar Tracking","Socal",5,6,0]
["Solar Tracking","Socal",5,7,0.13]
["Solar Tracking","Socal",5,8,0.52]
["Solar Tracking","Socal",5,9,0.71]
["Solar Tracking","Socal",5,10,0.77]
["Solar Tracking","Socal",5,11,0.81]
["Solar Tracking","Socal",5,12,0.8]
["Solar Tracking","Socal",5,13,0.8]
["Solar Tracking","Socal",5,14,0.8]
["Solar Tracking","Socal",5,15,0.79]
["Solar Tracking","Socal",5,16,0.77]
["Solar Tracking","Socal",5,17,0.73]
["Solar Tracking","Socal",5,18,0.62]
["Solar Tracking","Socal",5,19,0.31]
["Solar Tracking","Socal",5,20,0.02]
["Solar Tracking","Socal",5,21,0]
["Solar Tracking","Socal",5,22,0]
["Solar Tracking","Socal",5,23,0]
["Solar Tracking","Socal",5,24,0]
["Solar Tracking","Socal",6,1,0]
["Solar Tracking","Socal",6,2,0]
["Solar Tracking","Socal",6,3,0]
["Solar Tracking","Socal",6,4,0]
["Solar Tracking","Socal",6,5,0]
["Solar Tracking","Socal",6,6,0]
["Solar Tracking","Socal",6,7,0.19]
["Solar Tracking","Socal",6,8,0.56999999999999995]
["Solar Tracking","Socal",6,9,0.76]
["Solar Tracking","Socal",6,10,0.83]
["Solar Tracking","Socal",6,11,0.86]
["Solar Tracking","Socal",6,12,0.88]
["Solar Tracking","Socal",6,13,0.87]
["Solar Tracking","Socal",6,14,0.87]
["Solar Tracking","Socal",6,15,0.86]
["Solar Tracking","Socal",6,16,0.84]
["Solar Tracking","Socal",6,17,0.81]
["Solar Tracking","Socal",6,18,0.72]
["Solar Tracking","Socal",6,19,0.44]
["Solar Tracking","Socal",6,20,7.0000000000000007E-2]
["Solar Tracking","Socal",6,21,0]
["Solar Tracking","Socal",6,22,0]
["Solar Tracking","Socal",6,23,0]
["Solar Tracking","Socal",6,24,0]
["Solar Tracking","Socal",7,1,0]
["Solar Tracking","Socal",7,2,0]
["Solar Tracking","Socal",7,3,0]
["Solar Tracking","Socal",7,4,0]
["Solar Tracking","Socal",7,5,0]
["Solar Tracking","Socal",7,6,0]
["Solar Tracking","Socal",7,7,0.09]
["Solar Tracking","Socal",7,8,0.45]
["Solar Tracking","Socal",7,9,0.7]
["Solar Tracking","Socal",7,10,0.81]
["Solar Tracking","Socal",7,11,0.84]
["Solar Tracking","Socal",7,12,0.86]
["Solar Tracking","Socal",7,13,0.86]
["Solar Tracking","Socal",7,14,0.84]
["Solar Tracking","Socal",7,15,0.84]
["Solar Tracking","Socal",7,16,0.82]
["Solar Tracking","Socal",7,17,0.79]
["Solar Tracking","Socal",7,18,0.68]
["Solar Tracking","Socal",7,19,0.4]
["Solar Tracking","Socal",7,20,0.06]
["Solar Tracking","Socal",7,21,0]
["Solar Tracking","Socal",7,22,0]
["Solar Tracking","Socal",7,23,0]
["Solar Tracking","Socal",7,24,0]
["Solar Tracking","Socal",8,1,0]
["Solar Tracking","Socal",8,2,0]
["Solar Tracking","Socal",8,3,0]
["Solar Tracking","Socal",8,4,0]
["Solar Tracking","Socal",8,5,0]
["Solar Tracking","Socal",8,6,0]
["Solar Tracking","Socal",8,7,0.03]
["Solar Tracking","Socal",8,8,0.37]
["Solar Tracking","Socal",8,9,0.71]
["Solar Tracking","Socal",8,10,0.81]
["Solar Tracking","Socal",8,11,0.85]
["Solar Tracking","Socal",8,12,0.87]
["Solar Tracking","Socal",8,13,0.86]
["Solar Tracking","Socal",8,14,0.85]
["Solar Tracking","Socal",8,15,0.84]
["Solar Tracking","Socal",8,16,0.81]
["Solar Tracking","Socal",8,17,0.75]
["Solar Tracking","Socal",8,18,0.59]
["Solar Tracking","Socal",8,19,0.22]
["Solar Tracking","Socal",8,20,0.01]
["Solar Tracking","Socal",8,21,0]
["Solar Tracking","Socal",8,22,0]
["Solar Tracking","Socal",8,23,0]
["Solar Tracking","Socal",8,24,0]
["Solar Tracking","Socal",9,1,0]
["Solar Tracking","Socal",9,2,0]
["Solar Tracking","Socal",9,3,0]
["Solar Tracking","Socal",9,4,0]
["Solar Tracking","Socal",9,5,0]
["Solar Tracking","Socal",9,6,0]
["Solar Tracking","Socal",9,7,0.01]
["Solar Tracking","Socal",9,8,0.24]
["Solar Tracking","Socal",9,9,0.63]
["Solar Tracking","Socal",9,10,0.75]
["Solar Tracking","Socal",9,11,0.8]
["Solar Tracking","Socal",9,12,0.81]
["Solar Tracking","Socal",9,13,0.82]
["Solar Tracking","Socal",9,14,0.8]
["Solar Tracking","Socal",9,15,0.79]
["Solar Tracking","Socal",9,16,0.77]
["Solar Tracking","Socal",9,17,0.67]
["Solar Tracking","Socal",9,18,0.37]
["Solar Tracking","Socal",9,19,0.04]
["Solar Tracking","Socal",9,20,0]
["Solar Tracking","Socal",9,21,0]
["Solar Tracking","Socal",9,22,0]
["Solar Tracking","Socal",9,23,0]
["Solar Tracking","Socal",9,24,0]
["Solar Tracking","Socal",10,1,0]
["Solar Tracking","Socal",10,2,0]
["Solar Tracking","Socal",10,3,0]
["Solar Tracking","Socal",10,4,0]
["Solar Tracking","Socal",10,5,0]
["Solar Tracking","Socal",10,6,0]
["Solar Tracking","Socal",10,7,0]
["Solar Tracking","Socal",10,8,0.11]
["Solar Tracking","Socal",10,9,0.51]
["Solar Tracking","Socal",10,10,0.68]
["Solar Tracking","Socal",10,11,0.71]
["Solar Tracking","Socal",10,12,0.72]
["Solar Tracking","Socal",10,13,0.72]
["Solar Tracking","Socal",10,14,0.72]
["Solar Tracking","Socal",10,15,0.73]
["Solar Tracking","Socal",10,16,0.7]
["Solar Tracking","Socal",10,17,0.52]
["Solar Tracking","Socal",10,18,0.12]
["Solar Tracking","Socal",10,19,0]
["Solar Tracking","Socal",10,20,0]
["Solar Tracking","Socal",10,21,0]
["Solar Tracking","Socal",10,22,0]
["Solar Tracking","Socal",10,23,0]
["Solar Tracking","Socal",10,24,0]
["Solar Tracking","Socal",11,1,0]
["Solar Tracking","Socal",11,2,0]
["Solar Tracking","Socal",11,3,0]
["Solar Tracking","Socal",11,4,0]
["Solar Tracking","Socal",11,5,0]
["Solar Tracking","Socal",11,6,0]
["Solar Tracking","Socal",11,7,0.01]
["Solar Tracking","Socal",11,8,0.25]
["Solar Tracking","Socal",11,9,0.53]
["Solar Tracking","Socal",11,10,0.62]
["Solar Tracking","Socal",11,11,0.62]
["Solar Tracking","Socal",11,12,0.6]
["Solar Tracking","Socal",11,13,0.62]
["Solar Tracking","Socal",11,14,0.6]
["Solar Tracking","Socal",11,15,0.56000000000000005]
["Solar Tracking","Socal",11,16,0.32]
["Solar Tracking","Socal",11,17,0.03]
["Solar Tracking","Socal",11,18,0]
["Solar Tracking","Socal",11,19,0]
["Solar Tracking","Socal",11,20,0]
["Solar Tracking","Socal",11,21,0]
["Solar Tracking","Socal",11,22,0]
["Solar Tracking","Socal",11,23,0]
["Solar Tracking","Socal",11,24,0]
["Solar Tracking","Socal",12,1,0]
["Solar Tracking","Socal",12,2,0]
["Solar Tracking","Socal",12,3,0]
["Solar Tracking","Socal",12,4,0]
["Solar Tracking","Socal",12,5,0]
["Solar Tracking","Socal",12,6,0]
["Solar Tracking","Socal",12,7,0]
["Solar Tracking","Socal",12,8,0.11]
["Solar Tracking","Socal",12,9,0.35]
["Solar Tracking","Socal",12,10,0.44]
["Solar Tracking","Socal",12,11,0.46]
["Solar Tracking","Socal",12,12,0.47]
["Solar Tracking","Socal",12,13,0.5]
["Solar Tracking","Socal",12,14,0.46]
["Solar Tracking","Socal",12,15,0.4]
["Solar Tracking","Socal",12,16,0.22]
["Solar Tracking","Socal",12,17,0.02]
["Solar Tracking","Socal",12,18,0]
["Solar Tracking","Socal",12,19,0]
["Solar Tracking","Socal",12,20,0]
["Solar Tracking","Socal",12,21,0]
["Solar Tracking","Socal",12,22,0]
["Solar Tracking","Socal",12,23,0]
["Solar Tracking","Socal",12,24,0]
["Solar Thermal","Socal",1,1,0]
["Solar Thermal","Socal",1,2,0]
["Solar Thermal","Socal",1,3,0]
["Solar Thermal","Socal",1,4,0]
["Solar Thermal","Socal",1,5,0]
["Solar Thermal","Socal",1,6,0]
["Solar Thermal","Socal",1,7,0]
["Solar Thermal","Socal",1,8,0]
["Solar Thermal","Socal",1,9,0.01]
["Solar Thermal","Socal",1,10,0.09]
["Solar Thermal","Socal",1,11,0.19]
["Solar Thermal","Socal",1,12,0.2]
["Solar Thermal","Socal",1,13,0.18]
["Solar Thermal","Socal",1,14,0.18]
["Solar Thermal","Socal",1,15,0.19]
["Solar Thermal","Socal",1,16,0.14000000000000001]
["Solar Thermal","Socal",1,17,0.04]
["Solar Thermal","Socal",1,18,0]
["Solar Thermal","Socal",1,19,0]
["Solar Thermal","Socal",1,20,0]
["Solar Thermal","Socal",1,21,0]
["Solar Thermal","Socal",1,22,0]
["Solar Thermal","Socal",1,23,0]
["Solar Thermal","Socal",1,24,0]
["Solar Thermal","Socal",2,1,0]
["Solar Thermal","Socal",2,2,0]
["Solar Thermal","Socal",2,3,0]
["Solar Thermal","Socal",2,4,0]
["Solar Thermal","Socal",2,5,0]
["Solar Thermal","Socal",2,6,0]
["Solar Thermal","Socal",2,7,0]
["Solar Thermal","Socal",2,8,0]
["Solar Thermal","Socal",2,9,0.1]
["Solar Thermal","Socal",2,10,0.28999999999999998]
["Solar Thermal","Socal",2,11,0.33]
["Solar Thermal","Socal",2,12,0.32]
["Solar Thermal","Socal",2,13,0.28000000000000003]
["Solar Thermal","Socal",2,14,0.26]
["Solar Thermal","Socal",2,15,0.27]
["Solar Thermal","Socal",2,16,0.26]
["Solar Thermal","Socal",2,17,0.16]
["Solar Thermal","Socal",2,18,0.02]
["Solar Thermal","Socal",2,19,0]
["Solar Thermal","Socal",2,20,0]
["Solar Thermal","Socal",2,21,0]
["Solar Thermal","Socal",2,22,0]
["Solar Thermal","Socal",2,23,0]
["Solar Thermal","Socal",2,24,0]
["Solar Thermal","Socal",3,1,0]
["Solar Thermal","Socal",3,2,0]
["Solar Thermal","Socal",3,3,0]
["Solar Thermal","Socal",3,4,0]
["Solar Thermal","Socal",3,5,0]
["Solar Thermal","Socal",3,6,0]
["Solar Thermal","Socal",3,7,0]
["Solar Thermal","Socal",3,8,0]
["Solar Thermal","Socal",3,9,0.11]
["Solar Thermal","Socal",3,10,0.36]
["Solar Thermal","Socal",3,11,0.43]
["Solar Thermal","Socal",3,12,0.43]
["Solar Thermal","Socal",3,13,0.42]
["Solar Thermal","Socal",3,14,0.41]
["Solar Thermal","Socal",3,15,0.39]
["Solar Thermal","Socal",3,16,0.39]
["Solar Thermal","Socal",3,17,0.28000000000000003]
["Solar Thermal","Socal",3,18,0.13]
["Solar Thermal","Socal",3,19,0]
["Solar Thermal","Socal",3,20,0]
["Solar Thermal","Socal",3,21,0]
["Solar Thermal","Socal",3,22,0]
["Solar Thermal","Socal",3,23,0]
["Solar Thermal","Socal",3,24,0]
["Solar Thermal","Socal",4,1,0]
["Solar Thermal","Socal",4,2,0]
["Solar Thermal","Socal",4,3,0]
["Solar Thermal","Socal",4,4,0]
["Solar Thermal","Socal",4,5,0]
["Solar Thermal","Socal",4,6,0]
["Solar Thermal","Socal",4,7,0]
["Solar Thermal","Socal",4,8,0.02]
["Solar Thermal","Socal",4,9,0.31]
["Solar Thermal","Socal",4,10,0.55000000000000004]
["Solar Thermal","Socal",4,11,0.64]
["Solar Thermal","Socal",4,12,0.66]
["Solar Thermal","Socal",4,13,0.65]
["Solar Thermal","Socal",4,14,0.61]
["Solar Thermal","Socal",4,15,0.53]
["Solar Thermal","Socal",4,16,0.51]
["Solar Thermal","Socal",4,17,0.46]
["Solar Thermal","Socal",4,18,0.38]
["Solar Thermal","Socal",4,19,0.15]
["Solar Thermal","Socal",4,20,0.02]
["Solar Thermal","Socal",4,21,0]
["Solar Thermal","Socal",4,22,0]
["Solar Thermal","Socal",4,23,0]
["Solar Thermal","Socal",4,24,0]
["Solar Thermal","Socal",5,1,0]
["Solar Thermal","Socal",5,2,0]
["Solar Thermal","Socal",5,3,0]
["Solar Thermal","Socal",5,4,0]
["Solar Thermal","Socal",5,5,0]
["Solar Thermal","Socal",5,6,0]
["Solar Thermal","Socal",5,7,0.01]
["Solar Thermal","Socal",5,8,0.22]
["Solar Thermal","Socal",5,9,0.64]
["Solar Thermal","Socal",5,10,0.78]
["Solar Thermal","Socal",5,11,0.82]
["Solar Thermal","Socal",5,12,0.81]
["Solar Thermal","Socal",5,13,0.74]
["Solar Thermal","Socal",5,14,0.73]
["Solar Thermal","Socal",5,15,0.7]
["Solar Thermal","Socal",5,16,0.63]
["Solar Thermal","Socal",5,17,0.56000000000000005]
["Solar Thermal","Socal",5,18,0.5]
["Solar Thermal","Socal",5,19,0.32]
["Solar Thermal","Socal",5,20,7.0000000000000007E-2]
["Solar Thermal","Socal",5,21,0]
["Solar Thermal","Socal",5,22,0]
["Solar Thermal","Socal",5,23,0]
["Solar Thermal","Socal",5,24,0]
["Solar Thermal","Socal",6,1,0]
["Solar Thermal","Socal",6,2,0]
["Solar Thermal","Socal",6,3,0]
["Solar Thermal","Socal",6,4,0]
["Solar Thermal","Socal",6,5,0]
["Solar Thermal","Socal",6,6,0]
["Solar Thermal","Socal",6,7,0.03]
["Solar Thermal","Socal",6,8,0.34]
["Solar Thermal","Socal",6,9,0.71]
["Solar Thermal","Socal",6,10,0.8]
["Solar Thermal","Socal",6,11,0.83]
["Solar Thermal","Socal",6,12,0.83]
["Solar Thermal","Socal",6,13,0.83]
["Solar Thermal","Socal",6,14,0.79]
["Solar Thermal","Socal",6,15,0.74]
["Solar Thermal","Socal",6,16,0.72]
["Solar Thermal","Socal",6,17,0.7]
["Solar Thermal","Socal",6,18,0.62]
["Solar Thermal","Socal",6,19,0.43]
["Solar Thermal","Socal",6,20,0.15]
["Solar Thermal","Socal",6,21,0]
["Solar Thermal","Socal",6,22,0]
["Solar Thermal","Socal",6,23,0]
["Solar Thermal","Socal",6,24,0]
["Solar Thermal","Socal",7,1,0]
["Solar Thermal","Socal",7,2,0]
["Solar Thermal","Socal",7,3,0]
["Solar Thermal","Socal",7,4,0]
["Solar Thermal","Socal",7,5,0]
["Solar Thermal","Socal",7,6,0]
["Solar Thermal","Socal",7,7,0]
["Solar Thermal","Socal",7,8,0.06]
["Solar Thermal","Socal",7,9,0.35]
["Solar Thermal","Socal",7,10,0.53]
["Solar Thermal","Socal",7,11,0.62]
["Solar Thermal","Socal",7,12,0.63]
["Solar Thermal","Socal",7,13,0.64]
["Solar Thermal","Socal",7,14,0.6]
["Solar Thermal","Socal",7,15,0.56999999999999995]
["Solar Thermal","Socal",7,16,0.55000000000000004]
["Solar Thermal","Socal",7,17,0.52]
["Solar Thermal","Socal",7,18,0.47]
["Solar Thermal","Socal",7,19,0.33]
["Solar Thermal","Socal",7,20,0.11]
["Solar Thermal","Socal",7,21,0]
["Solar Thermal","Socal",7,22,0]
["Solar Thermal","Socal",7,23,0]
["Solar Thermal","Socal",7,24,0]
["Solar Thermal","Socal",8,1,0]
["Solar Thermal","Socal",8,2,0]
["Solar Thermal","Socal",8,3,0]
["Solar Thermal","Socal",8,4,0]
["Solar Thermal","Socal",8,5,0]
["Solar Thermal","Socal",8,6,0]
["Solar Thermal","Socal",8,7,0]
["Solar Thermal","Socal",8,8,0.05]
["Solar Thermal","Socal",8,9,0.38]
["Solar Thermal","Socal",8,10,0.65]
["Solar Thermal","Socal",8,11,0.72]
["Solar Thermal","Socal",8,12,0.76]
["Solar Thermal","Socal",8,13,0.74]
["Solar Thermal","Socal",8,14,0.68]
["Solar Thermal","Socal",8,15,0.62]
["Solar Thermal","Socal",8,16,0.56000000000000005]
["Solar Thermal","Socal",8,17,0.54]
["Solar Thermal","Socal",8,18,0.45]
["Solar Thermal","Socal",8,19,0.28000000000000003]
["Solar Thermal","Socal",8,20,0.04]
["Solar Thermal","Socal",8,21,0]
["Solar Thermal","Socal",8,22,0]
["Solar Thermal","Socal",8,23,0]
["Solar Thermal","Socal",8,24,0]
["Solar Thermal","Socal",9,1,0]
["Solar Thermal","Socal",9,2,0]
["Solar Thermal","Socal",9,3,0]
["Solar Thermal","Socal",9,4,0]
["Solar Thermal","Socal",9,5,0]
["Solar Thermal","Socal",9,6,0]
["Solar Thermal","Socal",9,7,0]
["Solar Thermal","Socal",9,8,0.01]
["Solar Thermal","Socal",9,9,0.31]
["Solar Thermal","Socal",9,10,0.63]
["Solar Thermal","Socal",9,11,0.72]
["Solar Thermal","Socal",9,12,0.73]
["Solar Thermal","Socal",9,13,0.71]
["Solar Thermal","Socal",9,14,0.68]
["Solar Thermal","Socal",9,15,0.67]
["Solar Thermal","Socal",9,16,0.65]
["Solar Thermal","Socal",9,17,0.57999999999999996]
["Solar Thermal","Socal",9,18,0.43]
["Solar Thermal","Socal",9,19,0.1]
["Solar Thermal","Socal",9,20,0]
["Solar Thermal","Socal",9,21,0]
["Solar Thermal","Socal",9,22,0]
["Solar Thermal","Socal",9,23,0]
["Solar Thermal","Socal",9,24,0]
["Solar Thermal","Socal",10,1,0]
["Solar Thermal","Socal",10,2,0]
["Solar Thermal","Socal",10,3,0]
["Solar Thermal","Socal",10,4,0]
["Solar Thermal","Socal",10,5,0]
["Solar Thermal","Socal",10,6,0]
["Solar Thermal","Socal",10,7,0]
["Solar Thermal","Socal",10,8,0]
["Solar Thermal","Socal",10,9,0.15]
["Solar Thermal","Socal",10,10,0.56000000000000005]
["Solar Thermal","Socal",10,11,0.69]
["Solar Thermal","Socal",10,12,0.68]
["Solar Thermal","Socal",10,13,0.68]
["Solar Thermal","Socal",10,14,0.67]
["Solar Thermal","Socal",10,15,0.68]
["Solar Thermal","Socal",10,16,0.67]
["Solar Thermal","Socal",10,17,0.56000000000000005]
["Solar Thermal","Socal",10,18,0.23]
["Solar Thermal","Socal",10,19,0.02]
["Solar Thermal","Socal",10,20,0]
["Solar Thermal","Socal",10,21,0]
["Solar Thermal","Socal",10,22,0]
["Solar Thermal","Socal",10,23,0]
["Solar Thermal","Socal",10,24,0]
["Solar Thermal","Socal",11,1,0]
["Solar Thermal","Socal",11,2,0]
["Solar Thermal","Socal",11,3,0]
["Solar Thermal","Socal",11,4,0]
["Solar Thermal","Socal",11,5,0]
["Solar Thermal","Socal",11,6,0]
["Solar Thermal","Socal",11,7,0]
["Solar Thermal","Socal",11,8,0]
["Solar Thermal","Socal",11,9,0.13]
["Solar Thermal","Socal",11,10,0.38]
["Solar Thermal","Socal",11,11,0.47]
["Solar Thermal","Socal",11,12,0.43]
["Solar Thermal","Socal",11,13,0.41]
["Solar Thermal","Socal",11,14,0.43]
["Solar Thermal","Socal",11,15,0.36]
["Solar Thermal","Socal",11,16,0.27]
["Solar Thermal","Socal",11,17,7.0000000000000007E-2]
["Solar Thermal","Socal",11,18,0]
["Solar Thermal","Socal",11,19,0]
["Solar Thermal","Socal",11,20,0]
["Solar Thermal","Socal",11,21,0]
["Solar Thermal","Socal",11,22,0]
["Solar Thermal","Socal",11,23,0]
["Solar Thermal","Socal",11,24,0]
["Solar Thermal","Socal",12,1,0]
["Solar Thermal","Socal",12,2,0]
["Solar Thermal","Socal",12,3,0]
["Solar Thermal","Socal",12,4,0]
["Solar Thermal","Socal",12,5,0]
["Solar Thermal","Socal",12,6,0]
["Solar Thermal","Socal",12,7,0]
["Solar Thermal","Socal",12,8,0]
["Solar Thermal","Socal",12,9,0]
["Solar Thermal","Socal",12,10,0.06]
["Solar Thermal","Socal",12,11,0.12]
["Solar Thermal","Socal",12,12,0.12]
["Solar Thermal","Socal",12,13,0.12]
["Solar Thermal","Socal",12,14,0.12]
["Solar Thermal","Socal",12,15,0.12]
["Solar Thermal","Socal",12,16,0.1]
["Solar Thermal","Socal",12,17,0.01]
["Solar Thermal","Socal",12,18,0]
["Solar Thermal","Socal",12,19,0]
["Solar Thermal","Socal",12,20,0]
["Solar Thermal","Socal",12,21,0]
["Solar Thermal","Socal",12,22,0]
["Solar Thermal","Socal",12,23,0]
["Solar Thermal","Socal",12,24,0]
["Wind","Norcal",1,1,0.04]
["Wind","Norcal",1,2,0.04]
["Wind","Norcal",1,3,0.03]
["Wind","Norcal",1,4,0.03]
["Wind","Norcal",1,5,0.04]
["Wind","Norcal",1,6,0.04]
["Wind","Norcal",1,7,0.03]
["Wind","Norcal",1,8,0.03]
["Wind","Norcal",1,9,0.03]
["Wind","Norcal",1,10,0.03]
["Wind","Norcal",1,11,0.03]
["Wind","Norcal",1,12,0.03]
["Wind","Norcal",1,13,0.02]
["Wind","Norcal",1,14,0.02]
["Wind","Norcal",1,15,0.02]
["Wind","Norcal",1,16,0.02]
["Wind","Norcal",1,17,0.02]
["Wind","Norcal",1,18,0.03]
["Wind","Norcal",1,19,0.03]
["Wind","Norcal",1,20,0.03]
["Wind","Norcal",1,21,0.03]
["Wind","Norcal",1,22,0.03]
["Wind","Norcal",1,23,0.04]
["Wind","Norcal",1,24,0.04]
["Wind","Norcal",2,1,0.08]
["Wind","Norcal",2,2,0.08]
["Wind","Norcal",2,3,7.0000000000000007E-2]
["Wind","Norcal",2,4,0.08]
["Wind","Norcal",2,5,0.06]
["Wind","Norcal",2,6,7.0000000000000007E-2]
["Wind","Norcal",2,7,7.0000000000000007E-2]
["Wind","Norcal",2,8,7.0000000000000007E-2]
["Wind","Norcal",2,9,7.0000000000000007E-2]
["Wind","Norcal",2,10,0.06]
["Wind","Norcal",2,11,0.05]
["Wind","Norcal",2,12,0.05]
["Wind","Norcal",2,13,0.04]
["Wind","Norcal",2,14,0.04]
["Wind","Norcal",2,15,0.04]
["Wind","Norcal",2,16,0.04]
["Wind","Norcal",2,17,0.04]
["Wind","Norcal",2,18,0.04]
["Wind","Norcal",2,19,0.06]
["Wind","Norcal",2,20,7.0000000000000007E-2]
["Wind","Norcal",2,21,7.0000000000000007E-2]
["Wind","Norcal",2,22,7.0000000000000007E-2]
["Wind","Norcal",2,23,0.08]
["Wind","Norcal",2,24,0.09]
["Wind","Norcal",3,1,0.09]
["Wind","Norcal",3,2,0.1]
["Wind","Norcal",3,3,0.08]
["Wind","Norcal",3,4,0.09]
["Wind","Norcal",3,5,7.0000000000000007E-2]
["Wind","Norcal",3,6,0.06]
["Wind","Norcal",3,7,0.05]
["Wind","Norcal",3,8,0.05]
["Wind","Norcal",3,9,0.05]
["Wind","Norcal",3,10,0.04]
["Wind","Norcal",3,11,0.03]
["Wind","Norcal",3,12,0.04]
["Wind","Norcal",3,13,0.04]
["Wind","Norcal",3,14,0.04]
["Wind","Norcal",3,15,0.04]
["Wind","Norcal",3,16,0.04]
["Wind","Norcal",3,17,0.04]
["Wind","Norcal",3,18,0.05]
["Wind","Norcal",3,19,0.06]
["Wind","Norcal",3,20,0.09]
["Wind","Norcal",3,21,0.11]
["Wind","Norcal",3,22,0.1]
["Wind","Norcal",3,23,0.12]
["Wind","Norcal",3,24,0.11]
["Wind","Norcal",4,1,0.28000000000000003]
["Wind","Norcal",4,2,0.27]
["Wind","Norcal",4,3,0.27]
["Wind","Norcal",4,4,0.22]
["Wind","Norcal",4,5,0.19]
["Wind","Norcal",4,6,0.16]
["Wind","Norcal",4,7,0.15]
["Wind","Norcal",4,8,0.12]
["Wind","Norcal",4,9,0.1]
["Wind","Norcal",4,10,0.09]
["Wind","Norcal",4,11,0.08]
["Wind","Norcal",4,12,7.0000000000000007E-2]
["Wind","Norcal",4,13,7.0000000000000007E-2]
["Wind","Norcal",4,14,7.0000000000000007E-2]
["Wind","Norcal",4,15,0.08]
["Wind","Norcal",4,16,0.1]
["Wind","Norcal",4,17,0.17]
["Wind","Norcal",4,18,0.22]
["Wind","Norcal",4,19,0.21]
["Wind","Norcal",4,20,0.24]
["Wind","Norcal",4,21,0.27]
["Wind","Norcal",4,22,0.27]
["Wind","Norcal",4,23,0.28999999999999998]
["Wind","Norcal",4,24,0.3]
["Wind","Norcal",5,1,0.41]
["Wind","Norcal",5,2,0.4]
["Wind","Norcal",5,3,0.39]
["Wind","Norcal",5,4,0.37]
["Wind","Norcal",5,5,0.33]
["Wind","Norcal",5,6,0.28000000000000003]
["Wind","Norcal",5,7,0.24]
["Wind","Norcal",5,8,0.2]
["Wind","Norcal",5,9,0.19]
["Wind","Norcal",5,10,0.16]
["Wind","Norcal",5,11,0.14000000000000001]
["Wind","Norcal",5,12,0.11]
["Wind","Norcal",5,13,0.11]
["Wind","Norcal",5,14,0.13]
["Wind","Norcal",5,15,0.17]
["Wind","Norcal",5,16,0.22]
["Wind","Norcal",5,17,0.31]
["Wind","Norcal",5,18,0.39]
["Wind","Norcal",5,19,0.41]
["Wind","Norcal",5,20,0.41]
["Wind","Norcal",5,21,0.42]
["Wind","Norcal",5,22,0.43]
["Wind","Norcal",5,23,0.42]
["Wind","Norcal",5,24,0.42]
["Wind","Norcal",6,1,0.38]
["Wind","Norcal",6,2,0.4]
["Wind","Norcal",6,3,0.37]
["Wind","Norcal",6,4,0.34]
["Wind","Norcal",6,5,0.31]
["Wind","Norcal",6,6,0.27]
["Wind","Norcal",6,7,0.23]
["Wind","Norcal",6,8,0.17]
["Wind","Norcal",6,9,0.13]
["Wind","Norcal",6,10,0.1]
["Wind","Norcal",6,11,0.08]
["Wind","Norcal",6,12,0.05]
["Wind","Norcal",6,13,0.05]
["Wind","Norcal",6,14,0.06]
["Wind","Norcal",6,15,0.06]
["Wind","Norcal",6,16,0.1]
["Wind","Norcal",6,17,0.17]
["Wind","Norcal",6,18,0.25]
["Wind","Norcal",6,19,0.32]
["Wind","Norcal",6,20,0.33]
["Wind","Norcal",6,21,0.36]
["Wind","Norcal",6,22,0.37]
["Wind","Norcal",6,23,0.36]
["Wind","Norcal",6,24,0.38]
["Wind","Norcal",7,1,0.6]
["Wind","Norcal",7,2,0.59]
["Wind","Norcal",7,3,0.54]
["Wind","Norcal",7,4,0.5]
["Wind","Norcal",7,5,0.48]
["Wind","Norcal",7,6,0.43]
["Wind","Norcal",7,7,0.36]
["Wind","Norcal",7,8,0.31]
["Wind","Norcal",7,9,0.22]
["Wind","Norcal",7,10,0.18]
["Wind","Norcal",7,11,0.12]
["Wind","Norcal",7,12,0.08]
["Wind","Norcal",7,13,0.08]
["Wind","Norcal",7,14,0.11]
["Wind","Norcal",7,15,0.14000000000000001]
["Wind","Norcal",7,16,0.19]
["Wind","Norcal",7,17,0.31]
["Wind","Norcal",7,18,0.4]
["Wind","Norcal",7,19,0.43]
["Wind","Norcal",7,20,0.45]
["Wind","Norcal",7,21,0.5]
["Wind","Norcal",7,22,0.53]
["Wind","Norcal",7,23,0.56999999999999995]
["Wind","Norcal",7,24,0.6]
["Wind","Norcal",8,1,0.49]
["Wind","Norcal",8,2,0.47]
["Wind","Norcal",8,3,0.44]
["Wind","Norcal",8,4,0.4]
["Wind","Norcal",8,5,0.35]
["Wind","Norcal",8,6,0.3]
["Wind","Norcal",8,7,0.26]
["Wind","Norcal",8,8,0.24]
["Wind","Norcal",8,9,0.15]
["Wind","Norcal",8,10,0.1]
["Wind","Norcal",8,11,0.08]
["Wind","Norcal",8,12,0.05]
["Wind","Norcal",8,13,0.04]
["Wind","Norcal",8,14,0.05]
["Wind","Norcal",8,15,0.05]
["Wind","Norcal",8,16,0.09]
["Wind","Norcal",8,17,0.15]
["Wind","Norcal",8,18,0.23]
["Wind","Norcal",8,19,0.3]
["Wind","Norcal",8,20,0.39]
["Wind","Norcal",8,21,0.47]
["Wind","Norcal",8,22,0.5]
["Wind","Norcal",8,23,0.5]
["Wind","Norcal",8,24,0.51]
["Wind","Norcal",9,1,0.19]
["Wind","Norcal",9,2,0.19]
["Wind","Norcal",9,3,0.18]
["Wind","Norcal",9,4,0.16]
["Wind","Norcal",9,5,0.13]
["Wind","Norcal",9,6,0.1]
["Wind","Norcal",9,7,0.1]
["Wind","Norcal",9,8,0.08]
["Wind","Norcal",9,9,0.06]
["Wind","Norcal",9,10,0.04]
["Wind","Norcal",9,11,0.03]
["Wind","Norcal",9,12,0.01]
["Wind","Norcal",9,13,0.01]
["Wind","Norcal",9,14,0.01]
["Wind","Norcal",9,15,0.02]
["Wind","Norcal",9,16,0.03]
["Wind","Norcal",9,17,0.05]
["Wind","Norcal",9,18,7.0000000000000007E-2]
["Wind","Norcal",9,19,0.08]
["Wind","Norcal",9,20,0.12]
["Wind","Norcal",9,21,0.15]
["Wind","Norcal",9,22,0.17]
["Wind","Norcal",9,23,0.18]
["Wind","Norcal",9,24,0.18]
["Wind","Norcal",10,1,0.08]
["Wind","Norcal",10,2,7.0000000000000007E-2]
["Wind","Norcal",10,3,0.06]
["Wind","Norcal",10,4,0.04]
["Wind","Norcal",10,5,0.03]
["Wind","Norcal",10,6,0.03]
["Wind","Norcal",10,7,0.03]
["Wind","Norcal",10,8,0.03]
["Wind","Norcal",10,9,0.03]
["Wind","Norcal",10,10,0.02]
["Wind","Norcal",10,11,0.01]
["Wind","Norcal",10,12,0.01]
["Wind","Norcal",10,13,0.01]
["Wind","Norcal",10,14,0.01]
["Wind","Norcal",10,15,0.01]
["Wind","Norcal",10,16,0.01]
["Wind","Norcal",10,17,0.01]
["Wind","Norcal",10,18,0.01]
["Wind","Norcal",10,19,0.02]
["Wind","Norcal",10,20,0.03]
["Wind","Norcal",10,21,0.04]
["Wind","Norcal",10,22,0.05]
["Wind","Norcal",10,23,0.06]
["Wind","Norcal",10,24,7.0000000000000007E-2]
["Wind","Norcal",11,1,0.04]
["Wind","Norcal",11,2,0.04]
["Wind","Norcal",11,3,0.04]
["Wind","Norcal",11,4,0.03]
["Wind","Norcal",11,5,0.03]
["Wind","Norcal",11,6,0.03]
["Wind","Norcal",11,7,0.03]
["Wind","Norcal",11,8,0.03]
["Wind","Norcal",11,9,0.03]
["Wind","Norcal",11,10,0.02]
["Wind","Norcal",11,11,0.02]
["Wind","Norcal",11,12,0.02]
["Wind","Norcal",11,13,0.02]
["Wind","Norcal",11,14,0.02]
["Wind","Norcal",11,15,0.02]
["Wind","Norcal",11,16,0.02]
["Wind","Norcal",11,17,0.02]
["Wind","Norcal",11,18,0.02]
["Wind","Norcal",11,19,0.02]
["Wind","Norcal",11,20,0.03]
["Wind","Norcal",11,21,0.03]
["Wind","Norcal",11,22,0.04]
["Wind","Norcal",11,23,0.04]
["Wind","Norcal",11,24,0.04]
["Wind","Norcal",12,1,0.04]
["Wind","Norcal",12,2,0.04]
["Wind","Norcal",12,3,0.04]
["Wind","Norcal",12,4,0.04]
["Wind","Norcal",12,5,0.04]
["Wind","Norcal",12,6,0.04]
["Wind","Norcal",12,7,0.04]
["Wind","Norcal",12,8,0.04]
["Wind","Norcal",12,9,0.04]
["Wind","Norcal",12,10,0.03]
["Wind","Norcal",12,11,0.03]
["Wind","Norcal",12,12,0.02]
["Wind","Norcal",12,13,0.03]
["Wind","Norcal",12,14,0.02]
["Wind","Norcal",12,15,0.02]
["Wind","Norcal",12,16,0.02]
["Wind","Norcal",12,17,0.03]
["Wind","Norcal",12,18,0.02]
["Wind","Norcal",12,19,0.03]
["Wind","Norcal",12,20,0.04]
["Wind","Norcal",12,21,0.04]
["Wind","Norcal",12,22,0.04]
["Wind","Norcal",12,23,0.04]
["Wind","Norcal",12,24,0.05]
["Wind","Socal",1,1,0.03]
["Wind","Socal",1,2,0.03]
["Wind","Socal",1,3,0.03]
["Wind","Socal",1,4,0.03]
["Wind","Socal",1,5,0.03]
["Wind","Socal",1,6,0.03]
["Wind","Socal",1,7,0.03]
["Wind","Socal",1,8,0.03]
["Wind","Socal",1,9,0.02]
["Wind","Socal",1,10,0.02]
["Wind","Socal",1,11,0.02]
["Wind","Socal",1,12,0.02]
["Wind","Socal",1,13,0.02]
["Wind","Socal",1,14,0.02]
["Wind","Socal",1,15,0.02]
["Wind","Socal",1,16,0.02]
["Wind","Socal",1,17,0.02]
["Wind","Socal",1,18,0.02]
["Wind","Socal",1,19,0.03]
["Wind","Socal",1,20,0.03]
["Wind","Socal",1,21,0.03]
["Wind","Socal",1,22,0.03]
["Wind","Socal",1,23,0.03]
["Wind","Socal",1,24,0.03]
["Wind","Socal",2,1,0.04]
["Wind","Socal",2,2,0.04]
["Wind","Socal",2,3,0.05]
["Wind","Socal",2,4,0.05]
["Wind","Socal",2,5,0.05]
["Wind","Socal",2,6,0.04]
["Wind","Socal",2,7,0.04]
["Wind","Socal",2,8,0.04]
["Wind","Socal",2,9,0.03]
["Wind","Socal",2,10,0.03]
["Wind","Socal",2,11,0.03]
["Wind","Socal",2,12,0.03]
["Wind","Socal",2,13,0.04]
["Wind","Socal",2,14,0.05]
["Wind","Socal",2,15,0.05]
["Wind","Socal",2,16,0.06]
["Wind","Socal",2,17,0.06]
["Wind","Socal",2,18,0.05]
["Wind","Socal",2,19,0.05]
["Wind","Socal",2,20,0.06]
["Wind","Socal",2,21,0.06]
["Wind","Socal",2,22,0.06]
["Wind","Socal",2,23,0.06]
["Wind","Socal",2,24,0.06]
["Wind","Socal",3,1,0.08]
["Wind","Socal",3,2,0.08]
["Wind","Socal",3,3,7.0000000000000007E-2]
["Wind","Socal",3,4,7.0000000000000007E-2]
["Wind","Socal",3,5,0.06]
["Wind","Socal",3,6,0.06]
["Wind","Socal",3,7,0.05]
["Wind","Socal",3,8,0.05]
["Wind","Socal",3,9,0.04]
["Wind","Socal",3,10,0.04]
["Wind","Socal",3,11,0.04]
["Wind","Socal",3,12,0.05]
["Wind","Socal",3,13,0.05]
["Wind","Socal",3,14,0.05]
["Wind","Socal",3,15,0.04]
["Wind","Socal",3,16,0.06]
["Wind","Socal",3,17,0.08]
["Wind","Socal",3,18,0.1]
["Wind","Socal",3,19,0.09]
["Wind","Socal",3,20,0.1]
["Wind","Socal",3,21,0.1]
["Wind","Socal",3,22,0.09]
["Wind","Socal",3,23,0.09]
["Wind","Socal",3,24,0.08]
["Wind","Socal",4,1,0.33]
["Wind","Socal",4,2,0.32]
["Wind","Socal",4,3,0.3]
["Wind","Socal",4,4,0.27]
["Wind","Socal",4,5,0.23]
["Wind","Socal",4,6,0.2]
["Wind","Socal",4,7,0.17]
["Wind","Socal",4,8,0.12]
["Wind","Socal",4,9,0.09]
["Wind","Socal",4,10,0.09]
["Wind","Socal",4,11,0.09]
["Wind","Socal",4,12,0.08]
["Wind","Socal",4,13,0.09]
["Wind","Socal",4,14,0.1]
["Wind","Socal",4,15,0.14000000000000001]
["Wind","Socal",4,16,0.22]
["Wind","Socal",4,17,0.27]
["Wind","Socal",4,18,0.31]
["Wind","Socal",4,19,0.34]
["Wind","Socal",4,20,0.36]
["Wind","Socal",4,21,0.36]
["Wind","Socal",4,22,0.36]
["Wind","Socal",4,23,0.33]
["Wind","Socal",4,24,0.34]
["Wind","Socal",5,1,0.39]
["Wind","Socal",5,2,0.36]
["Wind","Socal",5,3,0.35]
["Wind","Socal",5,4,0.34]
["Wind","Socal",5,5,0.28000000000000003]
["Wind","Socal",5,6,0.22]
["Wind","Socal",5,7,0.19]
["Wind","Socal",5,8,0.11]
["Wind","Socal",5,9,7.0000000000000007E-2]
["Wind","Socal",5,10,0.05]
["Wind","Socal",5,11,0.05]
["Wind","Socal",5,12,0.05]
["Wind","Socal",5,13,0.04]
["Wind","Socal",5,14,0.05]
["Wind","Socal",5,15,0.09]
["Wind","Socal",5,16,0.17]
["Wind","Socal",5,17,0.28999999999999998]
["Wind","Socal",5,18,0.35]
["Wind","Socal",5,19,0.36]
["Wind","Socal",5,20,0.36]
["Wind","Socal",5,21,0.39]
["Wind","Socal",5,22,0.41]
["Wind","Socal",5,23,0.41]
["Wind","Socal",5,24,0.39]
["Wind","Socal",6,1,0.4]
["Wind","Socal",6,2,0.4]
["Wind","Socal",6,3,0.36]
["Wind","Socal",6,4,0.34]
["Wind","Socal",6,5,0.27]
["Wind","Socal",6,6,0.23]
["Wind","Socal",6,7,0.19]
["Wind","Socal",6,8,0.12]
["Wind","Socal",6,9,7.0000000000000007E-2]
["Wind","Socal",6,10,0.04]
["Wind","Socal",6,11,0.03]
["Wind","Socal",6,12,0.04]
["Wind","Socal",6,13,0.05]
["Wind","Socal",6,14,0.06]
["Wind","Socal",6,15,0.09]
["Wind","Socal",6,16,0.15]
["Wind","Socal",6,17,0.21]
["Wind","Socal",6,18,0.3]
["Wind","Socal",6,19,0.35]
["Wind","Socal",6,20,0.4]
["Wind","Socal",6,21,0.41]
["Wind","Socal",6,22,0.43]
["Wind","Socal",6,23,0.43]
["Wind","Socal",6,24,0.43]
["Wind","Socal",7,1,0.33]
["Wind","Socal",7,2,0.28999999999999998]
["Wind","Socal",7,3,0.28000000000000003]
["Wind","Socal",7,4,0.23]
["Wind","Socal",7,5,0.19]
["Wind","Socal",7,6,0.14000000000000001]
["Wind","Socal",7,7,0.1]
["Wind","Socal",7,8,7.0000000000000007E-2]
["Wind","Socal",7,9,0.03]
["Wind","Socal",7,10,0.02]
["Wind","Socal",7,11,0.02]
["Wind","Socal",7,12,0.02]
["Wind","Socal",7,13,0.03]
["Wind","Socal",7,14,0.05]
["Wind","Socal",7,15,7.0000000000000007E-2]
["Wind","Socal",7,16,0.12]
["Wind","Socal",7,17,0.2]
["Wind","Socal",7,18,0.25]
["Wind","Socal",7,19,0.28999999999999998]
["Wind","Socal",7,20,0.32]
["Wind","Socal",7,21,0.37]
["Wind","Socal",7,22,0.38]
["Wind","Socal",7,23,0.37]
["Wind","Socal",7,24,0.35]
["Wind","Socal",8,1,0.3]
["Wind","Socal",8,2,0.26]
["Wind","Socal",8,3,0.22]
["Wind","Socal",8,4,0.18]
["Wind","Socal",8,5,0.15]
["Wind","Socal",8,6,0.12]
["Wind","Socal",8,7,0.09]
["Wind","Socal",8,8,0.05]
["Wind","Socal",8,9,0.03]
["Wind","Socal",8,10,0.02]
["Wind","Socal",8,11,0.02]
["Wind","Socal",8,12,0.02]
["Wind","Socal",8,13,0.03]
["Wind","Socal",8,14,0.05]
["Wind","Socal",8,15,7.0000000000000007E-2]
["Wind","Socal",8,16,0.1]
["Wind","Socal",8,17,0.15]
["Wind","Socal",8,18,0.22]
["Wind","Socal",8,19,0.27]
["Wind","Socal",8,20,0.31]
["Wind","Socal",8,21,0.35]
["Wind","Socal",8,22,0.35]
["Wind","Socal",8,23,0.34]
["Wind","Socal",8,24,0.32]
["Wind","Socal",9,1,0.1]
["Wind","Socal",9,2,0.08]
["Wind","Socal",9,3,7.0000000000000007E-2]
["Wind","Socal",9,4,0.05]
["Wind","Socal",9,5,0.05]
["Wind","Socal",9,6,0.04]
["Wind","Socal",9,7,0.03]
["Wind","Socal",9,8,0.02]
["Wind","Socal",9,9,0.02]
["Wind","Socal",9,10,0.02]
["Wind","Socal",9,11,0.02]
["Wind","Socal",9,12,0.03]
["Wind","Socal",9,13,0.03]
["Wind","Socal",9,14,0.05]
["Wind","Socal",9,15,0.04]
["Wind","Socal",9,16,0.04]
["Wind","Socal",9,17,0.05]
["Wind","Socal",9,18,0.08]
["Wind","Socal",9,19,0.13]
["Wind","Socal",9,20,0.14000000000000001]
["Wind","Socal",9,21,0.14000000000000001]
["Wind","Socal",9,22,0.11]
["Wind","Socal",9,23,0.11]
["Wind","Socal",9,24,0.1]
["Wind","Socal",10,1,0.04]
["Wind","Socal",10,2,0.04]
["Wind","Socal",10,3,0.04]
["Wind","Socal",10,4,0.04]
["Wind","Socal",10,5,0.04]
["Wind","Socal",10,6,0.03]
["Wind","Socal",10,7,0.03]
["Wind","Socal",10,8,0.02]
["Wind","Socal",10,9,0.01]
["Wind","Socal",10,10,0.01]
["Wind","Socal",10,11,0.01]
["Wind","Socal",10,12,0.02]
["Wind","Socal",10,13,0.02]
["Wind","Socal",10,14,0.02]
["Wind","Socal",10,15,0.02]
["Wind","Socal",10,16,0.03]
["Wind","Socal",10,17,0.03]
["Wind","Socal",10,18,0.03]
["Wind","Socal",10,19,0.04]
["Wind","Socal",10,20,0.04]
["Wind","Socal",10,21,0.04]
["Wind","Socal",10,22,0.04]
["Wind","Socal",10,23,0.04]
["Wind","Socal",10,24,0.04]
["Wind","Socal",11,1,0.02]
["Wind","Socal",11,2,0.02]
["Wind","Socal",11,3,0.02]
["Wind","Socal",11,4,0.02]
["Wind","Socal",11,5,0.02]
["Wind","Socal",11,6,0.02]
["Wind","Socal",11,7,0.02]
["Wind","Socal",11,8,0.02]
["Wind","Socal",11,9,0.01]
["Wind","Socal",11,10,0.02]
["Wind","Socal",11,11,0.02]
["Wind","Socal",11,12,0.02]
["Wind","Socal",11,13,0.02]
["Wind","Socal",11,14,0.02]
["Wind","Socal",11,15,0.02]
["Wind","Socal",11,16,0.02]
["Wind","Socal",11,17,0.02]
["Wind","Socal",11,18,0.02]
["Wind","Socal",11,19,0.02]
["Wind","Socal",11,20,0.03]
["Wind","Socal",11,21,0.03]
["Wind","Socal",11,22,0.03]
["Wind","Socal",11,23,0.02]
["Wind","Socal",11,24,0.02]
["Wind","Socal",12,1,0.02]
["Wind","Socal",12,2,0.02]
["Wind","Socal",12,3,0.02]
["Wind","Socal",12,4,0.02]
["Wind","Socal",12,5,0.02]
["Wind","Socal",12,6,0.02]
["Wind","Socal",12,7,0.02]
["Wind","Socal",12,8,0.02]
["Wind","Socal",12,9,0.02]
["Wind","Socal",12,10,0.02]
["Wind","Socal",12,11,0.02]
["Wind","Socal",12,12,0.02]
["Wind","Socal",12,13,0.02]
["Wind","Socal",12,14,0.02]
["Wind","Socal",12,15,0.02]
["Wind","Socal",12,16,0.02]
["Wind","Socal",12,17,0.02]
["Wind","Socal",12,18,0.02]
["Wind","Socal",12,19,0.02]
["Wind","Socal",12,20,0.03]
["Wind","Socal",12,21,0.03]
["Wind","Socal",12,22,0.02]
["Wind","Socal",12,23,0.02]
["Wind","Socal",12,24,0.02]
["Battery Storage","Any",1,1,0]
["Battery Storage","Any",1,2,0]
["Battery Storage","Any",1,3,0]
["Battery Storage","Any",1,4,0]
["Battery Storage","Any",1,5,0]
["Battery Storage","Any",1,6,0]
["Battery Storage","Any",1,7,0]
["Battery Storage","Any",1,8,0]
["Battery Storage","Any",1,9,0]
["Battery Storage","Any",1,10,0]
["Battery Storage","Any",1,11,0]
["Battery Storage","Any",1,12,0]
["Battery Storage","Any",1,13,0]
["Battery Storage","Any",1,14,0]
["Battery Storage","Any",1,15,0]
["Battery Storage","Any",1,16,0]
["Battery Storage","Any",1,17,0]
["Battery Storage","Any",1,18,1]
["Battery Storage","Any",1,19,1]
["Battery Storage","Any",1,20,1]
["Battery Storage","Any",1,21,1]
["Battery Storage","Any",1,22,0]
["Battery Storage","Any",1,23,0]
["Battery Storage","Any",1,24,0]
["Battery Storage","Any",2,1,0]
["Battery Storage","Any",2,2,0]
["Battery Storage","Any",2,3,0]
["Battery Storage","Any",2,4,0]
["Battery Storage","Any",2,5,0]
["Battery Storage","Any",2,6,0]
["Battery Storage","Any",2,7,0]
["Battery Storage","Any",2,8,0]
["Battery Storage","Any",2,9,0]
["Battery Storage","Any",2,10,0]
["Battery Storage","Any",2,11,0]
["Battery Storage","Any",2,12,0]
["Battery Storage","Any",2,13,0]
["Battery Storage","Any",2,14,0]
["Battery Storage","Any",2,15,0]
["Battery Storage","Any",2,16,0]
["Battery Storage","Any",2,17,0]
["Battery Storage","Any",2,18,1]
["Battery Storage","Any",2,19,1]
["Battery Storage","Any",2,20,1]
["Battery Storage","Any",2,21,1]
["Battery Storage","Any",2,22,0]
["Battery Storage","Any",2,23,0]
["Battery Storage","Any",2,24,0]
["Battery Storage","Any",3,1,0]
["Battery Storage","Any",3,2,0]
["Battery Storage","Any",3,3,0]
["Battery Storage","Any",3,4,0]
["Battery Storage","Any",3,5,0]
["Battery Storage","Any",3,6,0]
["Battery Storage","Any",3,7,0]
["Battery Storage","Any",3,8,0]
["Battery Storage","Any",3,9,0]
["Battery Storage","Any",3,10,0]
["Battery Storage","Any",3,11,0]
["Battery Storage","Any",3,12,0]
["Battery Storage","Any",3,13,0]
["Battery Storage","Any",3,14,0]
["Battery Storage","Any",3,15,0]
["Battery Storage","Any",3,16,0]
["Battery Storage","Any",3,17,0]
["Battery Storage","Any",3,18,0]
["Battery Storage","Any",3,19,1]
["Battery Storage","Any",3,20,1]
["Battery Storage","Any",3,21,1]
["Battery Storage","Any",3,22,1]
["Battery Storage","Any",3,23,0]
["Battery Storage","Any",3,24,0]
["Battery Storage","Any",4,1,0]
["Battery Storage","Any",4,2,0]
["Battery Storage","Any",4,3,0]
["Battery Storage","Any",4,4,0]
["Battery Storage","Any",4,5,0]
["Battery Storage","Any",4,6,0]
["Battery Storage","Any",4,7,0]
["Battery Storage","Any",4,8,0]
["Battery Storage","Any",4,9,0]
["Battery Storage","Any",4,10,0]
["Battery Storage","Any",4,11,0]
["Battery Storage","Any",4,12,0]
["Battery Storage","Any",4,13,0]
["Battery Storage","Any",4,14,0]
["Battery Storage","Any",4,15,0]
["Battery Storage","Any",4,16,0]
["Battery Storage","Any",4,17,0]
["Battery Storage","Any",4,18,0]
["Battery Storage","Any",4,19,1]
["Battery Storage","Any",4,20,1]
["Battery Storage","Any",4,21,1]
["Battery Storage","Any",4,22,1]
["Battery Storage","Any",4,23,0]
["Battery Storage","Any",4,24,0]
["Battery Storage","Any",5,1,0]
["Battery Storage","Any",5,2,0]
["Battery Storage","Any",5,3,0]
["Battery Storage","Any",5,4,0]
["Battery Storage","Any",5,5,0]
["Battery Storage","Any",5,6,0]
["Battery Storage","Any",5,7,0]
["Battery Storage","Any",5,8,0]
["Battery Storage","Any",5,9,0]
["Battery Storage","Any",5,10,0]
["Battery Storage","Any",5,11,0]
["Battery Storage","Any",5,12,0]
["Battery Storage","Any",5,13,0]
["Battery Storage","Any",5,14,0]
["Battery Storage","Any",5,15,0]
["Battery Storage","Any",5,16,0]
["Battery Storage","Any",5,17,0]
["Battery Storage","Any",5,18,0]
["Battery Storage","Any",5,19,1]
["Battery Storage","Any",5,20,1]
["Battery Storage","Any",5,21,1]
["Battery Storage","Any",5,22,1]
["Battery Storage","Any",5,23,0]
["Battery Storage","Any",5,24,0]
["Battery Storage","Any",6,1,0]
["Battery Storage","Any",6,2,0]
["Battery Storage","Any",6,3,0]
["Battery Storage","Any",6,4,0]
["Battery Storage","Any",6,5,0]
["Battery Storage","Any",6,6,0]
["Battery Storage","Any",6,7,0]
["Battery Storage","Any",6,8,0]
["Battery Storage","Any",6,9,0]
["Battery Storage","Any",6,10,0]
["Battery Storage","Any",6,11,0]
["Battery Storage","Any",6,12,0]
["Battery Storage","Any",6,13,0]
["Battery Storage","Any",6,14,0]
["Battery Storage","Any",6,15,0]
["Battery Storage","Any",6,16,0]
["Battery Storage","Any",6,17,0]
["Battery Storage","Any",6,18,1]
["Battery Storage","Any",6,19,1]
["Battery Storage","Any",6,20,1]
["Battery Storage","Any",6,21,1]
["Battery Storage","Any",6,22,0]
["Battery Storage","Any",6,23,0]
["Battery Storage","Any",6,24,0]
["Battery Storage","Any",7,1,0]
["Battery Storage","Any",7,2,0]
["Battery Storage","Any",7,3,0]
["Battery Storage","Any",7,4,0]
["Battery Storage","Any",7,5,0]
["Battery Storage","Any",7,6,0]
["Battery Storage","Any",7,7,0]
["Battery Storage","Any",7,8,0]
["Battery Storage","Any",7,9,0]
["Battery Storage","Any",7,10,0]
["Battery Storage","Any",7,11,0]
["Battery Storage","Any",7,12,0]
["Battery Storage","Any",7,13,0]
["Battery Storage","Any",7,14,0]
["Battery Storage","Any",7,15,0]
["Battery Storage","Any",7,16,0]
["Battery Storage","Any",7,17,0]
["Battery Storage","Any",7,18,1]
["Battery Storage","Any",7,19,1]
["Battery Storage","Any",7,20,1]
["Battery Storage","Any",7,21,1]
["Battery Storage","Any",7,22,0]
["Battery Storage","Any",7,23,0]
["Battery Storage","Any",7,24,0]
["Battery Storage","Any",8,1,0]
["Battery Storage","Any",8,2,0]
["Battery Storage","Any",8,3,0]
["Battery Storage","Any",8,4,0]
["Battery Storage","Any",8,5,0]
["Battery Storage","Any",8,6,0]
["Battery Storage","Any",8,7,0]
["Battery Storage","Any",8,8,0]
["Battery Storage","Any",8,9,0]
["Battery Storage","Any",8,10,0]
["Battery Storage","Any",8,11,0]
["Battery Storage","Any",8,12,0]
["Battery Storage","Any",8,13,0]
["Battery Storage","Any",8,14,0]
["Battery Storage","Any",8,15,0]
["Battery Storage","Any",8,16,0]
["Battery Storage","Any",8,17,0]
["Battery Storage","Any",8,18,1]
["Battery Storage","Any",8,19,1]
["Battery Storage","Any",8,20,1]
["Battery Storage","Any",8,21,1]
["Battery Storage","Any",8,22,0]
["Battery Storage","Any",8,23,0]
["Battery Storage","Any",8,24,0]
["Battery Storage","Any",9,1,0]
["Battery Storage","Any",9,2,0]
["Battery Storage","Any",9,3,0]
["Battery Storage","Any",9,4,0]
["Battery Storage","Any",9,5,0]
["Battery Storage","Any",9,6,0]
["Battery Storage","Any",9,7,0]
["Battery Storage","Any",9,8,0]
["Battery Storage","Any",9,9,0]
["Battery Storage","Any",9,10,0]
["Battery Storage","Any",9,11,0]
["Battery Storage","Any",9,12,0]
["Battery Storage","Any",9,13,0]
["Battery Storage","Any",9,14,0]
["Battery Storage","Any",9,15,0]
["Battery Storage","Any",9,16,0]
["Battery Storage","Any",9,17,0]
["Battery Storage","Any",9,18,1]
["Battery Storage","Any",9,19,1]
["Battery Storage","Any",9,20,1]
["Battery Storage","Any",9,21,1]
["Battery Storage","Any",9,22,0]
["Battery Storage","Any",9,23,0]
["Battery Storage","Any",9,24,0]
["Battery Storage","Any",10,1,0]
["Battery Storage","Any",10,2,0]
["Battery Storage","Any",10,3,0]
["Battery Storage","Any",10,4,0]
["Battery Storage","Any",10,5,0]
["Battery Storage","Any",10,6,0]
["Battery Storage","Any",10,7,0]
["Battery Storage","Any",10,8,0]
["Battery Storage","Any",10,9,0]
["Battery Storage","Any",10,10,0]
["Battery Storage","Any",10,11,0]
["Battery Storage","Any",10,12,0]
["Battery Storage","Any",10,13,0]
["Battery Storage","Any",10,14,0]
["Battery Storage","Any",10,15,0]
["Battery Storage","Any",10,16,0]
["Battery Storage","Any",10,17,0]
["Battery Storage","Any",10,18,1]
["Battery Storage","Any",10,19,1]
["Battery Storage","Any",10,20,1]
["Battery Storage","Any",10,21,1]
["Battery Storage","Any",10,22,0]
["Battery Storage","Any",10,23,0]
["Battery Storage","Any",10,24,0]
["Battery Storage","Any",11,1,0]
["Battery Storage","Any",11,2,0]
["Battery Storage","Any",11,3,0]
["Battery Storage","Any",11,4,0]
["Battery Storage","Any",11,5,0]
["Battery Storage","Any",11,6,0]
["Battery Storage","Any",11,7,0]
["Battery Storage","Any",11,8,0]
["Battery Storage","Any",11,9,0]
["Battery Storage","Any",11,10,0]
["Battery Storage","Any",11,11,0]
["Battery Storage","Any",11,12,0]
["Battery Storage","Any",11,13,0]
["Battery Storage","Any",11,14,0]
["Battery Storage","Any",11,15,0]
["Battery Storage","Any",11,16,0]
["Battery Storage","Any",11,17,0]
["Battery Storage","Any",11,18,1]
["Battery Storage","Any",11,19,1]
["Battery Storage","Any",11,20,1]
["Battery Storage","Any",11,21,1]
["Battery Storage","Any",11,22,0]
["Battery Storage","Any",11,23,0]
["Battery Storage","Any",11,24,0]
["Battery Storage","Any",12,1,0]
["Battery Storage","Any",12,2,0]
["Battery Storage","Any",12,3,0]
["Battery Storage","Any",12,4,0]
["Battery Storage","Any",12,5,0]
["Battery Storage","Any",12,6,0]
["Battery Storage","Any",12,7,0]
["Battery Storage","Any",12,8,0]
["Battery Storage","Any",12,9,0]
["Battery Storage","Any",12,10,0]
["Battery Storage","Any",12,11,0]
["Battery Storage","Any",12,12,0]
["Battery Storage","Any",12,13,0]
["Battery Storage","Any",12,14,0]
["Battery Storage","Any",12,15,0]
["Battery Storage","Any",12,16,0]
["Battery Storage","Any",12,17,0]
["Battery Storage","Any",12,18,1]
["Battery Storage","Any",12,19,1]
["Battery Storage","Any",12,20,1]
["Battery Storage","Any",12,21,1]
["Battery Storage","Any",12,22,0]
["Battery Storage","Any",12,23,0]
["Battery Storage","Any",12,24,0]

{"sheet":"Resource Profile Categories","index":29,"n_rows":28,"n_cols":2,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Resource Type","Profile Category"]
["Battery Storage","Battery Storage"]
["Biogas","Other"]
["Biomass","Other"]
["CCGT","Other"]
["CHP","Other"]
["Coal","Other"]
["Fuel Cell","Other"]
["Geothermal","Other"]
["Hybrid_Solar1Axis","Solar Tracking"]
["Hybrid_SolarFixed","Solar Fixed"]
["Hybrid_Storage","Battery Storage"]
["Hydro","Other"]
["Nuclear","Other"]
["Paired_BattStorage","Battery Storage"]
["Paired_Solar_1Axis","Solar Tracking"]
["Paired_Solar_Fixed","Solar Fixed"]
["Paired_Solar_Thermal","Solar Thermal"]
["Peaker","Other"]
["Pump","Other"]
["Pumped Hydro","Other"]
["Reciprocating Engine","Other"]
["Solar_1Axis","Solar Tracking"]
["Solar_2Axis","Solar Tracking"]
["Solar_Fixed","Solar Fixed"]
["Solar_Thermal","Solar Thermal"]
["Steam Turbine","Other"]
["Wind","Wind"]

{"sheet":"Regions","index":30,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["Path 26 Designation","Balancing Authority Area","Region"]
["North","CISO","Norcal"]
["South","CISO","Socal"]
[null,"CISO"]
[null,"IID","Socal"]
[null,"SRP","AZ/NM"]
[null,"AZPS","AZ/NM"]
[null,"PNM","AZ/NM"]
[null,"WALC","AZ/NM"]
[null,"BPAT","WA/OR"]
[null,"LADWP","Socal"]